(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(aux_axis_origin 150.12875 80.773)
		(grid_origin 150.12875 80.773)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "VBUS")
	(net 2 "/TX")
	(net 3 "/RX")
	(net 4 "/MISO")
	(net 5 "/MOSI")
	(net 6 "/SCK")
	(net 7 "/A3")
	(net 8 "/A2")
	(net 9 "/A1")
	(net 10 "/A0")
	(net 11 "GND")
	(net 12 "+3.3V")
	(net 13 "/SDA")
	(net 14 "/SCL")
	(footprint "Xiao:Conn_01x_07_Xiao"
		(layer "F.Cu")
		(at 148.602731 80.773 180)
		(property "Reference" "J2"
			(at 0 -0.5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Xiao Right"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x07, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "xiao-qtpy.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at -1.269999 -7.619999 180)
			(size 3.938 1.778)
			(drill 1
				(offset 0.191 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/RX")
			(pinfunction "Pin_1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "1" thru_hole circle
			(at 0 -7.620001 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/RX")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -1.269999 -5.08 180)
			(size 3.938 1.778)
			(drill 1
				(offset 0.191 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/SCK")
			(pinfunction "Pin_2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole circle
			(at -0.000001 -5.08 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/SCK")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at -1.269999 -2.54 180)
			(size 3.938 1.778)
			(drill 1
				(offset 0.191 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/MISO")
			(pinfunction "Pin_3")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole circle
			(at -0.000001 -2.539999 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/MISO")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at -1.270001 0 180)
			(size 3.938 1.778)
			(drill 1
				(offset 0.191 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/MOSI")
			(pinfunction "Pin_4")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole circle
			(at 0 0 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/MOSI")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at -1.269999 2.540001 180)
			(size 3.938 1.778)
			(drill 1
				(offset 0.191 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "+3.3V")
			(pinfunction "Pin_5")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "5" thru_hole circle
			(at 0 2.539999 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "+3.3V")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at -1.269999 5.079999 180)
			(size 3.938 1.778)
			(drill 1
				(offset 0.191 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "6" thru_hole circle
			(at -0.000001 5.08 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at -1.269999 7.62 180)
			(size 3.938 1.778)
			(drill 1
				(offset 0.191 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VBUS")
			(pinfunction "Pin_7")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "7" thru_hole circle
			(at 0 7.62 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VBUS")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
	)
	(footprint "Xiao:JLC Minimum Mouse Bites"
		(layer "F.Cu")
		(at 144.02875 80.823)
		(property "Reference" "REF**"
			(at -2.8 -4 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "JLC Minimum Mouse Bites"
			(at -2.8 4.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 -0.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 -0.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 -0.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -2.8 5.7 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 -2.5)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -1.8)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -1.1)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -0.4)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0.3)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 1)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 1.7)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 2.4)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu" "*.Mask")
		)
	)
	(footprint "Xiao:Conn_01x_07_Xiao"
		(layer "F.Cu")
		(at 142.50875 80.773)
		(property "Reference" "J1"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Xiao Left"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x07, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "xiao-qtpy.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at -1.269999 -7.619999)
			(size 3.938 1.778)
			(drill 1
				(offset 0.191 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/A0")
			(pinfunction "Pin_1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "1" thru_hole circle
			(at 0 -7.620001)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/A0")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -1.269999 -5.08)
			(size 3.938 1.778)
			(drill 1
				(offset 0.191 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/A1")
			(pinfunction "Pin_2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole circle
			(at -0.000001 -5.08)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/A1")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at -1.269999 -2.54)
			(size 3.938 1.778)
			(drill 1
				(offset 0.191 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/A2")
			(pinfunction "Pin_3")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole circle
			(at -0.000001 -2.539999)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/A2")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at -1.270001 0)
			(size 3.938 1.778)
			(drill 1
				(offset 0.191 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/A3")
			(pinfunction "Pin_4")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole circle
			(at 0 0)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/A3")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at -1.269999 2.540001)
			(size 3.938 1.778)
			(drill 1
				(offset 0.191 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/SDA")
			(pinfunction "Pin_5")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "5" thru_hole circle
			(at 0 2.539999)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/SDA")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at -1.269999 5.079999)
			(size 3.938 1.778)
			(drill 1
				(offset 0.191 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/SCL")
			(pinfunction "Pin_6")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "6" thru_hole circle
			(at -0.000001 5.08)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/SCL")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at -1.269999 7.62)
			(size 3.938 1.778)
			(drill 1
				(offset 0.191 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/TX")
			(pinfunction "Pin_7")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "7" thru_hole circle
			(at 0 7.62)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/TX")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
	)
	(footprint "Xiao:JLC Minimum Mouse Bites"
		(layer "F.Cu")
		(at 147.082731 80.823)
		(property "Reference" "REF**"
			(at -2.8 -4 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "JLC Minimum Mouse Bites"
			(at -2.8 4.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 -0.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 -0.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 -0.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at 0 -2.5)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -1.8)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -1.1)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -0.4)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0.3)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 1)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 1.7)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 2.4)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu" "*.Mask")
		)
	)
	(gr_arc
		(start 143.77875 91.1235)
		(mid 141.982699 90.379551)
		(end 141.23875 88.5835)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 147.332731 83.273)
		(end 147.332731 91.1235)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 147.332731 70.4225)
		(mid 149.12875 71.166466)
		(end 149.872731 72.9625)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 149.872731 88.5835)
		(mid 149.128785 90.379569)
		(end 147.332731 91.1235)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 147.332731 83.273)
		(end 143.77875 83.273)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 141.23875 72.9625)
		(mid 141.982699 71.166449)
		(end 143.77875 70.4225)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 147.332731 78.273)
		(end 143.77875 78.273)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 149.872731 72.9625)
		(end 149.872731 88.5835)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.77875 83.273)
		(end 143.77875 91.1235)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 141.23875 88.5835)
		(end 141.23875 72.9625)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.77875 70.4225)
		(end 143.77875 78.273)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 147.332731 78.273)
		(end 147.332731 70.4225)
		(layer "Edge.Cuts")
	)
	(gr_text ""
		(at 214.56855 88.5327 0)
		(layer "F.SilkS")
	)
)