(kicad_pcb (version 4) (host pcbnew 4.0.5-e0-6337~49~ubuntu14.04.1)
  (general
    (links 173)
    (no_connects 0)
    (area 174 88.4 289.942501 153.000001)
    (thickness 1.6)
    (drawings 107)
    (tracks 645)
    (zones 0)
    (modules 73)
    (nets 60)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 0.35)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 25)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C4-Pad1)")
  (net 5 VUSB)
  (net 6 "Net-(C8-Pad1)")
  (net 7 "Net-(C9-Pad1)")
  (net 8 +5V)
  (net 9 "Net-(C12-Pad1)")
  (net 10 RESET)
  (net 11 "Net-(D3-Pad1)")
  (net 12 "Net-(D4-Pad1)")
  (net 13 "Net-(F1-Pad2)")
  (net 14 "Net-(L1-Pad2)")
  (net 15 "Net-(LED1-Pad1)")
  (net 16 NEOPIXEL)
  (net 17 "Net-(LED2-Pad1)")
  (net 18 "Net-(LED3-Pad1)")
  (net 19 "Net-(P1-Pad2)")
  (net 20 "Net-(P1-Pad3)")
  (net 21 "Net-(P1-Pad4)")
  (net 22 "Net-(P3-Pad1)")
  (net 23 "Net-(P3-Pad2)")
  (net 24 "Net-(P3-Pad3)")
  (net 25 "Net-(P3-Pad4)")
  (net 26 MISO)
  (net 27 SCK)
  (net 28 MOSI)
  (net 29 "Net-(P5-Pad2)")
  (net 30 "Net-(P5-Pad1)")
  (net 31 "Net-(P6-Pad2)")
  (net 32 "Net-(P6-Pad1)")
  (net 33 SERVO)
  (net 34 "Net-(R6-Pad2)")
  (net 35 "Net-(R7-Pad2)")
  (net 36 "Net-(R8-Pad2)")
  (net 37 BUTTON_A)
  (net 38 BUTTON_B)
  (net 39 FIN1)
  (net 40 RIN1)
  (net 41 SCL)
  (net 42 SDA)
  (net 43 FIN2)
  (net 44 RIN2)
  (net 45 JOYSTICK_X)
  (net 46 JOYSTICK_Y)
  (net 47 D-)
  (net 48 D+)
  (net 49 "Net-(U2-Pad21)")
  (net 50 "Net-(U2-Pad28)")
  (net 51 "Net-(U2-Pad12)")
  (net 52 "Net-(P3-Pad5)")
  (net 53 "Net-(U9-Pad2)")
  (net 54 "Net-(U9-Pad3)")
  (net 55 "Net-(D5-Pad1)")
  (net 56 "Net-(C13-Pad1)")
  (net 57 "Net-(F2-Pad2)")
  (net 58 "Net-(U1-Pad3)")
  (net 59 "Net-(U1-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net BUTTON_A)
    (add_net BUTTON_B)
    (add_net D+)
    (add_net D-)
    (add_net FIN1)
    (add_net FIN2)
    (add_net GND)
    (add_net JOYSTICK_X)
    (add_net JOYSTICK_Y)
    (add_net MISO)
    (add_net MOSI)
    (add_net NEOPIXEL)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(F2-Pad2)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(LED1-Pad1)")
    (add_net "Net-(LED2-Pad1)")
    (add_net "Net-(LED3-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P6-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U9-Pad2)")
    (add_net "Net-(U9-Pad3)")
    (add_net RESET)
    (add_net RIN1)
    (add_net RIN2)
    (add_net SCK)
    (add_net SCL)
    (add_net SDA)
    (add_net SERVO)
    (add_net VUSB)
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 591A3B52)
    (at 202 103.25 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at -2.9 -0.15 180) (layer F.SilkS) hide)
    (fp_text value RXLED (at 0 1.55 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D3-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 251.3 116.7 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C20 (at 0 1.25 180) (layer B.SilkS))
    (fp_text value 0u1 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 +5V))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 228.1 105.9 225)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 -1.45 225) (layer F.SilkS))
    (fp_text value R (at 0 1.55 225) (layer F.Fab))
    (fp_text user %R (at 0 0 225) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 225) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.1 0 225) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DM_Custom:XV_Custom_BD621 (layer F.Cu) (tedit 591A3ADF)
    (at 257.5 102.9 270)
    (fp_text reference U7 (at -1.6 2.4 360) (layer F.SilkS))
    (fp_text value BD6212HFP-TR (at -0.635 -8.255 270) (layer F.Fab))
    (pad 1 smd rect (at -3.81 5.6055 270) (size 0.73 1.835) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
    (pad 2 smd rect (at -2.54 5.6055 270) (size 0.73 1.835) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(P6-Pad1)"))
    (pad 3 smd rect (at -1.27 5.6055 270) (size 0.73 1.835) (layers F.Cu F.Paste F.Mask)
      (net 43 FIN2))
    (pad 4 smd rect (at 0 5.6055 270) (size 0.73 1.835) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.27 5.6055 270) (size 0.73 1.835) (layers F.Cu F.Paste F.Mask)
      (net 44 RIN2))
    (pad 6 smd rect (at 2.54 5.6055 270) (size 0.73 1.835) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(P6-Pad2)"))
    (pad 7 smd rect (at 3.81 5.6055 270) (size 0.73 1.835) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
    (pad 8 smd rect (at 0 -2 270) (size 7.49 6.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 217.7 113.2 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0 -1.7 180) (layer B.SilkS))
    (fp_text value 1u0 (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.25 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad_Footprints:ZF_CONN_USB-MICRO-B-SMD-holes (layer F.Cu) (tedit 5825EC80)
    (at 201.5 108.75 270)
    (fp_text reference P1 (at 0 5.75 270) (layer Cmts.User))
    (fp_text value USB_OTG (at 0 -6.2 270) (layer F.Fab) hide)
    (pad 6 thru_hole oval (at 3.375 0 270) (size 2 2) (drill 1.15) (layers *.Cu *.Mask)
      (net 14 "Net-(L1-Pad2)"))
    (pad 6 thru_hole oval (at -3.375 0 270) (size 2 2) (drill 1.15) (layers *.Cu *.Mask)
      (net 14 "Net-(L1-Pad2)"))
    (pad 1 smd rect (at -1.3 -2.7 270) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(F1-Pad2)"))
    (pad 2 smd rect (at -0.65 -2.7 270) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P1-Pad2)"))
    (pad 3 smd rect (at 0 -2.7 270) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(P1-Pad3)"))
    (pad 4 smd rect (at 0.65 -2.7 270) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(P1-Pad4)"))
    (pad 5 smd rect (at 1.3 -2.7 270) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 2.5 -2.7 270) (size 1.25 1.75) (drill 0.85) (layers *.Cu *.Mask)
      (net 14 "Net-(L1-Pad2)"))
    (pad 6 thru_hole oval (at -2.5 -2.7 270) (size 1.25 1.75) (drill 0.85) (layers *.Cu *.Mask)
      (net 14 "Net-(L1-Pad2)"))
    (pad 6 smd rect (at -2.5 0 270) (size 1.5 2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(L1-Pad2)"))
    (pad 6 smd rect (at 2.5 0 270) (size 1.5 2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(L1-Pad2)"))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 216.2 109 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -4.25 -0.05 360) (layer B.SilkS))
    (fp_text value C (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 1.25 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 VUSB))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 221 124 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 1.7 180) (layer F.SilkS))
    (fp_text value 22p (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 216.2 124 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 1.8 360) (layer F.SilkS))
    (fp_text value 22p (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 209 119.5 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.5 180) (layer B.SilkS))
    (fp_text value 0u1 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 209 118 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 1.25 180) (layer B.SilkS))
    (fp_text value 0u1 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer B.Cu) (tedit 0)
    (at 214.2 109 270)
    (attr smd)
    (fp_text reference C6 (at 1.75 2.2 360) (layer B.SilkS))
    (fp_text value CP (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 5 VUSB))
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 219.3 109.5)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 2.45 0) (layer B.SilkS))
    (fp_text value 0u1 (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 1.25) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 219.1 113.2 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at -4.05 1.15 360) (layer B.SilkS))
    (fp_text value 1u0 (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.25 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 0)
    (at 228.25 118.25 90)
    (attr smd)
    (fp_text reference C14 (at 3.35 -0.15 180) (layer F.SilkS))
    (fp_text value CP (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0 90) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
    (pad 2 smd rect (at 1.651 0 90) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 251.4 108.3 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C24 (at 0 -1.45 180) (layer B.SilkS))
    (fp_text value 0u1 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 +5V))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_1206 (layer F.Cu) (tedit 587F7EF9)
    (at 209 117 180)
    (descr "Diode SMD 1206, reflow soldering")
    (tags "Diode 1206")
    (attr smd)
    (fp_text reference D1 (at -0.1 -0.1 180) (layer F.SilkS))
    (fp_text value CD1206-S01575 (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 10 RESET))
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 591A3B3C)
    (at 202 114.25 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at -2.9 -0.05 180) (layer F.SilkS) hide)
    (fp_text value TXLED (at 0 1.55 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D4-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 591C49B0)
    (at 208.2 111 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L1 (at -0.05 -1.75 180) (layer B.SilkS))
    (fp_text value Ferrite_Bead (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 -1.75 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(L1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 221.9 113.25 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L2 (at 0 -1.85 360) (layer B.SilkS))
    (fp_text value MH2029-300Y (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 +5V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DM_Custom:SR_CUSTOM_NEO_PIX (layer F.Cu) (tedit 58C6BC28)
    (at 231.5 118.25 270)
    (fp_text reference LED1 (at 3.55 0 360) (layer F.SilkS))
    (fp_text value NeoPixel (at 0 -7.112 270) (layer F.Fab))
    (pad 1 smd rect (at -1.85 -0.875 270) (size 2 0.85) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(LED1-Pad1)"))
    (pad 2 smd rect (at -1.85 0.875 270) (size 2 0.85) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.85 0.875 270) (size 2 0.85) (layers F.Cu F.Paste F.Mask)
      (net 16 NEOPIXEL))
    (pad 4 smd rect (at 1.85 -0.875 270) (size 2 0.85) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
  )
  (module DM_Custom:SR_CUSTOM_NEO_PIX (layer F.Cu) (tedit 58C6BC28)
    (at 235.75 118.25 270)
    (fp_text reference LED2 (at 3.55 -0.05 360) (layer F.SilkS))
    (fp_text value NeoPixel (at 0 -7.112 270) (layer F.Fab))
    (pad 1 smd rect (at -1.85 -0.875 270) (size 2 0.85) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(LED2-Pad1)"))
    (pad 2 smd rect (at -1.85 0.875 270) (size 2 0.85) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.85 0.875 270) (size 2 0.85) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(LED1-Pad1)"))
    (pad 4 smd rect (at 1.85 -0.875 270) (size 2 0.85) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
  )
  (module DM_Custom:SR_CUSTOM_NEO_PIX (layer F.Cu) (tedit 58C6BC28)
    (at 240 118.25 270)
    (fp_text reference LED3 (at 0.35 -3.7 360) (layer F.SilkS))
    (fp_text value NeoPixel (at 0 -7.112 270) (layer F.Fab))
    (pad 1 smd rect (at -1.85 -0.875 270) (size 2 0.85) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(LED3-Pad1)"))
    (pad 2 smd rect (at -1.85 0.875 270) (size 2 0.85) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.85 0.875 270) (size 2 0.85) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(LED2-Pad1)"))
    (pad 4 smd rect (at 1.85 -0.875 270) (size 2 0.85) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 209 115 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 1.4 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 RESET))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 219.3 108.1)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -0.05 -1.35) (layer B.SilkS))
    (fp_text value R (at 0 -1.550001) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 218.6 120.6 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -3 -0.1 180) (layer F.SilkS))
    (fp_text value 1M (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 209 107.6)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 3.6 -0.5) (layer F.SilkS))
    (fp_text value 1k (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 209 111.8)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -2.5 -1.3) (layer F.SilkS))
    (fp_text value 1k (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 266.2 112.5)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 1.45) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 37 BUTTON_A))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 258.4 112.5)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0 1.45) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 38 BUTTON_B))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 251.4 121.1 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 39 FIN1))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 251.4 123.1 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at -4.1 -0.15 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 40 RIN1))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 251.4 101.9 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 43 FIN2))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 251.4 103.9 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 3.15 -0.1 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 44 RIN2))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 591C49F7)
    (at 208.2 106.8)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference RV1 (at -1.7 -1.3) (layer B.SilkS))
    (fp_text value Varistor (at 0 -1.55) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(P1-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 591C49F3)
    (at 208.2 108.2)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference RV2 (at -3.7 0.8) (layer B.SilkS))
    (fp_text value Varistor (at 0 -1.55) (layer B.Fab) hide)
    (fp_text user %R (at 0 0.05) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(P1-Pad3)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DM_Custom:XV_Custom_BD621 (layer F.Cu) (tedit 591A3AE8)
    (at 257.5 122.1 270)
    (fp_text reference U5 (at -1.6 2.4 360) (layer F.SilkS))
    (fp_text value BD6212HFP-TR (at 0 -8.255 270) (layer F.Fab))
    (pad 1 smd rect (at -3.81 5.6055 270) (size 0.73 1.835) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
    (pad 2 smd rect (at -2.54 5.6055 270) (size 0.73 1.835) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(P5-Pad1)"))
    (pad 3 smd rect (at -1.27 5.6055 270) (size 0.73 1.835) (layers F.Cu F.Paste F.Mask)
      (net 39 FIN1))
    (pad 4 smd rect (at 0 5.6055 270) (size 0.73 1.835) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.27 5.6055 270) (size 0.73 1.835) (layers F.Cu F.Paste F.Mask)
      (net 40 RIN1))
    (pad 6 smd rect (at 2.54 5.6055 270) (size 0.73 1.835) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(P5-Pad2)"))
    (pad 7 smd rect (at 3.81 5.6055 270) (size 0.73 1.835) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
    (pad 8 smd rect (at 0 -2 270) (size 7.49 6.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Crystals:Crystal_SMD_3225-4pin_3.2x2.5mm (layer F.Cu) (tedit 58CD2E9C)
    (at 218.6 124.2 90)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y1 (at 2.7 -2.7 180) (layer F.SilkS))
    (fp_text value 16M (at 0 2.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0.85 90) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.1 0.85 90) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 -0.85 90) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 4 smd rect (at -1.1 -0.85 90) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_3225-4pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad_Footprints:ZF_IC_TQFP44-0-8 (layer F.Cu) (tedit 591A3963)
    (at 219 112.5)
    (fp_text reference U2 (at 5.8 5.9) (layer F.SilkS))
    (fp_text value ATMEGA32U4-A (at 0 -11) (layer F.Fab))
    (pad 1 smd rect (at -6 -4) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(P3-Pad1)"))
    (pad 2 smd rect (at -6 -3.2) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
    (pad 3 smd rect (at -6 -2.4) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 47 D-))
    (pad 4 smd rect (at -6 -1.6) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 48 D+))
    (pad 5 smd rect (at -6 -0.8) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -6 0) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C8-Pad1)"))
    (pad 7 smd rect (at -6 0.8) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 VUSB))
    (pad 8 smd rect (at -6 1.6) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R6-Pad2)"))
    (pad 9 smd rect (at -6 2.4) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 27 SCK))
    (pad 10 smd rect (at -6 3.2) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 28 MOSI))
    (pad 11 smd rect (at -6 4) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 26 MISO))
    (pad 12 smd rect (at -4 6 90) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U2-Pad12)"))
    (pad 13 smd rect (at -3.2 6 90) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 RESET))
    (pad 14 smd rect (at -2.4 6 90) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
    (pad 15 smd rect (at -1.6 6 90) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -0.8 6 90) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 17 smd rect (at 0 6 90) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 18 smd rect (at 0.8 6 90) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 41 SCL))
    (pad 19 smd rect (at 1.6 6 90) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 42 SDA))
    (pad 20 smd rect (at 2.4 6 90) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 16 NEOPIXEL))
    (pad 21 smd rect (at 3.2 6 90) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U2-Pad21)"))
    (pad 22 smd rect (at 4 6 90) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R7-Pad2)"))
    (pad 23 smd rect (at 6 4) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 6 3.2) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C12-Pad1)"))
    (pad 25 smd rect (at 6 2.4) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 38 BUTTON_B))
    (pad 26 smd rect (at 6 1.6) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 37 BUTTON_A))
    (pad 27 smd rect (at 6 0.8) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 33 SERVO))
    (pad 28 smd rect (at 6 0) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U2-Pad28)"))
    (pad 29 smd rect (at 6 -0.8) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 40 RIN1))
    (pad 30 smd rect (at 6 -1.6) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 39 FIN1))
    (pad 31 smd rect (at 6 -2.4) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 44 RIN2))
    (pad 32 smd rect (at 6 -3.2) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 43 FIN2))
    (pad 33 smd rect (at 6 -4) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R8-Pad2)"))
    (pad 34 smd rect (at 4 -6 90) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
    (pad 35 smd rect (at 3.2 -6 90) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 2.4 -6 90) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 46 JOYSTICK_Y))
    (pad 37 smd rect (at 1.6 -6 90) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 45 JOYSTICK_X))
    (pad 38 smd rect (at 0.8 -6 90) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(P3-Pad5)"))
    (pad 39 smd rect (at 0 -6 90) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(P3-Pad4)"))
    (pad 40 smd rect (at -0.8 -6 90) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(P3-Pad3)"))
    (pad 41 smd rect (at -1.6 -6 90) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(P3-Pad2)"))
    (pad 42 smd rect (at -2.4 -6 90) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C9-Pad1)"))
    (pad 43 smd rect (at -3.2 -6 90) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 44 smd rect (at -4 -6 90) (size 1.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C12-Pad1)"))
  )
  (module KiCad_Footprints:ZF_LOGO_PHHS (layer F.Cu) (tedit 0)
    (at 239.7 114)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module KiCad_Footprints:ZF_CONN_3x2_noshroud (layer F.Cu) (tedit 5912556F)
    (at 203 119 90)
    (fp_text reference P4 (at 0 5.25 90) (layer F.SilkS) hide)
    (fp_text value CONN_02X03 (at 0 -6.75 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -2.54 1.27 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 MISO))
    (pad 2 thru_hole circle (at -2.54 -1.27 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 +5V))
    (pad 3 thru_hole circle (at 0 1.27 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 27 SCK))
    (pad 4 thru_hole circle (at 0 -1.27 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 28 MOSI))
    (pad 5 thru_hole circle (at 2.54 1.27 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 RESET))
    (pad 6 thru_hole circle (at 2.54 -1.27 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module KiCad_Footprints:ZF_SW_LS38 (layer F.Cu) (tedit 590B3697)
    (at 209 120 180)
    (fp_text reference SW1 (at 0 6.25 180) (layer F.SilkS) hide)
    (fp_text value SWITCH (at 0 -5.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1.75 -1 180) (size 1.4 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.75 1 180) (size 1.4 0.7) (layers F.Cu F.Paste F.Mask)
      (net 10 RESET))
    (pad 2 smd rect (at 1.75 1 180) (size 1.4 0.7) (layers F.Cu F.Paste F.Mask)
      (net 10 RESET))
    (pad 1 smd rect (at 1.75 -1 180) (size 1.4 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module KiCad_Footprints:ZF_SMD_NonPol_0603 (layer F.Cu) (tedit 572E229D)
    (at 209 109 180)
    (fp_text reference R13 (at 0 1.5 180) (layer Cmts.User))
    (fp_text value R (at 0 -4.7 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 0 180) (size 1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 47 D-))
    (pad 2 smd rect (at 1 0 180) (size 1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P1-Pad2)"))
  )
  (module KiCad_Footprints:ZF_SMD_NonPol_0603 (layer F.Cu) (tedit 572E229D)
    (at 209 110.5 180)
    (fp_text reference R14 (at 0 1.5 180) (layer Cmts.User))
    (fp_text value R (at 0 -4.7 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 0 180) (size 1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 48 D+))
    (pad 2 smd rect (at 1 0 180) (size 1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(P1-Pad3)"))
  )
  (module KiCad_Footprints:ZF_STRUCT_M3-hole (layer F.Cu) (tedit 56B8C9D2)
    (at 267.5 100)
    (fp_text reference REF** (at 0 4.2) (layer F.SilkS) hide)
    (fp_text value ZF_STRUCT_M3-hole (at 0 -3.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module KiCad_Footprints:ZF_STRUCT_M3-hole (layer F.Cu) (tedit 56B8C9D2)
    (at 267.5 125)
    (fp_text reference REF** (at 0 4.2) (layer F.SilkS) hide)
    (fp_text value ZF_STRUCT_M3-hole (at 0 -3.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module KiCad_Footprints:ZF_STRUCT_M3-hole (layer F.Cu) (tedit 56B8C9D2)
    (at 202.5 125)
    (fp_text reference REF** (at 0 4.2) (layer F.SilkS) hide)
    (fp_text value ZF_STRUCT_M3-hole (at 0 -3.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module KiCad_Footprints:ZF_STRUCT_M3-hole (layer F.Cu) (tedit 56B8C9D2)
    (at 202.5 100)
    (fp_text reference REF** (at 0 4.2) (layer F.SilkS) hide)
    (fp_text value ZF_STRUCT_M3-hole (at 0 -3.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module KiCad_Footprints:ZF_SMD_pol_1206 (layer B.Cu) (tedit 591C4B36)
    (at 251.4 126 180)
    (fp_text reference C21 (at -4.35 0 180) (layer B.SilkS))
    (fp_text value 10u (at 0 3.6 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.3 0 180) (size 1.8 1.25) (layers B.Cu B.Paste B.Mask)
      (net 8 +5V))
    (pad 2 smd rect (at 1.3 0 180) (size 1.8 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module KiCad_Footprints:ZF_SMD_pol_1206 (layer B.Cu) (tedit 591C4B23)
    (at 251.4 106.7 180)
    (fp_text reference C25 (at 3.9 -0.05 180) (layer B.SilkS))
    (fp_text value 10u (at 0 3.6 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.3 0 180) (size 1.8 1.25) (layers B.Cu B.Paste B.Mask)
      (net 8 +5V))
    (pad 2 smd rect (at 1.3 0 180) (size 1.8 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module KiCad_Footprints:ZF_CONN_1x7-hdr locked (layer F.Cu) (tedit 59162724)
    (at 218.99 101.07)
    (fp_text reference P3 (at 0 5.08) (layer Cmts.User))
    (fp_text value CONN_01X07 (at 0 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at -7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(P3-Pad1)"))
    (pad 2 thru_hole circle (at -5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(P3-Pad2)"))
    (pad 3 thru_hole circle (at -2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(P3-Pad3)"))
    (pad 4 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(P3-Pad4)"))
    (pad 5 thru_hole circle (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(P3-Pad5)"))
    (pad 6 thru_hole circle (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 SCL))
    (pad 7 thru_hole circle (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 SDA))
  )
  (module KiCad_Footprints:ZF_SW_Metal_Ball_Tactile (layer F.Cu) (tedit 591A3AD7)
    (at 266.2 112.5 90)
    (fp_text reference SW2 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value SWITCH (at 0 -6.35 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.7 -2.5 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 BUTTON_A))
    (pad 2 thru_hole circle (at 3.7 -2.5 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 +5V))
    (pad 3 thru_hole circle (at 3.7 2.5 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -3.7 2.5 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  )
  (module KiCad_Footprints:ZF_SW_Metal_Ball_Tactile (layer F.Cu) (tedit 591A3AD0)
    (at 258.4 112.5 90)
    (fp_text reference SW3 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value SWITCH (at 0 -6.35 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.7 -2.5 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 BUTTON_B))
    (pad 2 thru_hole circle (at 3.7 -2.5 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 +5V))
    (pad 3 thru_hole circle (at 3.7 2.5 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -3.7 2.5 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  )
  (module KiCad_Footprints:ZF_SMD_NonPol_0603 (layer B.Cu) (tedit 591C4B6A)
    (at 247 119.5 90)
    (fp_text reference C3 (at 4.25 0 180) (layer B.SilkS))
    (fp_text value 0u1 (at 0 4.7 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0 90) (size 1 1.2) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module KiCad_Footprints:ZF_SMD_NonPol_0603 (layer B.Cu) (tedit 591C4AF1)
    (at 237 101.1)
    (fp_text reference C10 (at -3 0.4) (layer B.SilkS))
    (fp_text value C (at 0 4.7) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0) (size 1 1.2) (layers B.Cu B.Paste B.Mask)
      (net 8 +5V))
    (pad 2 smd rect (at 1 0) (size 1 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module KiCad_Footprints:ZF_SMD_pol_1206 (layer B.Cu) (tedit 591C4B8B)
    (at 245.5 119.5 90)
    (fp_text reference C13 (at 5.75 0 180) (layer B.SilkS))
    (fp_text value CP (at 0 3.6 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.3 0 90) (size 1.8 1.25) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 1.3 0 90) (size 1.8 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module KiCad_Footprints:ZF_SMD_pol_1206 (layer B.Cu) (tedit 591C4C1F)
    (at 237 119.5 90)
    (fp_text reference C15 (at 6 -0.75 180) (layer B.SilkS))
    (fp_text value 10u (at 0 3.6 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.3 0 90) (size 1.8 1.25) (layers B.Cu B.Paste B.Mask)
      (net 8 +5V))
    (pad 2 smd rect (at 1.3 0 90) (size 1.8 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module KiCad_Footprints:ZF_SMD_pol_1206 (layer B.Cu) (tedit 591C4C15)
    (at 235 119.5 90)
    (fp_text reference C16 (at -3.25 0 180) (layer B.SilkS))
    (fp_text value CP (at 0 3.6 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.3 0 90) (size 1.8 1.25) (layers B.Cu B.Paste B.Mask)
      (net 8 +5V))
    (pad 2 smd rect (at 1.3 0 90) (size 1.8 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module KiCad_Footprints:ZF_SMD_pol_0805 (layer B.Cu) (tedit 591C4B5D)
    (at 248.5 119.5 90)
    (fp_text reference D2 (at 2.75 0 180) (layer B.SilkS))
    (fp_text value D (at 0 3.3 90) (layer B.Fab) hide)
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(C13-Pad1)"))
  )
  (module KiCad_Footprints:ZF_SMD_pol_0805 (layer F.Cu) (tedit 591C5E85)
    (at 234.9 124.7 90)
    (fp_text reference D5 (at -0.8 -1.9 180) (layer F.SilkS))
    (fp_text value LED (at 0 -3.3 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(D5-Pad1)"))
  )
  (module KiCad_Footprints:ZF_SMD_pol_0805 (layer B.Cu) (tedit 591C4C07)
    (at 233 119.5 90)
    (fp_text reference D6 (at 3 0 180) (layer B.SilkS))
    (fp_text value D (at 0 3.3 90) (layer B.Fab) hide)
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 VUSB))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 8 +5V))
  )
  (module KiCad_Footprints:ZF_SMD_NonPol_0603 (layer B.Cu) (tedit 591C4AE6)
    (at 237 99.4)
    (fp_text reference R1 (at -2.5 -0.4) (layer B.SilkS))
    (fp_text value R (at 0 4.7) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0) (size 1 1.2) (layers B.Cu B.Paste B.Mask)
      (net 8 +5V))
    (pad 2 smd rect (at 1 0) (size 1 1.2) (layers B.Cu B.Paste B.Mask)
      (net 41 SCL))
  )
  (module KiCad_Footprints:ZF_SMD_NonPol_0603 (layer B.Cu) (tedit 591C4B00)
    (at 237 102.8)
    (fp_text reference R2 (at 0 1.45) (layer B.SilkS))
    (fp_text value R (at 0 4.7) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0) (size 1 1.2) (layers B.Cu B.Paste B.Mask)
      (net 8 +5V))
    (pad 2 smd rect (at 1 0) (size 1 1.2) (layers B.Cu B.Paste B.Mask)
      (net 42 SDA))
  )
  (module KiCad_Footprints:ZF_SMD_NonPol_0603 (layer B.Cu) (tedit 591C4BF5)
    (at 234.9 126.2 180)
    (fp_text reference R19 (at 2.9 -0.05 180) (layer B.SilkS))
    (fp_text value R (at 0 4.7 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0 180) (size 1 1.2) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module KiCad_Footprints:ZF_IC_DFN8-050 (layer F.Cu) (tedit 591A20D3)
    (at 237 101.1 180)
    (fp_text reference U1 (at 0 5.75 180) (layer F.SilkS))
    (fp_text value SHT30-DIS-B (at 0 -6.25 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.75 180) (size 1.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 SDA))
    (pad 2 smd rect (at -1.5 -0.25 180) (size 1.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.5 0.25 180) (size 1.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -1.5 0.75 180) (size 1.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 SCL))
    (pad 5 smd rect (at 1.5 0.75 180) (size 1.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
    (pad 6 smd rect (at 1.5 0.25 180) (size 1.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at 1.5 -0.25 180) (size 1.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 1.5 -0.75 180) (size 1.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module KiCad_Footprints:ZF_CONN_POWER_1x2 (layer F.Cu) (tedit 591A3A65)
    (at 240.25 124)
    (fp_text reference P2 (at 0 6.35) (layer F.SilkS) hide)
    (fp_text value POWER_IN (at 0 -6.35) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -1.27 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.27 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(F2-Pad2)"))
  )
  (module KiCad_Footprints:ZF_CONN_POWER_1x2 (layer F.Cu) (tedit 591A3A98)
    (at 266.5 120 270)
    (fp_text reference P5 (at 0 6.35 270) (layer F.SilkS) hide)
    (fp_text value MOTOR_1 (at 0 -6.35 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -1.27 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(P5-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(P5-Pad2)"))
  )
  (module KiCad_Footprints:ZF_CONN_POWER_1x2 (layer F.Cu) (tedit 591A3A98)
    (at 266.5 105 270)
    (fp_text reference P6 (at 0 6.35 270) (layer F.SilkS) hide)
    (fp_text value MOTOR_2 (at 0 -6.35 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -1.27 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(P6-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(P6-Pad2)"))
  )
  (module KiCad_Footprints:ZF_JOYSTICK locked (layer F.Cu) (tedit 591C48C6)
    (at 219 112.5 90)
    (fp_text reference U9 (at 0 3.75 90) (layer F.SilkS) hide)
    (fp_text value joystick (at 0 -4.25 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -11.43 -12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 +5V))
    (pad 2 thru_hole circle (at -11.43 -10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(U9-Pad2)"))
    (pad 3 thru_hole circle (at -11.43 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(U9-Pad3)"))
    (pad 4 thru_hole circle (at -11.43 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 11.43 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 11.43 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 JOYSTICK_Y))
    (pad 7 thru_hole circle (at 11.43 -10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 JOYSTICK_X))
    (pad 8 thru_hole circle (at 11.43 -12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 +5V))
  )
  (module KiCad_Footprints:ZF_SMD_1812 (layer B.Cu) (tedit 591C4937)
    (at 211.6 104.3 180)
    (fp_text reference F1 (at 0 -2.3 180) (layer B.SilkS))
    (fp_text value Polyfuse (at 0 4.6 180) (layer B.Fab) hide)
    (pad 2 smd rect (at 1.6 0 180) (size 2 3.2) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(F1-Pad2)"))
    (pad 1 smd rect (at -1.6 0 180) (size 2 3.2) (layers B.Cu B.Paste B.Mask)
      (net 5 VUSB))
  )
  (module KiCad_Footprints:ZF_SMD_1812 (layer B.Cu) (tedit 591C4B4E)
    (at 245.8 124 180)
    (fp_text reference F2 (at 0.05 -2.5 180) (layer B.SilkS))
    (fp_text value Polyfuse (at 0 4.6 180) (layer B.Fab) hide)
    (pad 2 smd rect (at 1.6 0 180) (size 2 3.2) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(F2-Pad2)"))
    (pad 1 smd rect (at -1.6 0 180) (size 2 3.2) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(C13-Pad1)"))
  )
  (module KiCad_Footprints:ZF_SMD_DPAK (layer B.Cu) (tedit 591C4BC7)
    (at 241 116 180)
    (fp_text reference U4 (at 0 6.5 180) (layer B.SilkS))
    (fp_text value LF33CDT-TRY (at 0 6.5 180) (layer B.Fab))
    (pad 2 smd rect (at 0 2.6 180) (size 6.3 6.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.2 -3.9 180) (size 1.5 3) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(C13-Pad1)"))
    (pad 3 smd rect (at 2.2 -3.9 180) (size 1.5 3) (layers B.Cu B.Paste B.Mask)
      (net 8 +5V))
  )
  (module KiCad_Footprints:ZF_CONN_1x3_servo (layer F.Cu) (tedit 591C5DE2)
    (at 244.4 101.1)
    (fp_text reference P7 (at 0.1 1.9) (layer Cmts.User))
    (fp_text value SERVO_HEADER (at 0 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 33 SERVO))
    (pad 2 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 +5V))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (gr_text "Patriot\nCompanion" (at 243.25 105.75) (layer F.Mask))
  (gr_text "DE '17" (at 225.7 126.2) (layer F.SilkS))
  (gr_text A0 (at 229.25 99) (layer B.SilkS))
  (gr_text A1 (at 208.75 99) (layer B.SilkS))
  (gr_text PWM6 (at 244.5 99) (layer B.SilkS))
  (gr_text PWM5/13 (at 263.25 103.25 90) (layer B.SilkS))
  (gr_text PWM9/10 (at 263.25 121.5 90) (layer B.SilkS))
  (gr_text D4 (at 258.5 110.5 360) (layer B.SilkS))
  (gr_text D12 (at 266.25 110.5 360) (layer B.SilkS))
  (gr_text M0 (at 264.25 101.5) (layer F.SilkS))
  (gr_text M1 (at 264.25 123.5) (layer F.SilkS))
  (gr_text "PCBs sponsored \nby OSHpark!!" (at 226.75 112 270) (layer B.Cu))
  (gr_text TEMP/HUM (at 235 103.6) (layer F.SilkS))
  (gr_text "6-12\nVDC" (at 245.3 122.9) (layer F.SilkS))
  (gr_text ISP (at 205.9 119.1 270) (layer F.SilkS))
  (gr_text SW1 (at 212.8 120) (layer F.SilkS))
  (gr_text RV1 (at 205.9 112.5) (layer F.SilkS))
  (gr_text RV2 (at 209 106.2) (layer F.SilkS))
  (gr_text RX (at 205 103.4) (layer F.SilkS))
  (gr_text TX (at 205 114.3) (layer F.SilkS))
  (gr_text - (at 236.6 125.9) (layer F.SilkS))
  (gr_text + (at 243.9 125.9) (layer F.SilkS))
  (gr_text SERVO (at 244.348 99.187) (layer F.SilkS))
  (gr_text D7 (at 211.455 99) (layer F.SilkS))
  (gr_text A5 (at 213.995 102.87) (layer F.SilkS))
  (gr_text A4 (at 216.408 99) (layer F.SilkS))
  (gr_text A3 (at 218.821 102.87) (layer F.SilkS))
  (gr_text A2 (at 221.5 99) (layer F.SilkS))
  (gr_text JX (at 208.661 102.997) (layer F.SilkS))
  (gr_text JY (at 229.235 102.997) (layer F.SilkS))
  (gr_text 5V (at 206.375 99) (layer F.SilkS))
  (gr_text SCL (at 224.028 102.87) (layer F.SilkS))
  (gr_text SDA (at 226.568 99) (layer F.SilkS))
  (gr_text GND (at 231.648 99) (layer F.SilkS))
  (dimension 30.000167 (width 0.3) (layer Cmts.User)
    (gr_text "30.000 mm" (at 283.442501 112.448358 270.1909852) (layer Cmts.User))
    (feature1 (pts (xy 268 127.5) (xy 284.842494 127.443858)))
    (feature2 (pts (xy 267.9 97.5) (xy 284.742494 97.443858)))
    (crossbar (pts (xy 282.042509 97.452858) (xy 282.142509 127.452858)))
    (arrow1a (pts (xy 282.142509 127.452858) (xy 281.552337 126.328315)))
    (arrow1b (pts (xy 282.142509 127.452858) (xy 282.725171 126.324406)))
    (arrow2a (pts (xy 282.042509 97.452858) (xy 281.459847 98.58131)))
    (arrow2b (pts (xy 282.042509 97.452858) (xy 282.632681 98.577401)))
  )
  (gr_line (start 200 100) (end 200 125) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 267.5 97.5) (end 202.5 97.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 270 125) (end 270 100) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 202.5 127.5) (end 267.5 127.5) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 267.5 100) (end 267.5 97.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 267.5 125) (end 270 125) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 202.5 125) (end 202.5 127.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 202.5 100) (end 200 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Patriot\nCompanion" (at 243.25 105.75) (layer F.Cu))
  (dimension 75 (width 0.3) (layer Cmts.User)
    (gr_text "75.000 mm" (at 237.5 141.35) (layer Cmts.User))
    (feature1 (pts (xy 275 130) (xy 275 142.7)))
    (feature2 (pts (xy 200 130) (xy 200 142.7)))
    (crossbar (pts (xy 200 140) (xy 275 140)))
    (arrow1a (pts (xy 275 140) (xy 273.873496 140.586421)))
    (arrow1b (pts (xy 275 140) (xy 273.873496 139.413579)))
    (arrow2a (pts (xy 200 140) (xy 201.126504 140.586421)))
    (arrow2b (pts (xy 200 140) (xy 201.126504 139.413579)))
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 221.9 127.4) (xy 221.9 117.6) (xy 215.4 117.6) (xy 215.4 127.3)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.3)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 193.4 92.6) (xy 280.2 88.4) (xy 283.4 153) (xy 174 139)
      )
    )
  )
)
