(kicad_pcb (version 20171130) (host pcbnew "(5.1.7)-1")
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 914)
    (zones 0)
    (modules 74)
    (nets 57)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2032)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.3556)
    (user_trace_width 0.381)
    (user_trace_width 0.4572)
    (user_trace_width 0.635)
    (user_trace_width 0.889)
    (user_trace_width 1.27)
    (trace_clearance 0.1778)
    (zone_clearance 0.635)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.635 0.3048)
    (user_via 0.889 0.508)
    (user_via 1.397 0.8128)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "/Harmonic Filters/F2_IN")
  (net 3 "/Harmonic Filters/F1_IN")
  (net 4 "/Harmonic Filters/F3_IN")
  (net 5 "/Harmonic Filters/F2_OUT")
  (net 6 "/Harmonic Filters/F1_OUT")
  (net 7 "/Harmonic Filters/F3_OUT")
  (net 8 "Net-(J1-Pad1)")
  (net 9 "Net-(J2-Pad11)")
  (net 10 "Net-(J2-Pad9)")
  (net 11 "Net-(J2-Pad7)")
  (net 12 "Net-(J2-Pad4)")
  (net 13 "Net-(J2-Pad3)")
  (net 14 "Net-(J2-Pad2)")
  (net 15 "Net-(J2-Pad1)")
  (net 16 "Net-(J7-Pad1)")
  (net 17 "Net-(J9-Pad1)")
  (net 18 "Net-(J11-Pad1)")
  (net 19 "Net-(U1-Pad23)")
  (net 20 +5.0V)
  (net 21 "Net-(C5-Pad2)")
  (net 22 "Net-(C5-Pad1)")
  (net 23 "Net-(C6-Pad2)")
  (net 24 "Net-(C6-Pad1)")
  (net 25 "Net-(C7-Pad1)")
  (net 26 "Net-(C8-Pad1)")
  (net 27 +3.3V)
  (net 28 "Net-(C13-Pad1)")
  (net 29 "Net-(C14-Pad1)")
  (net 30 "Net-(C15-Pad1)")
  (net 31 "Net-(C21-Pad1)")
  (net 32 "Net-(C22-Pad1)")
  (net 33 "Net-(C28-Pad1)")
  (net 34 "Net-(C29-Pad1)")
  (net 35 "Net-(J1-Pad11)")
  (net 36 "Net-(J1-Pad9)")
  (net 37 "Net-(J1-Pad7)")
  (net 38 "Net-(J1-Pad4)")
  (net 39 "Net-(J1-Pad3)")
  (net 40 "Net-(J1-Pad2)")
  (net 41 "Net-(J7-Pad11)")
  (net 42 "Net-(J7-Pad9)")
  (net 43 "Net-(J7-Pad7)")
  (net 44 "Net-(J7-Pad6)")
  (net 45 "Net-(J7-Pad4)")
  (net 46 "Net-(J7-Pad3)")
  (net 47 "Net-(J7-Pad2)")
  (net 48 "Net-(J12-Pad1)")
  (net 49 "Net-(J13-Pad1)")
  (net 50 "Net-(J14-Pad1)")
  (net 51 "Net-(J15-Pad1)")
  (net 52 "Net-(U2-Pad8)")
  (net 53 "Net-(U2-Pad23)")
  (net 54 "Net-(J16-Pad1)")
  (net 55 "Net-(C35-Pad2)")
  (net 56 "Net-(C35-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.2032)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3.3V)
    (add_net +5.0V)
    (add_net "/Harmonic Filters/F1_IN")
    (add_net "/Harmonic Filters/F1_OUT")
    (add_net "/Harmonic Filters/F2_IN")
    (add_net "/Harmonic Filters/F2_OUT")
    (add_net "/Harmonic Filters/F3_IN")
    (add_net "/Harmonic Filters/F3_OUT")
    (add_net GND)
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C28-Pad1)")
    (add_net "Net-(C29-Pad1)")
    (add_net "Net-(C35-Pad1)")
    (add_net "Net-(C35-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J12-Pad1)")
    (add_net "Net-(J13-Pad1)")
    (add_net "Net-(J14-Pad1)")
    (add_net "Net-(J15-Pad1)")
    (add_net "Net-(J16-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J7-Pad11)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(J7-Pad3)")
    (add_net "Net-(J7-Pad4)")
    (add_net "Net-(J7-Pad6)")
    (add_net "Net-(J7-Pad7)")
    (add_net "Net-(J7-Pad9)")
    (add_net "Net-(J9-Pad1)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U2-Pad23)")
    (add_net "Net-(U2-Pad8)")
  )
  (module t_logos:Thales_26x3_Cu (layer B.Cu) (tedit 0)
    (at 113.665 159.385 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 109.855 138.938)
    (descr "SMT capacitor, 0402")
    (fp_text reference C12 (at -2.032 0) (layer F.SilkS))
    (fp_text value 100pF (at 0 0.8636) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 +5.0V))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 109.855 137.795)
    (descr "SMT capacitor, 0402")
    (fp_text reference C11 (at -2.032 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 +5.0V))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 126.238 89.281 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference C4 (at -1.778 0 90) (layer F.SilkS))
    (fp_text value 100pF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 +5.0V))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 127.508 89.281 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference C3 (at -1.778 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 +5.0V))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 97.282 92.202 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C2 (at -1.651 0 90) (layer F.SilkS))
    (fp_text value 100pF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 +5.0V))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 98.425 92.202 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C1 (at -1.651 -0.127 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 +5.0V))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 134.874 71.755)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C35 (at 0 -1.1176) (layer F.SilkS))
    (fp_text value C_small (at 0 1.016) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C35-Pad2)"))
    (pad 1 smd rect (at 0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(C35-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_RF_conn:SMA_Edge_1 (layer F.Cu) (tedit 62165ADF)
    (at 83.82 167.005 90)
    (fp_text reference J17 (at -4.445 4.064) (layer F.SilkS))
    (fp_text value SMA_Edge (at 0.2 -1.3 90) (layer F.Fab))
    (pad 3 thru_hole rect (at 4.25 0 90) (size 1.4 5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole rect (at -4.25 0 90) (size 1.4 5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 90) (size 1.8 5) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(J16-Pad1)"))
    (model ${T_LIBS}/3d/t_RF_conn/32K145-400L5.stp
      (offset (xyz 0 0.4999999924907534 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module t_RF_conn:SMA_Edge_1 (layer F.Cu) (tedit 62165ADF)
    (at 140.97 167.005 270)
    (fp_text reference J16 (at -4.445 4.064) (layer F.SilkS))
    (fp_text value SMA_Edge (at 0.2 -1.3 90) (layer F.Fab))
    (pad 3 thru_hole rect (at 4.25 0 270) (size 1.4 5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole rect (at -4.25 0 270) (size 1.4 5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 270) (size 1.8 5) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(J16-Pad1)"))
    (model ${T_LIBS}/3d/t_RF_conn/32K145-400L5.stp
      (offset (xyz 0 0.4999999924907534 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module t_connectors:Banana_Horiz_Blk (layer F.Cu) (tedit 565486E4)
    (at 112.395 45.6946 90)
    (fp_text reference J10 (at -4.699 -3.429 90) (layer F.SilkS))
    (fp_text value BANANA_JACK_Black (at 0 -0.5 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 7.6454 0 90) (size 3.048 3.048) (drill 2.032) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -7.6454 0 90) (size 3.048 3.048) (drill 2.032) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ${T_LIBS}/3d/t_connectors/AB2_90DEG_4MM_JACK_PTH-BLK.wrl
      (offset (xyz -11.04899983406067 -4.825999927520752 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module t_connectors:Banana_Horiz_Yel (layer F.Cu) (tedit 56548771)
    (at 93.345 45.6946 90)
    (fp_text reference J8 (at -4.699 -3.429 90) (layer F.SilkS))
    (fp_text value BANANA_JACK_Yellow (at 0 -0.5 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 7.6454 0 90) (size 3.048 3.048) (drill 2.032) (layers *.Cu *.Mask F.SilkS)
      (net 27 +3.3V))
    (pad 2 thru_hole circle (at -7.6454 0 90) (size 3.048 3.048) (drill 2.032) (layers *.Cu *.Mask F.SilkS)
      (net 27 +3.3V))
    (model ${T_LIBS}/3d/t_connectors/AB2_90DEG_4MM_JACK_PTH-YEL.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_connectors:Banana_Horiz_Red (layer F.Cu) (tedit 56548724)
    (at 131.445 45.6946 90)
    (fp_text reference J6 (at -4.699 -3.429 90) (layer F.SilkS))
    (fp_text value BANANA_JACK_Red (at 0 -0.5 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 7.6454 0 90) (size 3.048 3.048) (drill 2.032) (layers *.Cu *.Mask F.SilkS)
      (net 20 +5.0V))
    (pad 2 thru_hole circle (at -7.6454 0 90) (size 3.048 3.048) (drill 2.032) (layers *.Cu *.Mask F.SilkS)
      (net 20 +5.0V))
    (model ${T_LIBS}/3d/t_connectors/AB2_90DEG_4MM_JACK_PTH-RED.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_RF_conn:SMA_Edge_1 (layer F.Cu) (tedit 62165ADF)
    (at 140.97 71.755 270)
    (fp_text reference J5 (at -4.445 4.064) (layer F.SilkS))
    (fp_text value SMA_Edge (at 0.2 -1.3 90) (layer F.Fab))
    (pad 3 thru_hole rect (at 4.25 0 270) (size 1.4 5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole rect (at -4.25 0 270) (size 1.4 5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 270) (size 1.8 5) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(C35-Pad1)"))
    (model ${T_LIBS}/3d/t_RF_conn/32K145-400L5.stp
      (offset (xyz 0 0.4999999924907534 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 114.681 137.795 180)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C13 (at 0 -1.1176) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.016) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0 180) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75 0 180) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C13-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 103.378 60.833 270)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C10 (at 0 -1.1176 90) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.016 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635 90) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 +3.3V))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 108.839 156.972 90)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C9 (at 0 -1.1176 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.016 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635 90) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 +3.3V))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 96.647 86.753 270)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C8 (at 0 -1.1176 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.016 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635 90) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C8-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 127.508 94.119 90)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C7 (at 0 -1.1176 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.016 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635 90) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C7-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 88.265 90.805 180)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C6 (at 0 -1.1176) (layer F.SilkS))
    (fp_text value C_small (at 0 1.016) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0 180) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C6-Pad2)"))
    (pad 1 smd rect (at 0.75 0 180) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C6-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 136.64 90.805 180)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C5 (at 0 -1.1176) (layer F.SilkS))
    (fp_text value C_small (at 0 1.016) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0 180) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C5-Pad2)"))
    (pad 1 smd rect (at 0.75 0 180) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C5-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 108.458 64.516 270)
    (descr "Through hole straight pin header, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x06 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_02x06_Odd_Even (at 1.27 15.03 90) (layer F.Fab))
    (fp_text user %R (at 1.27 6.35) (layer F.Fab))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 +3.3V))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J1-Pad11)"))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 +3.3V))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 +3.3V))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(C8-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 116.459 151.003 270)
    (descr "Through hole straight pin header, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x06 2.54mm double row")
    (fp_text reference J7 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_02x06_Odd_Even (at 1.27 15.03 90) (layer F.Fab))
    (fp_text user %R (at 1.27 6.35) (layer F.Fab))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 +3.3V))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J7-Pad11)"))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 +3.3V))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J7-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 +3.3V))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J7-Pad7)"))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J7-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(C13-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(J7-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J7-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(J7-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J7-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 129.921 64.643 270)
    (descr "Through hole straight pin header, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x06 2.54mm double row")
    (fp_text reference J2 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_02x06_Odd_Even (at 1.27 15.03 90) (layer F.Fab))
    (fp_text user %R (at 1.27 6.35) (layer F.Fab))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 +3.3V))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad11)"))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 +3.3V))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 +3.3V))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad7)"))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(C7-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_RF_conn:SMA_Edge_1 (layer F.Cu) (tedit 62165ADF)
    (at 83.82 90.805 90)
    (fp_text reference J4 (at -4.445 4.064) (layer F.SilkS))
    (fp_text value SMA_Edge (at 0.2 -1.3 90) (layer F.Fab))
    (pad 3 thru_hole rect (at 4.25 0 90) (size 1.4 5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole rect (at -4.25 0 90) (size 1.4 5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 90) (size 1.8 5) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C6-Pad1)"))
    (model ${T_LIBS}/3d/t_RF_conn/32K145-400L5.stp
      (offset (xyz 0 0.4999999924907534 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module t_RF_conn:SMA_Edge_1 (layer F.Cu) (tedit 62165ADF)
    (at 83.82 147.955 90)
    (fp_text reference J15 (at -4.445 4.064) (layer F.SilkS))
    (fp_text value SMA_Edge (at 0.2 -1.3 90) (layer F.Fab))
    (pad 3 thru_hole rect (at 4.25 0 90) (size 1.4 5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole rect (at -4.25 0 90) (size 1.4 5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 90) (size 1.8 5) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(J15-Pad1)"))
    (model ${T_LIBS}/3d/t_RF_conn/32K145-400L5.stp
      (offset (xyz 0 0.4999999924907534 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module t_RF_conn:SMA_Edge_1 (layer F.Cu) (tedit 62165ADF)
    (at 140.97 128.905 270)
    (fp_text reference J14 (at -4.445 4.064) (layer F.SilkS))
    (fp_text value SMA_Edge (at 0.2 -1.3 90) (layer F.Fab))
    (pad 3 thru_hole rect (at 4.25 0 270) (size 1.4 5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole rect (at -4.25 0 270) (size 1.4 5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 270) (size 1.8 5) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(J14-Pad1)"))
    (model ${T_LIBS}/3d/t_RF_conn/32K145-400L5.stp
      (offset (xyz 0 0.4999999924907534 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module t_RF_conn:SMA_Edge_1 (layer F.Cu) (tedit 62165ADF)
    (at 140.97 147.955 270)
    (fp_text reference J13 (at -4.445 4.064) (layer F.SilkS))
    (fp_text value SMA_Edge (at 0.2 -1.3 90) (layer F.Fab))
    (pad 3 thru_hole rect (at 4.25 0 270) (size 1.4 5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole rect (at -4.25 0 270) (size 1.4 5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 270) (size 1.8 5) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(J13-Pad1)"))
    (model ${T_LIBS}/3d/t_RF_conn/32K145-400L5.stp
      (offset (xyz 0 0.4999999924907534 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module t_RF_conn:SMA_Edge_1 (layer F.Cu) (tedit 62165ADF)
    (at 83.82 128.905 90)
    (fp_text reference J11 (at -4.445 4.064) (layer F.SilkS))
    (fp_text value SMA_Edge (at 0.2 -1.3 90) (layer F.Fab))
    (pad 3 thru_hole rect (at 4.25 0 90) (size 1.4 5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole rect (at -4.25 0 90) (size 1.4 5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 90) (size 1.8 5) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J11-Pad1)"))
    (model ${T_LIBS}/3d/t_RF_conn/32K145-400L5.stp
      (offset (xyz 0 0.4999999924907534 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module t_RF_conn:SMA_Edge_1 (layer F.Cu) (tedit 62165ADF)
    (at 83.82 109.855 90)
    (fp_text reference J9 (at -4.445 4.064) (layer F.SilkS))
    (fp_text value SMA_Edge (at 0.2 -1.3 90) (layer F.Fab))
    (pad 3 thru_hole rect (at 4.25 0 90) (size 1.4 5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole rect (at -4.25 0 90) (size 1.4 5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 90) (size 1.8 5) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J9-Pad1)"))
    (model ${T_LIBS}/3d/t_RF_conn/32K145-400L5.stp
      (offset (xyz 0 0.4999999924907534 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module t_RF_conn:SMA_Edge_1 (layer F.Cu) (tedit 62165ADF)
    (at 140.97 109.855 270)
    (fp_text reference J12 (at -4.445 4.064) (layer F.SilkS))
    (fp_text value SMA_Edge (at 0.2 -1.3 90) (layer F.Fab))
    (pad 3 thru_hole rect (at 4.25 0 270) (size 1.4 5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole rect (at -4.25 0 270) (size 1.4 5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 270) (size 1.8 5) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(J12-Pad1)"))
    (model ${T_LIBS}/3d/t_RF_conn/32K145-400L5.stp
      (offset (xyz 0 0.4999999924907534 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module t_RF_conn:SMA_Edge_1 (layer F.Cu) (tedit 62165ADF)
    (at 140.97 90.805 270)
    (fp_text reference J3 (at -4.445 4.064) (layer F.SilkS))
    (fp_text value SMA_Edge (at 0.2 -1.3 90) (layer F.Fab))
    (pad 3 thru_hole rect (at 4.25 0 270) (size 1.4 5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole rect (at -4.25 0 270) (size 1.4 5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 270) (size 1.8 5) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C5-Pad2)"))
    (model ${T_LIBS}/3d/t_RF_conn/32K145-400L5.stp
      (offset (xyz 0 0.4999999924907534 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module t_qfn:QFN-32_5mm (layer F.Cu) (tedit 6216457C)
    (at 93.484 91.071 90)
    (descr "Plastic QFP, TI S-PVQFN-N32 0.5mm Pitch")
    (fp_text reference U2 (at 2.286 -4.318 270) (layer F.SilkS))
    (fp_text value PE42850 (at 0 3.49758 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd rect (at -2.5 1.74752 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U2-Pad8)") (solder_mask_margin 0.06858))
    (pad 7 smd rect (at -2.5 1.24968 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 6 smd rect (at -2.5 0.7493 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 5 smd rect (at -2.5 0.24892 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 15 smd rect (at 1.24968 2.5 90) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J1-Pad11)") (solder_mask_margin 0.06858))
    (pad 14 smd rect (at 0.7493 2.5 90) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J1-Pad9)") (solder_mask_margin 0.06858))
    (pad 4 smd rect (at -2.5 -0.24892 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 2 "/Harmonic Filters/F2_IN") (solder_mask_margin 0.06858))
    (pad 3 smd rect (at -2.5 -0.7493 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 2 smd rect (at -2.5 -1.24968 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 4 "/Harmonic Filters/F3_IN") (solder_mask_margin 0.06858))
    (pad 1 smd rect (at -2.5 -1.74752 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 32 smd rect (at -1.74752 -2.5 90) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 31 smd rect (at -1.24968 -2.5 90) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 30 smd rect (at -0.7493 -2.5 90) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 29 smd rect (at -0.24892 -2.5 90) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 28 smd rect (at 0.24892 -2.5 90) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C6-Pad2)") (solder_mask_margin 0.06858))
    (pad 27 smd rect (at 0.7493 -2.5 90) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 26 smd rect (at 1.24968 -2.5 90) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 25 smd rect (at 1.74752 -2.5 90) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 24 smd rect (at 2.5 -1.74752 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 23 smd rect (at 2.5 -1.24968 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U2-Pad23)") (solder_mask_margin 0.06858))
    (pad 33 smd rect (at 0.75 -0.75 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858) (solder_paste_margin -0.09906))
    (pad 33 smd rect (at -0.75 -0.75 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858) (solder_paste_margin -0.09906))
    (pad 33 smd rect (at -0.75 0.75 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858) (solder_paste_margin -0.09906))
    (pad 33 smd rect (at 0.75 0.75 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858) (solder_paste_margin -0.09906))
    (pad 9 smd rect (at -1.74752 2.5 90) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 22 smd rect (at 2.5 -0.7493 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 21 smd rect (at 2.5 -0.24892 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 3 "/Harmonic Filters/F1_IN") (solder_mask_margin 0.06858))
    (pad 20 smd rect (at 2.5 0.24892 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 19 smd rect (at 2.5 0.7493 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 18 smd rect (at 2.5 1.24968 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 17 smd rect (at 2.5 1.74752 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 16 smd rect (at 1.74752 2.5 90) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C8-Pad1)") (solder_mask_margin 0.06858))
    (pad 13 smd rect (at 0.24892 2.5 90) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J1-Pad7)") (solder_mask_margin 0.06858))
    (pad 12 smd rect (at -0.24892 2.5 90) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 20 +5.0V) (solder_mask_margin 0.06858))
    (pad 11 smd rect (at -0.7493 2.5 90) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 10 smd rect (at -1.24968 2.5 90) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (model ${T_LIBS}/3d/t_qfn/QFNS32_OPT2.stp
      (offset (xyz 0 0 0.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_qfn:QFN-32_5mm (layer F.Cu) (tedit 6216457C)
    (at 111.125 133.731)
    (descr "Plastic QFP, TI S-PVQFN-N32 0.5mm Pitch")
    (fp_text reference U3 (at 2.286 -4.318 180) (layer F.SilkS))
    (fp_text value PE42850 (at 0 3.49758) (layer F.SilkS))
    (fp_text user %R (at 0.451 0.234) (layer F.Fab))
    (pad 8 smd rect (at -2.5 1.74752) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(J15-Pad1)") (solder_mask_margin 0.06858))
    (pad 7 smd rect (at -2.5 1.24968) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 6 smd rect (at -2.5 0.7493) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 5 smd rect (at -2.5 0.24892) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 15 smd rect (at 1.24968 2.5) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J7-Pad11)") (solder_mask_margin 0.06858))
    (pad 14 smd rect (at 0.7493 2.5) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(J7-Pad9)") (solder_mask_margin 0.06858))
    (pad 4 smd rect (at -2.5 -0.24892) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J11-Pad1)") (solder_mask_margin 0.06858))
    (pad 3 smd rect (at -2.5 -0.7493) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 2 smd rect (at -2.5 -1.24968) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J9-Pad1)") (solder_mask_margin 0.06858))
    (pad 1 smd rect (at -2.5 -1.74752) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 32 smd rect (at -1.74752 -2.5) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 31 smd rect (at -1.24968 -2.5) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 30 smd rect (at -0.7493 -2.5) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 29 smd rect (at -0.24892 -2.5) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 28 smd rect (at 0.24892 -2.5) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(J12-Pad1)") (solder_mask_margin 0.06858))
    (pad 27 smd rect (at 0.7493 -2.5) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 26 smd rect (at 1.24968 -2.5) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 25 smd rect (at 1.74752 -2.5) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 24 smd rect (at 2.5 -1.74752) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 23 smd rect (at 2.5 -1.24968) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(J14-Pad1)") (solder_mask_margin 0.06858))
    (pad 33 smd rect (at 0.75 -0.75) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858) (solder_paste_margin -0.09906))
    (pad 33 smd rect (at -0.75 -0.75) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858) (solder_paste_margin -0.09906))
    (pad 33 smd rect (at -0.75 0.75) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858) (solder_paste_margin -0.09906))
    (pad 33 smd rect (at 0.75 0.75) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858) (solder_paste_margin -0.09906))
    (pad 9 smd rect (at -1.74752 2.5) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 22 smd rect (at 2.5 -0.7493) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 21 smd rect (at 2.5 -0.24892) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(J13-Pad1)") (solder_mask_margin 0.06858))
    (pad 20 smd rect (at 2.5 0.24892) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 19 smd rect (at 2.5 0.7493) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 18 smd rect (at 2.5 1.24968) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 17 smd rect (at 2.5 1.74752) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 16 smd rect (at 1.74752 2.5) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C13-Pad1)") (solder_mask_margin 0.06858))
    (pad 13 smd rect (at 0.24892 2.5) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J7-Pad7)") (solder_mask_margin 0.06858))
    (pad 12 smd rect (at -0.24892 2.5) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 20 +5.0V) (solder_mask_margin 0.06858))
    (pad 11 smd rect (at -0.7493 2.5) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 10 smd rect (at -1.24968 2.5) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (model ${T_LIBS}/3d/t_qfn/QFNS32_OPT2.stp
      (offset (xyz 0 0 0.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_qfn:QFN-32_5mm (layer F.Cu) (tedit 6216457C)
    (at 131.445 90.551 270)
    (descr "Plastic QFP, TI S-PVQFN-N32 0.5mm Pitch")
    (fp_text reference U1 (at 2.286 -4.318 270) (layer F.SilkS))
    (fp_text value PE42850 (at 0 3.49758 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd rect (at -2.5 1.74752 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C35-Pad2)") (solder_mask_margin 0.06858))
    (pad 7 smd rect (at -2.5 1.24968 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 6 smd rect (at -2.5 0.7493 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 5 smd rect (at -2.5 0.24892 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 15 smd rect (at 1.24968 2.5 270) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J2-Pad11)") (solder_mask_margin 0.06858))
    (pad 14 smd rect (at 0.7493 2.5 270) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad9)") (solder_mask_margin 0.06858))
    (pad 4 smd rect (at -2.5 -0.24892 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 5 "/Harmonic Filters/F2_OUT") (solder_mask_margin 0.06858))
    (pad 3 smd rect (at -2.5 -0.7493 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 2 smd rect (at -2.5 -1.24968 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 6 "/Harmonic Filters/F1_OUT") (solder_mask_margin 0.06858))
    (pad 1 smd rect (at -2.5 -1.74752 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 32 smd rect (at -1.74752 -2.5 270) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 31 smd rect (at -1.24968 -2.5 270) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 30 smd rect (at -0.7493 -2.5 270) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 29 smd rect (at -0.24892 -2.5 270) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 28 smd rect (at 0.24892 -2.5 270) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C5-Pad1)") (solder_mask_margin 0.06858))
    (pad 27 smd rect (at 0.7493 -2.5 270) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 26 smd rect (at 1.24968 -2.5 270) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 25 smd rect (at 1.74752 -2.5 270) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 24 smd rect (at 2.5 -1.74752 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 23 smd rect (at 2.5 -1.24968 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-Pad23)") (solder_mask_margin 0.06858))
    (pad 33 smd rect (at 0.75 -0.75 270) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858) (solder_paste_margin -0.09906))
    (pad 33 smd rect (at -0.75 -0.75 270) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858) (solder_paste_margin -0.09906))
    (pad 33 smd rect (at -0.75 0.75 270) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858) (solder_paste_margin -0.09906))
    (pad 33 smd rect (at 0.75 0.75 270) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858) (solder_paste_margin -0.09906))
    (pad 9 smd rect (at -1.74752 2.5 270) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 22 smd rect (at 2.5 -0.7493 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 21 smd rect (at 2.5 -0.24892 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 7 "/Harmonic Filters/F3_OUT") (solder_mask_margin 0.06858))
    (pad 20 smd rect (at 2.5 0.24892 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 19 smd rect (at 2.5 0.7493 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 18 smd rect (at 2.5 1.24968 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 17 smd rect (at 2.5 1.74752 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 16 smd rect (at 1.74752 2.5 270) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C7-Pad1)") (solder_mask_margin 0.06858))
    (pad 13 smd rect (at 0.24892 2.5 270) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J2-Pad7)") (solder_mask_margin 0.06858))
    (pad 12 smd rect (at -0.24892 2.5 270) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 20 +5.0V) (solder_mask_margin 0.06858))
    (pad 11 smd rect (at -0.7493 2.5 270) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (pad 10 smd rect (at -1.24968 2.5 270) (size 0.2794 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.06858))
    (model ${T_LIBS}/3d/t_qfn/QFNS32_OPT2.stp
      (offset (xyz 0 0 0.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0603 (layer F.Cu) (tedit 5BB76B6F)
    (at 95.758 60.795 270)
    (descr "SMT resistor, 0603")
    (fp_text reference R6 (at 0 -1.05 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 0.9652 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.381 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.8 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.8 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J1-Pad11)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0603 (layer F.Cu) (tedit 5BB76B6F)
    (at 98.298 60.795 270)
    (descr "SMT resistor, 0603")
    (fp_text reference R5 (at 0 -1.05 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 0.9652 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.381 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.8 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.8 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J1-Pad9)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0603 (layer F.Cu) (tedit 5BB76B6F)
    (at 100.838 60.795 270)
    (descr "SMT resistor, 0603")
    (fp_text reference R4 (at 0 -1.05 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 0.9652 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.381 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.8 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.8 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J1-Pad7)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0603 (layer F.Cu) (tedit 5BB76B6F)
    (at 108.966 147.574 270)
    (descr "SMT resistor, 0603")
    (fp_text reference R9 (at 0 -1.05 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 0.9652 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.381 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.8 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.8 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J7-Pad7)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0603 (layer F.Cu) (tedit 5BB76B6F)
    (at 106.299 147.612 270)
    (descr "SMT resistor, 0603")
    (fp_text reference R8 (at 0 -1.05 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 0.9652 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.381 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.8 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.8 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(J7-Pad9)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0603 (layer F.Cu) (tedit 5BB76B6F)
    (at 103.759 147.701 270)
    (descr "SMT resistor, 0603")
    (fp_text reference R7 (at 0 -1.05 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 0.9652 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.381 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.8 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.8 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J7-Pad11)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0603 (layer F.Cu) (tedit 5BB76B6F)
    (at 122.301 60.833 270)
    (descr "SMT resistor, 0603")
    (fp_text reference R3 (at 0 -1.05 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 0.9652 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.381 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.8 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.8 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J2-Pad7)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0603 (layer F.Cu) (tedit 5BB76B6F)
    (at 119.761 60.833 270)
    (descr "SMT resistor, 0603")
    (fp_text reference R2 (at 0 -1.05 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 0.9652 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.381 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.8 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.8 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad9)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0603 (layer F.Cu) (tedit 5BB76B6F)
    (at 117.221 60.833 270)
    (descr "SMT resistor, 0603")
    (fp_text reference R1 (at 0 -1.05 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 0.9652 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.381 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.8 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.8 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J2-Pad11)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_coilcraft:MiniSpring_1512SP (layer F.Cu) (tedit 62164F4D)
    (at 118.491 98.3615 270)
    (fp_text reference L9 (at -1.8415 -2.413 180) (layer F.SilkS))
    (fp_text value Ind4x (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 1.4605 -1.397 270) (size 1.27 3.302) (layers F.Cu F.Paste F.Mask)
      (net 7 "/Harmonic Filters/F3_OUT"))
    (pad 1 smd rect (at -1.4605 1.397 270) (size 1.27 3.302) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C29-Pad1)"))
    (model ${T_LIBS}/3d/t_coilcraft/Coilcraft-1512SP-XXX.STEP
      (offset (xyz -1.3716 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module t_coilcraft:MiniSpring_1512SP (layer F.Cu) (tedit 62164F4D)
    (at 119.5705 81.788)
    (fp_text reference L3 (at 3.1115 -2.413) (layer F.SilkS))
    (fp_text value Ind4x (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 1.4605 -1.397) (size 1.27 3.302) (layers F.Cu F.Paste F.Mask)
      (net 6 "/Harmonic Filters/F1_OUT"))
    (pad 1 smd rect (at -1.4605 1.397) (size 1.27 3.302) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C15-Pad1)"))
    (model ${T_LIBS}/3d/t_coilcraft/Coilcraft-1512SP-XXX.STEP
      (offset (xyz -1.3716 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module t_coilcraft:B09T (layer F.Cu) (tedit 62165172)
    (at 119.3292 90.297)
    (fp_text reference L6 (at 1.3208 -3.048) (layer F.SilkS))
    (fp_text value Ind4x (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 2.9972 -1.397) (size 1.27 3.302) (layers F.Cu F.Paste F.Mask)
      (net 5 "/Harmonic Filters/F2_OUT"))
    (pad 1 smd rect (at -2.9972 1.397) (size 1.27 3.302) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C22-Pad1)"))
    (model ${T_LIBS}/3d/t_coilcraft/Coilcraft-B09T.STEP
      (offset (xyz -2.870200000000001 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module t_coilcraft:MiniSpring_1512SP (layer F.Cu) (tedit 62164F4D)
    (at 110.49 98.8695 270)
    (fp_text reference L8 (at -2.9845 0.635 180) (layer F.SilkS))
    (fp_text value Ind4x (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 1.4605 -1.397 270) (size 1.27 3.302) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C29-Pad1)"))
    (pad 1 smd rect (at -1.4605 1.397 270) (size 1.27 3.302) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C28-Pad1)"))
    (model ${T_LIBS}/3d/t_coilcraft/Coilcraft-1512SP-XXX.STEP
      (offset (xyz -1.3716 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module t_coilcraft:MiniSpring_1512SP (layer F.Cu) (tedit 62164F4D)
    (at 113.665 80.772 270)
    (fp_text reference L2 (at -2.159 -1.397 180) (layer F.SilkS))
    (fp_text value Ind4x (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 1.4605 -1.397 270) (size 1.27 3.302) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C15-Pad1)"))
    (pad 1 smd rect (at -1.4605 1.397 270) (size 1.27 3.302) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C14-Pad1)"))
    (model ${T_LIBS}/3d/t_coilcraft/Coilcraft-1512SP-XXX.STEP
      (offset (xyz -1.3716 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module t_coilcraft:MiniSpring_1512SP (layer F.Cu) (tedit 62164F4D)
    (at 112.268 89.916 270)
    (fp_text reference L5 (at 3.048 -0.635 180) (layer F.SilkS))
    (fp_text value Ind4x (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 1.4605 -1.397 270) (size 1.27 3.302) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C22-Pad1)"))
    (pad 1 smd rect (at -1.4605 1.397 270) (size 1.27 3.302) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C21-Pad1)"))
    (model ${T_LIBS}/3d/t_coilcraft/Coilcraft-1512SP-XXX.STEP
      (offset (xyz -1.3716 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module t_coilcraft:MiniSpring_1512SP (layer F.Cu) (tedit 62164F4D)
    (at 104.648 99.949)
    (fp_text reference L7 (at -3.048 -1.016) (layer F.SilkS))
    (fp_text value Ind4x (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 1.4605 -1.397) (size 1.27 3.302) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C28-Pad1)"))
    (pad 1 smd rect (at -1.4605 1.397) (size 1.27 3.302) (layers F.Cu F.Paste F.Mask)
      (net 4 "/Harmonic Filters/F3_IN"))
    (model ${T_LIBS}/3d/t_coilcraft/Coilcraft-1512SP-XXX.STEP
      (offset (xyz -1.3716 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module t_coilcraft:MiniSpring_2712 (layer F.Cu) (tedit 62164A17)
    (at 105.664 81.534)
    (fp_text reference L1 (at -1.016 2.667) (layer F.SilkS))
    (fp_text value Ind4x (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 2.9845 -1.397) (size 1.27 3.302) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C14-Pad1)"))
    (pad 1 smd rect (at -2.9845 1.397) (size 1.27 3.302) (layers F.Cu F.Paste F.Mask)
      (net 3 "/Harmonic Filters/F1_IN"))
    (model ${T_LIBS}/3d/t_coilcraft/Coilcraft-2712SP-121_4.STEP
      (offset (xyz -3 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module t_coilcraft:MiniSpring_2712 (layer F.Cu) (tedit 62164A17)
    (at 105.2195 90.805)
    (fp_text reference L4 (at -4.826 -1.016) (layer F.SilkS))
    (fp_text value Ind4x (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 2.9845 -1.397) (size 1.27 3.302) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C21-Pad1)"))
    (pad 1 smd rect (at -2.9845 1.397) (size 1.27 3.302) (layers F.Cu F.Paste F.Mask)
      (net 2 "/Harmonic Filters/F2_IN"))
    (model ${T_LIBS}/3d/t_coilcraft/Coilcraft-2712SP-121_4.STEP
      (offset (xyz -3 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 118.745 101.854)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C34 (at 2.413 0.127) (layer F.SilkS))
    (fp_text value C_small (at 0 1.016) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "/Harmonic Filters/F3_OUT"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 121.031 83.959 90)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C20 (at -0.115 1.651 180) (layer F.SilkS))
    (fp_text value C_small (at 0 1.016 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635 90) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "/Harmonic Filters/F1_OUT"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 122.428 93.103 90)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C27 (at -1.893 -0.254 180) (layer F.SilkS))
    (fp_text value C_small (at 0 1.016 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635 90) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "/Harmonic Filters/F2_OUT"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 115.951 99.568 270)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C30 (at 1.778 0.381 180) (layer F.SilkS))
    (fp_text value C_small (at 0 1.016 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635 90) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C29-Pad1)"))
    (pad 1 smd rect (at 0.75 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "/Harmonic Filters/F3_OUT"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0805 (layer F.Cu) (tedit 5CF041DB)
    (at 118.049 79.248)
    (descr "SMT capacitor, 0805")
    (attr smd)
    (fp_text reference C16 (at 0 -1.397) (layer F.SilkS))
    (fp_text value C_small (at 0 1.3462) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1 0) (layer F.Fab))
    (pad 2 smd rect (at -0.95 0) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C15-Pad1)"))
    (pad 1 smd rect (at 0.95 0) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "/Harmonic Filters/F1_OUT"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0805.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 119.253 92.964)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C23 (at -0.127 1.27) (layer F.SilkS))
    (fp_text value C_small (at 0 1.016) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C22-Pad1)"))
    (pad 1 smd rect (at 0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "/Harmonic Filters/F2_OUT"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 110.871 101.981)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C33 (at 2.286 0.127) (layer F.SilkS))
    (fp_text value C_small (at 0 1.016) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C29-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 115.443 84.201)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C19 (at -2.286 0) (layer F.SilkS))
    (fp_text value C_small (at 0 1.016) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C15-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 116.205 88.011)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C26 (at 2.286 -0.254) (layer F.SilkS))
    (fp_text value C_small (at 0 1.016) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C22-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0805 (layer F.Cu) (tedit 5CF041DB)
    (at 113.792 97.724 270)
    (descr "SMT capacitor, 0805")
    (attr smd)
    (fp_text reference C29 (at 2.347 0 180) (layer F.SilkS))
    (fp_text value C_small (at 0 1.3462 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.95 0 270) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C28-Pad1)"))
    (pad 1 smd rect (at 0.95 0 270) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C29-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0805.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 110.49 81.673 270)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C15 (at 0 -1.1176 90) (layer F.SilkS))
    (fp_text value C_small (at 0 1.016 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635 90) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C14-Pad1)"))
    (pad 1 smd rect (at 0.75 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C15-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0805 (layer F.Cu) (tedit 5CF041DB)
    (at 109.855 91.379 270)
    (descr "SMT capacitor, 0805")
    (attr smd)
    (fp_text reference C22 (at 2.22 0 180) (layer F.SilkS))
    (fp_text value C_small (at 0 1.3462 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.95 0 270) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C21-Pad1)"))
    (pad 1 smd rect (at 0.95 0 270) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C22-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0805.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 108.077 99.949 90)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C32 (at -1.778 0 180) (layer F.SilkS))
    (fp_text value C_small (at 0 1.016 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635 90) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C28-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 106.311 78.867)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C18 (at 0 -1.1176) (layer F.SilkS))
    (fp_text value C_small (at 0 1.016) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C14-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 107.188 93.218)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C25 (at -2.413 0) (layer F.SilkS))
    (fp_text value C_small (at 0 1.016) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0.0635) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C21-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 103.886 97.409)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C28 (at 0 -1.1176) (layer F.SilkS))
    (fp_text value C_small (at 0 1.016) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "/Harmonic Filters/F3_IN"))
    (pad 1 smd rect (at 0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C28-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 107.835 84.074)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C14 (at 2.274 0) (layer F.SilkS))
    (fp_text value C_small (at 0 1.016) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "/Harmonic Filters/F1_IN"))
    (pad 1 smd rect (at 0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C14-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 105.422 88.138)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C21 (at 0 -1.1176) (layer F.SilkS))
    (fp_text value C_small (at 0 1.016) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "/Harmonic Filters/F2_IN"))
    (pad 1 smd rect (at 0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C21-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 105.676 102.362 180)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C31 (at -2.274 -0.508) (layer F.SilkS))
    (fp_text value C_small (at 0 1.016) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0 180) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75 0 180) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "/Harmonic Filters/F3_IN"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 103.124 78.867 180)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C17 (at 2.286 0) (layer F.SilkS))
    (fp_text value C_small (at 0 1.016) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0 180) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75 0 180) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "/Harmonic Filters/F1_IN"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 102.616 88.138)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C24 (at 0 -1.1176) (layer F.SilkS))
    (fp_text value C_small (at 0 1.016) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "/Harmonic Filters/F2_IN"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 139.7 (width 0.15) (layer Dwgs.User)
    (gr_text "5.5000 in" (at 63.47 104.775 90) (layer Dwgs.User))
    (feature1 (pts (xy 80.645 34.925) (xy 64.183579 34.925)))
    (feature2 (pts (xy 80.645 174.625) (xy 64.183579 174.625)))
    (crossbar (pts (xy 64.77 174.625) (xy 64.77 34.925)))
    (arrow1a (pts (xy 64.77 34.925) (xy 65.356421 36.051504)))
    (arrow1b (pts (xy 64.77 34.925) (xy 64.183579 36.051504)))
    (arrow2a (pts (xy 64.77 174.625) (xy 65.356421 173.498496)))
    (arrow2b (pts (xy 64.77 174.625) (xy 64.183579 173.498496)))
  )
  (dimension 63.5 (width 0.15) (layer Dwgs.User)
    (gr_text "2.5000 in" (at 112.395 181.64) (layer Dwgs.User))
    (feature1 (pts (xy 144.145 174.625) (xy 144.145 180.926421)))
    (feature2 (pts (xy 80.645 174.625) (xy 80.645 180.926421)))
    (crossbar (pts (xy 80.645 180.34) (xy 144.145 180.34)))
    (arrow1a (pts (xy 144.145 180.34) (xy 143.018496 180.926421)))
    (arrow1b (pts (xy 144.145 180.34) (xy 143.018496 179.753579)))
    (arrow2a (pts (xy 80.645 180.34) (xy 81.771504 180.926421)))
    (arrow2b (pts (xy 80.645 180.34) (xy 81.771504 179.753579)))
  )
  (gr_line (start 80.645 174.625) (end 80.645 34.925) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 144.145 174.625) (end 80.645 174.625) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 144.145 34.925) (end 144.145 174.625) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 80.645 34.925) (end 144.145 34.925) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 20)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.51 173.99) (xy 81.28 173.99) (xy 81.28 35.56) (xy 143.51 35.56)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (priority 20)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.51 173.99) (xy 81.28 173.99) (xy 81.28 35.56) (xy 143.51 35.56)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (priority 20)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.51 173.99) (xy 81.28 173.99) (xy 81.28 35.56) (xy 143.51 35.56)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 20)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.51 173.929909) (xy 81.28 173.929909) (xy 81.28 35.499909) (xy 143.51 35.499909)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.985 93.218) (xy 128.651 93.218) (xy 128.651 87.757) (xy 133.985 87.757)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.139 93.853) (xy 90.805 93.853) (xy 90.805 88.392) (xy 96.139 88.392)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.792 136.398) (xy 108.458 136.398) (xy 108.458 130.937) (xy 113.792 130.937)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.396 83.82) (xy 102.108 83.82) (xy 101.981 78.359) (xy 120.269 78.359)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.6025 93.0275) (xy 102.341412 92.964) (xy 102.214412 87.503) (xy 114.173 87.503) (xy 114.173 88.265)
        (xy 115.824 88.265) (xy 115.824 87.503) (xy 121.539 87.503)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.376095 101.380999) (xy 102.997 101.317499) (xy 102.988007 95.856499) (xy 122.312595 95.856499)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.635))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.635 161.925) (xy 99.695 161.925) (xy 99.695 156.845) (xy 127.635 156.845)
      )
    )
  )
)
