(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 2)
    (no_connects 0)
    (area 135.199999 77.449999 142.800001 105.050001)
    (thickness 1.6)
    (drawings 9)
    (tracks 54)
    (zones 0)
    (modules 3)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.02548)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.9304 15)
    (pad_drill 0)
    (pad_to_mask_clearance 0.1)
    (solder_mask_min_width 0.05)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010c0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../../../../../../../1/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(U23-Pad1)")
  (net 3 "Net-(U24-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(U23-Pad1)")
    (add_net "Net-(U24-Pad3)")
  )
  (module aruj:smb3 (layer F.Cu) (tedit 5AC4BDE9)
    (at 139 80)
    (fp_text reference U23 (at -27.25 9) (layer F.SilkS) hide)
    (fp_text value smb3 (at -44.25 0) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1.9304 5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U23-Pad1)"))
  )
  (module aruj:Via.16 (layer F.Cu) (tedit 5A912C1B)
    (at 139 109)
    (fp_text reference U24 (at 0 8.89) (layer F.SilkS) hide)
    (fp_text value AEMIF-0805 (at 22.2 -28) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -24.5) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U23-Pad1)"))
    (pad 3 smd rect (at 0 -22.1) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U24-Pad3)"))
    (pad 2 smd rect (at 0 -23.3) (size 2.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module aruj:smb4 (layer B.Cu) (tedit 5A97193F)
    (at 139 119)
    (fp_text reference U25 (at -11.8 -0.9) (layer B.SilkS) hide)
    (fp_text value smb4 (at -11.8 0.1) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 -21.54) (size 1.9304 15) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(U24-Pad3)"))
  )
  (gr_line (start 135.25 105) (end 135.25 77.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.75 105) (end 135.25 105) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.75 77.5) (end 142.75 105) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.25 77.5) (end 142.75 77.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "SMD\nV 1.0" (at 180.8 91.6) (layer F.SilkS))
  (gr_text Out (at 176.1 96.7) (layer F.SilkS))
  (gr_text In (at 177 88.1) (layer F.SilkS))
  (gr_text In (at 180.2 84.2) (layer F.SilkS))
  (gr_text ch0 (at 172 83.6) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.02548))
    (min_thickness 0.02548)
    (fill yes (arc_segments 16) (thermal_gap 1) (thermal_bridge_width 0.02549))
    (polygon
      (pts
        (xy 142.75 105) (xy 135.25 105) (xy 135.25 77.5) (xy 142.75 77.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.02548))
    (min_thickness 0.02548)
    (fill yes (arc_segments 16) (thermal_gap 1) (thermal_bridge_width 0.02549))
    (polygon
      (pts
        (xy 142.75 105) (xy 135.25 105) (xy 135.25 77.5) (xy 142.75 77.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.02548))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.75 105) (xy 135.25 105) (xy 135.25 77.5) (xy 142.75 77.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.02548))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.75 105) (xy 135.25 105) (xy 135.25 77.5) (xy 142.75 77.5)
      )
    )
  )
)
