(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 16)
    (tracks 50)
    (zones 0)
    (modules 4)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.2032)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-PadA4)")
  (net 3 "Net-(J1-PadA5)")
  (net 4 "Net-(J1-PadA6)")
  (net 5 "Net-(J1-PadA7)")
  (net 6 "Net-(J1-PadA8)")
  (net 7 "Net-(J1-PadB5)")
  (net 8 "Net-(J1-PadB8)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-PadA4)")
    (add_net "Net-(J1-PadA5)")
    (add_net "Net-(J1-PadA6)")
    (add_net "Net-(J1-PadA7)")
    (add_net "Net-(J1-PadA8)")
    (add_net "Net-(J1-PadB5)")
    (add_net "Net-(J1-PadB8)")
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5EE28D78)
    (at 112.75 87 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x04_Female (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-PadA4)"))
    (pad 2 smd oval (at 0 2.54 90) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-PadA7)"))
    (pad 3 smd oval (at 0 5.08 90) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-PadA6)"))
    (pad 4 smd oval (at 0 7.62 90) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 118.3128 90.6552 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 1.43 270) (layer B.SilkS) hide)
    (fp_text value 5.1k (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J1-PadA5)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 121.3354 90.6552 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 1.43 90) (layer B.SilkS) hide)
    (fp_text value 5.1k (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(J1-PadB5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module misc_footprints:TYPE-C-31-M-12 (layer F.Cu) (tedit 5D75DCEA)
    (at 112.5 90.5)
    (fp_text reference J1 (at 0.01016 2.75082) (layer F.SilkS))
    (fp_text value USB_C_Receptacle_USB2.0 (at -2.8448 -3.63474) (layer F.Fab))
    (pad A4|B9 smd rect (at -2.45 0) (size 0.6 1.45) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-PadA4)"))
    (pad B8 smd rect (at -1.75 0) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-PadB8)"))
    (pad A5 smd rect (at -1.25 0) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-PadA5)"))
    (pad B7 smd rect (at -0.75 0) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-PadA7)"))
    (pad A6 smd rect (at -0.25 0) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-PadA6)"))
    (pad A7 smd rect (at 0.25 0) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-PadA7)"))
    (pad B6 smd rect (at 0.75 0) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-PadA6)"))
    (pad A8 smd rect (at 1.25 0) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-PadA8)"))
    (pad B5 smd rect (at 1.75 0) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-PadB5)"))
    (pad B4|A9 smd rect (at 2.45 0) (size 0.6 1.45) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-PadA4)"))
    (pad B1|A12 smd rect (at 3.25 0) (size 0.6 1.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A1|B12 smd rect (at -3.25 0) (size 0.6 1.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad GND thru_hole oval (at 4.32 5.095) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad GND thru_hole oval (at 4.32 0.915) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad GND thru_hole oval (at -4.32 0.915) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad GND thru_hole oval (at -4.32 5.095) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 2.89 1.445) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.89 1.445) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
  )
  (gr_text "makho - v1.0\niPod 4th gen\nUSB C PCB" (at 113.1 90.9 90) (layer B.SilkS))
  (gr_arc (start 109.5 87.25) (end 109.5 85.25) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 120.5 87.25) (end 122.5 87.25) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 120.5 94.5) (end 120.5 96.5) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 119.25 94.15) (end 120.07 94.15) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120.5 96.5) (end 110.75 96.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.5 87.25) (end 122.5 94.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.5 85.25) (end 120.5 85.25) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.5 90) (end 107.5 87.25) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.5 90) (end 106.5 91) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.5 90) (end 106.5 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.5 93.25) (end 106.5 91) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 110.75 93.25) (end 107.5 93.25) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_text "G + - V" (at 117.4 88.7 180) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.5 96.5) (xy 106.5 96.5) (xy 106.5 85.2) (xy 122.5 85.2)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.5 96.5) (xy 106.5 96.5) (xy 106.5 85.2) (xy 122.5 85.2)
      )
    )
  )
)
