(kicad_pcb (version 20171130) (host pcbnew 5.0.1+dfsg1-3~bpo9+1)
  (general
    (thickness 1.6)
    (drawings 20)
    (tracks 146)
    (zones 0)
    (modules 7)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.6 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 CS)
  (net 4 MOSI)
  (net 5 MISO)
  (net 6 SCK)
  (net 7 DIO0)
  (net 8 RESET)
  (net 9 DIO1)
  (net 10 DIO2)
  (net 11 ANT)
  (net 12 DIO5)
  (net 13 DIO4)
  (net 14 DIO3)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net ANT)
    (add_net CS)
    (add_net DIO0)
    (add_net DIO1)
    (add_net DIO2)
    (add_net DIO3)
    (add_net DIO4)
    (add_net DIO5)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net RESET)
    (add_net SCK)
    (add_net VCC)
  )
  (module parts:shutleworth (layer B.Cu) (tedit 5BFC2395)
    (at 118.85 117.05 180)
    (fp_text reference "" (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "" (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5BFC21F3)
    (at 113 106)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -0.025 -0.1) (layer B.SilkS))
    (fp_text value C1 (at 3.93 0.16) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module RFM95W-868S2:XCVR_RFM95W-868S2 (layer F.Cu) (tedit 0)
    (at 113.02 110.84 90)
    (attr smd)
    (fp_text reference U1 (at -6.86 -9.02 90) (layer F.SilkS))
    (fp_text value RFM95W-868S2 (at -0.26 9.08 90) (layer F.SilkS))
    (pad 1 smd rect (at -7.4 -7 90) (size 1.95 1.05) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -7.4 -5 90) (size 1.95 1.05) (layers F.Cu F.Paste F.Mask)
      (net 5 MISO))
    (pad 3 smd rect (at -7.4 -3 90) (size 1.95 1.05) (layers F.Cu F.Paste F.Mask)
      (net 4 MOSI))
    (pad 4 smd rect (at -7.4 -1 90) (size 1.95 1.05) (layers F.Cu F.Paste F.Mask)
      (net 6 SCK))
    (pad 5 smd rect (at -7.4 1 90) (size 1.95 1.05) (layers F.Cu F.Paste F.Mask)
      (net 3 CS))
    (pad 6 smd rect (at -7.4 3 90) (size 1.95 1.05) (layers F.Cu F.Paste F.Mask)
      (net 8 RESET))
    (pad 7 smd rect (at -7.4 5 90) (size 1.95 1.05) (layers F.Cu F.Paste F.Mask)
      (net 12 DIO5))
    (pad 8 smd rect (at -7.4 7 90) (size 1.95 1.05) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 7.4 7 270) (size 1.95 1.05) (layers F.Cu F.Paste F.Mask)
      (net 11 ANT))
    (pad 10 smd rect (at 7.4 5 270) (size 1.95 1.05) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 7.4 3 270) (size 1.95 1.05) (layers F.Cu F.Paste F.Mask)
      (net 14 DIO3))
    (pad 12 smd rect (at 7.4 1 270) (size 1.95 1.05) (layers F.Cu F.Paste F.Mask)
      (net 13 DIO4))
    (pad 13 smd rect (at 7.4 -1 270) (size 1.95 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 14 smd rect (at 7.4 -3 270) (size 1.95 1.05) (layers F.Cu F.Paste F.Mask)
      (net 7 DIO0))
    (pad 15 smd rect (at 7.4 -5 270) (size 1.95 1.05) (layers F.Cu F.Paste F.Mask)
      (net 9 DIO1))
    (pad 16 smd rect (at 7.4 -7 270) (size 1.95 1.05) (layers F.Cu F.Paste F.Mask)
      (net 10 DIO2))
    (model ${KIPRJMOD}/parts/RFM95/RFM95W-915S2--3DModel-STEP-56544.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Connectors:SMB_Straight (layer F.Cu) (tedit 586135E7)
    (at 127.5 110.5)
    (descr "SMB pcb mounting jack")
    (tags "SMB Jack  Striaght")
    (fp_text reference AE1 (at -0.1 4.725) (layer F.SilkS))
    (fp_text value Ant (at 0 5.05) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.24 2.24) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 ANT))
    (model Connectors.3dshapes/SMB_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Amphenol_132291-12_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 0.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_2x06 (layer F.Cu) (tedit 0)
    (at 100.665 117.145 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 1.265 6.345 180) (layer F.SilkS))
    (fp_text value PMOD_LoRa (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 SCK))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 DIO2))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 MISO))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 DIO1))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 MOSI))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 RESET))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 CS))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 DIO0))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_2x06_P1.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2.75 2.5 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.00mm (layer F.Cu) (tedit 56FA75DA)
    (at 130 103 270)
    (descr "Through hole pin header, 1x03, 2.00mm pitch, single row")
    (tags "pin header single row")
    (fp_text reference P2 (at 2.1 2) (layer F.SilkS))
    (fp_text value Ext (at -0.1 6.4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 DIO5))
    (pad 2 thru_hole circle (at 0 2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 DIO4))
    (pad 3 thru_hole circle (at 0 4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 DIO3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module parts:radiona-small (layer B.Cu) (tedit 5BFC234F)
    (at 119.875 103.675 180)
    (fp_text reference "" (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "" (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_line (start 94 121) (end 94 101) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.25 121) (end 94 121) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132 121) (end 125.75 121) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132 101) (end 132 121) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 94 101) (end 132 101) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 124 121) (end 125.75 121) (angle -180) (layer Edge.Cuts) (width 0.2))
  (gr_text "Ver.: 0.2" (at 99.6 119.9) (layer B.SilkS))
  (gr_text LoRa-PMOD (at 99.8 102) (layer B.SilkS))
  (gr_text IO0 (at 95.8 104.7) (layer B.SilkS))
  (gr_text 3V3 (at 95.5 117.3) (layer B.SilkS))
  (gr_text GND (at 95.6 114.9) (layer B.SilkS))
  (gr_text IO2 (at 95.7 112.2) (layer B.SilkS))
  (gr_text IO1 (at 95.7 109.7) (layer B.SilkS))
  (gr_text RST (at 95.8 107.1) (layer B.SilkS))
  (gr_text 3V3 (at 103.4 117.4) (layer B.SilkS))
  (gr_text GND (at 103.6 114.7) (layer B.SilkS))
  (gr_text SCK (at 103.6 112.2) (layer B.SilkS))
  (gr_text MISO (at 103.8 109.7) (layer B.SilkS))
  (gr_text MOSI (at 103.8 107.2) (layer B.SilkS))
  (gr_text CS (at 103.2 104.5) (layer B.SilkS))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132 101) (xy 94 101) (xy 94 121) (xy 132 121)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132 101) (xy 94 101) (xy 94 121) (xy 132 121)
      )
    )
  )
)
