(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 6)
    (zones 0)
    (modules 2)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (grid_origin 92.71 110.8)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /M1)
  (net 2 /M2)
  (net 3 "Net-(J1-Pad5)")
  (net 4 "Net-(J1-Pad6)")
  (net 5 /GND)
  (net 6 /3V3)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3V3)
    (add_net /GND)
    (add_net /M1)
    (add_net /M2)
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x06_P1.27mm_Vertical (layer F.Cu) (tedit 59FED6E3)
    (at 96.825 106.99 90)
    (descr "Through hole straight pin header, 1x06, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x06 1.27mm single row")
    (fp_text reference J3 (at 0 -1.695 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x06 (at 0 8.045 90) (layer F.Fab))
    (fp_text user %R (at 0 3.15) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 6.35 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 3.81 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 /3V3))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 /GND))
    (pad 2 thru_hole oval (at 0 1.27 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 /M2))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 /M1))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x06_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "wedo_2.0:WeDo 2.0 Female Socket" (layer F.Cu) (tedit 5E7CD3A7)
    (at 100 100)
    (fp_text reference J1 (at 0.33 4.394) (layer F.SilkS) hide)
    (fp_text value FemaleConnector (at 11.43 15.24) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 4.85 2.05) (size 2.286 2.286) (drill 2.286) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -4.85 0.58) (size 2.286 2.286) (drill 2.286) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 3.175 0.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad6)"))
    (pad 5 thru_hole circle (at 1.905 2.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad5)"))
    (pad 4 thru_hole circle (at 0.635 0.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 /3V3))
    (pad 3 thru_hole circle (at -0.635 2.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 /GND))
    (pad 2 thru_hole circle (at -1.905 0.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 /M2))
    (pad 1 thru_hole circle (at -3.175 2.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 /M1))
  )
  (gr_text ID2 (at 103.251 104.831 90) (layer F.SilkS))
  (gr_text ID1 (at 101.981 104.831 90) (layer F.SilkS))
  (gr_text 3v3 (at 100.711 104.831 90) (layer F.SilkS))
  (gr_text "Gnd\n" (at 99.441 104.831 90) (layer F.SilkS))
  (gr_text M2 (at 98.171 104.831 90) (layer F.SilkS))
  (gr_text M1 (at 96.901 104.831 90) (layer F.SilkS))
  (gr_text "V1.0\n2020-03-26" (at 94.234 108.387 270) (layer B.SilkS))
  (gr_text "Powered Up Extender" (at 101.219 104.704 180) (layer B.SilkS))
  (gr_line (start 107.315 98.1) (end 107.315 108.895) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.6 98.1) (end 107.315 98.1) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.6 108.895) (end 92.6 98.1) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 107.315 108.895) (end 92.6 108.895) (layer Edge.Cuts) (width 0.1))
  (zone (net 5) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.315 108.895) (xy 91.44 108.895) (xy 91.44 98.1) (xy 107.315 98.1)
      )
    )
  )
  (zone (net 5) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.315 108.895) (xy 92.075 108.895) (xy 92.075 98.1) (xy 107.315 98.1)
      )
    )
  )
)
