<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="40.64" y1="50.4825" x2="40.64" y2="1.5875" width="0" layer="20"/>
<wire x1="40.64" y1="1.5875" x2="39.0525" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="39.0525" y1="0" x2="1.5875" y2="0" width="0" layer="20"/>
<wire x1="1.5875" y1="0" x2="0" y2="1.5875" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="1.5875" x2="0" y2="50.4825" width="0" layer="20"/>
<wire x1="0" y1="50.4825" x2="1.5875" y2="52.07" width="0" layer="20" curve="-90"/>
<wire x1="1.5875" y1="52.07" x2="39.0525" y2="52.07" width="0" layer="20"/>
<wire x1="39.0525" y1="52.07" x2="40.64" y2="50.4825" width="0" layer="20" curve="-90"/>
<text>K3</text>
<text>EPCCS.ORG</text>
<text>0V</text>
<text>5V</text>
<text>K3</text>
<text>EPCCS.ORG</text>
<text>16276^0</text>
<text>5.3%BOOST</text>
<text>!EN</text>
<text>EN</text>
<text>A2</text>
<text>A1</text>
<text>A0</text>
<text>COM</text>
<text>K3</text>
<text>K2</text>
<text>K1</text>
<text>JMP 1-2: 24V</text>
<text>JMP NONE: 9V</text>
<text>JMP 2-3: 12V</text>
</plain>
<libraries>
<library name="H-Fiducial">
<description>&lt;pre&gt;Fiducianl Mark
USE AT YOUR OWN RISK...
Copyright (C) 2013 Ronald Steven Sutherland
Permission is granted to copy, distribute and/or modify this document 
under the terms of the GNU Free Documentation License, Version 1.2 or 
any later version published by the Free Software Foundation; with no 
Invariant Sections, no Front-Cover Texts, and no Back-Cover Texts. A 
copy of the license is included in the section entitled "GNU Free 
Documentation License".</description>
<packages>
<package name="FIDUCIAL-1.27">
<description>&lt;pre&gt;Fiducian R=1.27mm 
STOP=2.54mm
It is up to designer to not put traces under Fiducial (i.e. Void or sold plane only)
Autorouter restricted areas are defined as RECTangles, POLYGONs, or CIRCLEs on the 
tRestrict, bRestrict, or vRestrict layers.</description>
</package>
</packages>
</library>
<library name="HW-DINMnt">
<description>&lt;pre&gt;DIN Rail Adapters

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="USA10">
<description>&lt;pre&gt;USA10-4.6 [PhxCont,1202713] DINRAIL ADAPTER UNIVERSAL 10MM 4.6MM
with #6 screw size mounting holes</description>
</package>
</packages>
</library>
<library name="Q-NCH">
<description>&lt;pre&gt;N-CHANNEL MOSFET
ENHANCEMENT MODE is shown with a open/broken channel
DEPLETION MODE is shown with a closed/complete channel thus the idea of being on with zero gate voltage.

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="SOT23">
<description>&lt;pre&gt;SOT23 (based on SOT23-6) pin 3 is alone
http://www.diodes.com/_files/zetex_files/pack/SOT23-6.pdf
center(1) to center(2,3) 2.2 mm
center(2) to center(3) 1.9mm
pad .65X x 1.06Y mm</description>
</package>
</packages>
</library>
<library name="Q-PCH">
<description>&lt;pre&gt;N-CHANNEL MOSFET
ENHANCEMENT MODE is shown with a open/broken channel
DEPLETION MODE is shown with a closed/complete channel thus the idea of being on with zero gate voltage.

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="SOT23">
<description>&lt;pre&gt;SOT23 (based on SOT23-6) pin 3 is alone
http://www.diodes.com/_files/zetex_files/pack/SOT23-6.pdf
center(1) to center(2,3) 2.2 mm
center(2) to center(3) 1.9mm
pad .65X x 1.06Y mm</description>
</package>
</packages>
</library>
<library name="R-C">
<description>&lt;pre&gt;CHIP RESISTOR
NOTE: rounded pads... http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf
See section on Tombstoneing. Lead free solder may not wet edges, and IPC does not allow exposed copper. 
My (rsutherland@epccs) experience suggest highly rounded pads reduce solder beads that can be extruded along edges of larger capacitors (0805).

USE AT YOUR OWN RISK...
 
Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="C0805(2012)">
<description>&lt;pre&gt;EIA 0805 (Metric Code Size 2012) Ceramic Chip
rounded pads are added in IPC 782 rev A
http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf</description>
</package>
<package name="C1210(3225)">
<description>&lt;pre&gt;EIA 1210 (Metric Code Size 3225) Ceramic Chip
rounded pads are added in IPC 782 rev A.
http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf</description>
</package>
</packages>
</library>
<library name="Q-NPN">
<description>&lt;pre&gt;NPN Bipolar junction transistor

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="SOT23">
<description>&lt;pre&gt;SOT23 (based on SOT23-6) pin 1 is alone (Cathode)
http://www.diodes.com/_files/zetex_files/pack/SOT23-6.pdf
center(1) to center(2,3) 2.2 mm
center(2) to center(3) 1.9mm
pad .65X x 1.06Y mm</description>
</package>
</packages>
</library>
<library name="Q-PNP">
<description>&lt;pre&gt;PNP Bipolar junction transistor

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="SOT23">
<description>&lt;pre&gt;SOT23 (based on SOT23-6) pin 1 is alone (Cathode)
http://www.diodes.com/_files/zetex_files/pack/SOT23-6.pdf
center(1) to center(2,3) 2.2 mm
center(2) to center(3) 1.9mm
pad .65X x 1.06Y mm</description>
</package>
</packages>
</library>
<library name="J-HDR3.5mm">
<description>&lt;pre&gt;HEADER 3.5MM center to center
USE AT YOUR OWN RISK...
 
Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="MCV4">
<description>&lt;pre&gt;MCV 1,5/4-G-3,5-RN [PHOENIX CONTACT,1843622] CONN HEADER SHROUDED 4POS 3.5MM
PST 1,0/4-3,5 [PHOENIX CONTACT,1945119] CONN HEADER STRIP PIN 4POS 3.5MM

Drill Size 3/64": .0469" (1.2mm)</description>
</package>
<package name="MCV8">
<description>&lt;pre&gt;PHOENIX CONTACT 1843664
MCV 1,5/ 8-G-3,5
Drill Size 3/64": .0469" (1.2mm)</description>
</package>
</packages>
</library>
<library name="U-7400">
<description>&lt;b&gt;TTL Devices, 74xx Series with US Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="16SOIC">
<description>&lt;pre&gt;Small Outline (SO/SOIC) package 1.27mm [50 mil] pitch, 4mm wide body, 6.2mm wide pin-pin, 10mm long
e.g. 74HC151 [TI,SN74HC151D] LOGIC 8TO1 MUX 16SOIC</description>
</package>
</packages>
</library>
<library name="C-C">
<description>&lt;pre&gt; MULTILAYER CERAMIC CHIP CAPACITORS

Type: C1005 [EIA CC0402], C1608 [EIA CC0603], C2012 [EIA CC0805],
C3216 [EIA CC1206], C3225 [EIA CC1210], C4532 [EIA CC1812], C5750 [EIA CC2220]

CH 0±60 ppm/°C -25 to +85°C
C0G 0±30 ppm/°C -55 to +125°C
JB ±10% -25 to +85°C
X5R ±15% -55 to +85°C
X6S ±22% -55 to +105°C
X7R ±15% -55 to +125°C
X7S ±22% -55 to +125°C
X7T +22/-33% -55 to +125°C

TDK voltage cods
0G 4V
0J 6.3V
1A 10V
1C 16V
1E 25V
1V 35V
1H 50V
2A 100V
2E 250V
2V 350V
2W 450V
2J 630V

NOTE: rounded pads... http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf
See section on Tombstoneing. Lead free solder may not wet edges, and IPC does not allow exposed copper. 
My (rsutherland@epccs) experience suggest highly rounded pads reduce solder beads that can be extruded along edges of larger capacitors (0805).

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="C0603(1608)">
<description>&lt;pre&gt;EIA 0603 (Metric Code Size 1608) Ceramic Chip Capacitor
rounded pads are added in IPC 782 rev A, this pad was on Arduino Due and may have originated from Sparkfun.
http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf</description>
</package>
</packages>
</library>
<library name="U-Boost">
<description>&lt;pre&gt;Boost Regulator
For step-up DC-DC

USE AT YOUR OWN RISK...

Copyright (C) 2014 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="SOIC8">
<description>&lt;pre&gt;8POS Standard SMALLl OUTLINE Package (SO/SOIC) Narrow Body</description>
</package>
</packages>
</library>
<library name="D-SBR">
<description>&lt;pre&gt;Super Barrier Rectifier
Super barrier diodes are rectifier diodes that incorporate the low forward voltage
drop of the Schottky diode with the surge-handling capability and low reverse 
leakage current of a normal p–n junction diode.

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="SMA">
<description>&lt;pre&gt;SMB 
http://www.diodes.com/datasheets/ap02001.pdf
center to center 4 mm
pad 2.5X x 1.7Y mm</description>
</package>
</packages>
</library>
<library name="C-Al">
<description>&lt;pre&gt;Aluminum Electrolytic Capacitors

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="E7,5-18">
<description>&lt;pre&gt;ELECTROLYTIC CAPACITOR
pin spacing 7.5 mm, body diameter 18 mm
PW1J222 [NICHICON,UPW1J222MHD] CAP ALUM 63V 2200UF 20% RADIAL</description>
</package>
</packages>
</library>
<library name="D-LED">
<description>&lt;pre&gt;Light-emitting diode
http://en.wikipedia.org/wiki/Light-emitting_diode
USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="C0805(2012)">
<description>&lt;pre&gt;EIA 0805 (Metric Code Size 2012) Ceramic Chip
rounded pads are added in IPC 782 rev A, this pad was on Arduino and may have originated from Sparkfun.
http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf</description>
</package>
</packages>
</library>
<library name="L-PWR">
<description>&lt;pre&gt;Inductor Power

USE AT YOUR OWN RISK...
 
    Copyright (C) 2015 Ronald Sutherland
    Released under the Creative Commons 
    Attribution-ShareAlike 4.0 International
    http://creativecommons.org/licenses/by-sa/4.0</description>
<packages>
<package name="L2626">
<description>&lt;pre&gt;Dimension (mm): .26 x .26 (6.5 x 6.5)

SRR0604-101 [Bourns,SRR0604-101KL] INDUCTOR POWER SHIELDED 100UH SMD</description>
</package>
</packages>
</library>
<library name="J-HDR2.54mm">
<description>&lt;pre&gt;HEADER 2.54MM center to center

USE AT YOUR OWN RISK...
 
Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="1X3">
<description>&lt;pre&gt;4 PIN 
.1" CENTER 
0.040" DRILL
auto PAD

http://www.sullinscorp.com/catalogs/78_Page80-81_HEADER_.100_2.54mm_FEMALE.pdf</description>
</package>
</packages>
</library>
<library name="D-GP">
<description>&lt;pre&gt;GEN PURPOSE DIODE
USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="SOD123">
<description>&lt;pre&gt;SOD123
http://www.diodes.com/datasheets/ap02001.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="H-Fiducial" package="FIDUCIAL-1.27" value="FIDUCIAL1.27"/>
<element name="U$3" library="H-Fiducial" package="FIDUCIAL-1.27" value="FIDUCIAL1.27"/>
<element name="U$4" library="H-Fiducial" package="FIDUCIAL-1.27" value="FIDUCIAL1.27"/>
<element name="HW1" library="HW-DINMnt" package="USA10" value="USA10-4,6">
<attribute name="NAME"/>
</element>
<element name="HW2" library="HW-DINMnt" package="USA10" value="USA10-4,6">
<attribute name="NAME"/>
</element>
<element name="Q12" library="Q-NCH" package="SOT23" value="34N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="Q-PCH" package="SOT23" value="DMB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q6" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="Q-NCH" package="SOT23" value="34N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="Q-PCH" package="SOT23" value="DMB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="R-C" package="C0805(2012)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q11" library="Q-NCH" package="SOT23" value="34N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q10" library="Q-PCH" package="SOT23" value="DMB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q9" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="R-C" package="C0805(2012)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="R-C" package="C0805(2012)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q7" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q8" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q5" library="Q-PNP" package="SOT23" value="K3N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q13" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q14" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q15" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q23" library="Q-NCH" package="SOT23" value="34N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q22" library="Q-PCH" package="SOT23" value="DMB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q21" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="R-C" package="C0805(2012)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="J-HDR3.5mm" package="MCV4" value="PST1,0/4-3,5">
<attribute name="NAME"/>
</element>
<element name="U2" library="U-7400" package="16SOIC" value="74HC238">
<attribute name="NAME"/>
</element>
<element name="C6" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="U-Boost" package="SOIC8" value="MC34063A">
<attribute name="NAME"/>
</element>
<element name="Q24" library="Q-PCH" package="SOT23" value="K84">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="R-C" package="C0805(2012)" value="182">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="C-C" package="C0603(1608)" value="330pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="R-C" package="C0805(2012)" value="15.8k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="D-SBR" package="SMA" value="SQ4">
<attribute name="NAME"/>
</element>
<element name="R19" library="R-C" package="C1210(3225)" value="1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q18" library="Q-PCH" package="SOT23" value="DMB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q16" library="Q-NCH" package="SOT23" value="K38">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q17" library="Q-NCH" package="SOT23" value="K38">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="R-C" package="C0805(2012)" value="32.4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="R-C" package="C0805(2012)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="D-LED" package="C0805(2012)" value="0805RD">
<attribute name="NAME"/>
</element>
<element name="R25" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="R-C" package="C0805(2012)" value="5.62K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="L-PWR" package="L2626" value="150UH 0A3">
<attribute name="NAME"/>
</element>
<element name="R29" library="R-C" package="C0805(2012)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="J-HDR2.54mm" package="1X3" value="PBC03SAA">
<attribute name="NAME"/>
</element>
<element name="R31" library="R-C" package="C0805(2012)" value="43.2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="R-C" package="C0805(2012)" value="8.45k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="C-C" package="C0603(1608)" value=".01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="D-GP" package="SOD123" value="T4">
<attribute name="NAME"/>
</element>
<element name="Q20" library="Q-PNP" package="SOT23" value="K3N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q19" library="Q-PNP" package="SOT23" value="K3N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="R-C" package="C0805(2012)" value="49.9k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="C-Al" package="E7,5-18" value="2200uF">
<attribute name="NAME"/>
</element>
<element name="J2" library="J-HDR3.5mm" package="MCV8" value="">
<attribute name="NAME"/>
</element>
<element name="C1" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="0V">
<contactref element="Q1" pad="E"/>
<contactref element="Q3" pad="2(S)"/>
<contactref element="Q12" pad="2(S)"/>
<contactref element="Q6" pad="E"/>
<contactref element="Q7" pad="E"/>
<contactref element="Q8" pad="E"/>
<contactref element="Q11" pad="2(S)"/>
<contactref element="Q9" pad="E"/>
<contactref element="R15" pad="1"/>
<contactref element="Q13" pad="E"/>
<contactref element="Q15" pad="E"/>
<contactref element="Q14" pad="E"/>
<contactref element="Q23" pad="2(S)"/>
<contactref element="Q21" pad="E"/>
<contactref element="U2" pad="8"/>
<contactref element="C6" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="U1" pad="4"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="R26" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="R28" pad="1"/>
<contactref element="R31" pad="2"/>
<contactref element="R30" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="R21" pad="1"/>
<contactref element="C4" pad="-"/>
<contactref element="J2" pad="8"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="Q5" pad="E"/>
<contactref element="U2" pad="16"/>
<contactref element="C6" pad="1"/>
<contactref element="Q24" pad="2(S)"/>
<contactref element="R11" pad="1"/>
<contactref element="Q18" pad="2(S)"/>
<contactref element="R20" pad="2"/>
<contactref element="Q20" pad="E"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="N$9">
<contactref element="Q4" pad="1(G)"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="SET-K1">
<contactref element="Q3" pad="1(G)"/>
<contactref element="R6" pad="1"/>
<contactref element="U2" pad="13"/>
</signal>
<signal name="RESET-K1">
<contactref element="R9" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="U2" pad="12"/>
</signal>
<signal name="SET-K3">
<contactref element="R8" pad="1"/>
<contactref element="Q23" pad="1(G)"/>
<contactref element="U2" pad="9"/>
</signal>
<signal name="SET-K2">
<contactref element="R7" pad="1"/>
<contactref element="Q11" pad="1(G)"/>
<contactref element="U2" pad="11"/>
</signal>
<signal name="RESET-K3">
<contactref element="R17" pad="1"/>
<contactref element="R22" pad="1"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="N$27">
<contactref element="R5" pad="1"/>
<contactref element="Q6" pad="C"/>
<contactref element="Q7" pad="C"/>
<contactref element="Q8" pad="C"/>
</signal>
<signal name="N$28">
<contactref element="Q6" pad="B"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="K1">
<contactref element="Q3" pad="3(D)"/>
<contactref element="Q2" pad="3(D)"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="Q2" pad="1(G)"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$36">
<contactref element="R2" pad="1"/>
<contactref element="Q1" pad="C"/>
</signal>
<signal name="N$37">
<contactref element="Q1" pad="B"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="RESET-K2">
<contactref element="R10" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="U2" pad="10"/>
</signal>
<signal name="K2">
<contactref element="Q11" pad="3(D)"/>
<contactref element="Q10" pad="3(D)"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$43">
<contactref element="Q10" pad="1(G)"/>
<contactref element="R14" pad="1"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$44">
<contactref element="R13" pad="1"/>
<contactref element="Q9" pad="C"/>
</signal>
<signal name="N$45">
<contactref element="Q9" pad="B"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="BOOST">
<contactref element="Q4" pad="2(S)"/>
<contactref element="R4" pad="2"/>
<contactref element="Q2" pad="2(S)"/>
<contactref element="R3" pad="2"/>
<contactref element="Q10" pad="2(S)"/>
<contactref element="R14" pad="2"/>
<contactref element="Q22" pad="2(S)"/>
<contactref element="R24" pad="2"/>
<contactref element="C4" pad="+"/>
<contactref element="R27" pad="1"/>
<contactref element="D1" pad="K"/>
<contactref element="R25" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="R8" pad="2"/>
<contactref element="Q8" pad="B"/>
</signal>
<signal name="N$71">
<contactref element="R7" pad="2"/>
<contactref element="Q7" pad="B"/>
</signal>
<signal name="N$21">
<contactref element="Q12" pad="1(G)"/>
<contactref element="Q5" pad="C"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$72">
<contactref element="Q5" pad="B"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="N$73">
<contactref element="R16" pad="1"/>
<contactref element="Q13" pad="C"/>
<contactref element="Q14" pad="C"/>
<contactref element="Q15" pad="C"/>
</signal>
<signal name="N$79">
<contactref element="Q13" pad="B"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$81">
<contactref element="Q14" pad="B"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$87">
<contactref element="Q15" pad="B"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="K3">
<contactref element="Q23" pad="3(D)"/>
<contactref element="Q22" pad="3(D)"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="Q22" pad="1(G)"/>
<contactref element="R24" pad="1"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R23" pad="1"/>
<contactref element="Q21" pad="C"/>
</signal>
<signal name="N$5">
<contactref element="Q21" pad="B"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="COM">
<contactref element="Q4" pad="3(D)"/>
<contactref element="Q12" pad="3(D)"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="A0">
<contactref element="U2" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="SMPS">
<contactref element="U2" pad="14"/>
<contactref element="Q24" pad="1(G)"/>
<contactref element="Q16" pad="1(G)"/>
</signal>
<signal name="A1">
<contactref element="U2" pad="2"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="A2">
<contactref element="U2" pad="3"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="!EN">
<contactref element="U2" pad="5"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="EN">
<contactref element="U2" pad="6"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="5"/>
<contactref element="Q24" pad="3(D)"/>
<contactref element="R29" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="U1" pad="8"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="R18" pad="1"/>
<contactref element="U1" pad="7"/>
<contactref element="R19" pad="2"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="U1" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="U1" pad="3"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="6"/>
<contactref element="R19" pad="1"/>
<contactref element="Q17" pad="1(G)"/>
<contactref element="Q18" pad="3(D)"/>
<contactref element="C3" pad="1"/>
<contactref element="D3" pad="K"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="Q17" pad="3(D)"/>
<contactref element="Q16" pad="2(S)"/>
</signal>
<signal name="N$22">
<contactref element="R11" pad="2"/>
<contactref element="Q16" pad="3(D)"/>
<contactref element="Q18" pad="1(G)"/>
</signal>
<signal name="N$26">
<contactref element="R29" pad="1"/>
<contactref element="R27" pad="2"/>
<contactref element="R28" pad="2"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="5.3%BOOST">
<contactref element="R25" pad="2"/>
<contactref element="R26" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="N$120">
<contactref element="J3" pad="3"/>
<contactref element="R31" pad="1"/>
</signal>
<signal name="N$121">
<contactref element="J3" pad="1"/>
<contactref element="R30" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="Q17" pad="2(S)"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$128">
<contactref element="R20" pad="1"/>
<contactref element="Q19" pad="E"/>
<contactref element="Q20" pad="B"/>
</signal>
<signal name="N$132">
<contactref element="Q20" pad="C"/>
<contactref element="R21" pad="2"/>
<contactref element="Q19" pad="B"/>
</signal>
<signal name="N$86">
<contactref element="Q19" pad="C"/>
<contactref element="D3" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
