(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 0.1916)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen") (color "White"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "#808080D4") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (color "Polyimide") (thickness 0.1016) (material "Polyimide") (epsilon_r 3.2) (loss_tangent 0.004))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen") (color "#808080FF"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "output/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "/SCL")
  (net 3 "/SDA")
  (net 4 "/ANT")
  (net 5 "VDD")
  (net 6 "Net-(D1-A)")
  (net 7 "/SWIO")
  (net 8 "/PZ+")
  (net 9 "/PZ-")
  (net 10 "/FD")
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 129.54 106.68 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "JLC" "0805")
    (property "LCSC" "C126592")
    (property "MPN" "GCM21BR71H105KA03L")
    (property "Sheetfile" "b4handy.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C1" (at 3.175 0) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 5 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 142.24 101.6 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "JLC" "")
    (property "LCSC" "")
    (property "MPN" "")
    (property "Sheetfile" "b4handy.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd exclude_from_bom)
    (fp_text reference "C2" (at 0 -2.032 90) (layer "F.SilkS") hide)
    (fp_text value "DNP" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/ANT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/ANT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 90.805 81.28 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "JLC" "0805")
    (property "LCSC" "C114531")
    (property "MPN" "RC0805FR-073K3L")
    (property "Sheetfile" "b4handy.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -2.54 0 180) (layer "F.SilkS"))
    (fp_text value "3.3k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 5 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 6 "Net-(D1-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "custom:Buzzer_Murata_PKLCS1212E_handy" (layer "F.Cu")
    (at 133.35 116.205 -90)
    (descr "Murata Buzzer https://www.murata.com/~/media/webrenewal/support/library/catalog/products/sound/p37e.ashx")
    (tags "Murata Buzzer Beeper")
    (property "JLC" "")
    (property "LCSC" "C184513")
    (property "MPN" "PKLCS1212E20A0-R1")
    (property "Sheetfile" "b4handy.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Crystal speaker/transducer")
    (property "ki_keywords" "crystal speaker ultrasonic transducer")
    (attr smd)
    (fp_text reference "LS1" (at 0 0 -180) (layer "F.SilkS"))
    (fp_text value "Speaker_Crystal" (at 0 7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -6.6 0 270) (size 3.2 4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/PZ-") (pinfunction "1") (pintype "input"))
    (pad "2" smd rect (at 6.6 0 270) (size 3.2 4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/PZ+") (pinfunction "2") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Buzzer_Beeper.3dshapes/Buzzer_Murata_PKLCS1212E.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOP-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (at 128.905 101.6 90)
    (descr "SOP, 8 Pin (http://www.macronix.com/Lists/Datasheet/Attachments/7534/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.6.pdf#page=79), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOP SO")
    (property "JLC" "SO8_3.9mm")
    (property "LCSC" "C5346354")
    (property "MPN" "CH32V003J4M6")
    (property "Sheetfile" "b4handy.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 0 0 180) (layer "F.SilkS"))
    (fp_text value "CH32V003F4P6" (at -0.127 -29.083 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.625 -1.905 90) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/PZ+") (pinfunction "PA1_T1CH2_A1") (pintype "bidirectional"))
    (pad "2" smd roundrect (at -2.625 -0.635 90) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "3" smd roundrect (at -2.625 0.635 90) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/PZ-") (pinfunction "PA2_T1CH2N_A0") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -2.625 1.905 90) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "VDD") (pinfunction "VDD") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.625 1.905 90) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/SDA") (pinfunction "PC1_SDA") (pintype "bidirectional"))
    (pad "6" smd roundrect (at 2.625 0.635 90) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/SCL") (pinfunction "PC2_SCL") (pintype "bidirectional"))
    (pad "7" smd roundrect (at 2.625 -0.635 90) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/FD") (pinfunction "PC4_MCO_A2") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 2.625 -1.905 90) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/SWIO") (pinfunction "PD1_SWIO") (pintype "bidirectional"))
    (model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/SOP-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "custom:PinHeader_2x03_P2.54mm_Staggered" (layer "F.Cu")
    (at 96.525 104.125 180)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "JLC" "")
    (property "LCSC" "")
    (property "MPN" "")
    (property "Sheetfile" "b4handy.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole exclude_from_bom)
    (fp_text reference "J1" (at 1.27 -2.33) (layer "F.SilkS") hide)
    (fp_text value "DNP" (at 1.27 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -0.127 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "VDD") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.667 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0.127 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "/SDA") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.413 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "/SCL") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at -0.127 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "/SWIO") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.667 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "/FD") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Symbol:KiCad-Logo_12mm_Copper" locked (layer "F.Cu")
    (at 107.95 116.205)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -8.89) (layer "F.SilkS") hide)
    (fp_text value "KiCad-Logo_12mm_Copper" (at 1.27 8.89) (layer "F.Fab") hide)
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 133.35 99.06 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "JLC" "0805")
    (property "LCSC" "C114531")
    (property "MPN" "RC0805FR-073K3L")
    (property "Sheetfile" "b4handy.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 2.54 0 180) (layer "F.SilkS"))
    (fp_text value "3.3k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 5 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "/SCL") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Symbol:KiCad-Logo_12mm_SilkScreen" locked (layer "F.Cu")
    (at 107.95 116.205)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -8.89) (layer "F.SilkS") hide)
    (fp_text value "KiCad-Logo_12mm_SilkScreen" (at 1.27 8.89) (layer "F.Fab") hide)
  )
  (footprint "Package_SO:SO-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (at 137.795 101.6 -90)
    (descr "SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SO SO")
    (property "JLC" "SO8_3.9mm")
    (property "LCSC" "C2654821")
    (property "MPN" "NT3H2211W0FT1X")
    (property "Sheetfile" "b4handy.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "NFC/I2C EEPROM, SOIC-8/TSSOP-8/DFN-8")
    (property "ki_keywords" "NFC/I2C EEPROM")
    (attr smd)
    (fp_text reference "U1" (at 0 0) (layer "F.SilkS"))
    (fp_text value "NT3H2211" (at 0.127 37.846 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.575 -1.905 270) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/ANT") (pinfunction "LA") (pintype "input"))
    (pad "2" smd roundrect (at -2.575 -0.635 270) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "input"))
    (pad "3" smd roundrect (at -2.575 0.635 270) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "4" smd roundrect (at -2.575 1.905 270) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/FD") (pinfunction "FD") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.575 1.905 270) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "6" smd roundrect (at 2.575 0.635 270) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "VDD") (pinfunction "VCC") (pintype "input"))
    (pad "7" smd roundrect (at 2.575 -0.635 270) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "VDD") (pinfunction "VOUT") (pintype "input"))
    (pad "8" smd roundrect (at 2.575 -1.905 270) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/ANT") (pinfunction "LB") (pintype "power_in"))
    (model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/SO-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 133.35 104.14 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "JLC" "0805")
    (property "LCSC" "C114531")
    (property "MPN" "RC0805FR-073K3L")
    (property "Sheetfile" "b4handy.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at -2.54 0 180) (layer "F.SilkS"))
    (fp_text value "3.3k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 3 "/SDA") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 5 "VDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "custom:LED_3228_Reverse_HandSolder" (layer "F.Cu")
    (at 93.98 81.28 90)
    (descr "LED SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "JLC" "")
    (property "LCSC" "C5346037")
    (property "MPN" "VLRK31R1S2-GS08")
    (property "Sheetfile" "b4handy.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D1" (at -5.08 0 180) (layer "F.SilkS"))
    (fp_text value "VLRK31R1S2-GS08" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2 2) (drill 2.5) (layers "F&B.Cu" "*.Mask"))
    (pad "1" smd roundrect (at -2.75 0 90) (size 2.5 2.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754392)
      (net 10 "/FD") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2.75 0 90) (size 2.5 2.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754392)
      (net 6 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 88.9 80.01) (mid 90.015923 77.315923) (end 92.71 76.2)
    (layer "Edge.Cuts"))
  (gr_line (start 177.8 80.01) (end 177.8 123.19)
    (layer "Edge.Cuts"))
  (gr_arc (start 92.71 127) (mid 90.015923 125.884077) (end 88.9 123.19)
    (layer "Edge.Cuts"))
  (gr_line (start 88.9 123.19) (end 88.9 80.01)
    (layer "Edge.Cuts"))
  (gr_line (start 92.71 76.2) (end 173.99 76.2)
    (layer "Edge.Cuts"))
  (gr_arc (start 177.8 123.19) (mid 176.684077 125.884077) (end 173.99 127)
    (layer "Edge.Cuts"))
  (gr_arc (start 173.99 76.2) (mid 176.684077 77.315923) (end 177.8 80.01)
    (layer "Edge.Cuts"))
  (gr_line (start 173.99 127) (end 92.71 127)
    (layer "Edge.Cuts"))
  (gr_text "Beeping\nBlinking\nBusiness card\nBadge\n" (at 115.57 82.55) (layer "F.SilkS"))
  (gr_text "B4" (at 107.95 82.55) (layer "F.SilkS"))
  (gr_text "SDA" (at 100.076 101.6) (layer "F.SilkS"))
  (gr_text "NTAG\nI2C\nPlus" (at 137.795 93.345) (layer "F.SilkS"))
  (gr_text "VDD" (at 100.076 104.14) (layer "F.SilkS"))
  (gr_text "Designed with" (at 92.71 109.22) (layer "F.SilkS"))
  (gr_text "SCL" (at 90.932 101.6) (layer "F.SilkS"))
  (gr_text "SWIO" (at 100.076 99.06) (layer "F.SilkS"))
  (gr_text "GND" (at 90.932 104.14) (layer "F.SilkS"))
  (gr_text "FD" (at 90.932 99.06) (layer "F.SilkS"))
  (gr_text "WCH32V003" (at 116.84 101.6) (layer "F.SilkS"))
)
