<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="13.97" y1="0" x2="5.08" y2="0" width="0.2032" layer="20"/>
<wire x1="0" y1="5.08" x2="0" y2="25.4" width="0.2032" layer="20"/>
<text>http://pinocc.io</text>
<text>Design by: Eric Jennings for Pinoccio</text>
<text>Pinoccio(tm) Module v0.1</text>
<wire x1="0" y1="5.08" x2="5.08" y2="0" width="0.2032" layer="20"/>
<wire x1="0" y1="25.4" x2="19.05" y2="25.4" width="0.2032" layer="20"/>
<text>Licensed under CERN OHL v.1.1</text>
<wire x1="13.97" y1="0" x2="19.05" y2="5.08" width="0.2032" layer="20"/>
<wire x1="19.05" y1="5.08" x2="19.05" y2="25.4" width="0.2032" layer="20"/>
<text>pinoccio v0.1</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="ANTENNA-CHIP5">
</package>
</packages>
</library>
<library name="BeanLabs">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CRYSTAL-SMD-2.5X2-ABM10">
<description>Crystal package for ABM10 16MHz crystal</description>
</package>
<package name="CRYSTAL-SMD-2X1.2-ABS06">
<description>Package for the Abracon ABS06 32k crystal</description>
</package>
</packages>
</library>
<library name="Pinoccio">
<description>Pinoccio Board Devices</description>
<packages>
<package name="QFN-64">
<description>QFN package with a 6x8 pin configuration.</description>
</package>
<package name="BALUN">
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="SHIELDCAN-65X65">
<description>LAIRD: STANDARD SURFACE MOUNT SHIELD TWO-PIECE PART NO. BMI-S-202</description>
</package>
<package name="MICRO-FIDUCIAL">
</package>
<package name="PAD-63-31-RECT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U4" library="Pinoccio" package="QFN-64" value="ATMEGA128RFA1"/>
<element name="C7" library="Pinoccio" package="0402-CAP" value="1.0uF"/>
<element name="C8" library="Pinoccio" package="0402-CAP" value="1.0uF"/>
<element name="C13" library="Pinoccio" package="0402-CAP" value="22pF"/>
<element name="C12" library="Pinoccio" package="0402-CAP" value="22pF"/>
<element name="C15" library="Pinoccio" package="0402-CAP" value="12pF"/>
<element name="C14" library="Pinoccio" package="0402-CAP" value="12pF"/>
<element name="C9" library="Pinoccio" package="0402-CAP" value="1.0pF"/>
<element name="B1" library="Pinoccio" package="BALUN" value="BALUN0805"/>
<element name="Y2" library="SparkFun" package="ANTENNA-CHIP5" value="ANTENNA2SMD5"/>
<element name="C10" library="Pinoccio" package="0402-CAP" value="22pF"/>
<element name="Q1" library="BeanLabs" package="CRYSTAL-SMD-2.5X2-ABM10" value="16MHz"/>
<element name="Q2" library="BeanLabs" package="CRYSTAL-SMD-2X1.2-ABS06" value="32.768k"/>
<element name="C11" library="Pinoccio" package="0402-CAP" value="1.0uF"/>
<element name="C1" library="Pinoccio" package="0402-CAP" value="100nF"/>
<element name="R21" library="Pinoccio" package="0402-RES" value="DNI"/>
<element name="R22" library="Pinoccio" package="0402-RES" value="0"/>
<element name="R23" library="Pinoccio" package="0402-RES" value="DNI"/>
<element name="R24" library="Pinoccio" package="0402-RES" value="0"/>
<element name="C2" library="Pinoccio" package="0402-CAP" value="1.0uF"/>
<element name="U$1" library="Pinoccio" package="SHIELDCAN-65X65" value="SHIELDCAN"/>
<element name="JP1" library="Pinoccio" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
<element name="JP2" library="Pinoccio" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
<element name="PB0" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PB1" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PB2" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PB3" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PB4" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PB5" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PB6" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PB7" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PD0" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PD1" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PD2" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PD3" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PD4" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PD5" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PD6" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PD7" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PE0" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PE1" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PE2" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PE3" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PE4" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PE5" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PE6" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PE7" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PF0" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PF1" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PF2" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PF3" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PF4" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PF5" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PF6" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PF7" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="VCC" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="GND" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PG0" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PG1" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PG2" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="PG5" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="RSTON" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="AREF" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="RSTN" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="U$43" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
<element name="U$44" library="Pinoccio" package="PAD-63-31-RECT" value="PAD"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C12" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="U4" pad="61"/>
<contactref element="U4" pad="58"/>
<contactref element="U4" pad="7"/>
<contactref element="U4" pad="10"/>
<contactref element="U4" pad="20"/>
<contactref element="U4" pad="24"/>
<contactref element="U4" pad="35"/>
<contactref element="U4" pad="45"/>
<contactref element="U4" pad="55"/>
<contactref element="C10" pad="2"/>
<contactref element="U4" pad="11"/>
<contactref element="U4" pad="33"/>
<contactref element="C9" pad="2"/>
<contactref element="B1" pad="6"/>
<contactref element="B1" pad="5"/>
<contactref element="C13" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="R23" pad="2"/>
<contactref element="R21" pad="2"/>
<contactref element="U4" pad="PADDLE"/>
<contactref element="C8" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="GND" pad="P$1"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="U$1" pad="P$5"/>
<contactref element="U$1" pad="P$4"/>
<contactref element="U$1" pad="P$3"/>
<contactref element="U$1" pad="P$9"/>
<contactref element="U$1" pad="P$7"/>
<contactref element="U$1" pad="P$2"/>
<contactref element="U$1" pad="P$8"/>
<contactref element="U$1" pad="P$11"/>
<contactref element="U$1" pad="P$6"/>
<contactref element="U$1" pad="P$10"/>
<contactref element="U$1" pad="P$12"/>
</signal>
<signal name="N$4">
<contactref element="C9" pad="1"/>
<contactref element="B1" pad="1"/>
<contactref element="R22" pad="1"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="C12" pad="1"/>
<contactref element="U4" pad="57"/>
<contactref element="Q1" pad="P$1"/>
</signal>
<signal name="N$16">
<contactref element="C13" pad="1"/>
<contactref element="U4" pad="56"/>
<contactref element="Q1" pad="P$3"/>
</signal>
<signal name="N$17">
<contactref element="U4" pad="17"/>
<contactref element="C14" pad="1"/>
<contactref element="Q2" pad="P$1"/>
</signal>
<signal name="N$18">
<contactref element="C15" pad="1"/>
<contactref element="U4" pad="18"/>
<contactref element="Q2" pad="P$2"/>
</signal>
<signal name="N$20">
<contactref element="U4" pad="21"/>
<contactref element="U4" pad="22"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="U4" pad="60"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="R22" pad="2"/>
<contactref element="R24" pad="1"/>
<contactref element="R23" pad="1"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="R24" pad="2"/>
<contactref element="Y2" pad="FEED"/>
</signal>
<signal name="N$29">
<contactref element="U4" pad="47"/>
<contactref element="PE1" pad="P$1"/>
</signal>
<signal name="N$30">
<contactref element="U4" pad="48"/>
<contactref element="PE2" pad="P$1"/>
</signal>
<signal name="N$31">
<contactref element="U4" pad="49"/>
<contactref element="PE3" pad="P$1"/>
</signal>
<signal name="N$32">
<contactref element="U4" pad="50"/>
<contactref element="PE4" pad="P$1"/>
</signal>
<signal name="N$33">
<contactref element="U4" pad="51"/>
<contactref element="PE5" pad="P$1"/>
</signal>
<signal name="N$34">
<contactref element="U4" pad="52"/>
<contactref element="PE6" pad="P$1"/>
</signal>
<signal name="N$35">
<contactref element="U4" pad="53"/>
<contactref element="PE7" pad="P$1"/>
</signal>
<signal name="N$36">
<contactref element="U4" pad="63"/>
<contactref element="PF0" pad="P$1"/>
</signal>
<signal name="N$37">
<contactref element="U4" pad="64"/>
<contactref element="PF1" pad="P$1"/>
</signal>
<signal name="N$38">
<contactref element="U4" pad="1"/>
<contactref element="PF2" pad="P$1"/>
</signal>
<signal name="N$39">
<contactref element="U4" pad="2"/>
<contactref element="PF3" pad="P$1"/>
</signal>
<signal name="N$40">
<contactref element="U4" pad="3"/>
<contactref element="PF4" pad="P$1"/>
</signal>
<signal name="N$41">
<contactref element="U4" pad="4"/>
<contactref element="PF5" pad="P$1"/>
</signal>
<signal name="N$42">
<contactref element="U4" pad="5"/>
<contactref element="PF6" pad="P$1"/>
</signal>
<signal name="N$44">
<contactref element="U4" pad="14"/>
<contactref element="PG0" pad="P$1"/>
</signal>
<signal name="N$45">
<contactref element="U4" pad="15"/>
<contactref element="PG1" pad="P$1"/>
</signal>
<signal name="N$46">
<contactref element="U4" pad="16"/>
<contactref element="PG2" pad="P$1"/>
</signal>
<signal name="N$47">
<contactref element="U4" pad="19"/>
<contactref element="PG5" pad="P$1"/>
</signal>
<signal name="N$48">
<contactref element="U4" pad="13"/>
<contactref element="RSTON" pad="P$1"/>
</signal>
<signal name="N$49">
</signal>
<signal name="N$50">
</signal>
<signal name="N$13">
<contactref element="C10" pad="1"/>
<contactref element="B1" pad="2"/>
</signal>
<signal name="RFP">
<contactref element="U4" pad="8"/>
<contactref element="B1" pad="4"/>
</signal>
<signal name="RFN">
<contactref element="U4" pad="9"/>
<contactref element="B1" pad="3"/>
</signal>
<signal name="VIN">
</signal>
<signal name="N$1">
<contactref element="U4" pad="36"/>
<contactref element="PB0" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="U4" pad="37"/>
<contactref element="PB1" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="U4" pad="38"/>
<contactref element="PB2" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="U4" pad="39"/>
<contactref element="PB3" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="U4" pad="40"/>
<contactref element="PB4" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="U4" pad="41"/>
<contactref element="PB5" pad="P$1"/>
</signal>
<signal name="N$9">
<contactref element="U4" pad="42"/>
<contactref element="PB6" pad="P$1"/>
</signal>
<signal name="N$11">
<contactref element="U4" pad="43"/>
<contactref element="PB7" pad="P$1"/>
</signal>
<signal name="N$12">
<contactref element="U4" pad="25"/>
<contactref element="PD0" pad="P$1"/>
</signal>
<signal name="N$14">
<contactref element="U4" pad="26"/>
<contactref element="PD1" pad="P$1"/>
</signal>
<signal name="N$19">
<contactref element="U4" pad="27"/>
<contactref element="PD2" pad="P$1"/>
</signal>
<signal name="N$21">
<contactref element="U4" pad="28"/>
<contactref element="PD3" pad="P$1"/>
</signal>
<signal name="N$22">
<contactref element="U4" pad="29"/>
<contactref element="PD4" pad="P$1"/>
</signal>
<signal name="N$23">
<contactref element="U4" pad="30"/>
<contactref element="PD5" pad="P$1"/>
</signal>
<signal name="N$24">
<contactref element="U4" pad="31"/>
<contactref element="PD6" pad="P$1"/>
</signal>
<signal name="N$25">
<contactref element="U4" pad="32"/>
<contactref element="PD7" pad="P$1"/>
</signal>
<signal name="N$26">
<contactref element="U4" pad="46"/>
<contactref element="PE0" pad="P$1"/>
</signal>
<signal name="N$43">
<contactref element="U4" pad="6"/>
<contactref element="PF7" pad="P$1"/>
</signal>
<signal name="VCC">
<contactref element="U4" pad="59"/>
<contactref element="C11" pad="1"/>
<contactref element="VCC" pad="P$1"/>
<contactref element="U4" pad="54"/>
<contactref element="U4" pad="23"/>
<contactref element="C2" pad="1"/>
<contactref element="U4" pad="34"/>
<contactref element="U4" pad="44"/>
</signal>
<signal name="N$52">
<contactref element="U4" pad="62"/>
<contactref element="C1" pad="1"/>
<contactref element="AREF" pad="P$1"/>
</signal>
<signal name="N$53">
<contactref element="U4" pad="12"/>
<contactref element="RSTN" pad="P$1"/>
</signal>
<signal name="N$2">
</signal>
<signal name="N$51">
</signal>
<signal name="N$54">
</signal>
<signal name="N$55">
</signal>
<signal name="N$56">
</signal>
<signal name="N$57">
</signal>
<signal name="N$58">
</signal>
<signal name="N$59">
</signal>
<signal name="N$60">
</signal>
<signal name="N$61">
</signal>
<signal name="N$62">
</signal>
<signal name="N$63">
</signal>
<signal name="N$64">
</signal>
<signal name="N$65">
</signal>
<signal name="N$66">
</signal>
<signal name="N$67">
</signal>
<signal name="N$68">
</signal>
<signal name="N$69">
</signal>
<signal name="N$70">
</signal>
<signal name="N$71">
</signal>
<signal name="N$72">
</signal>
<signal name="N$73">
</signal>
<signal name="N$74">
</signal>
<signal name="N$75">
</signal>
<signal name="N$76">
</signal>
<signal name="N$77">
</signal>
<signal name="N$78">
</signal>
<signal name="N$79">
</signal>
<signal name="N$80">
</signal>
<signal name="N$81">
</signal>
<signal name="N$82">
</signal>
<signal name="N$83">
</signal>
<signal name="N$84">
</signal>
<signal name="N$85">
</signal>
<signal name="N$86">
</signal>
<signal name="N$87">
</signal>
<signal name="N$88">
</signal>
<signal name="N$89">
</signal>
<signal name="N$90">
</signal>
<signal name="N$91">
</signal>
<signal name="N$92">
</signal>
<signal name="N$93">
</signal>
<signal name="N$94">
</signal>
</signals>
</board>
</drawing>
</eagle>
