<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.7.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="18.649" y2="0" width="0" layer="20"/>
<wire x1="18.649" y1="0" x2="18.649" y2="55.931" width="0" layer="20"/>
<wire x1="18.649" y1="55.931" x2="0" y2="55.931" width="0" layer="20"/>
<wire x1="0" y1="55.931" x2="0" y2="0" width="0" layer="20"/>
<text>RPI3 Breakout Rev B (2018)</text>
<text>FF1</text>
<text>FF2</text>
<text>Aardvark</text>
<text>RPI3</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X20">
<description>&lt;h3&gt;Plated Through Hole - 2x20&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:40&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_20x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5">
<description>&lt;h3&gt;Plated Through Hole - 2x5&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="2X20" value="CONN_20X2">
<attribute name="NAME"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="2X5" value="2x5">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08499"/>
<attribute name="SF_ID" value="PRT-0778"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="2X5" value="2x5">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08499"/>
<attribute name="SF_ID" value="PRT-0778"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="2X5" value="2x5">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08499"/>
<attribute name="SF_ID" value="PRT-0778"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J1" pad="9"/>
<contactref element="J1" pad="25"/>
<contactref element="J1" pad="39"/>
<contactref element="J1" pad="6"/>
<contactref element="J1" pad="14"/>
<contactref element="J1" pad="20"/>
<contactref element="J1" pad="30"/>
<contactref element="J1" pad="34"/>
<contactref element="J2" pad="10"/>
<contactref element="J3" pad="10"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="SDA">
<contactref element="J1" pad="3"/>
<contactref element="J2" pad="3"/>
<contactref element="J3" pad="3"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="J1" pad="5"/>
<contactref element="J2" pad="4"/>
<contactref element="J3" pad="4"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="SELECTL1">
<contactref element="J2" pad="8"/>
<contactref element="J1" pad="37"/>
</signal>
<signal name="SELECTL2">
<contactref element="J3" pad="8"/>
<contactref element="J1" pad="32"/>
</signal>
<signal name="INTL1">
<contactref element="J2" pad="5"/>
<contactref element="J1" pad="31"/>
</signal>
<signal name="PRESENTL1">
<contactref element="J2" pad="7"/>
<contactref element="J1" pad="33"/>
</signal>
<signal name="RESETL1">
<contactref element="J2" pad="6"/>
<contactref element="J1" pad="35"/>
</signal>
<signal name="RESETL2">
<contactref element="J3" pad="6"/>
<contactref element="J1" pad="36"/>
</signal>
<signal name="INTL2">
<contactref element="J3" pad="5"/>
<contactref element="J1" pad="38"/>
</signal>
<signal name="PRESENTL2">
<contactref element="J3" pad="7"/>
<contactref element="J1" pad="40"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
