(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(aux_axis_origin 176.53 76.2)
		(pcbplotparams
			(layerselection 0x00010f0_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerbers/")
		)
	)
	(net 0 "")
	(net 1 "VCC")
	(net 2 "/a13?")
	(net 3 "/a13")
	(net 4 "/a15")
	(net 5 "/a1")
	(net 6 "/a11")
	(net 7 "/d3")
	(net 8 "unconnected-(CPU1-nc-Pad36)")
	(net 9 "/a14")
	(net 10 "/a8")
	(net 11 "/a2")
	(net 12 "/d0")
	(net 13 "/a7")
	(net 14 "GND")
	(net 15 "unconnected-(CPU1-SYNC-Pad7)")
	(net 16 "/d1")
	(net 17 "/d6")
	(net 18 "/d4")
	(net 19 "/r~{w}")
	(net 20 "/a12")
	(net 21 "/a5")
	(net 22 "/a9")
	(net 23 "unconnected-(CPU1-ϕ1-Pad3)")
	(net 24 "/a10")
	(net 25 "/a0")
	(net 26 "/d2")
	(net 27 "/a6")
	(net 28 "unconnected-(CPU1-nc-Pad5)")
	(net 29 "/a4")
	(net 30 "unconnected-(CPU1-nc-Pad35)")
	(net 31 "/ϕ0")
	(net 32 "/ϕ2")
	(net 33 "/d7")
	(net 34 "/a3")
	(net 35 "/~{res}")
	(net 36 "/d5")
	(net 37 "unconnected-(RAM1-NC-Pad1)")
	(net 38 "/r~{w}ϕ")
	(net 39 "/~{oe}")
	(net 40 "/~{ce1}")
	(net 41 "/~{ce0}")
	(net 42 "unconnected-(U9-RDY-Pad3)")
	(net 43 "/m12")
	(net 44 "unconnected-(U100-O2-Pad13)")
	(net 45 "unconnected-(U100-O5-Pad10)")
	(net 46 "unconnected-(U100-O4-Pad11)")
	(net 47 "unconnected-(U100-O6-Pad9)")
	(net 48 "unconnected-(U100-O3-Pad12)")
	(net 49 "unconnected-(U101-2A-Pad4)")
	(net 50 "unconnected-(U101-1A-Pad1)")
	(net 51 "unconnected-(U101-1Y-Pad3)")
	(net 52 "unconnected-(U101-2Y-Pad6)")
	(net 53 "unconnected-(U101-1B-Pad2)")
	(net 54 "unconnected-(U101-2B-Pad5)")
	(footprint "Open1050Duplicator:C_Disc_D7.5mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 165.314 85.09 180)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*2.5mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 2.5mm Capacitor")
		(property "Reference" "C2"
			(at 2.5 -1.001 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at 2.5 -1.016 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open1050Duplicator.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "GND")
			(pintype "passive")
		)
		(pad "1" smd rect
			(at 1.8415 0 180)
			(size 0.6096 1.016)
			(layers "F.Cu" "F.Mask")
			(net 14 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.175 0 180)
			(size 0.6096 1.016)
			(layers "F.Cu" "F.Mask")
			(net 1 "VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-14_W7.62mm_Socket_LongPads"
		(layer "F.Cu")
		(at 154.94 77.475 90)
		(descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
		(property "Reference" "U101"
			(at 3.815 7.62 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "74LS00"
			(at 3.81 7.62 180)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS00"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?16*")
		(sheetname "Root")
		(sheetfile "Open1050Duplicator.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 7.62 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "unconnected-(U101-1A-Pad1)")
			(pinfunction "1A")
			(pintype "no_connect")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "unconnected-(U101-1B-Pad2)")
			(pinfunction "1B")
			(pintype "no_connect")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "unconnected-(U101-1Y-Pad3)")
			(pinfunction "1Y")
			(pintype "no_connect")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "unconnected-(U101-2A-Pad4)")
			(pinfunction "2A")
			(pintype "no_connect")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "unconnected-(U101-2B-Pad5)")
			(pinfunction "2B")
			(pintype "no_connect")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "unconnected-(U101-2Y-Pad6)")
			(pinfunction "2Y")
			(pintype "no_connect")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" thru_hole oval
			(at 7.62 15.24 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/~{oe}")
			(pinfunction "3Y")
			(pintype "output")
		)
		(pad "9" thru_hole oval
			(at 7.62 12.7 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/r~{w}")
			(pinfunction "3A")
			(pintype "input")
		)
		(pad "10" thru_hole oval
			(at 7.62 10.16 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/r~{w}")
			(pinfunction "3B")
			(pintype "input")
		)
		(pad "11" thru_hole oval
			(at 7.62 7.62 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "/r~{w}ϕ")
			(pinfunction "4Y")
			(pintype "output")
		)
		(pad "12" thru_hole oval
			(at 7.62 5.08 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/~{oe}")
			(pinfunction "4A")
			(pintype "input")
		)
		(pad "13" thru_hole oval
			(at 7.62 2.54 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/ϕ2")
			(pinfunction "4B")
			(pintype "input")
		)
		(pad "14" thru_hole oval
			(at 7.62 0 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm_Socket.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-16_W7.62mm_Socket_LongPads"
		(layer "F.Cu")
		(at 133.345 77.475 90)
		(descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
		(property "Reference" "U100"
			(at 3.815 8.89 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "74LS138"
			(at 3.815 8.895 180)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS138"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?16*")
		(sheetname "Root")
		(sheetfile "Open1050Duplicator.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 8.89 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/a13")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/a14")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/a15")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "GND")
			(pinfunction "E1")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "GND")
			(pinfunction "E2")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
			(pinfunction "E3")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/~{ce0}")
			(pinfunction "O7")
			(pintype "output")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "9" thru_hole oval
			(at 7.62 17.78 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "unconnected-(U100-O6-Pad9)")
			(pinfunction "O6")
			(pintype "no_connect")
		)
		(pad "10" thru_hole oval
			(at 7.62 15.24 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "unconnected-(U100-O5-Pad10)")
			(pinfunction "O5")
			(pintype "no_connect")
		)
		(pad "11" thru_hole oval
			(at 7.62 12.7 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "unconnected-(U100-O4-Pad11)")
			(pinfunction "O4")
			(pintype "no_connect")
		)
		(pad "12" thru_hole oval
			(at 7.62 10.16 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "unconnected-(U100-O3-Pad12)")
			(pinfunction "O3")
			(pintype "no_connect")
		)
		(pad "13" thru_hole oval
			(at 7.62 7.62 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "unconnected-(U100-O2-Pad13)")
			(pinfunction "O2")
			(pintype "no_connect")
		)
		(pad "14" thru_hole oval
			(at 7.62 5.08 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "/~{ce1}")
			(pinfunction "O1")
			(pintype "output")
		)
		(pad "15" thru_hole oval
			(at 7.62 2.54 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/m12")
			(pinfunction "O0")
			(pintype "output")
		)
		(pad "16" thru_hole oval
			(at 7.62 0 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm_Socket.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 144.78 118.11 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 5.075 0.9652 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4k7"
			(at 5.08 -1.016 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open1050Duplicator.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/a13?")
			(pintype "passive")
		)
		(pad "1" smd rect
			(at 4.3561 0 180)
			(size 0.7366 1.016)
			(layers "F.Cu" "F.Mask")
			(net 2 "/a13?")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 5.8293 0 180)
			(size 0.7366 1.016)
			(layers "F.Cu" "F.Mask")
			(net 1 "VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Open1050Duplicator:C_Disc_D7.5mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 124.46 72.405 180)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*2.5mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 2.5mm Capacitor")
		(property "Reference" "C1"
			(at 2.5 -1.001 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at 2.54 -1.001 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open1050Duplicator.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
			(pintype "passive")
		)
		(pad "1" smd rect
			(at 1.8415 0 180)
			(size 0.6096 1.016)
			(layers "F.Cu" "F.Mask")
			(net 1 "VCC")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.175 0 180)
			(size 0.6096 1.016)
			(layers "F.Cu" "F.Mask")
			(net 14 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-28_W15.24mm_Socket_LongPads"
		(layer "F.Cu")
		(at 154.94 81.295)
		(descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads")
		(tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads")
		(property "Reference" "RAM1"
			(at 7.366 16.495 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "6264 (8x8)"
			(at 7.493 16.495 90)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W15.24mm*")
		(sheetname "Root")
		(sheetfile "Open1050Duplicator.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 16.51 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "unconnected-(RAM1-NC-Pad1)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/a12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/a7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/a6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/a5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/a4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/a3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/a2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/a1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/a0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "11" thru_hole oval
			(at 0 25.4)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/d0")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "12" thru_hole oval
			(at 0 27.94)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/d1")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "13" thru_hole oval
			(at 0 30.48)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/d2")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "14" thru_hole oval
			(at 0 33.02)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "15" thru_hole oval
			(at 15.24 33.02)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/d3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "16" thru_hole oval
			(at 15.24 30.48)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/d4")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "17" thru_hole oval
			(at 15.24 27.94)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/d5")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "18" thru_hole oval
			(at 15.24 25.4)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/d6")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "19" thru_hole oval
			(at 15.24 22.86)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/d7")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "20" thru_hole oval
			(at 15.24 20.32)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "/~{ce1}")
			(pinfunction "~{CE1}")
			(pintype "input")
		)
		(pad "21" thru_hole oval
			(at 15.24 17.78)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/a10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "22" thru_hole oval
			(at 15.24 15.24)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/~{oe}")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "23" thru_hole oval
			(at 15.24 12.7)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/a11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "24" thru_hole oval
			(at 15.24 10.16)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/a9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "25" thru_hole oval
			(at 15.24 7.62)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/a8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "26" thru_hole oval
			(at 15.24 5.08)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
			(pinfunction "CE2")
			(pintype "input")
		)
		(pad "27" thru_hole oval
			(at 15.24 2.54)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "/r~{w}ϕ")
			(pinfunction "RW")
			(pintype "input")
		)
		(pad "28" thru_hole oval
			(at 15.24 0)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-28_W15.24mm_Socket.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 150.749 118.11 -90)
		(descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x02 2.54mm single row")
		(property "Reference" "BS1"
			(at -1.793 1.021 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Bank Select"
			(at -1.778 1.016 180)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper* TestPoint*2Pads* TestPoint*Bridge*")
		(sheetname "Root")
		(sheetfile "Open1050Duplicator.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.77 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/a13?")
			(pinfunction "B")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-40_W15.24mm_Socket_LongPads"
		(layer "F.Cu")
		(at 129.545 118.125 180)
		(descr "40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads")
		(tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads")
		(property "Reference" "CPU1"
			(at 7.625 24.145 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "6502"
			(at 7.62 24.018 90)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.6502.org/documents/datasheets/mos/mos_6500_mpu_mar_1980.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP-40_W15.24mm*")
		(sheetname "Root")
		(sheetfile "Open1050Duplicator.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.366 24.13 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
			(pinfunction "RDY")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(CPU1-ϕ1-Pad3)")
			(pinfunction "ϕ1")
			(pintype "no_connect")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
			(pinfunction "~{IRQ}")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(CPU1-nc-Pad5)")
			(pinfunction "nc")
			(pintype "no_connect")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
			(pinfunction "~{NMI}")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(CPU1-SYNC-Pad7)")
			(pinfunction "SYNC")
			(pintype "no_connect")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/a0")
			(pinfunction "A0")
			(pintype "output")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/a1")
			(pinfunction "A1")
			(pintype "output")
		)
		(pad "11" thru_hole oval
			(at 0 25.4 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/a2")
			(pinfunction "A2")
			(pintype "output")
		)
		(pad "12" thru_hole oval
			(at 0 27.94 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/a3")
			(pinfunction "A3")
			(pintype "output")
		)
		(pad "13" thru_hole oval
			(at 0 30.48 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/a4")
			(pinfunction "A4")
			(pintype "output")
		)
		(pad "14" thru_hole oval
			(at 0 33.02 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/a5")
			(pinfunction "A5")
			(pintype "output")
		)
		(pad "15" thru_hole oval
			(at 0 35.56 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/a6")
			(pinfunction "A6")
			(pintype "output")
		)
		(pad "16" thru_hole oval
			(at 0 38.1 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/a7")
			(pinfunction "A7")
			(pintype "output")
		)
		(pad "17" thru_hole oval
			(at 0 40.64 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/a8")
			(pinfunction "A8")
			(pintype "output")
		)
		(pad "18" thru_hole oval
			(at 0 43.18 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/a9")
			(pinfunction "A9")
			(pintype "output")
		)
		(pad "19" thru_hole oval
			(at 0 45.72 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/a10")
			(pinfunction "A10")
			(pintype "output")
		)
		(pad "20" thru_hole oval
			(at 0 48.26 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/a11")
			(pinfunction "A11")
			(pintype "output")
		)
		(pad "21" thru_hole oval
			(at 15.24 48.26 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "22" thru_hole oval
			(at 15.24 45.72 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/a12")
			(pinfunction "A12")
			(pintype "output")
		)
		(pad "23" thru_hole oval
			(at 15.24 43.18 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/a13")
			(pinfunction "A13")
			(pintype "output")
		)
		(pad "24" thru_hole oval
			(at 15.24 40.64 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/a14")
			(pinfunction "A14")
			(pintype "output")
		)
		(pad "25" thru_hole oval
			(at 15.24 38.1 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/a15")
			(pinfunction "A15")
			(pintype "output")
		)
		(pad "26" thru_hole oval
			(at 15.24 35.56 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/d7")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "27" thru_hole oval
			(at 15.24 33.02 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/d6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "28" thru_hole oval
			(at 15.24 30.48 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/d5")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "29" thru_hole oval
			(at 15.24 27.94 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/d4")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "30" thru_hole oval
			(at 15.24 25.4 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/d3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "31" thru_hole oval
			(at 15.24 22.86 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/d2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "32" thru_hole oval
			(at 15.24 20.32 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/d1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "33" thru_hole oval
			(at 15.24 17.78 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/d0")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "34" thru_hole oval
			(at 15.24 15.24 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/r~{w}")
			(pinfunction "R/~{W}")
			(pintype "output")
		)
		(pad "35" thru_hole oval
			(at 15.24 12.7 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "unconnected-(CPU1-nc-Pad35)")
			(pinfunction "nc")
			(pintype "no_connect")
		)
		(pad "36" thru_hole oval
			(at 15.24 10.16 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "unconnected-(CPU1-nc-Pad36)")
			(pinfunction "nc")
			(pintype "no_connect")
		)
		(pad "37" thru_hole oval
			(at 15.24 7.62 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/ϕ0")
			(pinfunction "ϕ0")
			(pintype "input")
		)
		(pad "38" thru_hole oval
			(at 15.24 5.08 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
			(pinfunction "~{SO}")
			(pintype "input")
		)
		(pad "39" thru_hole oval
			(at 15.24 2.54 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/ϕ2")
			(pinfunction "ϕ2")
			(pintype "output")
		)
		(pad "40" thru_hole oval
			(at 15.24 0 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/~{res}")
			(pinfunction "~{RES}")
			(pintype "input")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-40_W15.24mm_Socket.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-28_W15.24mm_Socket_LongPads"
		(layer "F.Cu")
		(at 134.62 81.295)
		(descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads")
		(tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads")
		(property "Reference" "ROM1"
			(at 7.62 16.495 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2764 (EPROM)"
			(at 7.747 16.495 90)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://downloads.reactivemicro.com/Electronics/ROM/2764%20EPROM.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W15.24mm*")
		(sheetname "Root")
		(sheetfile "Open1050Duplicator.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 16.51 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
			(pinfunction "VPP")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/a12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/a7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/a6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/a5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/a4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/a3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/a2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/a1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/a0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "11" thru_hole oval
			(at 0 25.4)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/d0")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "12" thru_hole oval
			(at 0 27.94)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/d1")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "13" thru_hole oval
			(at 0 30.48)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/d2")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "14" thru_hole oval
			(at 0 33.02)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "15" thru_hole oval
			(at 15.24 33.02)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/d3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "16" thru_hole oval
			(at 15.24 30.48)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/d4")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "17" thru_hole oval
			(at 15.24 27.94)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/d5")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "18" thru_hole oval
			(at 15.24 25.4)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/d6")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "19" thru_hole oval
			(at 15.24 22.86)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/d7")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "20" thru_hole oval
			(at 15.24 20.32)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/~{ce0}")
			(pinfunction "~{CE}")
			(pintype "input")
		)
		(pad "21" thru_hole oval
			(at 15.24 17.78)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/a10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "22" thru_hole oval
			(at 15.24 15.24)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/~{oe}")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "23" thru_hole oval
			(at 15.24 12.7)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/a11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "24" thru_hole oval
			(at 15.24 10.16)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/a9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "25" thru_hole oval
			(at 15.24 7.62)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/a8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "26" thru_hole oval
			(at 15.24 5.08)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/a13?")
			(pinfunction "NC")
			(pintype "input")
		)
		(pad "27" thru_hole oval
			(at 15.24 2.54)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "/r~{w}ϕ")
			(pinfunction "~{PGM}")
			(pintype "input")
		)
		(pad "28" thru_hole oval
			(at 15.24 0)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-28_W15.24mm_Socket.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-28_W15.24mm_LongPads"
		(layer "F.Cu")
		(at 139.685 114.305 180)
		(descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), LongPads")
		(tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil LongPads")
		(property "Reference" "U9"
			(at 12.446 16.51 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "6507 Header"
			(at 7.62 35.35 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.6502.org/documents/datasheets/mos/mos_6500_mpu_mar_1980.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP-28_W15.24mm*")
		(sheetname "Root")
		(sheetfile "Open1050Duplicator.kicad_sch")
		(attr through_hole)
		(fp_text user "Headers to 1050 U9 socket"
			(at 7.62 16.764 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "Pin 1"
			(at -3.698 0 180)
			(layer "B.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 7.62 16.51 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/~{res}")
			(pinfunction "~{RES}")
			(pintype "output")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "unconnected-(U9-RDY-Pad3)")
			(pinfunction "RDY")
			(pintype "no_connect")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/a0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/a1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/a2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/a3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/a4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/a5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "11" thru_hole oval
			(at 0 25.4 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/a6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "12" thru_hole oval
			(at 0 27.94 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/a7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "13" thru_hole oval
			(at 0 30.48 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/a8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "14" thru_hole oval
			(at 0 33.02 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/a9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "15" thru_hole oval
			(at 15.24 33.02 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/a10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "16" thru_hole oval
			(at 15.24 30.48 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/a11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "17" thru_hole oval
			(at 15.24 27.94 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/m12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "18" thru_hole oval
			(at 15.24 25.4 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/d7")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "19" thru_hole oval
			(at 15.24 22.86 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/d6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "20" thru_hole oval
			(at 15.24 20.32 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/d5")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "21" thru_hole oval
			(at 15.24 17.78 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/d4")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "22" thru_hole oval
			(at 15.24 15.24 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/d3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "23" thru_hole oval
			(at 15.24 12.7 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/d2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "24" thru_hole oval
			(at 15.24 10.16 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/d1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "25" thru_hole oval
			(at 15.24 7.62 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/d0")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "26" thru_hole oval
			(at 15.24 5.08 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/r~{w}")
			(pinfunction "R/~{W}")
			(pintype "input")
		)
		(pad "27" thru_hole oval
			(at 15.24 2.54 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/ϕ0")
			(pinfunction "ϕ0")
			(pintype "output")
		)
		(pad "28" thru_hole oval
			(at 15.24 0 180)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/ϕ2")
			(pinfunction "ϕ2")
			(pintype "input")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-28_W15.24mm.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 164.084 109.22 -90)
		(property "Reference" "G***"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 163.449 95.377 -90)
		(property "Reference" "G***"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(gr_arc
		(start 112.395 120.65)
		(mid 111.945987 120.464013)
		(end 111.76 120.015)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.395 120.65)
		(end 172.085 120.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 172.72 120.015)
		(mid 172.534013 120.464013)
		(end 172.085 120.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.085 67.31)
		(end 112.395 67.31)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.76 67.945)
		(end 111.76 120.015)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 111.76 67.945)
		(mid 111.945987 67.495987)
		(end 112.395 67.31)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.72 67.945)
		(end 172.72 120.015)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 172.085 67.31)
		(mid 172.534013 67.495987)
		(end 172.72 67.945)
		(layer "Edge.Cuts")
	)
	(gr_text "To Front\n"
		(at 121.92 118.872 0)
		(layer "B.SilkS")
	)
	(gr_text "Open 1050 Duplicator Redux\nRev 4.2502 Nezgar / Kludgy\n"
		(at 162.814 118.11 0)
		(layer "F.SilkS")
	)
	(zone
		(net 14)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 172.72 120.65) (xy 111.76 120.65) (xy 111.76 67.31) (xy 172.72 67.31)
			)
		)
	)
)
