(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 46)
    (zones 0)
    (modules 13)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 /AGND)
  (net 2 /Audio-Right)
  (net 3 /Audio-Left)
  (net 4 GND)
  (net 5 /SPK-)
  (net 6 /SPK+)
  (net 7 "Net-(R11-Pad2)")
  (net 8 "Net-(R11-Pad1)")
  (net 9 "Net-(R12-Pad2)")
  (net 10 "Net-(T1-Pad5)")
  (net 11 "Net-(T1-Pad2)")
  (net 12 "Net-(T2-Pad2)")
  (net 13 "Net-(T2-Pad5)")
  (net 14 "Net-(J1-Pad10)")
  (net 15 "Net-(J1-Pad11)")
  (net 16 "Net-(R10-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.508)
    (diff_pair_gap 0.508)
    (add_net /AGND)
    (add_net /Audio-Left)
    (add_net /Audio-Right)
    (add_net /SPK+)
    (add_net /SPK-)
    (add_net GND)
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(T1-Pad2)")
    (add_net "Net-(T1-Pad5)")
    (add_net "Net-(T2-Pad2)")
    (add_net "Net-(T2-Pad5)")
  )
  (module SamacSys:400UDP1R1BLKM2RE (layer F.Cu) (tedit 0)
    (at 137.16 49.53 270)
    (descr 400UDP1R1BLKM2RE-3)
    (tags Switch)
    (fp_text reference SW1 (at -1.27 -7.62 90) (layer F.SilkS))
    (fp_text value Mono_Switch (at 2 0.95 90) (layer F.SilkS) hide)
    (fp_text user %R (at 2 0.95 90) (layer F.Fab))
    (pad 6 thru_hole circle (at -2.54 -5.08 270) (size 1.446 1.446) (drill 0.89) (layers *.Cu *.Mask)
      (net 5 /SPK-))
    (pad 5 thru_hole circle (at -2.54 -2.54 270) (size 1.446 1.446) (drill 0.89) (layers *.Cu *.Mask)
      (net 9 "Net-(R12-Pad2)"))
    (pad 4 thru_hole circle (at -2.54 0 270) (size 1.446 1.446) (drill 0.89) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at 0 -5.08 270) (size 1.446 1.446) (drill 0.89) (layers *.Cu *.Mask)
      (net 6 /SPK+))
    (pad 2 thru_hole circle (at 0 -2.54 270) (size 1.446 1.446) (drill 0.89) (layers *.Cu *.Mask)
      (net 8 "Net-(R11-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.446 1.446) (drill 0.89) (layers *.Cu *.Mask)
      (net 5 /SPK-))
    (model "C:\\Users\\ander\\Documents\\Library Loader\\SamacSys_Parts.3dshapes\\400UDP1R1BLKM2RE.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.5mm_Pad_Via (layer F.Cu) (tedit 56DDBAEA)
    (at 210.875825 72.445825)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm_Pad_Via (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.325825 -1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -1.875) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.325825 -1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.875 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.325825 1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 1.875) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.325825 1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.875 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm_Pad_Via (layer F.Cu) (tedit 56DDBAEA)
    (at 138.43 72.39)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm_Pad_Via (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.325825 -1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -1.875) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.325825 -1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.875 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.325825 1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 1.875) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.325825 1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.875 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm_Pad_Via (layer F.Cu) (tedit 56DDBAEA)
    (at 210.82 40.64)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm_Pad_Via (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.325825 -1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -1.875) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.325825 -1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.875 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.325825 1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 1.875) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.325825 1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.875 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm_Pad_Via (layer F.Cu) (tedit 56DDBAEA)
    (at 138.43 40.64)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm_Pad_Via (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.325825 -1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -1.875) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.325825 -1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.875 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.325825 1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 1.875) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.325825 1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.875 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module SamacSys:SHDR3W100P0X500_1X3_1500X900X1290P (layer F.Cu) (tedit 0)
    (at 140.97 55.88 270)
    (descr TB001-500-03BE)
    (tags Connector)
    (fp_text reference J2 (at 3.65 -5.35 90) (layer F.SilkS))
    (fp_text value "JAMMA Audio" (at 3.65 5.55 90) (layer F.Fab))
    (fp_text user %R (at 3.65 3.65 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 10 0 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 /SPK+))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 /SPK-))
    (model "C:\\Users\\ander\\Documents\\Library Loader\\SamacSys_Parts.3dshapes\\TB001-500-03BE.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys:TY145P (layer F.Cu) (tedit 0)
    (at 181.61 52.07 270)
    (descr TY-145P-2)
    (tags Transformer)
    (fp_text reference T2 (at 4.75 -5.334 90) (layer F.SilkS))
    (fp_text value Transformer_1P_SS_2T (at 4.75 -5.334 90) (layer F.SilkS) hide)
    (fp_text user %R (at 4.75 -5.334 90) (layer F.Fab))
    (pad 6 thru_hole circle (at 0 -10.668 270) (size 2.286 2.286) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 /Audio-Right))
    (pad 5 thru_hole circle (at 4.75 -10.668 270) (size 2.286 2.286) (drill 1.524) (layers *.Cu *.Mask)
      (net 13 "Net-(T2-Pad5)"))
    (pad 4 thru_hole circle (at 9.5 -10.668 270) (size 2.286 2.286) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 /AGND))
    (pad 3 thru_hole circle (at 9.5 0 270) (size 2.286 2.286) (drill 1.524) (layers *.Cu *.Mask)
      (net 9 "Net-(R12-Pad2)"))
    (pad 2 thru_hole circle (at 4.75 0 270) (size 2.286 2.286) (drill 1.524) (layers *.Cu *.Mask)
      (net 12 "Net-(T2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.286 2.286) (drill 1.524) (layers *.Cu *.Mask)
      (net 7 "Net-(R11-Pad2)"))
    (model "C:\\Users\\ander\\Documents\\Library Loader\\SamacSys_Parts.3dshapes\\TY-145P.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys:TY145P (layer F.Cu) (tedit 0)
    (at 160.02 52.07 270)
    (descr TY-145P-2)
    (tags Transformer)
    (fp_text reference T1 (at 4.75 -5.334 90) (layer F.SilkS))
    (fp_text value Transformer_1P_SS_2T (at 4.75 -5.334 90) (layer F.SilkS) hide)
    (fp_text user %R (at 4.75 -5.334 90) (layer F.Fab))
    (pad 6 thru_hole circle (at 0 -10.668 270) (size 2.286 2.286) (drill 1.524) (layers *.Cu *.Mask)
      (net 3 /Audio-Left))
    (pad 5 thru_hole circle (at 4.75 -10.668 270) (size 2.286 2.286) (drill 1.524) (layers *.Cu *.Mask)
      (net 10 "Net-(T1-Pad5)"))
    (pad 4 thru_hole circle (at 9.5 -10.668 270) (size 2.286 2.286) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 /AGND))
    (pad 3 thru_hole circle (at 9.5 0 270) (size 2.286 2.286) (drill 1.524) (layers *.Cu *.Mask)
      (net 9 "Net-(R12-Pad2)"))
    (pad 2 thru_hole circle (at 4.75 0 270) (size 2.286 2.286) (drill 1.524) (layers *.Cu *.Mask)
      (net 11 "Net-(T1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.286 2.286) (drill 1.524) (layers *.Cu *.Mask)
      (net 16 "Net-(R10-Pad1)"))
    (model "C:\\Users\\ander\\Documents\\Library Loader\\SamacSys_Parts.3dshapes\\TY-145P.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 148.59 48.26 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R10 (at 2.54 -1.92 90) (layer F.SilkS))
    (fp_text value 390 (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 "Net-(R10-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 /SPK+))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 148.59 60.96 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R11 (at 2.54 -1.92 90) (layer F.SilkS))
    (fp_text value 390 (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(R11-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(R11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 152.4 48.26 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R12 (at 2.54 -1.92 90) (layer F.SilkS))
    (fp_text value 47 (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(R12-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 152.4 60.96 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R13 (at 2.54 -1.92 90) (layer F.SilkS))
    (fp_text value 47 (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(R11-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(R12-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys:SJ13523N (layer F.Cu) (tedit 0)
    (at 210.82 57.15 180)
    (descr SJ1-3523N-1)
    (tags Connector)
    (fp_text reference J1 (at 4.375 0) (layer F.SilkS))
    (fp_text value "Phono Out" (at 4.375 0) (layer F.SilkS) hide)
    (fp_text user %R (at 4.375 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 4.5 0 180) (size 2.55 2.55) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 /AGND))
    (pad 2 thru_hole circle (at 9.5 5 180) (size 2.55 2.55) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 /Audio-Right))
    (pad 3 thru_hole circle (at 9.5 -5 180) (size 2.55 2.55) (drill 1.7) (layers *.Cu *.Mask)
      (net 3 /Audio-Left))
    (pad 10 thru_hole circle (at 9.5 2 180) (size 2.4 2.4) (drill 1.7) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad10)"))
    (pad 11 thru_hole circle (at 9.5 -2 180) (size 2.4 2.4) (drill 1.7) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad11)"))
    (pad MH1 np_thru_hole circle (at 2 -5 180) (size 1.2 0) (drill 1.2) (layers *.Cu *.Mask))
    (pad MH2 np_thru_hole circle (at 4.5 -5 180) (size 1.2 0) (drill 1.2) (layers *.Cu *.Mask))
    (pad MH3 np_thru_hole circle (at 9.5 0 180) (size 1.2 0) (drill 1.2) (layers *.Cu *.Mask))
    (pad MH4 np_thru_hole circle (at 2 5 180) (size 1.2 0) (drill 1.2) (layers *.Cu *.Mask))
    (pad MH5 np_thru_hole circle (at 4.5 5 180) (size 1.2 0) (drill 1.2) (layers *.Cu *.Mask))
    (model "C:\\Users\\ander\\Documents\\Library Loader\\SamacSys_Parts.3dshapes\\SJ1-3523N.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Anders Conbere <anders@conbere.org>" (at 198.12 48.26) (layer B.SilkS))
  (gr_text "Line Converter: V0.1" (at 205.74 46.99) (layer B.SilkS))
  (gr_line (start 215.9 35.56) (end 215.9 77.47) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.35 35.56) (end 215.9 35.56) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.35 77.47) (end 133.35 35.56) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 215.9 77.47) (end 133.35 77.47) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name /AGND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 215.9 77.47) (xy 133.35 77.47) (xy 133.35 35.56) (xy 215.9 35.56)
      )
    )
  )
)
