(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+12V")
  (net 2 "GND")
  (net 3 "-12V")
  (net 4 "Net-(D1-COM)")
  (net 5 "Net-(D2-COM)")
  (net 6 "/FACE")
  (net 7 "Net-(J1-Pin_1)")
  (net 8 "Net-(J1-Pin_10)")
  (net 9 "/+12")
  (net 10 "/-12")
  (net 11 "Net-(C5-Pad1)")
  (net 12 "Net-(Q1-E)")
  (net 13 "Net-(Q2A-B1)")
  (net 14 "Net-(Q2A-C1)")
  (net 15 "Net-(C8-Pad2)")
  (net 16 "Net-(U1A--)")
  (net 17 "Net-(C9-Pad2)")
  (net 18 "Net-(Q2B-C2)")
  (net 19 "Net-(Q2B-B2)")
  (net 20 "Net-(C12-Pad2)")
  (net 21 "Net-(C13-Pad2)")
  (net 22 "Net-(U1B--)")
  (net 23 "Net-(C14-Pad2)")
  (net 24 "Net-(C15-Pad1)")
  (net 25 "Net-(U1C--)")
  (net 26 "Net-(U1C-+)")
  (net 27 "Net-(U1D--)")
  (net 28 "Net-(C17-Pad2)")
  (net 29 "Net-(C19-Pad1)")
  (net 30 "Net-(D3-K)")
  (net 31 "Net-(Q3-D)")
  (net 32 "Net-(D4-K)")
  (net 33 "Net-(D4-A)")
  (net 34 "/IN")
  (net 35 "/RAND")
  (net 36 "unconnected-(J3-PadTN)")
  (net 37 "/GATE")
  (net 38 "/CLK")
  (net 39 "/OUT")
  (net 40 "unconnected-(J5-PadTN)")
  (net 41 "unconnected-(Q1-C-Pad1)")
  (net 42 "Net-(Q3-S)")
  (net 43 "/WHITE")
  (net 44 "/PINK")
  (net 45 "/RANDOM")
  (net 46 "Net-(U2B--)")
  (net 47 "Net-(U2A-+)")
  (net 48 "Net-(U2C--)")
  (net 49 "Net-(SW1A-B)")
  (net 50 "Net-(U2D--)")
  (net 51 "unconnected-(J6-PadTN)")
  (net 52 "Net-(R33-Pad2)")
  (net 53 "Net-(U2D-+)")
  (net 54 "Net-(D5-K)")
  (net 55 "Net-(D5-A)")
  (net 56 "/+12V'")
  (net 57 "/-12V'")
  (net 58 "/WHITE'")
  (net 59 "/RANDOM'")
  (net 60 "/PINK'")
  (net 61 "/GND'")
  (net 62 "Net-(C10-Pad2)")
  (net 63 "Net-(C11-Pad2)")
  (net 64 "Net-(R29-Pad1)")
  (net 65 "Net-(R38-Pad2)")
  (net 66 "Net-(U2A--)")
  (net 67 "unconnected-(RV1-Pad1)")
  (footprint "Eurorack:Mech-AudioJack-Hole-Output-Voct" (layer "F.Cu")
    (at 82.804 129.794)
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H8" (at 0.4 0.1 unlocked) (layer "F.Fab"))
    (fp_text value "out" (at 0 -10.3 unlocked) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 7.7 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 0 -1.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Switch_DPDT_Tayda_A-5752" (layer "F.Cu")
    (at 58.42 85.003)
    (property "PartNum" "A-6677")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Switch, dual pole double throw, separate symbols")
    (property "ki_keywords" "switch dual-pole double-throw DPDT spdt ON-ON")
    (attr through_hole)
    (fp_text reference "SW1" (at 0 -5.08 unlocked) (layer "F.SilkS"))
    (fp_text value "ON-ON-ON" (at 0 5.08 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 2.54 -2.54) (size 1.9 1.9) (drill 1) (layers "*.Cu" "*.Mask")
      (net 60 "/PINK'") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.9 1.9) (drill 1) (layers "*.Cu" "*.Mask")
      (net 49 "Net-(SW1A-B)") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole circle (at 2.54 2.54) (size 1.9 1.9) (drill 1) (layers "*.Cu" "*.Mask")
      (net 59 "/RANDOM'") (pinfunction "C") (pintype "passive"))
    (pad "4" thru_hole circle (at -2.54 -2.54) (size 1.9 1.9) (drill 1) (layers "*.Cu" "*.Mask")
      (net 49 "Net-(SW1A-B)") (pinfunction "A") (pintype "passive"))
    (pad "5" thru_hole circle (at -2.54 0) (size 1.9 1.9) (drill 1) (layers "*.Cu" "*.Mask")
      (net 35 "/RAND") (pinfunction "B") (pintype "passive"))
    (pad "6" thru_hole circle (at -2.54 2.54) (size 1.9 1.9) (drill 1) (layers "*.Cu" "*.Mask")
      (net 58 "/WHITE'") (pinfunction "C") (pintype "passive"))
  )
  (footprint "Eurorack:Mech-Potentiometer-Hole_level_90deg" (layer "F.Cu")
    (at 106.424 124.286)
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H11" (at 0 -9.906 unlocked) (layer "F.Fab"))
    (fp_text value "rate" (at 0 11.43 unlocked) (layer "F.SilkS"))
    (fp_text user "0" (at -5.08 6.35 unlocked) (layer "F.SilkS"))
    (fp_text user "10" (at 6.35 6.35 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 7.62 unlocked) (layer "F.Fab"))
    (pad "" thru_hole oval (at 0 -7.8) (size 3.2 1.4) (drill oval 3 1.2) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 0) (size 12 12) (drill 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (at 55.023 106.983)
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H1" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "mount0" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "output"))
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (at 55.023 140.633)
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H4" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "mount1" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 113.284 60.979 180)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J12" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x03_Socket" (at 0 7.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Input-Gate" (layer "F.Cu")
    (at 70.612 118.618)
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H5" (at 0.4 0.1 unlocked) (layer "F.Fab"))
    (fp_text value "gate" (at 0 -10.3 unlocked) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 7.7 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 0 -1.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Output-Clock" (layer "F.Cu")
    (at 82.804 118.618)
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H10" (at 0.4 0.1 unlocked) (layer "F.Fab"))
    (fp_text value "clock" (at 0 -10.3 unlocked) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 7.7 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 0 -1.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Potentiometer_RV16AF-41-15R1" (layer "F.Cu")
    (at 106.424 90.671 -90)
    (descr "Alpha 16mm Potentiometer Single -- Tayda Electronics ")
    (property "PartNum" "A-3940")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Potentiometer")
    (property "ki_keywords" "resistor variable")
    (attr through_hole)
    (fp_text reference "RV1" (at -9.906 3.556 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "C500K" (at 0 3.556 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.334 -90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -5 16 270) (size 2.2 2.2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 67 "unconnected-(RV1-Pad1)") (pinfunction "1") (pintype "passive+no_connect"))
    (pad "2" thru_hole circle (at 0 16 270) (size 2.2 2.2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 52 "Net-(R33-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 16 270) (size 2.2 2.2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 55 "Net-(D5-A)") (pinfunction "3") (pintype "passive"))
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 82.804 96.179)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J5" (at 5.969 3.302 unlocked) (layer "F.SilkS"))
    (fp_text value "AudioJack2_SwitchT" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 61 "/GND'") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 61 "/GND'") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 39 "/OUT") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 40 "unconnected-(J5-PadTN)") (pintype "passive+no_connect"))
    (model "/home/pstiverson/Projects/AR-808/hardware/EurorackKiCAD/Eurorack.pretty/models3d/A-2566.wrl"
      (offset (xyz 0 -0.15 11.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-2M_Switch-Hole" (layer "F.Cu")
    (at 58.42 118.618)
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H9" (at 0 -4.445 unlocked) (layer "F.SilkS") hide)
    (fp_text value "switch" (at 0 4.445 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 7 7) (drill 4.95) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (at 110.723 106.983)
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H2" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "mount1" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 52.324 62.503)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J8" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x03_Socket" (at 0 7.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 43 "/WHITE") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 45 "/RANDOM") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 44 "/PINK") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 113.538 74.441 180)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J10" (at 0 7.351) (layer "F.SilkS"))
    (fp_text value "Conn_01x03_Socket" (at 0 7.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (at 110.723 140.633)
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H3" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "mount1" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Input-Voct" (layer "F.Cu")
    (at 70.612 129.794)
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H6" (at 0.4 0.1 unlocked) (layer "F.Fab"))
    (fp_text value "in" (at 0 -10.3 unlocked) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 7.7 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 0 -1.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 70.612 85.003)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J4" (at 5.842 -4.572 unlocked) (layer "F.SilkS"))
    (fp_text value "AudioJack2_SwitchT" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 61 "/GND'") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 61 "/GND'") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 37 "/GATE") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 38 "/CLK") (pintype "passive"))
    (model "/home/pstiverson/Projects/AR-808/hardware/EurorackKiCAD/Eurorack.pretty/models3d/A-2566.wrl"
      (offset (xyz 0 -0.15 11.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Output-Voct" (layer "F.Cu")
    (at 58.42 129.794)
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H7" (at 0.4 0.1 unlocked) (layer "F.Fab"))
    (fp_text value "rand" (at 0 -10.3 unlocked) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 7.7 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 0 -1.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 70.612 96.179)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J2" (at 5.842 -4.572 unlocked) (layer "F.SilkS"))
    (fp_text value "AudioJack2_SwitchT" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 61 "/GND'") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 61 "/GND'") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 34 "/IN") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 35 "/RAND") (pintype "passive"))
    (model "/home/pstiverson/Projects/AR-808/hardware/EurorackKiCAD/Eurorack.pretty/models3d/A-2566.wrl"
      (offset (xyz 0 -0.15 11.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 82.804 85.003)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J6" (at 5.842 -4.826 unlocked) (layer "F.SilkS"))
    (fp_text value "AudioJack2_SwitchT" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 61 "/GND'") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 61 "/GND'") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 38 "/CLK") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 51 "unconnected-(J6-PadTN)") (pintype "passive+no_connect"))
    (model "/home/pstiverson/Projects/AR-808/hardware/EurorackKiCAD/Eurorack.pretty/models3d/A-2566.wrl"
      (offset (xyz 0 -0.15 11.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 58.42 96.179)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J3" (at 5.842 -4.572 unlocked) (layer "F.SilkS"))
    (fp_text value "AudioJack2_SwitchT" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 61 "/GND'") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 61 "/GND'") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 35 "/RAND") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 36 "unconnected-(J3-PadTN)") (pintype "passive+no_connect"))
    (model "/home/pstiverson/Projects/AR-808/hardware/EurorackKiCAD/Eurorack.pretty/models3d/A-2566.wrl"
      (offset (xyz 0 -0.15 11.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "B.Cu")
    (at 52.324 87.543 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J7" (at 0 2.33) (layer "B.SilkS"))
    (fp_text value "Conn_01x03_Pin" (at 0 -7.41) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.54 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 58 "/WHITE'") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 59 "/RANDOM'") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 60 "/PINK'") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 70.612 96.687 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R29" (at -2.286 -1.524) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 64 "Net-(R29-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 61 "/GND'") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm" (layer "B.Cu")
    (at 88.545 67.706621 -90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C5" (at 1.944379 -4.318 -180) (layer "B.SilkS"))
    (fp_text value "47u 50V" (at 1.25 -4.4 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 99.3981 69.8977)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 1.651 1.651) (layer "B.SilkS"))
    (fp_text value "10" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(D1-COM)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 7 "Net-(J1-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 97.028 88.559 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R27" (at 0.254 -1.778 90) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 56 "/+12V'") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 48 "Net-(U2C--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "B.Cu")
    (at 93.599 83.374113 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C21" (at 1.586113 -4.064 180) (layer "B.SilkS"))
    (fp_text value "10u 35V" (at 1.25 -3.75 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 50 "Net-(U2D--)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 57 "/-12V'") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm" (layer "B.Cu")
    (at 87.021 58.475 -90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C6" (at 4.826 2.794 -180) (layer "B.SilkS"))
    (fp_text value "47u 50V" (at 1.25 -4.4 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(Q1-E)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(Q2A-B1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 64.923 56.443 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R10" (at 0.127 -1.524 90) (layer "B.SilkS"))
    (fp_text value "470K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 16 "Net-(U1A--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 17 "Net-(C9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 56.287 68.127)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R20" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "33K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 23 "Net-(C14-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 24 "Net-(C15-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 93.599 86.741 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R33" (at 1.397 1.524 -90) (layer "B.SilkS"))
    (fp_text value "2.2K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 50 "Net-(U2D--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 52 "Net-(R33-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323_HandSoldering" (layer "B.Cu")
    (at 87.249 92.583 -90)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D5" (at 0 1.85 90) (layer "B.SilkS"))
    (fp_text value "1N4148" (at 0.1 -1.9 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.85 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.25 0 270) (size 1 1) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(D5-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.25 0 270) (size 1 1) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(D5-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323_HandSoldering" (layer "B.Cu")
    (at 100.076 83.733 90)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D3" (at 3.048 0 90) (layer "B.SilkS"))
    (fp_text value "1N4148" (at 0.1 -1.9 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.85 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.25 0 90) (size 1 1) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(D3-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.25 0 90) (size 1 1) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 61 "/GND'") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 103.124 97.663 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R38" (at 2.54 -0.127) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 47 "Net-(U2A-+)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 65 "Net-(R38-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 68.987 64.063 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C7" (at 2.794 -0.254 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "/+12") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "/-12") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 56.287 64.825 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R19" (at 0 -1.524) (layer "B.SilkS"))
    (fp_text value "1K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 23 "Net-(C14-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 44 "/PINK") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "B.Cu")
    (at 76.796112 56.951 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C13" (at -2.070888 2.341) (layer "B.SilkS"))
    (fp_text value "10u 35V" (at 1.25 -3.75) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(Q2B-C2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(C13-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (at 98.1281 63.5477 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PartNum" "863-BAT54SLT1G")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Vr 30V, If 200mA, Dual schottky barrier diode, in series, SOT-323")
    (property "ki_keywords" "schottky diode")
    (attr smd)
    (fp_text reference "D2" (at -1.0087 2.4 90) (layer "B.SilkS"))
    (fp_text value "BAT54S" (at 0 -2.4 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "K") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D2-COM)") (pinfunction "COM") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 106.934 83.733 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R35" (at -3.048 0 90) (layer "B.SilkS"))
    (fp_text value "120K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 53 "Net-(U2D-+)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 55 "Net-(D5-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 106.2755 98.679 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R40" (at 0 -1.778) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 61 "/GND'") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 66 "Net-(U2A--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 61.621 56.443 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C9" (at 1.397 -1.524 90) (layer "B.SilkS"))
    (fp_text value "10p" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(U1A--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(C9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (layer "B.Cu")
    (at 94.234 96.647 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C20" (at -2.072 -0.762) (layer "B.SilkS"))
    (fp_text value "100n box" (at 2.5 -2.5 270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 270) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(Q3-D)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 61 "/GND'") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 99.3981 67.3577)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 1.651 -1.778) (layer "B.SilkS"))
    (fp_text value "10" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 5 "Net-(D2-COM)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 8 "Net-(J1-Pin_10)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (at 98.1281 73.7077 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PartNum" "863-BAT54SLT1G")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Vr 30V, If 200mA, Dual schottky barrier diode, in series, SOT-323")
    (property "ki_keywords" "schottky diode")
    (attr smd)
    (fp_text reference "D1" (at -2.667 1.524) (layer "B.SilkS"))
    (fp_text value "BAT54S" (at 0 -2.4 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "K") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D1-COM)") (pinfunction "COM") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 95.7386 69.2627 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 2.5635 0.762) (layer "B.SilkS"))
    (fp_text value "10" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 3 "-12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 10 "/-12") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 89.053 55.173 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at -1.016 -1.524) (layer "B.SilkS"))
    (fp_text value "47K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 11 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 12 "Net-(Q1-E)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 104.648 83.733 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R34" (at 3.048 0 90) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 53 "Net-(U2D-+)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 61 "/GND'") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 97.79 83.733 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R28" (at -3.048 0 -270) (layer "B.SilkS"))
    (fp_text value "10K" (at 0 -1.65 -270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 61 "/GND'") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 48 "Net-(U2C--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:PinHeader_2x05_P2.54mm_Vertical" (layer "B.Cu")
    (at 105.7354 70.4946)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (property "PartNum" "A-2939")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at -4.4323 4.4831) (layer "B.SilkS"))
    (fp_text value "Conn_02x05_Odd_Even" (at 1.2446 -16.2052) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -5.08 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J1-Pin_1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 -5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 -7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J1-Pin_10)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 2.54 -10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J1-Pin_10)") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 71.527 56.443 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R17" (at 0 1.65 -270) (layer "B.SilkS"))
    (fp_text value "8.2K" (at 0 -1.65 -270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 21 "Net-(C13-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 22 "Net-(U1B--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (layer "B.Cu")
    (at 75.337 74.223)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C11" (at -3.175 1.524 180) (layer "B.SilkS"))
    (fp_text value "1n box" (at 2.5 -2.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(Q2B-B2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 63 "Net-(C11-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 56.287 61.523 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R24" (at 0 -1.524) (layer "B.SilkS"))
    (fp_text value "1K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 28 "Net-(C17-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 45 "/RANDOM") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 78.3355 64.897)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R12" (at 3.022 -0.127) (layer "B.SilkS"))
    (fp_text value "82K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 19 "Net-(Q2B-B2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 14 "Net-(Q2A-C1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 70.612 83.225 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R25" (at -3.048 0) (layer "B.SilkS"))
    (fp_text value "1K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 37 "/GATE") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 29 "Net-(C19-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 52.731 59.745 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R11" (at -3.048 0.254) (layer "B.SilkS"))
    (fp_text value "1K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 17 "Net-(C9-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 43 "/WHITE") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "B.Cu")
    (at 63.145 62.539 -90)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PartNum" "595-TL074CDR")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Quad Low-Noise JFET-Input Operational Amplifiers, DIP-14/SOIC-14")
    (property "ki_keywords" "quad opamp")
    (attr smd)
    (fp_text reference "U1" (at -2.794 5.28 90) (layer "B.SilkS"))
    (fp_text value "TL074" (at 0 -5.28 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.475 3.81 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(C9-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -2.475 2.54 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(U1A--)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 1.27 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 0 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "/+12") (pinfunction "V+") (pintype "power_in"))
    (pad "5" smd roundrect (at -2.475 -1.27 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at -2.475 -2.54 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(U1B--)") (pinfunction "-") (pintype "input"))
    (pad "7" smd roundrect (at -2.475 -3.81 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(C14-Pad2)") (pintype "output"))
    (pad "8" smd roundrect (at 2.475 -3.81 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(U1C--)") (pintype "output"))
    (pad "9" smd roundrect (at 2.475 -2.54 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(U1C--)") (pinfunction "-") (pintype "input"))
    (pad "10" smd roundrect (at 2.475 -1.27 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(U1C-+)") (pinfunction "+") (pintype "input"))
    (pad "11" smd roundrect (at 2.475 0 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "/-12") (pinfunction "V-") (pintype "power_in"))
    (pad "12" smd roundrect (at 2.475 1.27 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "+") (pintype "input"))
    (pad "13" smd roundrect (at 2.475 2.54 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(U1D--)") (pinfunction "-") (pintype "input"))
    (pad "14" smd roundrect (at 2.475 3.81 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(C17-Pad2)") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "B.Cu")
    (at 113.538 99.481)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J9" (at -0.254 -7.62) (layer "B.SilkS"))
    (fp_text value "Conn_01x03_Pin" (at 0 -7.41) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.54 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 56 "/+12V'") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 56 "/+12V'") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 61 "/GND'") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 72.035 60.253 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C14" (at 0.326 -1.625 90) (layer "B.SilkS"))
    (fp_text value "10p" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(U1B--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(C14-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 59.589 68.381 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R23" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "220K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 27 "Net-(U1D--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 28 "Net-(C17-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 87.529 64.317 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at 2.794 -0.508) (layer "B.SilkS"))
    (fp_text value "10K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 11 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 14 "Net-(Q2A-C1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 109.8785 94.488)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R42" (at 1.1195 -2.413 90) (layer "B.SilkS"))
    (fp_text value "24K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 65 "Net-(R38-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 61 "/GND'") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 82.804 83.733 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R36" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "1K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 54 "Net-(D5-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 38 "/CLK") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 70.612 93.893)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R30" (at 3.048 0) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 34 "/IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 64 "Net-(R29-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 88.545 73.715 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at 0.254 -1.778) (layer "B.SilkS"))
    (fp_text value "22" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 9 "/+12") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 11 "Net-(C5-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 109.855 96.647 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R43" (at -0.127 -1.778 180) (layer "B.SilkS"))
    (fp_text value "33K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 56 "/+12V'") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 65 "Net-(R38-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 102.362 83.733 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R26" (at 3.048 0 90) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 30 "Net-(D3-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 61 "/GND'") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 82.917 74.477 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R14" (at 0 -1.524 -90) (layer "B.SilkS"))
    (fp_text value "18K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 18 "Net-(Q2B-C2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 63 "Net-(C11-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "B.Cu")
    (at 103.124 90.78 90)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PartNum" "595-TL074CDR")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Quad Low-Noise JFET-Input Operational Amplifiers, DIP-14/SOIC-14")
    (property "ki_keywords" "quad opamp")
    (attr smd)
    (fp_text reference "U2" (at -2.184 5.588 180) (layer "B.SilkS"))
    (fp_text value "TL074" (at 0 -5.28 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.475 3.81 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(Q3-S)") (pintype "output"))
    (pad "2" smd roundrect (at -2.475 2.54 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(U2A--)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 1.27 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(U2A-+)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 0 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 56 "/+12V'") (pinfunction "V+") (pintype "power_in"))
    (pad "5" smd roundrect (at -2.475 -1.27 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(Q3-D)") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at -2.475 -2.54 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(U2B--)") (pinfunction "-") (pintype "input"))
    (pad "7" smd roundrect (at -2.475 -3.81 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(U2B--)") (pintype "output"))
    (pad "8" smd roundrect (at 2.475 -3.81 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(D4-K)") (pintype "output"))
    (pad "9" smd roundrect (at 2.475 -2.54 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(U2C--)") (pinfunction "-") (pintype "input"))
    (pad "10" smd roundrect (at 2.475 -1.27 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(D3-K)") (pinfunction "+") (pintype "input"))
    (pad "11" smd roundrect (at 2.475 0 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 57 "/-12V'") (pinfunction "V-") (pintype "power_in"))
    (pad "12" smd roundrect (at 2.475 1.27 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(U2D-+)") (pinfunction "+") (pintype "input"))
    (pad "13" smd roundrect (at 2.475 2.54 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(U2D--)") (pinfunction "-") (pintype "input"))
    (pad "14" smd roundrect (at 2.475 3.81 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(D5-A)") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.2mm_W5.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (layer "B.Cu")
    (at 52.009 73.461)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C15" (at 7.072 -1.778 -90) (layer "B.SilkS"))
    (fp_text value "1u box" (at 2.5 -4) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(C15-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(U1C--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W5.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 82.917 70.921 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R13" (at 0 -1.524 -270) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65 -270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 18 "Net-(Q2B-C2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 20 "Net-(C12-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSOP-6_1.65x3.05mm_P0.95mm" (layer "B.Cu")
    (at 74.575 64.063 -90)
    (descr "TSOP-6 package (comparable to TSOT-23), https://www.vishay.com/docs/71200/71200.pdf")
    (tags "Jedec MO-193C TSOP-6L")
    (property "PartNum" "771-BCM847DS135")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Dual NPN transistor, 6 pin package")
    (property "ki_keywords" "transistor NPN")
    (attr smd)
    (fp_text reference "Q2" (at -1.198 -2.387 -90) (layer "B.SilkS"))
    (fp_text value "BCM847" (at 0 -2.5 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect (at -1.16 0.95 270) (size 0.7 0.51) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "E1") (pintype "passive"))
    (pad "2" smd rect (at -1.16 0 270) (size 0.7 0.51) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "Net-(Q2A-B1)") (pinfunction "B1") (pintype "input"))
    (pad "3" smd rect (at -1.16 -0.95 270) (size 0.7 0.51) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "Net-(Q2B-C2)") (pinfunction "C2") (pintype "passive"))
    (pad "4" smd rect (at 1.16 -0.95 270) (size 0.7 0.51) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "E2") (pintype "passive"))
    (pad "5" smd rect (at 1.16 0 270) (size 0.7 0.51) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "Net-(Q2B-B2)") (pinfunction "B2") (pintype "input"))
    (pad "6" smd rect (at 1.16 0.95 270) (size 0.7 0.51) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "Net-(Q2A-C1)") (pinfunction "C1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSOP-6_1.65x3.05mm_P0.95mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.2mm_W3.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (layer "B.Cu")
    (at 57.049 56.443 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*3.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 3.5mm Capacitor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C17" (at -2.032 -0.762 90) (layer "B.SilkS"))
    (fp_text value "150n box" (at 2.5 -3) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(U1D--)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(C17-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W3.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "B.Cu")
    (at 99.467 59.1027 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at -2.1663 1.524) (layer "B.SilkS"))
    (fp_text value "22u 50V" (at 1.25 -3.75 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323_HandSoldering" (layer "B.Cu")
    (at 97.028 92.877 -90)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D4" (at 2.5 0 -180) (layer "B.SilkS"))
    (fp_text value "1N4148" (at 0.1 -1.9 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.85 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.25 0 270) (size 1 1) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(D4-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.25 0 270) (size 1 1) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(D4-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "B.Cu")
    (at 93.625 56.5627 -90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C2" (at 4.445 -1.905) (layer "B.SilkS"))
    (fp_text value "22u 50V" (at 1.25 -3.75 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 82.804 94.909 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R32" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "1K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 46 "Net-(U2B--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 39 "/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 69.749 60.253 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R18" (at 0 1.397 -270) (layer "B.SilkS"))
    (fp_text value "470K" (at 0 -1.65 -270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 22 "Net-(U1B--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 23 "Net-(C14-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 106.299 96.52 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R39" (at 0 1.397 180) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 42 "Net-(Q3-S)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 66 "Net-(U2A--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (layer "B.Cu")
    (at 75.337 67.619)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C10" (at -2.794 -0.508 180) (layer "B.SilkS"))
    (fp_text value "47n box" (at 2.5 -2.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(Q2B-B2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 62 "Net-(C10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "B.Cu")
    (at 113.284 86.019)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J11" (at 0 2.33) (layer "B.SilkS"))
    (fp_text value "Conn_01x03_Pin" (at 0 -7.41) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.54 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 61 "/GND'") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 57 "/-12V'") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 57 "/-12V'") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 76.2235 60.706)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R41" (at 2.3895 1.397 -90) (layer "B.SilkS"))
    (fp_text value "3.9K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 9 "/+12") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 18 "Net-(Q2B-C2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "B.Cu")
    (at 71.019 73.650113 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C8" (at -1.842887 -1.778 180) (layer "B.SilkS"))
    (fp_text value "10u 35V" (at 1.25 -3.75 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(Q2A-C1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(C8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (at 98.171 97.703 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PartNum" "863-MMBF4393LT1G")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "5mA min, 30V, 100mOhm max, 0.5-3V Vgs(off), N-Channel JFET, SOT-23")
    (property "ki_keywords" "N-Channel FET Transistor")
    (attr smd)
    (fp_text reference "Q3" (at 2.54 1.016 -180) (layer "B.SilkS"))
    (fp_text value "MMBFJ111" (at 0 -2.4 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(Q3-D)") (pinfunction "D") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(Q3-S)") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(D4-A)") (pinfunction "G") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline_Wide" (layer "B.Cu")
    (at 80.565 61.015 90)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "PartNum" "637-BC547C")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "0.1A Ic, 45V Vce, Small Signal NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (attr through_hole)
    (fp_text reference "Q1" (at -0.58 2.239 180) (layer "B.SilkS"))
    (fp_text value "BC547C" (at 2.54 -2.79 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 41 "unconnected-(Q1-C-Pad1)") (pinfunction "C") (pintype "passive+no_connect"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole circle (at 5.08 0 90) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(Q1-E)") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "B.Cu")
    (at 93.3021 74.404812 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C4" (at -1.342188 -2.4711) (layer "B.SilkS"))
    (fp_text value "22u 50V" (at 1.25 -3.75 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "/-12") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 108.966 90.591 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C18" (at 3.215 0 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 56 "/+12V'") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 57 "/-12V'") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 70.612 85.511)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C19" (at 2.286 1.524) (layer "B.SilkS"))
    (fp_text value "1n" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(C19-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(D3-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 95.7386 66.7227 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 2.5635 -0.508) (layer "B.SilkS"))
    (fp_text value "10" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 9 "/+12") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (layer "B.Cu")
    (at 75.337 70.921)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C12" (at -2.794 -2.032 180) (layer "B.SilkS"))
    (fp_text value "3.3n box" (at 2.5 -2.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(Q2B-B2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(C12-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 100.965 97.703 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R31" (at -2.5 -0.635 180) (layer "B.SilkS"))
    (fp_text value "2.2M" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 33 "Net-(D4-A)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 42 "Net-(Q3-S)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 62.891 68.381 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R22" (at 0 -1.524 -270) (layer "B.SilkS"))
    (fp_text value "10K" (at 0 -1.65 -270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 25 "Net-(U1C--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 27 "Net-(U1D--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 66.193 68.381 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R21" (at -0.254 1.65 90) (layer "B.SilkS"))
    (fp_text value "33K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 24 "Net-(C15-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 26 "Net-(U1C-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 71.527 64.063 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R16" (at 3.302 1.016 90) (layer "B.SilkS"))
    (fp_text value "1M" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 18 "Net-(Q2B-C2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 19 "Net-(Q2B-B2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 85.243 55.173 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 2.54 0.254) (layer "B.SilkS"))
    (fp_text value "150K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 14 "Net-(Q2A-C1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 13 "Net-(Q2A-B1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.2mm_W5.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (layer "B.Cu")
    (at 61.661 73.461)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C16" (at -1.818 1.27 90) (layer "B.SilkS"))
    (fp_text value "1u box" (at 2.5 -4) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(U1C-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W5.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "B.Cu")
    (at 92.1591 64.879812 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C3" (at -0.199188 3.4979) (layer "B.SilkS"))
    (fp_text value "22u 50V" (at 1.2265 -3.115 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "/+12") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 76.581 91.313)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R37" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 64 "Net-(R29-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 47 "Net-(U2A-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 82.917 67.111 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R15" (at 0 1.524 90) (layer "B.SilkS"))
    (fp_text value "390K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 18 "Net-(Q2B-C2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 62 "Net-(C10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 68.225 56.443 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sample-hold.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R9" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "33K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 15 "Net-(C8-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 16 "Net-(U1A--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 50.023 103.983) (end 115.723 143.633)
    (fill none) (layer "Edge.Cuts"))
  (gr_rect (start 50.023 53.903) (end 115.723 76.403)
    (fill none) (layer "Edge.Cuts"))
  (gr_rect (start 50.023 78.943) (end 115.723 101.443)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "thismatters/sample-hold/v0" (at 114.935 65.405 90) (layer "B.SilkS"))
  (gr_text "thismatters/sample-hold/v0" (at 51.054 126.492 90) (layer "F.SilkS"))
  (gr_text "wht" (at 58.418 113.364) (layer "F.SilkS"))
  (gr_text "sample" (at 70.61 135.97) (layer "F.SilkS"))
  (gr_text "gate" (at 70.61 111.76) (layer "F.SilkS"))
  (gr_text "clk" (at 82.802 111.76) (layer "F.SilkS"))
  (gr_text "pink" (at 58.418 123.524) (layer "F.SilkS"))
  (gr_text "slo" (at 63.752 118.444 90) (layer "F.SilkS"))
  (gr_text "held" (at 82.802 135.97) (layer "F.SilkS"))
  (gr_text "noise" (at 58.418 135.97) (layer "F.SilkS"))
  (gr_text "noise / sample" (at 83.564 142.574) (layer "F.SilkS"))
  (gr_text "thismatters/sample-hold/v0" (at 100.838 100.33) (layer "F.SilkS"))
  (zone (net 6) (net_name "/FACE") (layers "F&B.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 116.655 103.221)
        (xy 116.655 144.75)
        (xy 49.218 144.75)
        (xy 49.218 103.221)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 116.231 53.268)
        (xy 116.231 77.144)
        (xy 49.302 77.144)
        (xy 49.302 53.268)
      )
    )
  )
  (zone (net 61) (net_name "/GND'") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 116.332 78.399)
        (xy 116.332 102.275)
        (xy 49.53 102.275)
        (xy 49.53 78.399)
      )
    )
  )
)
