(kicad_pcb (version 4) (host pcbnew 4.0.7-e1-6374~58~ubuntu16.04.1)
  (general
    (links 23)
    (no_connects 0)
    (area 96.957599 60.179952 141.280001 105.164089)
    (thickness 1.6)
    (drawings 24)
    (tracks 66)
    (zones 0)
    (modules 16)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(F1-Pad1)")
  (net 3 "Net-(F1-Pad2)")
  (net 4 "Net-(J1-Pad1)")
  (net 5 +3V3)
  (net 6 "Net-(J3-Pad1)")
  (net 7 "Net-(J4-Pad1)")
  (net 8 "Net-(D1-Pad2)")
  (net 9 "Net-(J5-Pad1)")
  (net 10 "Net-(D2-Pad2)")
  (net 11 "Net-(Q1-Pad1)")
  (net 12 "Net-(R1-Pad1)")
  (net 13 "Net-(R1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R1-Pad2)")
  )
  (net_class 240V_B_CU ""
    (clearance 0.2)
    (trace_width 1.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J3-Pad1)")
  )
  (net_class 240V_F_CU ""
    (clearance 0.2)
    (trace_width 2.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J5-Pad1)")
  )
  (module suf_power_module:HLK-PM01 (layer F.Cu) (tedit 5987F362)
    (at 128.28 77.36 90)
    (fp_text reference U1 (at 0.13 -3.78 270) (layer F.SilkS))
    (fp_text value HLK-PM05 (at -0.03 -2.05 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -14.7 -2.5 90) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(F1-Pad2)"))
    (pad 2 thru_hole circle (at -14.7 2.5 90) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J3-Pad1)"))
    (pad 3 thru_hole circle (at 14.7 -7.7 90) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole circle (at 14.7 7.8 90) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 +3V3))
  )
  (module wemos_d1_mini:D1_mini_board (layer B.Cu) (tedit 5977340D)
    (at 128.28 76.64)
    (fp_text reference U2 (at 6.76 0.44 180) (layer B.SilkS))
    (fp_text value WeMos_mini (at 0.12 17.31) (layer B.Fab))
    (pad 8 thru_hole circle (at -11.43 10.16) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 7 thru_hole circle (at -11.43 7.62) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 6 thru_hole circle (at -11.43 5.08) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 5 thru_hole circle (at -11.43 2.54) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 4 thru_hole circle (at -11.43 0) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 3 thru_hole circle (at -11.43 -2.54) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 2 thru_hole circle (at -11.43 -5.08) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 1 thru_hole circle (at -11.43 -7.62) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 16 thru_hole circle (at 11.43 -7.62) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 15 thru_hole circle (at 11.43 -5.08) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 14 thru_hole circle (at 11.43 -2.54) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 13 thru_hole circle (at 11.43 0) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 8 "Net-(D1-Pad2)"))
    (pad 12 thru_hole circle (at 11.43 2.54) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 12 "Net-(R1-Pad1)"))
    (pad 11 thru_hole circle (at 11.43 5.08) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 10 thru_hole circle (at 11.43 7.62) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
    (pad 9 thru_hole circle (at 11.43 10.16) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 59732B88)
    (at 99.53 102.21)
    (fp_text reference J1 (at 1.58 -2.94) (layer F.SilkS))
    (fp_text value LOAD_NO (at 9.21 0.16) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)"))
  )
  (module Fuse_Holders_and_Fuses:Fuseholder_Fuse_TR5_Littlefuse-No560_No460 (layer F.Cu) (tedit 59732BCA)
    (at 122.94 102.36 90)
    (descr "Fuse, Fuseholder, TR5, Littlefuse/Wickmann, No. 460, No560,")
    (tags "Fuse Fuseholder TR5 Littlefuse/Wickmann No. 460 No560 ")
    (fp_text reference F1 (at 0.93 -2.48 360) (layer F.SilkS))
    (fp_text value TR5-50ma (at 2.42 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(F1-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0.01 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(F1-Pad2)"))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 59732627)
    (at 130.85 102.37)
    (fp_text reference J2 (at -2.79 1.89) (layer F.SilkS))
    (fp_text value PHASE_IN (at 0.13 6.99 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 2 "Net-(F1-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 5973276D)
    (at 138.42 102.37)
    (fp_text reference J3 (at -2.68 2.14) (layer F.SilkS))
    (fp_text value NEUTRAL_IN (at 0.14 7.49 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad1)"))
  )
  (module Relays_THT:Relay_SPDT_Schrack-RT1_RM5mm (layer F.Cu) (tedit 5973271C)
    (at 104.81 76.81 270)
    (descr "Relay SPST Schrack-RT1 RM5mm")
    (tags "Relay SPST Schrack-RT1 RM5mm Reais 1x um")
    (fp_text reference RL1 (at 3.39 -2.76 360) (layer F.SilkS))
    (fp_text value SCHRACK_16A_5V_COIL (at 1.51 6.58 270) (layer F.Fab))
    (pad A1 thru_hole circle (at 0 -7.62 270) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (pad A2 thru_hole circle (at 0 0 270) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 12 thru_hole circle (at 15.24 0 270) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask)
      (net 9 "Net-(J5-Pad1)"))
    (pad 11 thru_hole circle (at 20.32 0 270) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask)
      (net 7 "Net-(J4-Pad1)"))
    (pad 14 thru_hole circle (at 25.4 0 270) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (pad 12 thru_hole circle (at 15.24 -7.62 270) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask)
      (net 9 "Net-(J5-Pad1)"))
    (pad 11 thru_hole circle (at 20.32 -7.62 270) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask)
      (net 7 "Net-(J4-Pad1)"))
    (pad 14 thru_hole circle (at 25.4 -7.62 270) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)"))
  )
  (module Varistors:RV_Disc_D12_W3.9_P7.5 (layer F.Cu) (tedit 59732652)
    (at 138.43 97.66 180)
    (tags "varistor SIOV")
    (fp_text reference RV1 (at 4.26 -0.02 360) (layer F.SilkS))
    (fp_text value Varistor (at 1.41 1.88 360) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad1)"))
    (pad 2 thru_hole circle (at 7.5 1.4 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(F1-Pad2)"))
  )
  (module Capacitors_THT:CP_Radial_D8.0mm_P3.50mm (layer F.Cu) (tedit 597326DF)
    (at 101.97 63.3 270)
    (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C1 (at 0.18 -2.31 270) (layer F.SilkS))
    (fp_text value "470uf 16v" (at 1.86 -5.42 450) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_THT.3dshapes/CP_Radial_D8.0mm_P3.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_MELF_Handsoldering (layer B.Cu) (tedit 59732750)
    (at 108.39 71.74)
    (descr "Diode MELF Handsoldering")
    (tags "Diode MELF Handsoldering")
    (attr smd)
    (fp_text reference D2 (at -0.03 0.01) (layer B.SilkS))
    (fp_text value 1N4148 (at 2.4 2.46) (layer B.Fab))
    (pad 1 smd rect (at -3.4 0) (size 3.5 2.7) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 3.4 0) (size 3.5 2.7) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (model Diodes_SMD.3dshapes/D_MELF_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer B.Cu) (tedit 5987F26B)
    (at 128.88 61.3)
    (descr "LED 1206 smd package")
    (tags "LED led 1206 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 3.42 1.04) (layer B.SilkS))
    (fp_text value LED_Small (at 1.27 2.33) (layer B.Fab))
    (pad 2 smd rect (at 1.65 0 180) (size 1.5 1.5) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.65 0 180) (size 1.5 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 59732B83)
    (at 99.53 95.57)
    (fp_text reference J4 (at 1.53 -2.92) (layer F.SilkS))
    (fp_text value LOAD_COM (at 9.38 1.83) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 7 "Net-(J4-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 59732BA4)
    (at 99.51 89.52)
    (fp_text reference J5 (at 1.6 -2.98) (layer F.SilkS))
    (fp_text value LOAD_NC (at 9.34 2.68) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 9 "Net-(J5-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5883B105)
    (at 112.7 65.53 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 2.5 90) (layer B.SilkS))
    (fp_text value 2N7002 (at 0 -2.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 5987F279)
    (at 135.26 70.52 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 0.04 90) (layer B.SilkS))
    (fp_text value "1 OHM" (at 0 -1.9 90) (layer B.Fab))
    (fp_text user %R (at -0.08 1.86 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 5987F271)
    (at 122.11 66.75 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 0.08 180) (layer B.SilkS))
    (fp_text value "3.25 OHM" (at 0 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0.08 -3.47 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(Q1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text NO (at 108.63 99.97) (layer F.SilkS))
  (gr_text COM (at 108.57 94.88) (layer F.SilkS))
  (gr_text NC (at 108.85 89.8) (layer F.SilkS))
  (gr_line (start 140.15 60.23) (end 101.92 60.23) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.23 102.49) (end 141.23 61.29) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 138.48 102.36) (end 141.23 102.51) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.43 105.11) (end 138.3 105.11) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 97.01 102.2) (end 97.01 102.49) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 99.53 102.59) (end 99.42 105.11) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 97.01 65.23) (end 97.01 102.2) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 101.96 65.18) (end 97.01 65.23) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 140.16 61.3) (end 140.15 60.23) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text Switchy (at 130.06 74.62 270) (layer B.SilkS))
)
