(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 21)
    (no_connects 2)
    (area 206.578999 86.817999 226.999001 113.588001)
    (thickness 1.6)
    (drawings 16)
    (tracks 82)
    (zones 0)
    (modules 10)
    (nets 10)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3048)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.381)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.27 1.27)
    (mod_edge_width 0.15)
    (mod_text_size 1.016 1.016)
    (mod_text_width 0.127)
    (pad_size 1.7 1.7)
    (pad_drill 0.5)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 111.76 109.855)
    (grid_origin 0.889 0.508)
    (visible_elements 7FFFFBFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +BATT)
  (net 3 "Net-(IC1-Pad2)")
  (net 4 "Net-(CON1-Pad5)")
  (net 5 "Net-(CON1-Pad4)")
  (net 6 "Net-(CON1-Pad1)")
  (net 7 "Net-(CON1-Pad3)")
  (net 8 "Net-(D1-Pad1)")
  (net 9 "Net-(IC1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +BATT)
    (add_net GND)
    (add_net "Net-(CON1-Pad1)")
    (add_net "Net-(CON1-Pad3)")
    (add_net "Net-(CON1-Pad4)")
    (add_net "Net-(CON1-Pad5)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad3)")
  )
  (module myFootPrints:SW_SMD_TOUCH (layer F.Cu) (tedit 5A9F829B)
    (at 209.389 98.508 180)
    (fp_text reference J1 (at 0.127 4.572 180) (layer F.SilkS) hide)
    (fp_text value JMP (at 0.254 -4.572 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 -2 180) (size 3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 0.635 180) (size 1.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(IC1-Pad2)"))
    (pad 3 smd circle (at 0 -0.75 180) (size 3.5 3.5) (layers F.Paste F.Mask))
  )
  (module Opto-Devices:PhotoDiode_SMD-DIL2_4.5x4 (layer F.Cu) (tedit 5A9E0CC7)
    (at 225.044 109.093 90)
    (descr "PhotoDiode, plastic SMD DIL, 4.5x4mm²")
    (tags "PhotoDiode plastic SMD DIL")
    (attr smd)
    (fp_text reference Q1 (at 0 -1.25 90) (layer F.SilkS))
    (fp_text value LIGHT (at 0 1 90) (layer F.Fab))
    (pad 2 smd rect (at 0.85 0 270) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad3)"))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad3)"))
  )
  (module LEDs:LED_0805_HandSoldering (layer F.Cu) (tedit 5A9E0B35)
    (at 225.044 98.298 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D1 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(CON1-Pad3)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5A9E09B6)
    (at 214.889 89.008 270)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference CON1 (at 1.2 2.5 360) (layer F.SilkS) hide)
    (fp_text value ISP (at 1.5 -2 270) (layer F.SilkS))
    (fp_text user - (at 3.5 6 270) (layer F.SilkS))
    (fp_text user + (at 3.5 -1.5 270) (layer F.SilkS))
    (fp_text user %R (at 1.27 2.54 360) (layer F.Fab))
    (pad 1 smd circle (at 0 0 270) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(CON1-Pad1)"))
    (pad 2 smd oval (at 2.54 0 270) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT))
    (pad 3 smd oval (at 0 2.54 270) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(CON1-Pad3)"))
    (pad 4 smd oval (at 2.54 2.54 270) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(CON1-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 0.5) (layers *.Cu F.Mask)
      (net 4 "Net-(CON1-Pad5)"))
    (pad 6 smd oval (at 2.54 5.08 270) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module myFootPrints:CR2032 (layer B.Cu) (tedit 5A7D35AF)
    (at 216.789 100.203 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
    (pad 3 smd circle (at 0 0 90) (size 17.78 17.78) (layers B.Paste B.Mask))
  )
  (module footprints:BATT_CR2032_SMD locked (layer B.Cu) (tedit 5A7D2CD7)
    (at 216.535 100.076 90)
    (tags battery)
    (fp_text reference BT1 (at 0 -5.08 90) (layer B.SilkS) hide)
    (fp_text value Battery (at 0 2.54 90) (layer B.SilkS) hide)
    (pad 2 smd circle (at 0 0 90) (size 2.54 2.54) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -11.43 0 90) (size 2.54 5.08) (layers B.Cu B.Paste B.Mask)
      (net 2 +BATT))
    (pad 1 smd rect (at 11.43 0 90) (size 2.54 5.08) (layers B.Cu B.Paste B.Mask)
      (net 2 +BATT))
  )
  (module footprints:PS1240_piezo (layer F.Cu) (tedit 5A7D0A37)
    (at 216.889 108.508)
    (descr "piezo speaker 12 mm")
    (tags "buzzer speaker piezo")
    (fp_text reference SP1 (at 0 -0.4) (layer F.SilkS))
    (fp_text value SPEAKER (at 0 1.3) (layer F.SilkS))
    (pad 1 smd rect (at -4.3 0) (size 1.3 3.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 4.3 0) (size 1.3 3.4) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(CON1-Pad4)"))
  )
  (module footprints:SOIJ-8_5.3x5.3mm_Pitch1.27mm (layer F.Cu) (tedit 5A94E6CD)
    (at 217.8685 99.568)
    (descr "8-Lead Plastic Small Outline (SM) - Medium, 5.28 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference IC1 (at 0.265 0.06) (layer F.SilkS))
    (fp_text value ATTINY85 (at 0 3.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -3.65 -1.905) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(CON1-Pad5)"))
    (pad 2 smd rect (at -3.65 -0.635) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -3.65 0.635) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad3)"))
    (pad 4 smd rect (at -3.65 1.905) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 3.65 1.905) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(CON1-Pad4)"))
    (pad 6 smd rect (at 3.65 0.635) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(CON1-Pad1)"))
    (pad 7 smd rect (at 3.65 -0.635) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(CON1-Pad3)"))
    (pad 8 smd rect (at 3.65 -1.905) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIJ-8_5.3x5.3mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 225.044 104.013 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 330 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5A9E0520)
    (at 221.889 91.508 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 2 180) (layer F.SilkS))
    (fp_text value "0.1 uF" (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 2 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Press\nMe?" (at 209.423 104.648 270) (layer F.SilkS))
  (gr_text V0.3 (at 225.679 90.678 90) (layer B.SilkS))
  (gr_text http://v.ht/rroll (at 216.889 95.008) (layer F.SilkS))
  (gr_line (start 211.709 113.538) (end 221.869 113.538) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 206.629 91.948) (end 206.629 108.458) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 221.869 86.868) (end 211.709 86.868) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 226.949 108.458) (end 226.949 91.948) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 211.709 91.948) (end 206.629 91.948) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 221.869 91.948) (end 221.869 86.868) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 211.709 108.458) (end 211.709 113.538) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 221.869 108.458) (end 226.949 108.458) (angle 90) (layer Edge.Cuts) (width 0.1))
)
