(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(PS1-VIN)")
  (net 2 "Earth")
  (net 3 "Net-(U1--VIN)")
  (net 4 "Net-(F1-Pad2)")
  (net 5 "Net-(F2-Pad2)")
  (net 6 "Net-(IC1-INPUT)")
  (net 7 "Net-(IC1-OUTPUT)")
  (net 8 "Net-(IC2-IN)")
  (net 9 "Net-(IC2-OUT)")
  (net 10 "Net-(D1-A)")
  (net 11 "Net-(D2-A)")
  (footprint "Fuse:Fuseholder_Clip-5x20mm_Bel_FC-203-22_Lateral_P17.80x5.00mm_D1.17mm_Horizontal" (layer "F.Cu")
    (at 142.2 126.98 -90)
    (descr "Fuseholder Clips, 5x20mm Cylinder Fuse, Pins Lateral, Horizontal, Bel FC-203-22, https://www.belfuse.com/resources/datasheets/circuitprotection/ds-cp-0672-fuse-clips-series.pdf")
    (tags "fuse clip open")
    (property "Sheetfile" "parrot.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Fuse")
    (property "ki_keywords" "fuse")
    (attr through_hole)
    (fp_text reference "F1" (at 8.9 -2 -90) (layer "F.SilkS"))
    (fp_text value "Fuse" (at 8.9 7 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 8.9 2.5 -90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 2.2 2.2) (drill 1.17) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(PS1-VIN)") (pintype "passive"))
    (pad "1" thru_hole roundrect (at 0 5 270) (size 2.2 2.2) (drill 1.17) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(PS1-VIN)") (pintype "passive"))
    (pad "2" thru_hole circle (at 17.8 0 270) (size 2.2 2.2) (drill 1.17) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(F1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 17.8 5 270) (size 2.2 2.2) (drill 1.17) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(F1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Clip-5x20mm_Bel_FC-203-22_Lateral_P17.80x5.00mm_D1.17mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LIB_PV-T2X-38E:PVT2X38E" (layer "F.Cu")
    (at 168.148 105.52 90)
    (descr "PV-T2X-38E-1")
    (tags "Hardware")
    (property "Height" "38.1")
    (property "Manufacturer_Name" "Ohmite")
    (property "Manufacturer_Part_Number" "PV-T2X-38E")
    (property "Mouser Part Number" "588-PV-T2X-38E")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Ohmite/PV-T2X-38E?qs=W0yvOO0ixfHuhDcxaNjIaw%3D%3D")
    (property "Sheetfile" "parrot.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Heat Sinks 38mm Heatsink Degreased")
    (attr through_hole)
    (fp_text reference "H1" (at 22.352 0 90) (layer "F.SilkS"))
    (fp_text value "PV-T2X-38E" (at 9.144 -3.683 90) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0.254 90) (size 4.005 4.005) (drill 2.67) (layers "*.Cu" "*.Mask")
      (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 18 0.254 90) (size 4.005 4.005) (drill 2.67) (layers "*.Cu" "*.Mask")
      (pinfunction "2") (pintype "passive"))
    (model "PV-T2X-38E.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (at 158.75 71.12)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "parrot.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D2" (at 1.27 -3.96) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D2-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "RDEC71E226K3K1H03B:CAP_RDEC71E226K3K1H03B" (layer "F.Cu")
    (at 153.67 118.11)
    (property "Check_prices" "https://www.snapeda.com/parts/RDEC71E226K3K1H03B/Murata/view-part/?ref=eda")
    (property "Description" "\nLead capacitor X7S(EIA) with Capacitance 22F, Rated Voltage 25Vdc\n")
    (property "DigiKey_Part_Number" "490-14507-ND")
    (property "MANUFACTURER" "Murata")
    (property "MAXIMUM_PACKAGE_HEIGHT" "9.5mm")
    (property "MF" "Murata")
    (property "MP" "RDEC71E226K3K1H03B")
    (property "PARTREV" "")
    (property "Package" "NONSTANDARD")
    (property "Purchase-URL" "https://pricing.snapeda.com/search?q=RDEC71E226K3K1H03B&ref=eda")
    (property "STANDARD" "IPC-7351B")
    (property "Sheetfile" "parrot.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/RDEC71E226K3K1H03B/Murata/view-part/?ref=snap")
    (attr through_hole)
    (fp_text reference "C5" (at -0.225 -3.135) (layer "F.SilkS"))
    (fp_text value "RDEC71E226K3K1H03B" (at 10.57 3.065) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at -2.5 0) (size 1.15 1.15) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(IC2-IN)") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.15 1.15) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pintype "passive") (solder_mask_margin 0.102))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 142.24 68.58 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "parrot.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 5.08 -2.37 90) (layer "F.SilkS"))
    (fp_text value "47k" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D1-A)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(IC1-OUTPUT)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuseholder_Clip-5x20mm_Bel_FC-203-22_Lateral_P17.80x5.00mm_D1.17mm_Horizontal" (layer "F.Cu")
    (at 157.4 126.98 -90)
    (descr "Fuseholder Clips, 5x20mm Cylinder Fuse, Pins Lateral, Horizontal, Bel FC-203-22, https://www.belfuse.com/resources/datasheets/circuitprotection/ds-cp-0672-fuse-clips-series.pdf")
    (tags "fuse clip open")
    (property "Sheetfile" "parrot.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Fuse")
    (property "ki_keywords" "fuse")
    (attr through_hole)
    (fp_text reference "F2" (at 8.9 -2 -90) (layer "F.SilkS"))
    (fp_text value "Fuse" (at 8.9 7 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 8.9 2.5 -90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 2.2 2.2) (drill 1.17) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(U1--VIN)") (pintype "passive"))
    (pad "1" thru_hole roundrect (at 0 5 270) (size 2.2 2.2) (drill 1.17) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(U1--VIN)") (pintype "passive"))
    (pad "2" thru_hole circle (at 17.8 0 270) (size 2.2 2.2) (drill 1.17) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(F2-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 17.8 5 270) (size 2.2 2.2) (drill 1.17) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(F2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Clip-5x20mm_Bel_FC-203-22_Lateral_P17.80x5.00mm_D1.17mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "7908:TO270P460X1020X2008-3P" (layer "F.Cu")
    (at 162.6028 92.55 -90)
    (descr "TO-220 TYPE A")
    (tags "Integrated Circuit")
    (property "Height" "4.6")
    (property "Manufacturer_Name" "STMicroelectronics")
    (property "Manufacturer_Part_Number" "L7908CV")
    (property "Mouser Part Number" "511-L7908CV")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/STMicroelectronics/L7908CV?qs=W%252B4obUA0F3a1iCcgpeCvfA%3D%3D")
    (property "Sheetfile" "parrot.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "L7908CV, Linear Voltage Regulator, Negative 1.5A -8 V, 3-Pin TO-220")
    (attr through_hole)
    (fp_text reference "IC2" (at 0 0 90) (layer "F.SilkS"))
    (fp_text value "L7908CV" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.98 1.98) (drill 1.32) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "GND") (pintype "power_in"))
    (pad "2" thru_hole circle (at 2.7 0 270) (size 1.98 1.98) (drill 1.32) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(IC2-IN)") (pinfunction "IN") (pintype "power_in"))
    (pad "3" thru_hole circle (at 5.4 0 270) (size 1.98 1.98) (drill 1.32) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(IC2-OUT)") (pinfunction "OUT") (pintype "power_in"))
    (model "L7908CV.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "RDEC71E226K3K1H03B:CAP_RDEC71E226K3K1H03B" (layer "F.Cu")
    (at 140.97 83.82)
    (property "Check_prices" "https://www.snapeda.com/parts/RDEC71E226K3K1H03B/Murata/view-part/?ref=eda")
    (property "Description" "\nLead capacitor X7S(EIA) with Capacitance 22F, Rated Voltage 25Vdc\n")
    (property "DigiKey_Part_Number" "490-14507-ND")
    (property "MANUFACTURER" "Murata")
    (property "MAXIMUM_PACKAGE_HEIGHT" "9.5mm")
    (property "MF" "Murata")
    (property "MP" "RDEC71E226K3K1H03B")
    (property "PARTREV" "")
    (property "Package" "NONSTANDARD")
    (property "Purchase-URL" "https://pricing.snapeda.com/search?q=RDEC71E226K3K1H03B&ref=eda")
    (property "STANDARD" "IPC-7351B")
    (property "Sheetfile" "parrot.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/RDEC71E226K3K1H03B/Murata/view-part/?ref=snap")
    (attr through_hole)
    (fp_text reference "C3" (at -5.08 0) (layer "F.SilkS"))
    (fp_text value "RDEC71E226K3K1H03B" (at 10.57 3.065) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at -2.5 0) (size 1.15 1.15) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(IC1-OUTPUT)") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.15 1.15) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pintype "passive") (solder_mask_margin 0.102))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (at 128.27 165.1)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers "*.Mask" "B.Cu"))
  )
  (footprint "RDEC71E226K3K1H03B:CAP_RDEC71E226K3K1H03B" (layer "F.Cu")
    (at 143.51 117.9068 180)
    (property "Check_prices" "https://www.snapeda.com/parts/RDEC71E226K3K1H03B/Murata/view-part/?ref=eda")
    (property "Description" "\nLead capacitor X7S(EIA) with Capacitance 22F, Rated Voltage 25Vdc\n")
    (property "DigiKey_Part_Number" "490-14507-ND")
    (property "MANUFACTURER" "Murata")
    (property "MAXIMUM_PACKAGE_HEIGHT" "9.5mm")
    (property "MF" "Murata")
    (property "MP" "RDEC71E226K3K1H03B")
    (property "PARTREV" "")
    (property "Package" "NONSTANDARD")
    (property "Purchase-URL" "https://pricing.snapeda.com/search?q=RDEC71E226K3K1H03B&ref=eda")
    (property "STANDARD" "IPC-7351B")
    (property "Sheetfile" "parrot.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/RDEC71E226K3K1H03B/Murata/view-part/?ref=snap")
    (attr through_hole)
    (fp_text reference "C2" (at 0 -0.2032) (layer "F.SilkS"))
    (fp_text value "RDEC71E226K3K1H03B" (at 10.57 3.065) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at -2.5 0 180) (size 1.15 1.15) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(IC1-INPUT)") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.15 1.15) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pintype "passive") (solder_mask_margin 0.102))
  )
  (footprint "K7803-2000R3:CONV_K7803-2000R3" (layer "F.Cu")
    (at 138.43 110.3)
    (property "Check_prices" "https://www.snapeda.com/parts/K7803-2000R3/MORNSUN/view-part/?ref=eda")
    (property "Description" "\nLinear Regulator Replacement DC DC Converter 1 Output 3.3V - - - 2A 6V - 36V Input\n")
    (property "DigiKey_Part_Number" "2725-K7803-2000R3-ND")
    (property "MANUFACTURER" "Mornsun")
    (property "MAXIMUM_PACKAGE_HEIGHT" "18 mm")
    (property "MF" "Mornsun America, LLC")
    (property "MP" "K7803-2000R3")
    (property "PARTREV" "2019.10.24-A/5")
    (property "Package" "SIP-3-3 MORNSUN")
    (property "Purchase-URL" "https://pricing.snapeda.com/search?q=K7803-2000R3&ref=eda")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "parrot.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/K7803-2000R3/MORNSUN/view-part/?ref=snap")
    (attr through_hole)
    (fp_text reference "PS1" (at 0 -6.16) (layer "F.SilkS"))
    (fp_text value "K7803-2000R3" (at 7.62 -1.08 90) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -2.54 -2.35) (size 1.8 1.8) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(PS1-VIN)") (pinfunction "VIN") (pintype "input") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at 0 -2.35) (size 1.8 1.8) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "3" thru_hole circle (at 2.54 -2.35) (size 1.8 1.8) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(IC1-INPUT)") (pinfunction "+VO") (pintype "output") (solder_mask_margin 0.102))
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (at 134.62 71.12)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "parrot.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D1" (at 1.27 -3.96) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (at 168.91 46.99)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "7808:TO270P460X1020X2008-3P" (layer "F.Cu")
    (at 134.628 97.7976 90)
    (descr "TO-220 TYPE A")
    (tags "Integrated Circuit")
    (property "Height" "4.6")
    (property "Manufacturer_Name" "STMicroelectronics")
    (property "Manufacturer_Part_Number" "L7808ACV")
    (property "Mouser Part Number" "511-L7808ACV")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/STMicroelectronics/L7808ACV?qs=Mu9A%252BxKg3hQSf%252Bc%252BkCz4Aw%3D%3D")
    (property "Sheetfile" "parrot.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "L7808ACV, Voltage Regulator, 1A 8 V, 2%, 3-Pin TO-220")
    (attr through_hole)
    (fp_text reference "IC1" (at 0 0 90) (layer "F.SilkS"))
    (fp_text value "L7808ACV" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.98 1.98) (drill 1.32) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(IC1-INPUT)") (pinfunction "INPUT") (pintype "input"))
    (pad "2" thru_hole circle (at 2.7 0 90) (size 1.98 1.98) (drill 1.32) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "GROUND") (pintype "power_in"))
    (pad "3" thru_hole circle (at 5.4 0 90) (size 1.98 1.98) (drill 1.32) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(IC1-OUTPUT)") (pinfunction "OUTPUT") (pintype "output"))
    (model "L7808ACV.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:CONN4_282847-4_TEC" (layer "F.Cu")
    (at 139.7 156.21)
    (tags "282847-4 ")
    (property "Sheetfile" "parrot.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "282847-4")
    (attr through_hole)
    (fp_text reference "J1" (at -8.89 -0.508 90 unlocked) (layer "F.SilkS"))
    (fp_text value "282847-4" (at -6.35 0 90 unlocked) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(F1-Pad2)") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 5.08 0) (size 2.032 2.032) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole circle (at 10.16 0) (size 2.032 2.032) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "3") (pintype "unspecified"))
    (pad "4" thru_hole circle (at 15.24 0) (size 2.032 2.032) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(F2-Pad2)") (pinfunction "4") (pintype "unspecified"))
  )
  (footprint "LIB_PV-T2X-38E:PVT2X38E" (layer "F.Cu")
    (at 129.032 87.74 -90)
    (descr "PV-T2X-38E-1")
    (tags "Hardware")
    (property "Height" "38.1")
    (property "Manufacturer_Name" "Ohmite")
    (property "Manufacturer_Part_Number" "PV-T2X-38E")
    (property "Mouser Part Number" "588-PV-T2X-38E")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Ohmite/PV-T2X-38E?qs=W0yvOO0ixfHuhDcxaNjIaw%3D%3D")
    (property "Sheetfile" "parrot.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Heat Sinks 38mm Heatsink Degreased")
    (attr through_hole)
    (fp_text reference "H2" (at -4.936 0 90) (layer "F.SilkS"))
    (fp_text value "PV-T2X-38E" (at 9.144 -3.683 90) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0.254 270) (size 4.005 4.005) (drill 2.67) (layers "*.Cu" "*.Mask")
      (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 18 0.254 270) (size 4.005 4.005) (drill 2.67) (layers "*.Cu" "*.Mask")
      (pinfunction "2") (pintype "passive"))
    (model "PV-T2X-38E.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 153.67 78.74 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "parrot.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 5.08 -2.37 90) (layer "F.SilkS"))
    (fp_text value "47k" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D2-A)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(IC2-OUT)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (at 168.91 165.1)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers "F&B.Cu" "*.Mask"))
  )
  (footprint "TSN-1-24120:TSN 1_TRP" (layer "F.Cu")
    (at 156.21 110.490001)
    (tags "TSN 1-24120 ")
    (property "Sheetfile" "parrot.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "TSN 1-24120")
    (attr through_hole)
    (fp_text reference "U1" (at 2.54 -0.65 unlocked) (layer "F.SilkS"))
    (fp_text value "TSN 1-24120" (at 2.54 -0.65 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -4.3307 0) (layer "F.SilkS"))
    (fp_text user "*" (at -4.3307 0 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at -3.0607 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -0.65 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -3.0607 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 -0.000001) (size 1.27 1.27) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "GND") (pintype "power_out"))
    (pad "2" thru_hole circle (at 2.54 -0.000001) (size 1.27 1.27) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(U1--VIN)") (pinfunction "-VIN") (pintype "power_in"))
    (pad "3" thru_hole circle (at 5.08 -0.000001) (size 1.27 1.27) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(IC2-IN)") (pinfunction "-VOUT") (pintype "output"))
  )
  (footprint "RDEC71E226K3K1H03B:CAP_RDEC71E226K3K1H03B" (layer "F.Cu")
    (at 156.21 83.82)
    (property "Check_prices" "https://www.snapeda.com/parts/RDEC71E226K3K1H03B/Murata/view-part/?ref=eda")
    (property "Description" "\nLead capacitor X7S(EIA) with Capacitance 22F, Rated Voltage 25Vdc\n")
    (property "DigiKey_Part_Number" "490-14507-ND")
    (property "MANUFACTURER" "Murata")
    (property "MAXIMUM_PACKAGE_HEIGHT" "9.5mm")
    (property "MF" "Murata")
    (property "MP" "RDEC71E226K3K1H03B")
    (property "PARTREV" "")
    (property "Package" "NONSTANDARD")
    (property "Purchase-URL" "https://pricing.snapeda.com/search?q=RDEC71E226K3K1H03B&ref=eda")
    (property "STANDARD" "IPC-7351B")
    (property "Sheetfile" "parrot.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/RDEC71E226K3K1H03B/Murata/view-part/?ref=snap")
    (attr through_hole)
    (fp_text reference "C6" (at -5.08 0) (layer "F.SilkS"))
    (fp_text value "RDEC71E226K3K1H03B" (at 10.57 3.065) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at -2.5 0) (size 1.15 1.15) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(IC2-OUT)") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.15 1.15) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pintype "passive") (solder_mask_margin 0.102))
  )
  (footprint "RDEC71E226K3K1H03B:CAP_RDEC71E226K3K1H03B" (layer "F.Cu")
    (at 133.4008 118.11)
    (property "Check_prices" "https://www.snapeda.com/parts/RDEC71E226K3K1H03B/Murata/view-part/?ref=eda")
    (property "Description" "\nLead capacitor X7S(EIA) with Capacitance 22F, Rated Voltage 25Vdc\n")
    (property "DigiKey_Part_Number" "490-14507-ND")
    (property "MANUFACTURER" "Murata")
    (property "MAXIMUM_PACKAGE_HEIGHT" "9.5mm")
    (property "MF" "Murata")
    (property "MP" "RDEC71E226K3K1H03B")
    (property "PARTREV" "")
    (property "Package" "NONSTANDARD")
    (property "Purchase-URL" "https://pricing.snapeda.com/search?q=RDEC71E226K3K1H03B&ref=eda")
    (property "STANDARD" "IPC-7351B")
    (property "Sheetfile" "parrot.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/RDEC71E226K3K1H03B/Murata/view-part/?ref=snap")
    (attr through_hole)
    (fp_text reference "C1" (at -0.0508 0) (layer "F.SilkS"))
    (fp_text value "RDEC71E226K3K1H03B" (at 10.57 3.065) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at -2.5 0) (size 1.15 1.15) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(PS1-VIN)") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.15 1.15) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pintype "passive") (solder_mask_margin 0.102))
  )
  (footprint "RDEC71E226K3K1H03B:CAP_RDEC71E226K3K1H03B" (layer "F.Cu")
    (at 162.56 118.11)
    (property "Check_prices" "https://www.snapeda.com/parts/RDEC71E226K3K1H03B/Murata/view-part/?ref=eda")
    (property "Description" "\nLead capacitor X7S(EIA) with Capacitance 22F, Rated Voltage 25Vdc\n")
    (property "DigiKey_Part_Number" "490-14507-ND")
    (property "MANUFACTURER" "Murata")
    (property "MAXIMUM_PACKAGE_HEIGHT" "9.5mm")
    (property "MF" "Murata")
    (property "MP" "RDEC71E226K3K1H03B")
    (property "PARTREV" "")
    (property "Package" "NONSTANDARD")
    (property "Purchase-URL" "https://pricing.snapeda.com/search?q=RDEC71E226K3K1H03B&ref=eda")
    (property "STANDARD" "IPC-7351B")
    (property "Sheetfile" "parrot.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/RDEC71E226K3K1H03B/Murata/view-part/?ref=snap")
    (attr through_hole)
    (fp_text reference "C4" (at -0.225 -3.135) (layer "F.SilkS"))
    (fp_text value "RDEC71E226K3K1H03B" (at 10.57 3.065) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at -2.5 0) (size 1.15 1.15) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(U1--VIN)") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.15 1.15) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pintype "passive") (solder_mask_margin 0.102))
  )
  (footprint "footprints:CONN4_282847-4_TEC" (layer "F.Cu")
    (at 140.97 57.15)
    (tags "282847-4 ")
    (property "Sheetfile" "parrot.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "282847-4")
    (attr through_hole)
    (fp_text reference "J2" (at -7.903401 0 90 unlocked) (layer "F.SilkS"))
    (fp_text value "282847-4" (at -5.363401 0 90 unlocked) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(IC1-OUTPUT)") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 5.08 0) (size 2.032 2.032) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole circle (at 10.16 0) (size 2.032 2.032) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "3") (pintype "unspecified"))
    (pad "4" thru_hole circle (at 15.24 0) (size 2.032 2.032) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(IC2-OUT)") (pinfunction "4") (pintype "unspecified"))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (at 128.27 46.99)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers "F&B.Cu" "*.Mask"))
  )
  (gr_rect (start 124.46 43.18) (end 172.72 168.91)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "+" (at 138.43 166.37) (layer "F.SilkS"))
  (gr_text "PV-72X-38E Heatsink" (at 129.032 126.238 90) (layer "F.SilkS"))
  (gr_text "GND" (at 146.05 46.99) (layer "F.SilkS"))
  (gr_text "GND" (at 144.78 167.64) (layer "F.SilkS"))
  (gr_text "Input Rails" (at 159.766 150.622 270) (layer "F.SilkS"))
  (gr_text "0.1 μF Capacitors" (at 141.986 88.392) (layer "F.SilkS"))
  (gr_text "-" (at 153.67 166.37) (layer "F.SilkS"))
  (gr_text "Dual 8V Supply Board\nVer 3.0 6-11-2024 by A.J." (at 170.18 156.21 90) (layer "F.SilkS"))
  (gr_text "-" (at 154.94 49.53) (layer "F.SilkS"))
  (gr_text "L7807ACV" (at 138.43 97.79 90) (layer "F.SilkS"))
  (gr_text "22 μF Capacitors" (at 133.35 123.19) (layer "F.SilkS"))
  (gr_text "Output Rails" (at 160.782 50.8 270) (layer "F.SilkS"))
  (gr_text "L7907CV" (at 154.94 91.694 270) (layer "F.SilkS"))
  (gr_text "+" (at 139.7 49.53) (layer "F.SilkS"))
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 124.46 43.18)
        (xy 172.72 43.18)
        (xy 172.72 168.91)
        (xy 124.46 168.91)
      )
    )
  )
  (zone (net 2) (net_name "Earth") (layer "B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 172.72 43.18)
        (xy 124.46 43.18)
        (xy 124.46 168.91)
        (xy 172.72 168.91)
      )
    )
  )
  (zone (net 2) (net_name "Earth") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 124.46 43.18)
        (xy 172.72 43.18)
        (xy 172.72 168.91)
        (xy 124.46 168.91)
      )
    )
  )
)
