(kicad_pcb (version 4) (host pcbnew "(2015-08-07 BZR 6071, Git 6018bb6)-product")
  (general
    (links 202)
    (no_connects 0)
    (area 105.891359 94.855159 161.041361 130.005161)
    (thickness 1.6)
    (drawings 35)
    (tracks 1042)
    (zones 0)
    (modules 65)
    (nets 386)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power)
    (2 In2.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.127)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 1.27)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.508)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.9 1.3)
    (pad_drill 0)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(U2-PadA2)")
  (net 3 "Net-(U2-PadA3)")
  (net 4 "Net-(U2-PadA4)")
  (net 5 "Net-(U2-PadA5)")
  (net 6 "Net-(U2-PadA6)")
  (net 7 "Net-(U2-PadA7)")
  (net 8 "Net-(U2-PadA8)")
  (net 9 "Net-(U2-PadA9)")
  (net 10 "Net-(C2-Pad1)")
  (net 11 "Net-(U2-PadA11)")
  (net 12 "Net-(U2-PadA12)")
  (net 13 "Net-(U2-PadA13)")
  (net 14 "Net-(U2-PadA14)")
  (net 15 "Net-(U2-PadA15)")
  (net 16 "Net-(U2-PadA18)")
  (net 17 "Net-(U2-PadA19)")
  (net 18 PMIC_PGOOD)
  (net 19 "Net-(U2-PadB2)")
  (net 20 "Net-(U2-PadB20)")
  (net 21 "Net-(U2-PadB3)")
  (net 22 "Net-(R5-Pad1)")
  (net 23 "Net-(U2-PadB1)")
  (net 24 "Net-(U2-PadB6)")
  (net 25 "Net-(U2-PadB7)")
  (net 26 "Net-(U2-PadB8)")
  (net 27 "Net-(U2-PadB9)")
  (net 28 TRSTN)
  (net 29 "Net-(U2-PadB11)")
  (net 30 "Net-(U2-PadB12)")
  (net 31 "Net-(U2-PadB13)")
  (net 32 "Net-(U2-PadB14)")
  (net 33 "Net-(U2-PadB18)")
  (net 34 "Net-(U2-PadC2)")
  (net 35 "Net-(U2-PadC3)")
  (net 36 "Net-(U2-PadC4)")
  (net 37 "Net-(U2-PadC1)")
  (net 38 "Net-(U2-PadC6)")
  (net 39 "Net-(U2-PadC7)")
  (net 40 "Net-(U2-PadC8)")
  (net 41 "Net-(U2-PadC9)")
  (net 42 "Net-(U2-PadC10)")
  (net 43 "Net-(U2-PadC11)")
  (net 44 "Net-(U2-PadC12)")
  (net 45 "Net-(U2-PadC13)")
  (net 46 "Net-(U2-PadC14)")
  (net 47 MMC0_CD)
  (net 48 I2C0_SCL)
  (net 49 I2C0_SDA)
  (net 50 "Net-(U2-PadC18)")
  (net 51 "Net-(U2-PadD2)")
  (net 52 "Net-(U2-PadD5)")
  (net 53 "Net-(U2-PadD3)")
  (net 54 "Net-(U2-PadD4)")
  (net 55 "Net-(U2-PadD1)")
  (net 56 "Net-(U2-PadD6)")
  (net 57 "Net-(U2-PadD7)")
  (net 58 "Net-(U2-PadD8)")
  (net 59 "Net-(U2-PadD9)")
  (net 60 VDD_1V8)
  (net 61 "Net-(U2-PadD11)")
  (net 62 "Net-(U2-PadD12)")
  (net 63 "Net-(U2-PadD13)")
  (net 64 "Net-(U2-PadD14)")
  (net 65 "Net-(U2-PadD15)")
  (net 66 "Net-(U2-PadD16)")
  (net 67 "Net-(U2-PadD17)")
  (net 68 "Net-(U2-PadD18)")
  (net 69 "Net-(SW1-Pad2)")
  (net 70 "Net-(U2-PadE2)")
  (net 71 "Net-(U2-PadE5)")
  (net 72 "Net-(U2-PadE3)")
  (net 73 "Net-(U2-PadE4)")
  (net 74 "Net-(U2-PadE1)")
  (net 75 "Net-(U2-PadE6)")
  (net 76 "Net-(U2-PadE7)")
  (net 77 "Net-(U2-PadE8)")
  (net 78 "Net-(U2-PadE10)")
  (net 79 "Net-(U2-PadE11)")
  (net 80 "Net-(U2-PadE12)")
  (net 81 "Net-(U2-PadE13)")
  (net 82 VDD_RTC)
  (net 83 "Net-(U2-PadE17)")
  (net 84 "Net-(U2-PadE18)")
  (net 85 "Net-(U2-PadE19)")
  (net 86 "Net-(U2-PadE20)")
  (net 87 "Net-(U2-PadF2)")
  (net 88 "Net-(U2-PadF5)")
  (net 89 "Net-(U2-PadF3)")
  (net 90 "Net-(U2-PadF4)")
  (net 91 "Net-(U2-PadF1)")
  (net 92 "Net-(U2-PadF6)")
  (net 93 "Net-(U2-PadF7)")
  (net 94 "Net-(U2-PadF8)")
  (net 95 "Net-(U2-PadF9)")
  (net 96 "Net-(U2-PadF10)")
  (net 97 "Net-(U2-PadF11)")
  (net 98 "Net-(U2-PadF12)")
  (net 99 "Net-(U2-PadF13)")
  (net 100 "Net-(U2-PadF14)")
  (net 101 USB1_DRVVBUS)
  (net 102 "Net-(U2-PadF16)")
  (net 103 MMC0_DAT3)
  (net 104 MMC0_DAT2)
  (net 105 "Net-(U2-PadF19)")
  (net 106 "Net-(U2-PadG2)")
  (net 107 "Net-(U2-PadG5)")
  (net 108 "Net-(U2-PadG3)")
  (net 109 "Net-(U2-PadG4)")
  (net 110 "Net-(U2-PadG1)")
  (net 111 "Net-(U2-PadG6)")
  (net 112 "Net-(U2-PadG7)")
  (net 113 "Net-(U2-PadG8)")
  (net 114 "Net-(U2-PadG9)")
  (net 115 "Net-(U2-PadG10)")
  (net 116 "Net-(U2-PadG11)")
  (net 117 "Net-(U2-PadG12)")
  (net 118 "Net-(U2-PadG13)")
  (net 119 "Net-(U2-PadG14)")
  (net 120 MMC0_DAT1)
  (net 121 MMC0_DAT0)
  (net 122 MMC0_CLK)
  (net 123 MMC0_CMD)
  (net 124 "Net-(U2-PadG19)")
  (net 125 "Net-(U2-PadH2)")
  (net 126 "Net-(U2-PadH5)")
  (net 127 "Net-(U2-PadH3)")
  (net 128 "Net-(U2-PadH4)")
  (net 129 "Net-(U2-PadH1)")
  (net 130 "Net-(U2-PadH6)")
  (net 131 "Net-(U2-PadH7)")
  (net 132 "Net-(U2-PadH8)")
  (net 133 "Net-(U2-PadH9)")
  (net 134 "Net-(U2-PadH10)")
  (net 135 "Net-(U2-PadH11)")
  (net 136 "Net-(U2-PadH12)")
  (net 137 "Net-(U2-PadH13)")
  (net 138 "Net-(U2-PadH14)")
  (net 139 "Net-(U2-PadH15)")
  (net 140 "Net-(U2-PadH16)")
  (net 141 "Net-(U2-PadH17)")
  (net 142 "Net-(U2-PadH18)")
  (net 143 "Net-(U2-PadH19)")
  (net 144 "Net-(U2-PadJ2)")
  (net 145 "Net-(U2-PadJ5)")
  (net 146 "Net-(U2-PadJ3)")
  (net 147 "Net-(U2-PadJ4)")
  (net 148 "Net-(U2-PadJ1)")
  (net 149 "Net-(U2-PadJ7)")
  (net 150 "Net-(U2-PadJ8)")
  (net 151 "Net-(U2-PadJ9)")
  (net 152 "Net-(U2-PadJ10)")
  (net 153 "Net-(U2-PadJ11)")
  (net 154 "Net-(U2-PadJ12)")
  (net 155 "Net-(U2-PadJ13)")
  (net 156 "Net-(U2-PadJ14)")
  (net 157 "Net-(U2-PadJ15)")
  (net 158 "Net-(U2-PadJ16)")
  (net 159 "Net-(U2-PadJ17)")
  (net 160 "Net-(U2-PadJ18)")
  (net 161 "Net-(U2-PadJ19)")
  (net 162 "Net-(U2-PadJ20)")
  (net 163 "Net-(U2-PadK2)")
  (net 164 "Net-(U2-PadK5)")
  (net 165 "Net-(U2-PadK3)")
  (net 166 "Net-(U2-PadK4)")
  (net 167 "Net-(U2-PadK1)")
  (net 168 "Net-(U2-PadK6)")
  (net 169 "Net-(U2-PadK7)")
  (net 170 "Net-(U2-PadK8)")
  (net 171 "Net-(U2-PadK9)")
  (net 172 "Net-(U2-PadK10)")
  (net 173 "Net-(U2-PadK11)")
  (net 174 "Net-(U2-PadK12)")
  (net 175 "Net-(U2-PadK13)")
  (net 176 "Net-(U2-PadK14)")
  (net 177 "Net-(U2-PadK15)")
  (net 178 "Net-(U2-PadK16)")
  (net 179 "Net-(U2-PadK17)")
  (net 180 "Net-(U2-PadK18)")
  (net 181 "Net-(U2-PadK19)")
  (net 182 "Net-(C13-Pad1)")
  (net 183 "Net-(U2-PadL13)")
  (net 184 "Net-(U2-PadL11)")
  (net 185 "Net-(U2-PadL12)")
  (net 186 "Net-(U2-PadL10)")
  (net 187 "Net-(U2-PadL8)")
  (net 188 "Net-(U2-PadL9)")
  (net 189 "Net-(U2-PadL7)")
  (net 190 "Net-(U2-PadL3)")
  (net 191 "Net-(U2-PadL1)")
  (net 192 "Net-(U2-PadL2)")
  (net 193 "Net-(U2-PadL4)")
  (net 194 "Net-(U2-PadL5)")
  (net 195 "Net-(U2-PadL6)")
  (net 196 "Net-(U2-PadL15)")
  (net 197 "Net-(U2-PadL16)")
  (net 198 "Net-(U2-PadL14)")
  (net 199 "Net-(U2-PadL17)")
  (net 200 "Net-(U2-PadL18)")
  (net 201 OSC0_GND)
  (net 202 "Net-(U2-PadM13)")
  (net 203 "Net-(U2-PadM11)")
  (net 204 "Net-(U2-PadM12)")
  (net 205 "Net-(U2-PadM8)")
  (net 206 "Net-(U2-PadM9)")
  (net 207 "Net-(U2-PadM7)")
  (net 208 "Net-(U2-PadM3)")
  (net 209 "Net-(U2-PadM1)")
  (net 210 "Net-(U2-PadM2)")
  (net 211 "Net-(U2-PadM4)")
  (net 212 "Net-(U2-PadM5)")
  (net 213 "Net-(U2-PadM6)")
  (net 214 "Net-(U2-PadM15)")
  (net 215 "Net-(U2-PadM16)")
  (net 216 "Net-(U2-PadM14)")
  (net 217 "Net-(U2-PadM17)")
  (net 218 "Net-(U2-PadM18)")
  (net 219 "Net-(C10-Pad1)")
  (net 220 "Net-(U2-PadN13)")
  (net 221 "Net-(U2-PadN11)")
  (net 222 "Net-(U2-PadN12)")
  (net 223 "Net-(U2-PadN10)")
  (net 224 "Net-(U2-PadN8)")
  (net 225 "Net-(U2-PadN9)")
  (net 226 "Net-(U2-PadN3)")
  (net 227 "Net-(U2-PadN1)")
  (net 228 "Net-(U2-PadN2)")
  (net 229 "Net-(U2-PadN4)")
  (net 230 "Net-(U2-PadN5)")
  (net 231 "Net-(U2-PadN6)")
  (net 232 "Net-(U2-PadN15)")
  (net 233 "Net-(U2-PadN16)")
  (net 234 "Net-(U2-PadN14)")
  (net 235 "Net-(U2-PadN19)")
  (net 236 "Net-(U2-PadN20)")
  (net 237 "Net-(U2-PadP13)")
  (net 238 "Net-(U2-PadP11)")
  (net 239 "Net-(U2-PadP12)")
  (net 240 "Net-(U2-PadP10)")
  (net 241 "Net-(U2-PadP8)")
  (net 242 "Net-(U2-PadP9)")
  (net 243 "Net-(U2-PadP7)")
  (net 244 "Net-(U2-PadP3)")
  (net 245 "Net-(U2-PadP1)")
  (net 246 "Net-(U2-PadP2)")
  (net 247 "Net-(U2-PadP4)")
  (net 248 "Net-(U2-PadP5)")
  (net 249 "Net-(U2-PadP6)")
  (net 250 USB0_VBUS)
  (net 251 USB0_ID)
  (net 252 "Net-(U2-PadP14)")
  (net 253 USB1_ID)
  (net 254 "Net-(U2-PadP18)")
  (net 255 "Net-(U2-PadP19)")
  (net 256 "Net-(U2-PadP20)")
  (net 257 "Net-(U2-PadR13)")
  (net 258 "Net-(U2-PadR11)")
  (net 259 "Net-(U2-PadR12)")
  (net 260 "Net-(U2-PadR10)")
  (net 261 "Net-(U2-PadR8)")
  (net 262 "Net-(U2-PadR9)")
  (net 263 "Net-(U2-PadR7)")
  (net 264 "Net-(U2-PadR5)")
  (net 265 "Net-(U2-PadR6)")
  (net 266 "Net-(U2-PadR15)")
  (net 267 "Net-(U2-PadR16)")
  (net 268 "Net-(U2-PadR14)")
  (net 269 "Net-(U2-PadR19)")
  (net 270 "Net-(U2-PadR20)")
  (net 271 "Net-(U2-PadT13)")
  (net 272 "Net-(U2-PadT11)")
  (net 273 "Net-(U2-PadT12)")
  (net 274 "Net-(U2-PadT10)")
  (net 275 "Net-(U2-PadT8)")
  (net 276 "Net-(U2-PadT9)")
  (net 277 "Net-(U2-PadT7)")
  (net 278 "Net-(U2-PadT6)")
  (net 279 USR2_LED)
  (net 280 "Net-(U2-PadT16)")
  (net 281 "Net-(U2-PadT14)")
  (net 282 "Net-(U2-PadT17)")
  (net 283 USB1_VBUS)
  (net 284 "Net-(U2-PadT19)")
  (net 285 "Net-(U2-PadT20)")
  (net 286 "Net-(U2-PadU13)")
  (net 287 "Net-(U2-PadU11)")
  (net 288 "Net-(U2-PadU12)")
  (net 289 "Net-(U2-PadU10)")
  (net 290 "Net-(U2-PadU8)")
  (net 291 "Net-(U2-PadU9)")
  (net 292 "Net-(U2-PadU7)")
  (net 293 "Net-(U2-PadU5)")
  (net 294 "Net-(U2-PadU6)")
  (net 295 USR1_LED)
  (net 296 "Net-(U2-PadU16)")
  (net 297 "Net-(U2-PadU14)")
  (net 298 "Net-(U2-PadU17)")
  (net 299 "Net-(U2-PadU18)")
  (net 300 "Net-(U2-PadU19)")
  (net 301 +3V3)
  (net 302 "Net-(U2-PadV13)")
  (net 303 "Net-(U2-PadV11)")
  (net 304 "Net-(U2-PadV12)")
  (net 305 "Net-(U2-PadV10)")
  (net 306 "Net-(U2-PadV8)")
  (net 307 "Net-(U2-PadV9)")
  (net 308 "Net-(U2-PadV7)")
  (net 309 "Net-(U2-PadV5)")
  (net 310 "Net-(U2-PadV6)")
  (net 311 USR0_LED)
  (net 312 USR3_LED)
  (net 313 "Net-(U2-PadV14)")
  (net 314 "Net-(U2-PadV17)")
  (net 315 "Net-(U2-PadV18)")
  (net 316 "Net-(U2-PadW10)")
  (net 317 "Net-(U2-PadW9)")
  (net 318 "Net-(U2-PadW8)")
  (net 319 SYS_5V)
  (net 320 "Net-(U2-PadW3)")
  (net 321 "Net-(U2-PadW5)")
  (net 322 "Net-(U2-PadW7)")
  (net 323 "Net-(U2-PadW6)")
  (net 324 "Net-(U2-PadW16)")
  (net 325 "Net-(U2-PadW15)")
  (net 326 "Net-(U2-PadW13)")
  (net 327 "Net-(U2-PadW14)")
  (net 328 "Net-(U2-PadW12)")
  (net 329 "Net-(U2-PadW19)")
  (net 330 "Net-(U2-PadW18)")
  (net 331 "Net-(U2-PadW17)")
  (net 332 "Net-(U2-PadY10)")
  (net 333 +5V)
  (net 334 "Net-(U2-PadY7)")
  (net 335 "Net-(U2-PadY16)")
  (net 336 "Net-(U2-PadY15)")
  (net 337 "Net-(U2-PadY13)")
  (net 338 "Net-(U2-PadY14)")
  (net 339 "Net-(U2-PadY12)")
  (net 340 3P3AUX)
  (net 341 "Net-(U2-PadY19)")
  (net 342 "Net-(U2-PadY17)")
  (net 343 "Net-(U2-PadY20)")
  (net 344 "Net-(R4-Pad2)")
  (net 345 "Net-(U4-Pad3)")
  (net 346 "Net-(U1-Pad1)")
  (net 347 "Net-(D1-Pad1)")
  (net 348 "Net-(D2-Pad1)")
  (net 349 "Net-(D3-Pad1)")
  (net 350 "Net-(D4-Pad1)")
  (net 351 "Net-(D5-Pad1)")
  (net 352 "Net-(FB1-Pad2)")
  (net 353 "Net-(FB2-Pad2)")
  (net 354 USB1_D_N)
  (net 355 USB1_D_P)
  (net 356 USB0_D_N)
  (net 357 USB0_D_P)
  (net 358 "Net-(U2-PadF20)")
  (net 359 "Net-(U2-PadG20)")
  (net 360 "Net-(U2-PadH20)")
  (net 361 UART0_TXD)
  (net 362 UART0_RXD)
  (net 363 SPI_CS0)
  (net 364 SPI_CLK)
  (net 365 SPI_MOSI)
  (net 366 SPI_MISO)
  (net 367 "Net-(RN1-Pad8)")
  (net 368 "Net-(RN1-Pad7)")
  (net 369 "Net-(RN1-Pad6)")
  (net 370 "Net-(RN1-Pad5)")
  (net 371 "Net-(RN2-Pad2)")
  (net 372 "Net-(RN2-Pad3)")
  (net 373 "Net-(RN2-Pad1)")
  (net 374 "Net-(RN2-Pad4)")
  (net 375 "Net-(RN3-Pad8)")
  (net 376 "Net-(RN3-Pad7)")
  (net 377 "Net-(RN3-Pad6)")
  (net 378 "Net-(RN3-Pad5)")
  (net 379 "Net-(RN4-Pad8)")
  (net 380 "Net-(RN4-Pad7)")
  (net 381 "Net-(RN4-Pad6)")
  (net 382 "Net-(RN4-Pad5)")
  (net 383 VBAT)
  (net 384 TS)
  (net 385 BAT_SENSE)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net 3P3AUX)
    (add_net BAT_SENSE)
    (add_net GND)
    (add_net I2C0_SCL)
    (add_net I2C0_SDA)
    (add_net MMC0_CD)
    (add_net MMC0_CLK)
    (add_net MMC0_CMD)
    (add_net MMC0_DAT0)
    (add_net MMC0_DAT1)
    (add_net MMC0_DAT2)
    (add_net MMC0_DAT3)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(FB1-Pad2)")
    (add_net "Net-(FB2-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(RN1-Pad5)")
    (add_net "Net-(RN1-Pad6)")
    (add_net "Net-(RN1-Pad7)")
    (add_net "Net-(RN1-Pad8)")
    (add_net "Net-(RN2-Pad1)")
    (add_net "Net-(RN2-Pad2)")
    (add_net "Net-(RN2-Pad3)")
    (add_net "Net-(RN2-Pad4)")
    (add_net "Net-(RN3-Pad5)")
    (add_net "Net-(RN3-Pad6)")
    (add_net "Net-(RN3-Pad7)")
    (add_net "Net-(RN3-Pad8)")
    (add_net "Net-(RN4-Pad5)")
    (add_net "Net-(RN4-Pad6)")
    (add_net "Net-(RN4-Pad7)")
    (add_net "Net-(RN4-Pad8)")
    (add_net "Net-(SW1-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U2-PadA11)")
    (add_net "Net-(U2-PadA12)")
    (add_net "Net-(U2-PadA13)")
    (add_net "Net-(U2-PadA14)")
    (add_net "Net-(U2-PadA15)")
    (add_net "Net-(U2-PadA18)")
    (add_net "Net-(U2-PadA19)")
    (add_net "Net-(U2-PadA2)")
    (add_net "Net-(U2-PadA3)")
    (add_net "Net-(U2-PadA4)")
    (add_net "Net-(U2-PadA5)")
    (add_net "Net-(U2-PadA6)")
    (add_net "Net-(U2-PadA7)")
    (add_net "Net-(U2-PadA8)")
    (add_net "Net-(U2-PadA9)")
    (add_net "Net-(U2-PadB1)")
    (add_net "Net-(U2-PadB11)")
    (add_net "Net-(U2-PadB12)")
    (add_net "Net-(U2-PadB13)")
    (add_net "Net-(U2-PadB14)")
    (add_net "Net-(U2-PadB18)")
    (add_net "Net-(U2-PadB2)")
    (add_net "Net-(U2-PadB20)")
    (add_net "Net-(U2-PadB3)")
    (add_net "Net-(U2-PadB6)")
    (add_net "Net-(U2-PadB7)")
    (add_net "Net-(U2-PadB8)")
    (add_net "Net-(U2-PadB9)")
    (add_net "Net-(U2-PadC1)")
    (add_net "Net-(U2-PadC10)")
    (add_net "Net-(U2-PadC11)")
    (add_net "Net-(U2-PadC12)")
    (add_net "Net-(U2-PadC13)")
    (add_net "Net-(U2-PadC14)")
    (add_net "Net-(U2-PadC18)")
    (add_net "Net-(U2-PadC2)")
    (add_net "Net-(U2-PadC3)")
    (add_net "Net-(U2-PadC4)")
    (add_net "Net-(U2-PadC6)")
    (add_net "Net-(U2-PadC7)")
    (add_net "Net-(U2-PadC8)")
    (add_net "Net-(U2-PadC9)")
    (add_net "Net-(U2-PadD1)")
    (add_net "Net-(U2-PadD11)")
    (add_net "Net-(U2-PadD12)")
    (add_net "Net-(U2-PadD13)")
    (add_net "Net-(U2-PadD14)")
    (add_net "Net-(U2-PadD15)")
    (add_net "Net-(U2-PadD16)")
    (add_net "Net-(U2-PadD17)")
    (add_net "Net-(U2-PadD18)")
    (add_net "Net-(U2-PadD2)")
    (add_net "Net-(U2-PadD3)")
    (add_net "Net-(U2-PadD4)")
    (add_net "Net-(U2-PadD5)")
    (add_net "Net-(U2-PadD6)")
    (add_net "Net-(U2-PadD7)")
    (add_net "Net-(U2-PadD8)")
    (add_net "Net-(U2-PadD9)")
    (add_net "Net-(U2-PadE1)")
    (add_net "Net-(U2-PadE10)")
    (add_net "Net-(U2-PadE11)")
    (add_net "Net-(U2-PadE12)")
    (add_net "Net-(U2-PadE13)")
    (add_net "Net-(U2-PadE17)")
    (add_net "Net-(U2-PadE18)")
    (add_net "Net-(U2-PadE19)")
    (add_net "Net-(U2-PadE2)")
    (add_net "Net-(U2-PadE20)")
    (add_net "Net-(U2-PadE3)")
    (add_net "Net-(U2-PadE4)")
    (add_net "Net-(U2-PadE5)")
    (add_net "Net-(U2-PadE6)")
    (add_net "Net-(U2-PadE7)")
    (add_net "Net-(U2-PadE8)")
    (add_net "Net-(U2-PadF1)")
    (add_net "Net-(U2-PadF10)")
    (add_net "Net-(U2-PadF11)")
    (add_net "Net-(U2-PadF12)")
    (add_net "Net-(U2-PadF13)")
    (add_net "Net-(U2-PadF14)")
    (add_net "Net-(U2-PadF16)")
    (add_net "Net-(U2-PadF19)")
    (add_net "Net-(U2-PadF2)")
    (add_net "Net-(U2-PadF20)")
    (add_net "Net-(U2-PadF3)")
    (add_net "Net-(U2-PadF4)")
    (add_net "Net-(U2-PadF5)")
    (add_net "Net-(U2-PadF6)")
    (add_net "Net-(U2-PadF7)")
    (add_net "Net-(U2-PadF8)")
    (add_net "Net-(U2-PadF9)")
    (add_net "Net-(U2-PadG1)")
    (add_net "Net-(U2-PadG10)")
    (add_net "Net-(U2-PadG11)")
    (add_net "Net-(U2-PadG12)")
    (add_net "Net-(U2-PadG13)")
    (add_net "Net-(U2-PadG14)")
    (add_net "Net-(U2-PadG19)")
    (add_net "Net-(U2-PadG2)")
    (add_net "Net-(U2-PadG20)")
    (add_net "Net-(U2-PadG3)")
    (add_net "Net-(U2-PadG4)")
    (add_net "Net-(U2-PadG5)")
    (add_net "Net-(U2-PadG6)")
    (add_net "Net-(U2-PadG7)")
    (add_net "Net-(U2-PadG8)")
    (add_net "Net-(U2-PadG9)")
    (add_net "Net-(U2-PadH1)")
    (add_net "Net-(U2-PadH10)")
    (add_net "Net-(U2-PadH11)")
    (add_net "Net-(U2-PadH12)")
    (add_net "Net-(U2-PadH13)")
    (add_net "Net-(U2-PadH14)")
    (add_net "Net-(U2-PadH15)")
    (add_net "Net-(U2-PadH16)")
    (add_net "Net-(U2-PadH17)")
    (add_net "Net-(U2-PadH18)")
    (add_net "Net-(U2-PadH19)")
    (add_net "Net-(U2-PadH2)")
    (add_net "Net-(U2-PadH20)")
    (add_net "Net-(U2-PadH3)")
    (add_net "Net-(U2-PadH4)")
    (add_net "Net-(U2-PadH5)")
    (add_net "Net-(U2-PadH6)")
    (add_net "Net-(U2-PadH7)")
    (add_net "Net-(U2-PadH8)")
    (add_net "Net-(U2-PadH9)")
    (add_net "Net-(U2-PadJ1)")
    (add_net "Net-(U2-PadJ10)")
    (add_net "Net-(U2-PadJ11)")
    (add_net "Net-(U2-PadJ12)")
    (add_net "Net-(U2-PadJ13)")
    (add_net "Net-(U2-PadJ14)")
    (add_net "Net-(U2-PadJ15)")
    (add_net "Net-(U2-PadJ16)")
    (add_net "Net-(U2-PadJ17)")
    (add_net "Net-(U2-PadJ18)")
    (add_net "Net-(U2-PadJ19)")
    (add_net "Net-(U2-PadJ2)")
    (add_net "Net-(U2-PadJ20)")
    (add_net "Net-(U2-PadJ3)")
    (add_net "Net-(U2-PadJ4)")
    (add_net "Net-(U2-PadJ5)")
    (add_net "Net-(U2-PadJ7)")
    (add_net "Net-(U2-PadJ8)")
    (add_net "Net-(U2-PadJ9)")
    (add_net "Net-(U2-PadK1)")
    (add_net "Net-(U2-PadK10)")
    (add_net "Net-(U2-PadK11)")
    (add_net "Net-(U2-PadK12)")
    (add_net "Net-(U2-PadK13)")
    (add_net "Net-(U2-PadK14)")
    (add_net "Net-(U2-PadK15)")
    (add_net "Net-(U2-PadK16)")
    (add_net "Net-(U2-PadK17)")
    (add_net "Net-(U2-PadK18)")
    (add_net "Net-(U2-PadK19)")
    (add_net "Net-(U2-PadK2)")
    (add_net "Net-(U2-PadK3)")
    (add_net "Net-(U2-PadK4)")
    (add_net "Net-(U2-PadK5)")
    (add_net "Net-(U2-PadK6)")
    (add_net "Net-(U2-PadK7)")
    (add_net "Net-(U2-PadK8)")
    (add_net "Net-(U2-PadK9)")
    (add_net "Net-(U2-PadL1)")
    (add_net "Net-(U2-PadL10)")
    (add_net "Net-(U2-PadL11)")
    (add_net "Net-(U2-PadL12)")
    (add_net "Net-(U2-PadL13)")
    (add_net "Net-(U2-PadL14)")
    (add_net "Net-(U2-PadL15)")
    (add_net "Net-(U2-PadL16)")
    (add_net "Net-(U2-PadL17)")
    (add_net "Net-(U2-PadL18)")
    (add_net "Net-(U2-PadL2)")
    (add_net "Net-(U2-PadL3)")
    (add_net "Net-(U2-PadL4)")
    (add_net "Net-(U2-PadL5)")
    (add_net "Net-(U2-PadL6)")
    (add_net "Net-(U2-PadL7)")
    (add_net "Net-(U2-PadL8)")
    (add_net "Net-(U2-PadL9)")
    (add_net "Net-(U2-PadM1)")
    (add_net "Net-(U2-PadM11)")
    (add_net "Net-(U2-PadM12)")
    (add_net "Net-(U2-PadM13)")
    (add_net "Net-(U2-PadM14)")
    (add_net "Net-(U2-PadM15)")
    (add_net "Net-(U2-PadM16)")
    (add_net "Net-(U2-PadM17)")
    (add_net "Net-(U2-PadM18)")
    (add_net "Net-(U2-PadM2)")
    (add_net "Net-(U2-PadM3)")
    (add_net "Net-(U2-PadM4)")
    (add_net "Net-(U2-PadM5)")
    (add_net "Net-(U2-PadM6)")
    (add_net "Net-(U2-PadM7)")
    (add_net "Net-(U2-PadM8)")
    (add_net "Net-(U2-PadM9)")
    (add_net "Net-(U2-PadN1)")
    (add_net "Net-(U2-PadN10)")
    (add_net "Net-(U2-PadN11)")
    (add_net "Net-(U2-PadN12)")
    (add_net "Net-(U2-PadN13)")
    (add_net "Net-(U2-PadN14)")
    (add_net "Net-(U2-PadN15)")
    (add_net "Net-(U2-PadN16)")
    (add_net "Net-(U2-PadN19)")
    (add_net "Net-(U2-PadN2)")
    (add_net "Net-(U2-PadN20)")
    (add_net "Net-(U2-PadN3)")
    (add_net "Net-(U2-PadN4)")
    (add_net "Net-(U2-PadN5)")
    (add_net "Net-(U2-PadN6)")
    (add_net "Net-(U2-PadN8)")
    (add_net "Net-(U2-PadN9)")
    (add_net "Net-(U2-PadP1)")
    (add_net "Net-(U2-PadP10)")
    (add_net "Net-(U2-PadP11)")
    (add_net "Net-(U2-PadP12)")
    (add_net "Net-(U2-PadP13)")
    (add_net "Net-(U2-PadP14)")
    (add_net "Net-(U2-PadP18)")
    (add_net "Net-(U2-PadP19)")
    (add_net "Net-(U2-PadP2)")
    (add_net "Net-(U2-PadP20)")
    (add_net "Net-(U2-PadP3)")
    (add_net "Net-(U2-PadP4)")
    (add_net "Net-(U2-PadP5)")
    (add_net "Net-(U2-PadP6)")
    (add_net "Net-(U2-PadP7)")
    (add_net "Net-(U2-PadP8)")
    (add_net "Net-(U2-PadP9)")
    (add_net "Net-(U2-PadR10)")
    (add_net "Net-(U2-PadR11)")
    (add_net "Net-(U2-PadR12)")
    (add_net "Net-(U2-PadR13)")
    (add_net "Net-(U2-PadR14)")
    (add_net "Net-(U2-PadR15)")
    (add_net "Net-(U2-PadR16)")
    (add_net "Net-(U2-PadR19)")
    (add_net "Net-(U2-PadR20)")
    (add_net "Net-(U2-PadR5)")
    (add_net "Net-(U2-PadR6)")
    (add_net "Net-(U2-PadR7)")
    (add_net "Net-(U2-PadR8)")
    (add_net "Net-(U2-PadR9)")
    (add_net "Net-(U2-PadT10)")
    (add_net "Net-(U2-PadT11)")
    (add_net "Net-(U2-PadT12)")
    (add_net "Net-(U2-PadT13)")
    (add_net "Net-(U2-PadT14)")
    (add_net "Net-(U2-PadT16)")
    (add_net "Net-(U2-PadT17)")
    (add_net "Net-(U2-PadT19)")
    (add_net "Net-(U2-PadT20)")
    (add_net "Net-(U2-PadT6)")
    (add_net "Net-(U2-PadT7)")
    (add_net "Net-(U2-PadT8)")
    (add_net "Net-(U2-PadT9)")
    (add_net "Net-(U2-PadU10)")
    (add_net "Net-(U2-PadU11)")
    (add_net "Net-(U2-PadU12)")
    (add_net "Net-(U2-PadU13)")
    (add_net "Net-(U2-PadU14)")
    (add_net "Net-(U2-PadU16)")
    (add_net "Net-(U2-PadU17)")
    (add_net "Net-(U2-PadU18)")
    (add_net "Net-(U2-PadU19)")
    (add_net "Net-(U2-PadU5)")
    (add_net "Net-(U2-PadU6)")
    (add_net "Net-(U2-PadU7)")
    (add_net "Net-(U2-PadU8)")
    (add_net "Net-(U2-PadU9)")
    (add_net "Net-(U2-PadV10)")
    (add_net "Net-(U2-PadV11)")
    (add_net "Net-(U2-PadV12)")
    (add_net "Net-(U2-PadV13)")
    (add_net "Net-(U2-PadV14)")
    (add_net "Net-(U2-PadV17)")
    (add_net "Net-(U2-PadV18)")
    (add_net "Net-(U2-PadV5)")
    (add_net "Net-(U2-PadV6)")
    (add_net "Net-(U2-PadV7)")
    (add_net "Net-(U2-PadV8)")
    (add_net "Net-(U2-PadV9)")
    (add_net "Net-(U2-PadW10)")
    (add_net "Net-(U2-PadW12)")
    (add_net "Net-(U2-PadW13)")
    (add_net "Net-(U2-PadW14)")
    (add_net "Net-(U2-PadW15)")
    (add_net "Net-(U2-PadW16)")
    (add_net "Net-(U2-PadW17)")
    (add_net "Net-(U2-PadW18)")
    (add_net "Net-(U2-PadW19)")
    (add_net "Net-(U2-PadW3)")
    (add_net "Net-(U2-PadW5)")
    (add_net "Net-(U2-PadW6)")
    (add_net "Net-(U2-PadW7)")
    (add_net "Net-(U2-PadW8)")
    (add_net "Net-(U2-PadW9)")
    (add_net "Net-(U2-PadY10)")
    (add_net "Net-(U2-PadY12)")
    (add_net "Net-(U2-PadY13)")
    (add_net "Net-(U2-PadY14)")
    (add_net "Net-(U2-PadY15)")
    (add_net "Net-(U2-PadY16)")
    (add_net "Net-(U2-PadY17)")
    (add_net "Net-(U2-PadY19)")
    (add_net "Net-(U2-PadY20)")
    (add_net "Net-(U2-PadY7)")
    (add_net "Net-(U4-Pad3)")
    (add_net OSC0_GND)
    (add_net PMIC_PGOOD)
    (add_net SPI_CLK)
    (add_net SPI_CS0)
    (add_net SPI_MISO)
    (add_net SPI_MOSI)
    (add_net SYS_5V)
    (add_net TRSTN)
    (add_net TS)
    (add_net UART0_RXD)
    (add_net UART0_TXD)
    (add_net USB0_D_N)
    (add_net USB0_D_P)
    (add_net USB0_ID)
    (add_net USB0_VBUS)
    (add_net USB1_DRVVBUS)
    (add_net USB1_D_N)
    (add_net USB1_D_P)
    (add_net USB1_ID)
    (add_net USB1_VBUS)
    (add_net USR0_LED)
    (add_net USR1_LED)
    (add_net USR2_LED)
    (add_net USR3_LED)
    (add_net VBAT)
    (add_net VDD_1V8)
    (add_net VDD_RTC)
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58929B49)
    (at 145.72742 120.71858 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R37 (at 0.635 1.64592 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 301 +3V3))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 MMC0_CD))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pocketbone-kicad:BGA-400-1-27mm (layer F.Cu) (tedit 5892A008)
    (at 131.13512 112.90554 90)
    (fp_text reference U2 (at 12.1158 14.4526 180) (layer F.SilkS))
    (fp_text value OSD3358 (at 0 -14.478 90) (layer F.Fab))
    (pad A1 smd circle (at -12.065 12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A2 smd circle (at -12.065 10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U2-PadA2)"))
    (pad A3 smd circle (at -12.065 9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U2-PadA3)"))
    (pad A4 smd circle (at -12.065 8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U2-PadA4)"))
    (pad A5 smd circle (at -12.065 6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U2-PadA5)"))
    (pad A6 smd circle (at -12.065 5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U2-PadA6)"))
    (pad A7 smd circle (at -12.065 4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U2-PadA7)"))
    (pad A8 smd circle (at -12.065 3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U2-PadA8)"))
    (pad A9 smd circle (at -12.065 1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U2-PadA9)"))
    (pad A10 smd circle (at -12.065 0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C2-Pad1)"))
    (pad A11 smd circle (at -12.065 -0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U2-PadA11)"))
    (pad A12 smd circle (at -12.065 -1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U2-PadA12)"))
    (pad A13 smd circle (at -12.065 -3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U2-PadA13)"))
    (pad A14 smd circle (at -12.065 -4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U2-PadA14)"))
    (pad A15 smd circle (at -12.065 -5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U2-PadA15)"))
    (pad A16 smd circle (at -12.065 -6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 363 SPI_CS0))
    (pad A17 smd circle (at -12.065 -8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 364 SPI_CLK))
    (pad A18 smd circle (at -12.065 -9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U2-PadA18)"))
    (pad A19 smd circle (at -12.065 -10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U2-PadA19)"))
    (pad A20 smd circle (at -12.065 -12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 PMIC_PGOOD))
    (pad B2 smd circle (at -10.795 10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U2-PadB2)"))
    (pad B5 smd circle (at -10.795 6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U2-PadB20)"))
    (pad B3 smd circle (at -10.795 9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U2-PadB3)"))
    (pad B4 smd circle (at -10.795 8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R5-Pad1)"))
    (pad B1 smd circle (at -10.795 12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U2-PadB1)"))
    (pad B6 smd circle (at -10.795 5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U2-PadB6)"))
    (pad B7 smd circle (at -10.795 4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U2-PadB7)"))
    (pad B8 smd circle (at -10.795 3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U2-PadB8)"))
    (pad B9 smd circle (at -10.795 1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U2-PadB9)"))
    (pad B10 smd circle (at -10.795 0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 TRSTN))
    (pad B11 smd circle (at -10.795 -0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U2-PadB11)"))
    (pad B12 smd circle (at -10.795 -1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U2-PadB12)"))
    (pad B13 smd circle (at -10.795 -3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U2-PadB13)"))
    (pad B14 smd circle (at -10.795 -4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U2-PadB14)"))
    (pad B15 smd circle (at -10.795 -5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 PMIC_PGOOD))
    (pad B16 smd circle (at -10.795 -6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 365 SPI_MOSI))
    (pad B17 smd circle (at -10.795 -8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 366 SPI_MISO))
    (pad B18 smd circle (at -10.795 -9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U2-PadB18)"))
    (pad B19 smd circle (at -10.795 -10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U2-PadB18)"))
    (pad B20 smd circle (at -10.795 -12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U2-PadB20)"))
    (pad C2 smd circle (at -9.525 10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U2-PadC2)"))
    (pad C5 smd circle (at -9.525 6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U2-PadA19)"))
    (pad C3 smd circle (at -9.525 9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U2-PadC3)"))
    (pad C4 smd circle (at -9.525 8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U2-PadC4)"))
    (pad C1 smd circle (at -9.525 12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U2-PadC1)"))
    (pad C6 smd circle (at -9.525 5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U2-PadC6)"))
    (pad C7 smd circle (at -9.525 4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U2-PadC7)"))
    (pad C8 smd circle (at -9.525 3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U2-PadC8)"))
    (pad C9 smd circle (at -9.525 1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U2-PadC9)"))
    (pad C10 smd circle (at -9.525 0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U2-PadC10)"))
    (pad C11 smd circle (at -9.525 -0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U2-PadC11)"))
    (pad C12 smd circle (at -9.525 -1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U2-PadC12)"))
    (pad C13 smd circle (at -9.525 -3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U2-PadC13)"))
    (pad C14 smd circle (at -9.525 -4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U2-PadC14)"))
    (pad C15 smd circle (at -9.525 -5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 MMC0_CD))
    (pad C16 smd circle (at -9.525 -6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 I2C0_SCL))
    (pad C17 smd circle (at -9.525 -8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 I2C0_SDA))
    (pad C18 smd circle (at -9.525 -9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U2-PadC18)"))
    (pad C19 smd circle (at -9.525 -10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 I2C0_SDA))
    (pad C20 smd circle (at -9.525 -12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 I2C0_SCL))
    (pad D2 smd circle (at -8.255 10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U2-PadD2)"))
    (pad D5 smd circle (at -8.255 6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U2-PadD5)"))
    (pad D3 smd circle (at -8.255 9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U2-PadD3)"))
    (pad D4 smd circle (at -8.255 8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U2-PadD4)"))
    (pad D1 smd circle (at -8.255 12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U2-PadD1)"))
    (pad D6 smd circle (at -8.255 5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U2-PadD6)"))
    (pad D7 smd circle (at -8.255 4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U2-PadD7)"))
    (pad D8 smd circle (at -8.255 3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U2-PadD8)"))
    (pad D9 smd circle (at -8.255 1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U2-PadD9)"))
    (pad D10 smd circle (at -8.255 0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 60 VDD_1V8))
    (pad D11 smd circle (at -8.255 -0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(U2-PadD11)"))
    (pad D12 smd circle (at -8.255 -1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(U2-PadD12)"))
    (pad D13 smd circle (at -8.255 -3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U2-PadD13)"))
    (pad D14 smd circle (at -8.255 -4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U2-PadD14)"))
    (pad D15 smd circle (at -8.255 -5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(U2-PadD15)"))
    (pad D16 smd circle (at -8.255 -6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(U2-PadD16)"))
    (pad D17 smd circle (at -8.255 -8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(U2-PadD17)"))
    (pad D18 smd circle (at -8.255 -9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(U2-PadD18)"))
    (pad D19 smd circle (at -8.255 -10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U2-PadC6)"))
    (pad D20 smd circle (at -8.255 -12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(SW1-Pad2)"))
    (pad E2 smd circle (at -6.985 10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U2-PadE2)"))
    (pad E5 smd circle (at -6.985 6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U2-PadE5)"))
    (pad E3 smd circle (at -6.985 9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U2-PadE3)"))
    (pad E4 smd circle (at -6.985 8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U2-PadE4)"))
    (pad E1 smd circle (at -6.985 12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U2-PadE1)"))
    (pad E6 smd circle (at -6.985 5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U2-PadE6)"))
    (pad E7 smd circle (at -6.985 4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U2-PadE7)"))
    (pad E8 smd circle (at -6.985 3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U2-PadE8)"))
    (pad E9 smd circle (at -6.985 1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 60 VDD_1V8))
    (pad E10 smd circle (at -6.985 0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U2-PadE10)"))
    (pad E11 smd circle (at -6.985 -0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U2-PadE11)"))
    (pad E12 smd circle (at -6.985 -1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U2-PadE12)"))
    (pad E13 smd circle (at -6.985 -3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U2-PadE13)"))
    (pad E14 smd circle (at -6.985 -4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 82 VDD_RTC))
    (pad E15 smd circle (at -6.985 -5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 362 UART0_RXD))
    (pad E16 smd circle (at -6.985 -6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 361 UART0_TXD))
    (pad E17 smd circle (at -6.985 -8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U2-PadE17)"))
    (pad E18 smd circle (at -6.985 -9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(U2-PadE18)"))
    (pad E19 smd circle (at -6.985 -10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(U2-PadE19)"))
    (pad E20 smd circle (at -6.985 -12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(U2-PadE20)"))
    (pad F2 smd circle (at -5.715 10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(U2-PadF2)"))
    (pad F5 smd circle (at -5.715 6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(U2-PadF5)"))
    (pad F3 smd circle (at -5.715 9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(U2-PadF3)"))
    (pad F4 smd circle (at -5.715 8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(U2-PadF4)"))
    (pad F1 smd circle (at -5.715 12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(U2-PadF1)"))
    (pad F6 smd circle (at -5.715 5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(U2-PadF6)"))
    (pad F7 smd circle (at -5.715 4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(U2-PadF7)"))
    (pad F8 smd circle (at -5.715 3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(U2-PadF8)"))
    (pad F9 smd circle (at -5.715 1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(U2-PadF9)"))
    (pad F10 smd circle (at -5.715 0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(U2-PadF10)"))
    (pad F11 smd circle (at -5.715 -0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(U2-PadF11)"))
    (pad F12 smd circle (at -5.715 -1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(U2-PadF12)"))
    (pad F13 smd circle (at -5.715 -3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(U2-PadF13)"))
    (pad F14 smd circle (at -5.715 -4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(U2-PadF14)"))
    (pad F15 smd circle (at -5.715 -5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 101 USB1_DRVVBUS))
    (pad F16 smd circle (at -5.715 -6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(U2-PadF16)"))
    (pad F17 smd circle (at -5.715 -8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 103 MMC0_DAT3))
    (pad F18 smd circle (at -5.715 -9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 104 MMC0_DAT2))
    (pad F19 smd circle (at -5.715 -10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(U2-PadF19)"))
    (pad F20 smd circle (at -5.715 -12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 358 "Net-(U2-PadF20)"))
    (pad G2 smd circle (at -4.445 10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(U2-PadG2)"))
    (pad G5 smd circle (at -4.445 6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(U2-PadG5)"))
    (pad G3 smd circle (at -4.445 9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 108 "Net-(U2-PadG3)"))
    (pad G4 smd circle (at -4.445 8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(U2-PadG4)"))
    (pad G1 smd circle (at -4.445 12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(U2-PadG1)"))
    (pad G6 smd circle (at -4.445 5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(U2-PadG6)"))
    (pad G7 smd circle (at -4.445 4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(U2-PadG7)"))
    (pad G8 smd circle (at -4.445 3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(U2-PadG8)"))
    (pad G9 smd circle (at -4.445 1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(U2-PadG9)"))
    (pad G10 smd circle (at -4.445 0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(U2-PadG10)"))
    (pad G11 smd circle (at -4.445 -0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(U2-PadG11)"))
    (pad G12 smd circle (at -4.445 -1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(U2-PadG12)"))
    (pad G13 smd circle (at -4.445 -3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(U2-PadG13)"))
    (pad G14 smd circle (at -4.445 -4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(U2-PadG14)"))
    (pad G15 smd circle (at -4.445 -5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 120 MMC0_DAT1))
    (pad G16 smd circle (at -4.445 -6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 121 MMC0_DAT0))
    (pad G17 smd circle (at -4.445 -8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 122 MMC0_CLK))
    (pad G18 smd circle (at -4.445 -9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 123 MMC0_CMD))
    (pad G19 smd circle (at -4.445 -10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(U2-PadG19)"))
    (pad G20 smd circle (at -4.445 -12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 359 "Net-(U2-PadG20)"))
    (pad H2 smd circle (at -3.175 10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(U2-PadH2)"))
    (pad H5 smd circle (at -3.175 6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(U2-PadH5)"))
    (pad H3 smd circle (at -3.175 9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(U2-PadH3)"))
    (pad H4 smd circle (at -3.175 8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(U2-PadH4)"))
    (pad H1 smd circle (at -3.175 12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(U2-PadH1)"))
    (pad H6 smd circle (at -3.175 5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(U2-PadH6)"))
    (pad H7 smd circle (at -3.175 4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(U2-PadH7)"))
    (pad H8 smd circle (at -3.175 3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(U2-PadH8)"))
    (pad H9 smd circle (at -3.175 1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(U2-PadH9)"))
    (pad H10 smd circle (at -3.175 0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(U2-PadH10)"))
    (pad H11 smd circle (at -3.175 -0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 135 "Net-(U2-PadH11)"))
    (pad H12 smd circle (at -3.175 -1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 136 "Net-(U2-PadH12)"))
    (pad H13 smd circle (at -3.175 -3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 137 "Net-(U2-PadH13)"))
    (pad H14 smd circle (at -3.175 -4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(U2-PadH14)"))
    (pad H15 smd circle (at -3.175 -5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(U2-PadH15)"))
    (pad H16 smd circle (at -3.175 -6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(U2-PadH16)"))
    (pad H17 smd circle (at -3.175 -8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(U2-PadH17)"))
    (pad H18 smd circle (at -3.175 -9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(U2-PadH18)"))
    (pad H19 smd circle (at -3.175 -10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(U2-PadH19)"))
    (pad H20 smd circle (at -3.175 -12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 360 "Net-(U2-PadH20)"))
    (pad J2 smd circle (at -1.905 10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(U2-PadJ2)"))
    (pad J5 smd circle (at -1.905 6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(U2-PadJ5)"))
    (pad J3 smd circle (at -1.905 9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(U2-PadJ3)"))
    (pad J4 smd circle (at -1.905 8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(U2-PadJ4)"))
    (pad J1 smd circle (at -1.905 12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(U2-PadJ1)"))
    (pad J6 smd circle (at -1.905 5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad J7 smd circle (at -1.905 4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(U2-PadJ7)"))
    (pad J8 smd circle (at -1.905 3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(U2-PadJ8)"))
    (pad J9 smd circle (at -1.905 1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 151 "Net-(U2-PadJ9)"))
    (pad J10 smd circle (at -1.905 0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(U2-PadJ10)"))
    (pad J11 smd circle (at -1.905 -0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(U2-PadJ11)"))
    (pad J12 smd circle (at -1.905 -1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(U2-PadJ12)"))
    (pad J13 smd circle (at -1.905 -3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(U2-PadJ13)"))
    (pad J14 smd circle (at -1.905 -4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(U2-PadJ14)"))
    (pad J15 smd circle (at -1.905 -5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(U2-PadJ15)"))
    (pad J16 smd circle (at -1.905 -6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(U2-PadJ16)"))
    (pad J17 smd circle (at -1.905 -8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(U2-PadJ17)"))
    (pad J18 smd circle (at -1.905 -9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(U2-PadJ18)"))
    (pad J19 smd circle (at -1.905 -10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(U2-PadJ19)"))
    (pad J20 smd circle (at -1.905 -12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(U2-PadJ20)"))
    (pad K2 smd circle (at -0.635 10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(U2-PadK2)"))
    (pad K5 smd circle (at -0.635 6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(U2-PadK5)"))
    (pad K3 smd circle (at -0.635 9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(U2-PadK3)"))
    (pad K4 smd circle (at -0.635 8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 166 "Net-(U2-PadK4)"))
    (pad K1 smd circle (at -0.635 12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(U2-PadK1)"))
    (pad K6 smd circle (at -0.635 5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 168 "Net-(U2-PadK6)"))
    (pad K7 smd circle (at -0.635 4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 169 "Net-(U2-PadK7)"))
    (pad K8 smd circle (at -0.635 3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 170 "Net-(U2-PadK8)"))
    (pad K9 smd circle (at -0.635 1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 171 "Net-(U2-PadK9)"))
    (pad K10 smd circle (at -0.635 0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 172 "Net-(U2-PadK10)"))
    (pad K11 smd circle (at -0.635 -0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 173 "Net-(U2-PadK11)"))
    (pad K12 smd circle (at -0.635 -1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 174 "Net-(U2-PadK12)"))
    (pad K13 smd circle (at -0.635 -3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(U2-PadK13)"))
    (pad K14 smd circle (at -0.635 -4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 176 "Net-(U2-PadK14)"))
    (pad K15 smd circle (at -0.635 -5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(U2-PadK15)"))
    (pad K16 smd circle (at -0.635 -6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(U2-PadK16)"))
    (pad K17 smd circle (at -0.635 -8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(U2-PadK17)"))
    (pad K18 smd circle (at -0.635 -9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 180 "Net-(U2-PadK18)"))
    (pad K19 smd circle (at -0.635 -10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(U2-PadK19)"))
    (pad K20 smd circle (at -0.635 -12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(C13-Pad1)"))
    (pad L13 smd circle (at 0.635 -3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 183 "Net-(U2-PadL13)"))
    (pad L11 smd circle (at 0.635 -0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 184 "Net-(U2-PadL11)"))
    (pad L12 smd circle (at 0.635 -1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 185 "Net-(U2-PadL12)"))
    (pad L10 smd circle (at 0.635 0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(U2-PadL10)"))
    (pad L8 smd circle (at 0.635 3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(U2-PadL8)"))
    (pad L9 smd circle (at 0.635 1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 188 "Net-(U2-PadL9)"))
    (pad L7 smd circle (at 0.635 4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(U2-PadL7)"))
    (pad L3 smd circle (at 0.635 9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(U2-PadL3)"))
    (pad L1 smd circle (at 0.635 12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(U2-PadL1)"))
    (pad L2 smd circle (at 0.635 10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 192 "Net-(U2-PadL2)"))
    (pad L4 smd circle (at 0.635 8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(U2-PadL4)"))
    (pad L5 smd circle (at 0.635 6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(U2-PadL5)"))
    (pad L6 smd circle (at 0.635 5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(U2-PadL6)"))
    (pad L15 smd circle (at 0.635 -5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(U2-PadL15)"))
    (pad L16 smd circle (at 0.635 -6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(U2-PadL16)"))
    (pad L14 smd circle (at 0.635 -4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 198 "Net-(U2-PadL14)"))
    (pad L17 smd circle (at 0.635 -8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 199 "Net-(U2-PadL17)"))
    (pad L18 smd circle (at 0.635 -9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(U2-PadL18)"))
    (pad L19 smd circle (at 0.635 -10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad L20 smd circle (at 0.635 -12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 201 OSC0_GND))
    (pad M13 smd circle (at 1.905 -3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 202 "Net-(U2-PadM13)"))
    (pad M11 smd circle (at 1.905 -0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 203 "Net-(U2-PadM11)"))
    (pad M12 smd circle (at 1.905 -1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 204 "Net-(U2-PadM12)"))
    (pad M10 smd circle (at 1.905 0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad M8 smd circle (at 1.905 3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 205 "Net-(U2-PadM8)"))
    (pad M9 smd circle (at 1.905 1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 206 "Net-(U2-PadM9)"))
    (pad M7 smd circle (at 1.905 4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 207 "Net-(U2-PadM7)"))
    (pad M3 smd circle (at 1.905 9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(U2-PadM3)"))
    (pad M1 smd circle (at 1.905 12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(U2-PadM1)"))
    (pad M2 smd circle (at 1.905 10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(U2-PadM2)"))
    (pad M4 smd circle (at 1.905 8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(U2-PadM4)"))
    (pad M5 smd circle (at 1.905 6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 212 "Net-(U2-PadM5)"))
    (pad M6 smd circle (at 1.905 5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 213 "Net-(U2-PadM6)"))
    (pad M15 smd circle (at 1.905 -5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 214 "Net-(U2-PadM15)"))
    (pad M16 smd circle (at 1.905 -6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 215 "Net-(U2-PadM16)"))
    (pad M14 smd circle (at 1.905 -4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 216 "Net-(U2-PadM14)"))
    (pad M17 smd circle (at 1.905 -8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 217 "Net-(U2-PadM17)"))
    (pad M18 smd circle (at 1.905 -9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 218 "Net-(U2-PadM18)"))
    (pad M19 smd circle (at 1.905 -10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad M20 smd circle (at 1.905 -12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 219 "Net-(C10-Pad1)"))
    (pad N13 smd circle (at 3.175 -3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 220 "Net-(U2-PadN13)"))
    (pad N11 smd circle (at 3.175 -0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 221 "Net-(U2-PadN11)"))
    (pad N12 smd circle (at 3.175 -1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(U2-PadN12)"))
    (pad N10 smd circle (at 3.175 0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 223 "Net-(U2-PadN10)"))
    (pad N8 smd circle (at 3.175 3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(U2-PadN8)"))
    (pad N9 smd circle (at 3.175 1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 225 "Net-(U2-PadN9)"))
    (pad N7 smd circle (at 3.175 4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad N3 smd circle (at 3.175 9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 226 "Net-(U2-PadN3)"))
    (pad N1 smd circle (at 3.175 12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 227 "Net-(U2-PadN1)"))
    (pad N2 smd circle (at 3.175 10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 228 "Net-(U2-PadN2)"))
    (pad N4 smd circle (at 3.175 8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 229 "Net-(U2-PadN4)"))
    (pad N5 smd circle (at 3.175 6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 230 "Net-(U2-PadN5)"))
    (pad N6 smd circle (at 3.175 5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 231 "Net-(U2-PadN6)"))
    (pad N15 smd circle (at 3.175 -5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 232 "Net-(U2-PadN15)"))
    (pad N16 smd circle (at 3.175 -6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 233 "Net-(U2-PadN16)"))
    (pad N14 smd circle (at 3.175 -4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 234 "Net-(U2-PadN14)"))
    (pad N17 smd circle (at 3.175 -8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 357 USB0_D_P))
    (pad N18 smd circle (at 3.175 -9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 356 USB0_D_N))
    (pad N19 smd circle (at 3.175 -10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 235 "Net-(U2-PadN19)"))
    (pad N20 smd circle (at 3.175 -12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 236 "Net-(U2-PadN20)"))
    (pad P13 smd circle (at 4.445 -3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 237 "Net-(U2-PadP13)"))
    (pad P11 smd circle (at 4.445 -0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 238 "Net-(U2-PadP11)"))
    (pad P12 smd circle (at 4.445 -1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 239 "Net-(U2-PadP12)"))
    (pad P10 smd circle (at 4.445 0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 240 "Net-(U2-PadP10)"))
    (pad P8 smd circle (at 4.445 3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 241 "Net-(U2-PadP8)"))
    (pad P9 smd circle (at 4.445 1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 242 "Net-(U2-PadP9)"))
    (pad P7 smd circle (at 4.445 4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 243 "Net-(U2-PadP7)"))
    (pad P3 smd circle (at 4.445 9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 244 "Net-(U2-PadP3)"))
    (pad P1 smd circle (at 4.445 12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 245 "Net-(U2-PadP1)"))
    (pad P2 smd circle (at 4.445 10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 246 "Net-(U2-PadP2)"))
    (pad P4 smd circle (at 4.445 8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 247 "Net-(U2-PadP4)"))
    (pad P5 smd circle (at 4.445 6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 248 "Net-(U2-PadP5)"))
    (pad P6 smd circle (at 4.445 5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 249 "Net-(U2-PadP6)"))
    (pad P15 smd circle (at 4.445 -5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 250 USB0_VBUS))
    (pad P16 smd circle (at 4.445 -6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 251 USB0_ID))
    (pad P14 smd circle (at 4.445 -4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 252 "Net-(U2-PadP14)"))
    (pad P17 smd circle (at 4.445 -8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 253 USB1_ID))
    (pad P18 smd circle (at 4.445 -9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 254 "Net-(U2-PadP18)"))
    (pad P19 smd circle (at 4.445 -10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 255 "Net-(U2-PadP19)"))
    (pad P20 smd circle (at 4.445 -12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 256 "Net-(U2-PadP20)"))
    (pad R13 smd circle (at 5.715 -3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 257 "Net-(U2-PadR13)"))
    (pad R11 smd circle (at 5.715 -0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 258 "Net-(U2-PadR11)"))
    (pad R12 smd circle (at 5.715 -1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 259 "Net-(U2-PadR12)"))
    (pad R10 smd circle (at 5.715 0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 260 "Net-(U2-PadR10)"))
    (pad R8 smd circle (at 5.715 3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 261 "Net-(U2-PadR8)"))
    (pad R9 smd circle (at 5.715 1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 262 "Net-(U2-PadR9)"))
    (pad R7 smd circle (at 5.715 4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 263 "Net-(U2-PadR7)"))
    (pad R3 smd circle (at 5.715 9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 369 "Net-(RN1-Pad6)"))
    (pad R1 smd circle (at 5.715 12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 367 "Net-(RN1-Pad8)"))
    (pad R2 smd circle (at 5.715 10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 368 "Net-(RN1-Pad7)"))
    (pad R4 smd circle (at 5.715 8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 373 "Net-(RN2-Pad1)"))
    (pad R5 smd circle (at 5.715 6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 264 "Net-(U2-PadR5)"))
    (pad R6 smd circle (at 5.715 5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 265 "Net-(U2-PadR6)"))
    (pad R15 smd circle (at 5.715 -5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 266 "Net-(U2-PadR15)"))
    (pad R16 smd circle (at 5.715 -6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 267 "Net-(U2-PadR16)"))
    (pad R14 smd circle (at 5.715 -4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 268 "Net-(U2-PadR14)"))
    (pad R17 smd circle (at 5.715 -8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 355 USB1_D_P))
    (pad R18 smd circle (at 5.715 -9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 354 USB1_D_N))
    (pad R19 smd circle (at 5.715 -10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 269 "Net-(U2-PadR19)"))
    (pad R20 smd circle (at 5.715 -12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 270 "Net-(U2-PadR20)"))
    (pad T13 smd circle (at 6.985 -3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 271 "Net-(U2-PadT13)"))
    (pad T11 smd circle (at 6.985 -0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 272 "Net-(U2-PadT11)"))
    (pad T12 smd circle (at 6.985 -1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 273 "Net-(U2-PadT12)"))
    (pad T10 smd circle (at 6.985 0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 274 "Net-(U2-PadT10)"))
    (pad T8 smd circle (at 6.985 3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 275 "Net-(U2-PadT8)"))
    (pad T9 smd circle (at 6.985 1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 276 "Net-(U2-PadT9)"))
    (pad T7 smd circle (at 6.985 4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 277 "Net-(U2-PadT7)"))
    (pad T3 smd circle (at 6.985 9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 370 "Net-(RN1-Pad5)"))
    (pad T1 smd circle (at 6.985 12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 371 "Net-(RN2-Pad2)"))
    (pad T2 smd circle (at 6.985 10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 372 "Net-(RN2-Pad3)"))
    (pad T4 smd circle (at 6.985 8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 375 "Net-(RN3-Pad8)"))
    (pad T5 smd circle (at 6.985 6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 382 "Net-(RN4-Pad5)"))
    (pad T6 smd circle (at 6.985 5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 278 "Net-(U2-PadT6)"))
    (pad T15 smd circle (at 6.985 -5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 279 USR2_LED))
    (pad T16 smd circle (at 6.985 -6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 280 "Net-(U2-PadT16)"))
    (pad T14 smd circle (at 6.985 -4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 281 "Net-(U2-PadT14)"))
    (pad T17 smd circle (at 6.985 -8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 282 "Net-(U2-PadT17)"))
    (pad T18 smd circle (at 6.985 -9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 283 USB1_VBUS))
    (pad T19 smd circle (at 6.985 -10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 284 "Net-(U2-PadT19)"))
    (pad T20 smd circle (at 6.985 -12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 285 "Net-(U2-PadT20)"))
    (pad U13 smd circle (at 8.255 -3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 286 "Net-(U2-PadU13)"))
    (pad U11 smd circle (at 8.255 -0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 287 "Net-(U2-PadU11)"))
    (pad U12 smd circle (at 8.255 -1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 288 "Net-(U2-PadU12)"))
    (pad U10 smd circle (at 8.255 0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 289 "Net-(U2-PadU10)"))
    (pad U8 smd circle (at 8.255 3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 290 "Net-(U2-PadU8)"))
    (pad U9 smd circle (at 8.255 1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 291 "Net-(U2-PadU9)"))
    (pad U7 smd circle (at 8.255 4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 292 "Net-(U2-PadU7)"))
    (pad U3 smd circle (at 8.255 9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 378 "Net-(RN3-Pad5)"))
    (pad U1 smd circle (at 8.255 12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 376 "Net-(RN3-Pad7)"))
    (pad U2 smd circle (at 8.255 10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 377 "Net-(RN3-Pad6)"))
    (pad U4 smd circle (at 8.255 8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 379 "Net-(RN4-Pad8)"))
    (pad U5 smd circle (at 8.255 6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 293 "Net-(U2-PadU5)"))
    (pad U6 smd circle (at 8.255 5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 294 "Net-(U2-PadU6)"))
    (pad U15 smd circle (at 8.255 -5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 295 USR1_LED))
    (pad U16 smd circle (at 8.255 -6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 296 "Net-(U2-PadU16)"))
    (pad U14 smd circle (at 8.255 -4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 297 "Net-(U2-PadU14)"))
    (pad U17 smd circle (at 8.255 -8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 298 "Net-(U2-PadU17)"))
    (pad U18 smd circle (at 8.255 -9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 299 "Net-(U2-PadU18)"))
    (pad U19 smd circle (at 8.255 -10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 300 "Net-(U2-PadU19)"))
    (pad U20 smd circle (at 8.255 -12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 301 +3V3))
    (pad V13 smd circle (at 9.525 -3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 302 "Net-(U2-PadV13)"))
    (pad V11 smd circle (at 9.525 -0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 303 "Net-(U2-PadV11)"))
    (pad V12 smd circle (at 9.525 -1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 304 "Net-(U2-PadV12)"))
    (pad V10 smd circle (at 9.525 0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 305 "Net-(U2-PadV10)"))
    (pad V8 smd circle (at 9.525 3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 306 "Net-(U2-PadV8)"))
    (pad V9 smd circle (at 9.525 1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 307 "Net-(U2-PadV9)"))
    (pad V7 smd circle (at 9.525 4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 308 "Net-(U2-PadV7)"))
    (pad V3 smd circle (at 9.525 9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 381 "Net-(RN4-Pad6)"))
    (pad V1 smd circle (at 9.525 12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad V2 smd circle (at 9.525 10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 380 "Net-(RN4-Pad7)"))
    (pad V4 smd circle (at 9.525 8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 374 "Net-(RN2-Pad4)"))
    (pad V5 smd circle (at 9.525 6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 309 "Net-(U2-PadV5)"))
    (pad V6 smd circle (at 9.525 5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 310 "Net-(U2-PadV6)"))
    (pad V15 smd circle (at 9.525 -5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 311 USR0_LED))
    (pad V16 smd circle (at 9.525 -6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 312 USR3_LED))
    (pad V14 smd circle (at 9.525 -4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 313 "Net-(U2-PadV14)"))
    (pad V17 smd circle (at 9.525 -8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 314 "Net-(U2-PadV17)"))
    (pad V18 smd circle (at 9.525 -9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 315 "Net-(U2-PadV18)"))
    (pad V19 smd circle (at 9.525 -10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad V20 smd circle (at 9.525 -12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 301 +3V3))
    (pad W10 smd circle (at 10.795 0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 316 "Net-(U2-PadW10)"))
    (pad W9 smd circle (at 10.795 1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 317 "Net-(U2-PadW9)"))
    (pad W8 smd circle (at 10.795 3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 318 "Net-(U2-PadW8)"))
    (pad W1 smd circle (at 10.795 12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 384 TS))
    (pad W2 smd circle (at 10.795 10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad W4 smd circle (at 10.795 8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 319 SYS_5V))
    (pad W3 smd circle (at 10.795 9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 320 "Net-(U2-PadW3)"))
    (pad W5 smd circle (at 10.795 6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 321 "Net-(U2-PadW5)"))
    (pad W7 smd circle (at 10.795 4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 322 "Net-(U2-PadW7)"))
    (pad W6 smd circle (at 10.795 5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 323 "Net-(U2-PadW6)"))
    (pad W16 smd circle (at 10.795 -6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 324 "Net-(U2-PadW16)"))
    (pad W15 smd circle (at 10.795 -5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 325 "Net-(U2-PadW15)"))
    (pad W13 smd circle (at 10.795 -3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 326 "Net-(U2-PadW13)"))
    (pad W14 smd circle (at 10.795 -4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 327 "Net-(U2-PadW14)"))
    (pad W12 smd circle (at 10.795 -1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 328 "Net-(U2-PadW12)"))
    (pad W11 smd circle (at 10.795 -0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad W19 smd circle (at 10.795 -10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 329 "Net-(U2-PadW19)"))
    (pad W18 smd circle (at 10.795 -9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 330 "Net-(U2-PadW18)"))
    (pad W17 smd circle (at 10.795 -8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 331 "Net-(U2-PadW17)"))
    (pad W20 smd circle (at 10.795 -12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad Y10 smd circle (at 12.065 0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 332 "Net-(U2-PadY10)"))
    (pad Y9 smd circle (at 12.065 1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 250 USB0_VBUS))
    (pad Y8 smd circle (at 12.065 3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 250 USB0_VBUS))
    (pad Y1 smd circle (at 12.065 12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 385 BAT_SENSE))
    (pad Y2 smd circle (at 12.065 10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 383 VBAT))
    (pad Y4 smd circle (at 12.065 8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 319 SYS_5V))
    (pad Y3 smd circle (at 12.065 9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 383 VBAT))
    (pad Y5 smd circle (at 12.065 6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 333 +5V))
    (pad Y7 smd circle (at 12.065 4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 334 "Net-(U2-PadY7)"))
    (pad Y6 smd circle (at 12.065 5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 333 +5V))
    (pad Y16 smd circle (at 12.065 -6.985 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 335 "Net-(U2-PadY16)"))
    (pad Y15 smd circle (at 12.065 -5.715 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 336 "Net-(U2-PadY15)"))
    (pad Y13 smd circle (at 12.065 -3.175 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 337 "Net-(U2-PadY13)"))
    (pad Y14 smd circle (at 12.065 -4.445 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 338 "Net-(U2-PadY14)"))
    (pad Y12 smd circle (at 12.065 -1.905 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 339 "Net-(U2-PadY12)"))
    (pad Y11 smd circle (at 12.065 -0.635 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 340 3P3AUX))
    (pad Y19 smd circle (at 12.065 -10.795 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 341 "Net-(U2-PadY19)"))
    (pad Y18 smd circle (at 12.065 -9.525 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad Y17 smd circle (at 12.065 -8.255 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 342 "Net-(U2-PadY17)"))
    (pad Y20 smd circle (at 12.065 -12.065 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 343 "Net-(U2-PadY20)"))
  )
  (module SOT-23-5 (layer F.Cu) (tedit 589299ED)
    (at 115.0112 122.2756 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at -1.1684 2.0066 180) (layer F.SilkS))
    (fp_text value 24LC32AT-I/OT (at -0.05 2.35 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 48 I2C0_SCL))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 49 I2C0_SDA))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 301 +3V3))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 344 "Net-(R4-Pad2)"))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 90))
    )
  )
  (module SOT-23-5 (layer F.Cu) (tedit 58929F42)
    (at 115.7503 103.35496 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U4 (at -2.41064 0.0737 180) (layer F.SilkS))
    (fp_text value TPS2051C (at -0.05 2.35 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 283 USB1_VBUS))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 345 "Net-(U4-Pad3)"))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 101 USB1_DRVVBUS))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 319 SYS_5V))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 90))
    )
  )
  (module SOT-23-5 (layer F.Cu) (tedit 589298C1)
    (at 114.9604 126.4412 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at -1.2446 2.0574 180) (layer F.SilkS))
    (fp_text value SN74LVC1G07 (at -0.05 2.35 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 346 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 PMIC_PGOOD))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C2-Pad1)"))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 82 VDD_RTC))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 589298CE)
    (at 112.4712 126.5428 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 0.0254 -1.1684 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 82 VDD_RTC))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5892964E)
    (at 145.542 125.34528 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 1.609 0.0508 360) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 589299E5)
    (at 112.4204 121.0564 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at 1.8542 0.0254 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 301 +3V3))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58929F34)
    (at 115.1636 100.22196 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at 1.92396 0.00762 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 319 SYS_5V))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58929F48)
    (at 113.0808 103.2256 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at -2.3368 0.0254 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 283 USB1_VBUS))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58929F18)
    (at 110.9472 99.568 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at -2.2352 -0.1016 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 283 USB1_VBUS))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58929A74)
    (at 110.3884 112.4458 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C9 (at 1.9392 -0.0254 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 250 USB0_VBUS))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58929A30)
    (at 116.86032 109.97556 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C10 (at 0.06468 -1.07442 270) (layer F.SilkS))
    (fp_text value 18pF (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 219 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 201 OSC0_GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58929F2A)
    (at 110.9472 98.1964 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at -2.4892 -0.1016 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 283 USB1_VBUS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58929A5D)
    (at 110.3884 111.0996 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 0.0254 1.1684 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 250 USB0_VBUS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58929A24)
    (at 116.86032 114.48796 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C13 (at 0.0508 1.0668 450) (layer F.SilkS))
    (fp_text value 18pF (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 201 OSC0_GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 589297B7)
    (at 159.1564 121.7588 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C14 (at -0.0928 -1.0668 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 301 +3V3))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 589297C5)
    (at 156.7688 125.3744 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 0.1016 -1.27 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 301 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 58929C46)
    (at 132.3848 97.8408 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at -2.0828 0 270) (layer F.SilkS))
    (fp_text value BLUE (at 0 1.5 270) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 340 3P3AUX))
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 347 "Net-(D1-Pad1)"))
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 58929C5A)
    (at 123.6472 97.8408 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at -2.0828 0 270) (layer F.SilkS))
    (fp_text value BLUE (at 0 1.5 270) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 312 USR3_LED))
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 348 "Net-(D2-Pad1)"))
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 58929C54)
    (at 125.1966 97.8408 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at -2.0828 0.04064 270) (layer F.SilkS))
    (fp_text value BLUE (at 0 1.5 270) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 279 USR2_LED))
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 349 "Net-(D3-Pad1)"))
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 58929C50)
    (at 126.746 97.8408 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at -2.0828 0.02032 270) (layer F.SilkS))
    (fp_text value BLUE (at 0 1.5 270) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 295 USR1_LED))
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 350 "Net-(D4-Pad1)"))
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 58929C4B)
    (at 128.2954 97.8408 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D5 (at -2.0828 0.00762 270) (layer F.SilkS))
    (fp_text value BLUE (at 0 1.5 270) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 311 USR0_LED))
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 351 "Net-(D5-Pad1)"))
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5892965C)
    (at 145.54708 123.25816 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at -1.3407 0.01016 360) (layer F.SilkS))
    (fp_text value 10K (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 301 +3V3))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58929A06)
    (at 114.4905 117.62994)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 1.651 0.0254) (layer F.SilkS))
    (fp_text value 1.5K (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 301 +3V3))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 I2C0_SCL))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58929A0D)
    (at 114.4905 118.9863)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 1.651 0.0508) (layer F.SilkS))
    (fp_text value 1.5K (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 301 +3V3))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 I2C0_SDA))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 589299D7)
    (at 112.4204 123.2408 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at -0.0508 1.143 270) (layer F.SilkS))
    (fp_text value 1.5K (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 301 +3V3))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 344 "Net-(R4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 589296BB)
    (at 145.51152 128.33096 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at 0 1.1176 450) (layer F.SilkS))
    (fp_text value 10K (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58929F3A)
    (at 116.6876 100.2792 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R21 (at 2.04216 -0.04064 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 101 USB1_DRVVBUS))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58929A9A)
    (at 116.86032 112.25276 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R24 (at 0.0508 -1.0668 90) (layer F.SilkS))
    (fp_text value 1M (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 219 "Net-(C10-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 589298B5)
    (at 115.8312 128.9812)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R25 (at -2.0392 -0.1524) (layer F.SilkS))
    (fp_text value 4.87K (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 TRSTN))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58929783)
    (at 155.2448 121.5572 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R26 (at -1.9812 0 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 301 +3V3))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 104 MMC0_DAT2))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58929789)
    (at 156.5656 121.5572 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R27 (at -1.9884 0 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 301 +3V3))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 103 MMC0_DAT3))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58929790)
    (at 157.8864 121.5572 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R28 (at -1.9884 0.0508 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 301 +3V3))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 123 MMC0_CMD))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58929B5B)
    (at 158.3944 103.5812 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R29 (at -2.04174 0.02032 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 301 +3V3))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 122 MMC0_CLK))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58929C86)
    (at 130.9116 98.298 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R30 (at 2.032 0 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 347 "Net-(D1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58929C98)
    (at 122.184686 98.31073 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R31 (at 1.99393 0.040114 90) (layer F.SilkS))
    (fp_text value 240 (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 348 "Net-(D2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58929C94)
    (at 120.838486 98.31073 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R32 (at 1.99393 0.065514 90) (layer F.SilkS))
    (fp_text value 240 (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 349 "Net-(D3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58929C8F)
    (at 119.492286 98.31073 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R33 (at 1.99393 0.0254 90) (layer F.SilkS))
    (fp_text value 240 (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 350 "Net-(D4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58929C8B)
    (at 118.146086 98.31073 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R34 (at 1.99393 -0.036086 90) (layer F.SilkS))
    (fp_text value 240 (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 351 "Net-(D5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58929B56)
    (at 157.0736 103.5812 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R35 (at -2.0375 0.01778 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 301 +3V3))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 121 MMC0_DAT0))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58929B52)
    (at 155.7528 103.5812 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R36 (at -2.04216 0.02032 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 301 +3V3))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 120 MMC0_DAT1))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pocketbone-kicad:SCHA5B0200 (layer F.Cu) (tedit 58929B39)
    (at 159.5628 112.6236 90)
    (fp_text reference SOK1 (at 9.2964 0.3556 270) (layer F.SilkS))
    (fp_text value SCHA5B0200 (at 0 -16.51 90) (layer F.Fab))
    (pad 11 smd rect (at 7.1875 0 90) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -7.1875 0 90) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -7.1875 -1.265 90) (size 0.9 0.45) (layers F.Cu F.Paste F.Mask)
      (net 301 +3V3))
    (pad 5 smd rect (at 7.1875 -1.265 90) (size 0.9 0.45) (layers F.Cu F.Paste F.Mask)
      (net 122 MMC0_CLK))
    (pad 3 smd rect (at -7.1875 -1.965 90) (size 0.9 0.45) (layers F.Cu F.Paste F.Mask)
      (net 123 MMC0_CMD))
    (pad 6 smd rect (at 7.1875 -1.965 90) (size 0.9 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 7.1875 -2.665 90) (size 0.9 0.45) (layers F.Cu F.Paste F.Mask)
      (net 121 MMC0_DAT0))
    (pad 2 smd rect (at -7.1875 -2.665 90) (size 0.9 0.45) (layers F.Cu F.Paste F.Mask)
      (net 103 MMC0_DAT3))
    (pad 8 smd rect (at 7.1875 -3.365 90) (size 0.9 0.45) (layers F.Cu F.Paste F.Mask)
      (net 120 MMC0_DAT1))
    (pad 1 smd rect (at -7.1875 -3.365 90) (size 0.9 0.45) (layers F.Cu F.Paste F.Mask)
      (net 104 MMC0_DAT2))
    (pad 11 smd rect (at 7.1875 -9.7 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -7.1875 -11 90) (size 0.9 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -5.975 -13.35 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 MMC0_CD))
    (pad 11 smd rect (at -3.425 -13.925 90) (size 1.2 0.95) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 2.575 -13.925 90) (size 1.2 0.95) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 3.775 -13.35 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module pocketbone-kicad:445C33D24M00000 (layer F.Cu) (tedit 58929A4E)
    (at 113.54562 112.26546 270)
    (fp_text reference Y2 (at -3.4036 0.1016 360) (layer F.SilkS))
    (fp_text value 24MHz (at 0.01 -2.19 270) (layer F.Fab))
    (pad 1 smd rect (at -1.9 0 270) (size 1.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 219 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.9 0 270) (size 1.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(C13-Pad1)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58929F0F)
    (at 110.9472 100.9396 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference FB1 (at -2.4892 0 180) (layer F.SilkS))
    (fp_text value FILTER (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 283 USB1_VBUS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 352 "Net-(FB1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58929A66)
    (at 110.3884 113.792 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference FB2 (at -0.0762 -1.2192 180) (layer F.SilkS))
    (fp_text value FILTER (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 250 USB0_VBUS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 353 "Net-(FB2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 (layer F.Cu) (tedit 58929620)
    (at 148.4376 125.3236 90)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 0.0508 270) (layer F.SilkS))
    (fp_text value SW_PUSH_SMALL_H (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 2.7 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(SW1-Pad2)"))
    (pad 1 smd rect (at -2.7 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 (layer F.Cu) (tedit 58929628)
    (at 152.5016 125.3236 90)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW2 (at 0 0.0508 270) (layer F.SilkS))
    (fp_text value SW_PUSH_SMALL_H (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 2.7 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C2-Pad1)"))
    (pad 1 smd rect (at -2.7 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 5892B199)
    (at 136.18718 97.62236)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference TP1 (at 0 2.54 90) (layer B.SilkS) hide)
    (fp_text value 5V (at 1.27 -2.54) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 333 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 5892B1C6)
    (at 111.16564 124.17552)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference TP2 (at 1.9304 -0.0254) (layer B.SilkS) hide)
    (fp_text value WP (at 1.27 -2.54) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 344 "Net-(R4-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 5892B1C3)
    (at 111.16564 121.63552)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference TP3 (at 1.9812 0.0254) (layer B.SilkS) hide)
    (fp_text value GND (at 1.27 -2.54) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 5892B19D)
    (at 138.72718 97.62236)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference TP4 (at 0 2.54 90) (layer B.SilkS) hide)
    (fp_text value 3P3 (at 1.27 -2.54) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 301 +3V3))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 5892B19F)
    (at 141.26718 97.62236)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference TP5 (at 0 2.54 90) (layer B.SilkS) hide)
    (fp_text value SYS_5V (at 1.27 -2.54) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 319 SYS_5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 5892B1A2)
    (at 143.80718 97.62236)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference TP6 (at 0 2.54 90) (layer B.SilkS) hide)
    (fp_text value GND (at 1.27 -2.54) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Sensors:USB_MICRO_B_ST-USB-001E (layer F.Cu) (tedit 589C9A8D)
    (at 106.5008 105.7086 270)
    (descr "USB Micro-B 5-pin SMD connector")
    (tags "USB, Micro-B, connector")
    (attr smd)
    (fp_text reference P1 (at 4.5274 -0.1284 450) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 2 270) (layer F.SilkS) hide)
    (pad 4 smd rect (at 0.65 -4.175 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 253 USB1_ID))
    (pad 2 smd rect (at -0.65 -4.175 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 354 USB1_D_N))
    (pad 3 smd rect (at 0 -4.175 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 355 USB1_D_P))
    (pad 1 smd rect (at -1.3 -4.175 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 352 "Net-(FB1-Pad2)"))
    (pad 5 smd rect (at 1.3 -4.175 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 3.95 -1.5 270) (size 1.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 1.2 -1.5 270) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -1.2 -1.5 270) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -3.95 -1.5 270) (size 1.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Sensors:USB_MICRO_B_ST-USB-001E (layer F.Cu) (tedit 589C9B33)
    (at 106.4754 119.183 270)
    (descr "USB Micro-B 5-pin SMD connector")
    (tags "USB, Micro-B, connector")
    (attr smd)
    (fp_text reference P2 (at -4.5782 -0.1538 450) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 2 270) (layer F.SilkS) hide)
    (pad 4 smd rect (at 0.65 -4.175 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 251 USB0_ID))
    (pad 2 smd rect (at -0.65 -4.175 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 356 USB0_D_N))
    (pad 3 smd rect (at 0 -4.175 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 357 USB0_D_P))
    (pad 1 smd rect (at -1.3 -4.175 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 353 "Net-(FB2-Pad2)"))
    (pad 5 smd rect (at 1.3 -4.175 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 3.95 -1.5 270) (size 1.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 1.2 -1.5 270) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -1.2 -1.5 270) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -3.95 -1.5 270) (size 1.9 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Resistors_SMD:R_Array_Concave_4x0603 (layer F.Cu) (tedit 5892970A)
    (at 146.7548 97.5224 270)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN1 (at -1.9676 -0.019 360) (layer F.SilkS))
    (fp_text value 100K (at 0 2.6 270) (layer F.Fab))
    (pad 2 smd rect (at -0.85 -0.4 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -0.85 0.4 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.85 -1.2 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.85 1.2 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 0.85 -1.2 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 367 "Net-(RN1-Pad8)"))
    (pad 7 smd rect (at 0.85 -0.4 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 368 "Net-(RN1-Pad7)"))
    (pad 6 smd rect (at 0.85 0.4 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 369 "Net-(RN1-Pad6)"))
    (pad 5 smd rect (at 0.85 1.2 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 370 "Net-(RN1-Pad5)"))
    (model Resistors_SMD.3dshapes/R_Array_Concave_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0603 (layer F.Cu) (tedit 58929710)
    (at 143.186 97.5242 90)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN2 (at 2.02528 -0.0062 180) (layer F.SilkS))
    (fp_text value 100K (at 0 2.6 90) (layer F.Fab))
    (pad 2 smd rect (at -0.85 -0.4 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 371 "Net-(RN2-Pad2)"))
    (pad 3 smd rect (at -0.85 0.4 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 372 "Net-(RN2-Pad3)"))
    (pad 1 smd rect (at -0.85 -1.2 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 373 "Net-(RN2-Pad1)"))
    (pad 4 smd rect (at -0.85 1.2 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 374 "Net-(RN2-Pad4)"))
    (pad 8 smd rect (at 0.85 -1.2 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 301 +3V3))
    (pad 7 smd rect (at 0.85 -0.4 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 301 +3V3))
    (pad 6 smd rect (at 0.85 0.4 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 301 +3V3))
    (pad 5 smd rect (at 0.85 1.2 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 301 +3V3))
    (model Resistors_SMD.3dshapes/R_Array_Concave_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0603 (layer F.Cu) (tedit 58929716)
    (at 139.6046 97.5224 270)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN3 (at -2.0184 0.057 360) (layer F.SilkS))
    (fp_text value 100K (at 0 2.6 270) (layer F.Fab))
    (pad 2 smd rect (at -0.85 -0.4 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -0.85 0.4 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.85 -1.2 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.85 1.2 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 0.85 -1.2 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 375 "Net-(RN3-Pad8)"))
    (pad 7 smd rect (at 0.85 -0.4 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 376 "Net-(RN3-Pad7)"))
    (pad 6 smd rect (at 0.85 0.4 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 377 "Net-(RN3-Pad6)"))
    (pad 5 smd rect (at 0.85 1.2 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 378 "Net-(RN3-Pad5)"))
    (model Resistors_SMD.3dshapes/R_Array_Concave_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0603 (layer F.Cu) (tedit 5892971C)
    (at 136.0362 97.5242 270)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN4 (at -1.9694 -0.1078 360) (layer F.SilkS))
    (fp_text value 100K (at 0 2.6 270) (layer F.Fab))
    (pad 2 smd rect (at -0.85 -0.4 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -0.85 0.4 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.85 -1.2 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.85 1.2 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 0.85 -1.2 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 379 "Net-(RN4-Pad8)"))
    (pad 7 smd rect (at 0.85 -0.4 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 380 "Net-(RN4-Pad7)"))
    (pad 6 smd rect (at 0.85 0.4 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 381 "Net-(RN4-Pad6)"))
    (pad 5 smd rect (at 0.85 1.2 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 382 "Net-(RN4-Pad5)"))
    (model Resistors_SMD.3dshapes/R_Array_Concave_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x10 (layer F.Cu) (tedit 589298AD)
    (at 142.34668 128.1176 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P3 (at 24.61006 0.08382 270) (layer F.SilkS))
    (fp_text value CONN_01X10 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 301 +3V3))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 361 UART0_TXD))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 362 UART0_RXD))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 I2C0_SCL))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 I2C0_SDA))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 364 SPI_CLK))
    (pad 7 thru_hole oval (at 15.24 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 363 SPI_CS0))
    (pad 8 thru_hole oval (at 17.78 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 366 SPI_MISO))
    (pad 9 thru_hole oval (at 20.32 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 365 SPI_MOSI))
    (pad 10 thru_hole oval (at 22.86 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x10.wrl
      (at (xyz 0.45 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x02 (layer F.Cu) (tedit 5892A706)
    (at 153.2128 100.6348 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P4 (at 1.27 -2.3368 180) (layer F.SilkS))
    (fp_text value CONN_02X02 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 383 VBAT))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 384 TS))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 385 BAT_SENSE))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x02.wrl
      (at (xyz 0.05 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module libs:boris (layer B.Cu) (tedit 0)
    (at 151.13 112.7252 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module libs:oshpark (layer B.Cu) (tedit 0)
    (at 135.62584 111.79556 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module libs:qwerty (layer B.Cu) (tedit 0)
    (at 112.93856 111.75492 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (gr_text m_w (at 156.68244 125.13056 45) (layer B.SilkS))
  (gr_text "PocketBone KiCAD\nRev. 0 2017" (at 121.0564 112.014 90) (layer B.SilkS))
  (gr_text TS (at 155.30322 98.06686 90) (layer B.SilkS))
  (gr_text VBAT (at 155.34386 100.838 90) (layer B.SilkS))
  (gr_text BS (at 148.51888 100.63988 90) (layer B.SilkS))
  (gr_text GND (at 148.55444 98.00082 90) (layer B.SilkS))
  (gr_text SPI0_CS0 (at 127.22606 123.02998 90) (layer B.SilkS))
  (gr_text BATTERY (at 151.9428 96.0628) (layer F.SilkS))
  (gr_text GND (at 119.53494 125.05436 90) (layer B.SilkS))
  (gr_text SPI0_MOSI (at 122.10034 122.73534 90) (layer B.SilkS))
  (gr_text SPI0_MISO (at 124.6632 122.69978 90) (layer B.SilkS))
  (gr_text SPI0_SCLK (at 129.78892 122.59056 90) (layer B.SilkS))
  (gr_text I2C0_SDA (at 132.24256 123.02998 90) (layer B.SilkS))
  (gr_text I2C0_SCL (at 134.80542 123.10364 90) (layer B.SilkS))
  (gr_text UART0_RXD (at 137.36828 122.55246 90) (layer B.SilkS))
  (gr_text UART0_TXD (at 139.9667 122.66422 90) (layer B.SilkS))
  (gr_text +3V3 (at 142.38478 124.60478 90) (layer B.SilkS))
  (gr_text WP (at 112.86236 124.32792 90) (layer B.SilkS))
  (gr_text GND (at 112.82934 121.6406 90) (layer B.SilkS))
  (gr_text +5V (at 136.398 100.5332 90) (layer B.SilkS))
  (gr_text +3V3 (at 138.8872 101.0412 90) (layer B.SilkS))
  (gr_text SYS_5V (at 141.478 101.8032 90) (layer B.SilkS))
  (gr_text GND (at 144.018 100.584 90) (layer B.SilkS))
  (gr_text USR (at 129.5654 97.71888 90) (layer F.SilkS))
  (gr_text PWR (at 133.67766 97.663 90) (layer F.SilkS))
  (gr_text POWER (at 148.5392 120.904) (layer F.SilkS))
  (gr_text RESET (at 152.40508 120.89892) (layer F.SilkS))
  (gr_arc (start 150.96636 104.93016) (end 150.96636 94.93016) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 150.96636 119.93016) (end 160.96636 119.93016) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 115.96636 104.93016) (end 105.96636 104.93016) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 115.96636 119.93016) (end 115.96636 129.93016) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.96636 129.93016) (end 150.96636 129.93016) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.96636 104.93016) (end 160.96636 119.93016) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.96636 94.93016) (end 150.96636 94.93016) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 105.96636 104.93016) (end 105.96636 119.93016) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.08158 93.91396) (xy 104.08158 132.01396) (xy 162.50158 132.01396) (xy 162.50158 93.91396)
      )
    )
  )
  (zone (net 301) (net_name +3V3) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162.50158 93.91396) (xy 104.08158 93.91396) (xy 104.08158 132.01396) (xy 162.50158 132.01396)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.08158 93.91396) (xy 104.08158 132.01396) (xy 162.50158 132.01396) (xy 162.50158 93.91396)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.08158 93.91396) (xy 104.08158 132.01396) (xy 162.50158 132.01396) (xy 162.50158 93.91396)
      )
    )
  )
)
