(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6)
    (drawings 23)
    (tracks 58)
    (zones 0)
    (modules 14)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.635)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1 0.7)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4 4)
    (pad_drill 2.5)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 171.6 90.1)
    (visible_elements 7FFDFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 GND)
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(D1-Pad1)")
  (net 6 "Net-(D2-Pad1)")
  (net 7 "Net-(R1-Pad2)")
  (net 8 "Net-(R2-Pad1)")
  (net 9 "Net-(R3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
  )
  (module modules:CK_MINI_SLIDE_SWITCH (layer F.Cu) (tedit 5C88CD12)
    (at 180.3 87.3 90)
    (fp_text reference SW1 (at 0.1 -1.3 90) (layer F.SilkS) hide)
    (fp_text value POWER (at 0 1.27 90) (layer F.Fab) hide)
    (pad 4 thru_hole oval (at -4.1 0 90) (size 2 4) (drill 1.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at -2 0 90) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 3 thru_hole circle (at 2 0 90) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 4 thru_hole oval (at 4.1 0 90) (size 2 4) (drill 1.5) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C352302)
    (at 169.3 91.6 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 0 1.1938 270) (layer F.SilkS) hide)
    (fp_text value BAT (at -1.905 1.27) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5C88CFF9)
    (at 172 86.4 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D2 (at 0.1 1.5 180) (layer B.SilkS))
    (fp_text value CHG (at 0.0508 1.6002 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 5C88C9CE)
    (at 156 87.4)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value "Mounting Holes" (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.75) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module Mounting_Holes:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 5C88C9C9)
    (at 186 87.4)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.75) (layers *.Cu *.Mask))
  )
  (module modules:SOIC-8-N-POWERPAD (layer F.Cu) (tedit 5C88CF27)
    (at 164.7 85.7 270)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at -3 3.5) (layer F.SilkS))
    (fp_text value TP4056 (at 0 1.27 270) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 7 smd rect (at -0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R3-Pad1)"))
    (pad 6 smd rect (at 0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R2-Pad1)"))
    (pad 5 smd rect (at 1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 4 smd rect (at 1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 3 smd rect (at 0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R1-Pad2)"))
    (pad 1 smd rect (at -1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 thru_hole rect (at 0 0 270) (size 4 4) (drill 2.5) (layers *.Cu *.Mask)
      (net 3 GND) (zone_connect 2))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C88CFDE)
    (at 166.8 89.2 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 2.2 -1.4 180) (layer B.SilkS))
    (fp_text value 10u (at -0.0254 0 180) (layer B.Fab))
    (fp_text user %R (at 2.9 -1.3 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C88CFE4)
    (at 161.2 89.2)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -3 1.2) (layer B.SilkS))
    (fp_text value 10u (at 0 -0.0254) (layer B.Fab))
    (fp_text user %R (at -3.1 0.4) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5C87AAA6)
    (at 172 88.4 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D1 (at 0 -1.7 180) (layer B.SilkS))
    (fp_text value STBY (at -0.0254 -1.7526 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C352304)
    (at 175.8 91.6 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at -0.0508 1.2446 270) (layer F.SilkS) hide)
    (fp_text value OUT (at -1.905 1.27) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C352308)
    (at 160.1 91.6 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J3 (at 0 1.27 90) (layer F.SilkS) hide)
    (fp_text value IN (at 1.905 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5C87AAE2)
    (at 161.1 85.7 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 3 0) (layer B.SilkS))
    (fp_text value PRG (at 0.1016 0.1016 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(R1-Pad2)"))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C87AA4B)
    (at 173.417 85.852)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 3.383 0.048) (layer F.SilkS))
    (fp_text value 1K (at 0.1016 0.0254) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C87AA4D)
    (at 173.417 83.312)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 3.283 0.088) (layer F.SilkS))
    (fp_text value 1K (at 0.1778 0.0254) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 11.1 (width 0.3) (layer Cmts.User)
    (gr_text "11.100 mm" (at 194.1 87.35 90) (layer Cmts.User))
    (feature1 (pts (xy 189.5 81.8) (xy 192.586421 81.8)))
    (feature2 (pts (xy 189.5 92.9) (xy 192.586421 92.9)))
    (crossbar (pts (xy 192 92.9) (xy 192 81.8)))
    (arrow1a (pts (xy 192 81.8) (xy 192.586421 82.926504)))
    (arrow1b (pts (xy 192 81.8) (xy 191.413579 82.926504)))
    (arrow2a (pts (xy 192 92.9) (xy 192.586421 91.773496)))
    (arrow2b (pts (xy 192 92.9) (xy 191.413579 91.773496)))
  )
  (dimension 5 (width 0.3) (layer Cmts.User)
    (gr_text "5.000 mm" (at 183.5 79.2) (layer Cmts.User))
    (feature1 (pts (xy 181 87.4) (xy 181 80.713579)))
    (feature2 (pts (xy 186 87.4) (xy 186 80.713579)))
    (crossbar (pts (xy 186 81.3) (xy 181 81.3)))
    (arrow1a (pts (xy 181 81.3) (xy 182.126504 80.713579)))
    (arrow1b (pts (xy 181 81.3) (xy 182.126504 81.886421)))
    (arrow2a (pts (xy 186 81.3) (xy 184.873496 80.713579)))
    (arrow2b (pts (xy 186 81.3) (xy 184.873496 81.886421)))
  )
  (dimension 13.3 (width 0.3) (layer Cmts.User)
    (gr_text "13.300 mm" (at 179.35 96.7) (layer Cmts.User))
    (feature1 (pts (xy 172.7 87.4) (xy 172.7 95.186421)))
    (feature2 (pts (xy 186 87.4) (xy 186 95.186421)))
    (crossbar (pts (xy 186 94.6) (xy 172.7 94.6)))
    (arrow1a (pts (xy 172.7 94.6) (xy 173.826504 94.013579)))
    (arrow1b (pts (xy 172.7 94.6) (xy 173.826504 95.186421)))
    (arrow2a (pts (xy 186 94.6) (xy 184.873496 94.013579)))
    (arrow2b (pts (xy 186 94.6) (xy 184.873496 95.186421)))
  )
  (dimension 37 (width 0.3) (layer Cmts.User)
    (gr_text "37.000 mm" (at 171 104.8) (layer Cmts.User))
    (feature1 (pts (xy 152.5 92.9) (xy 152.5 103.286421)))
    (feature2 (pts (xy 189.5 92.9) (xy 189.5 103.286421)))
    (crossbar (pts (xy 189.5 102.7) (xy 152.5 102.7)))
    (arrow1a (pts (xy 152.5 102.7) (xy 153.626504 102.113579)))
    (arrow1b (pts (xy 152.5 102.7) (xy 153.626504 103.286421)))
    (arrow2a (pts (xy 189.5 102.7) (xy 188.373496 102.113579)))
    (arrow2b (pts (xy 189.5 102.7) (xy 188.373496 103.286421)))
  )
  (dimension 30 (width 0.3) (layer Cmts.User)
    (gr_text "30.000 mm" (at 171 100.9) (layer Cmts.User))
    (feature1 (pts (xy 186 87.4) (xy 186 99.386421)))
    (feature2 (pts (xy 156 87.4) (xy 156 99.386421)))
    (crossbar (pts (xy 156 98.8) (xy 186 98.8)))
    (arrow1a (pts (xy 186 98.8) (xy 184.873496 99.386421)))
    (arrow1b (pts (xy 186 98.8) (xy 184.873496 98.213579)))
    (arrow2a (pts (xy 156 98.8) (xy 157.126504 99.386421)))
    (arrow2b (pts (xy 156 98.8) (xy 157.126504 98.213579)))
  )
  (gr_line (start 189.5 92.9) (end 152.5 92.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.5 81.8) (end 189.5 81.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 189.5 81.8) (end 189.5 92.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.5 81.8) (end 152.5 92.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text 5V (at 156.7 91.6) (layer F.SilkS))
  (gr_text CHG (at 176.6 86.5) (layer B.SilkS))
  (gr_text STBY (at 176.9 88.4) (layer B.SilkS))
  (gr_text J313 (at 156 83.3) (layer B.SilkS))
  (gr_text - (at 165.9 89.2) (layer F.SilkS))
  (gr_text - (at 172.1 89.1) (layer F.SilkS))
  (gr_text - (at 162.9 89.1) (layer F.SilkS))
  (gr_text + (at 159.9 89.1) (layer F.SilkS))
  (gr_text + (at 176.5 89.1) (layer F.SilkS))
  (gr_text + (at 169.9 89.2) (layer F.SilkS))
  (gr_text OUT (at 174.4 89.2) (layer F.SilkS))
  (gr_text IN (at 161.4 89.2) (layer F.SilkS))
  (gr_text BAT (at 167.9 89.2) (layer F.SilkS))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.5 81.8) (xy 152.5 92.9) (xy 189.5 92.9) (xy 189.5 81.8)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.5 81.8) (xy 152.5 92.9) (xy 189.5 92.9) (xy 189.5 81.8)
      )
    )
  )
)
