(kicad_pcb (version 20171130) (host pcbnew 5.1.5-52549c5~84~ubuntu19.10.1)
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 102)
    (zones 0)
    (modules 2)
    (nets 33)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1.6)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "zip/"))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad1)")
  (net 2 "Net-(U1-Pad17)")
  (net 3 "Net-(U1-Pad2)")
  (net 4 "Net-(U1-Pad18)")
  (net 5 "Net-(U1-Pad3)")
  (net 6 "Net-(U1-Pad19)")
  (net 7 "Net-(U1-Pad4)")
  (net 8 "Net-(U1-Pad20)")
  (net 9 "Net-(U1-Pad5)")
  (net 10 "Net-(U1-Pad21)")
  (net 11 "Net-(U1-Pad6)")
  (net 12 "Net-(U1-Pad22)")
  (net 13 "Net-(U1-Pad7)")
  (net 14 "Net-(U1-Pad23)")
  (net 15 "Net-(U1-Pad8)")
  (net 16 "Net-(U1-Pad24)")
  (net 17 "Net-(U1-Pad9)")
  (net 18 "Net-(U1-Pad25)")
  (net 19 "Net-(U1-Pad10)")
  (net 20 "Net-(U1-Pad26)")
  (net 21 "Net-(U1-Pad11)")
  (net 22 "Net-(U1-Pad27)")
  (net 23 "Net-(U1-Pad12)")
  (net 24 "Net-(U1-Pad28)")
  (net 25 "Net-(U1-Pad13)")
  (net 26 "Net-(U1-Pad29)")
  (net 27 "Net-(U1-Pad14)")
  (net 28 "Net-(U1-Pad30)")
  (net 29 "Net-(U1-Pad15)")
  (net 30 "Net-(U1-Pad31)")
  (net 31 "Net-(U1-Pad16)")
  (net 32 "Net-(U1-Pad32)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
  )
  (module Package_DIP:DIP-32_W15.24mm_Socket (layer F.Cu) (tedit 5E5B6EB0)
    (at 122.555 86.995)
    (descr "32-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket")
    (fp_text reference "plcc32 adaptor" (at 7.62 3.67) (layer F.SilkS))
    (fp_text value 27C040 (at 7.62 40.43) (layer F.Fab) hide)
    (fp_text user %R (at 7.62 19.05) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(U1-Pad1)"))
    (pad 17 thru_hole oval (at 15.24 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad17)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad2)"))
    (pad 18 thru_hole oval (at 15.24 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad18)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(U1-Pad3)"))
    (pad 19 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(U1-Pad19)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(U1-Pad4)"))
    (pad 20 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(U1-Pad20)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(U1-Pad5)"))
    (pad 21 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(U1-Pad21)"))
    (pad 6 thru_hole circle (at 0 12.7) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(U1-Pad6)"))
    (pad 22 thru_hole circle (at 15.24 25.4) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(U1-Pad22)"))
    (pad 7 thru_hole circle (at 0 15.24) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad7)"))
    (pad 23 thru_hole circle (at 15.24 22.86) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(U1-Pad23)"))
    (pad 8 thru_hole circle (at 0 17.78) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(U1-Pad8)"))
    (pad 24 thru_hole circle (at 15.24 20.32) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(U1-Pad24)"))
    (pad 9 thru_hole circle (at 0 20.32) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad9)"))
    (pad 25 thru_hole circle (at 15.24 17.78) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(U1-Pad25)"))
    (pad 10 thru_hole circle (at 0 22.86) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(U1-Pad10)"))
    (pad 26 thru_hole circle (at 15.24 15.24) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(U1-Pad26)"))
    (pad 11 thru_hole circle (at 0 25.4) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(U1-Pad11)"))
    (pad 27 thru_hole circle (at 15.24 12.7) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(U1-Pad27)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(U1-Pad12)"))
    (pad 28 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(U1-Pad28)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(U1-Pad13)"))
    (pad 29 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(U1-Pad29)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(U1-Pad14)"))
    (pad 30 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(U1-Pad30)"))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad15)"))
    (pad 31 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(U1-Pad31)"))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(U1-Pad16)"))
    (pad 32 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(U1-Pad32)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-32_W15.24mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_PLCC:PLCC-32_THT-Socket (layer F.Cu) (tedit 5E5B6D36)
    (at 130.175 106.045)
    (descr "Socket PLCC 32 pins,  round pads")
    (tags PLCC)
    (fp_text reference U2 (at 0 12.065) (layer F.SilkS) hide)
    (fp_text value 27C040 (at 0 0 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 1.27 -5.08) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "Net-(U1-Pad1)"))
    (pad 2 thru_hole circle (at -1.27 -7.62) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad2)"))
    (pad 3 thru_hole circle (at -1.27 -5.08) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 "Net-(U1-Pad3)"))
    (pad 4 thru_hole circle (at -3.81 -7.62) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 7 "Net-(U1-Pad4)"))
    (pad 5 thru_hole circle (at -6.35 -5.08) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 9 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at -3.81 -5.08) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 "Net-(U1-Pad6)"))
    (pad 7 thru_hole circle (at -6.35 -2.54) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad7)"))
    (pad 8 thru_hole circle (at -3.81 -2.54) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 15 "Net-(U1-Pad8)"))
    (pad 9 thru_hole circle (at -6.35 0) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad9)"))
    (pad 10 thru_hole circle (at -3.81 0) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 19 "Net-(U1-Pad10)"))
    (pad 11 thru_hole circle (at -6.35 2.54) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 21 "Net-(U1-Pad11)"))
    (pad 12 thru_hole circle (at -3.81 2.54) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 23 "Net-(U1-Pad12)"))
    (pad 13 thru_hole circle (at -6.35 5.08) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 25 "Net-(U1-Pad13)"))
    (pad 14 thru_hole circle (at -3.81 7.62) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 27 "Net-(U1-Pad14)"))
    (pad 15 thru_hole circle (at -3.81 5.08) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad15)"))
    (pad 16 thru_hole circle (at -1.27 7.62) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 31 "Net-(U1-Pad16)"))
    (pad 17 thru_hole circle (at -1.27 5.08) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad17)"))
    (pad 18 thru_hole circle (at 1.27 7.62) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad18)"))
    (pad 19 thru_hole circle (at 1.27 5.08) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 6 "Net-(U1-Pad19)"))
    (pad 20 thru_hole circle (at 3.81 7.62) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 8 "Net-(U1-Pad20)"))
    (pad 21 thru_hole circle (at 6.35 5.08) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 10 "Net-(U1-Pad21)"))
    (pad 22 thru_hole circle (at 3.81 5.08) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 12 "Net-(U1-Pad22)"))
    (pad 23 thru_hole circle (at 6.35 2.54) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 14 "Net-(U1-Pad23)"))
    (pad 24 thru_hole circle (at 3.81 2.54) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 16 "Net-(U1-Pad24)"))
    (pad 25 thru_hole circle (at 6.35 0) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 18 "Net-(U1-Pad25)"))
    (pad 26 thru_hole circle (at 3.81 0) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 20 "Net-(U1-Pad26)"))
    (pad 27 thru_hole circle (at 6.35 -2.54) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 22 "Net-(U1-Pad27)"))
    (pad 28 thru_hole circle (at 3.81 -2.54) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 24 "Net-(U1-Pad28)"))
    (pad 31 thru_hole circle (at 3.81 -5.08) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 30 "Net-(U1-Pad31)"))
    (pad 32 thru_hole circle (at 1.27 -7.62) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 32 "Net-(U1-Pad32)"))
    (pad 29 thru_hole circle (at 6.35 -5.08) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 26 "Net-(U1-Pad29)"))
    (pad 30 thru_hole circle (at 3.81 -7.62) (size 1.2 1.2) (drill 0.8128) (layers *.Cu *.Mask)
      (net 28 "Net-(U1-Pad30)"))
  )
  (gr_line (start 120.9548 85.344) (end 139.3952 85.344) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 120.9548 126.746) (end 120.9548 85.344) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 139.3952 126.746) (end 120.9548 126.746) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 139.3952 85.344) (end 139.3952 126.746) (layer Edge.Cuts) (width 0.05))
)
