(kicad_pcb (version 20171130) (host pcbnew 5.1.4+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 108)
    (zones 0)
    (modules 16)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.154)
    (user_trace_width 0.254)
    (user_trace_width 0.635)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.15)
    (via_size 0.635)
    (via_drill 0.381)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 0.762 0.381)
    (user_via 1.27 0.635)
    (uvia_size 0.381)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1.6)
    (pad_drill 1.1)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 SDA)
  (net 4 SCL)
  (net 5 /TxD)
  (net 6 /RxD)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 0.381)
    (uvia_drill 0.254)
    (diff_pair_width 0.254)
    (diff_pair_gap 0.254)
    (add_net +3V3)
    (add_net /RxD)
    (add_net /TxD)
    (add_net GND)
    (add_net "Net-(S3-Pad3)")
    (add_net "Net-(S3-Pad4)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad33)")
    (add_net "Net-(U1-Pad34)")
    (add_net "Net-(U1-Pad35)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
    (add_net SCL)
    (add_net SDA)
  )
  (net_class Minimum ""
    (clearance 0.154)
    (trace_width 0.154)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.254)
    (diff_pair_gap 0.254)
  )
  (net_class Power ""
    (clearance 0.635)
    (trace_width 1.27)
    (via_dia 0.635)
    (via_drill 0.508)
    (uvia_dia 0.381)
    (uvia_drill 0.254)
    (diff_pair_width 0.254)
    (diff_pair_gap 0.254)
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 173.99 91.44)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H5 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 123.19 110.49)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H4 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 123.19 72.39)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H3 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5EB0E103)
    (at 135.89 73.66 90)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference S2 (at 0 -2.77 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 0 10.39 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 SDA))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 4 SCL))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLX90614ESF-DCA-000-TU:TO254P942H425-4 (layer F.Cu) (tedit 5EB0E139)
    (at 139.7 83.82)
    (fp_text reference S1 (at -5.715 -1.905) (layer F.SilkS))
    (fp_text value MLX90614ESF-DCA-000-TU (at 13.224 5.496) (layer F.Fab) hide)
    (pad 4 thru_hole circle (at 0 -2.54) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 SDA))
    (pad 1 thru_hole roundrect (at -2.54 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 4 SCL))
    (model ${KIPRJMOD}/MLX90614ESF-DAA-000-TU--3DModel-STEP-56544.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 5EB0E108)
    (at 156.21 86.995 90)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference S42 (at 0 16.51) (layer F.SilkS))
    (fp_text value TOF10120 (at 0 15.47 90) (layer F.Fab))
    (fp_text user %R (at 0 6.35) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SCL))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 SDA))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /TxD))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /RxD))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module teensy:Teensy30_31_32_LC (layer F.Cu) (tedit 5EB0E147)
    (at 152.4 101.6)
    (fp_text reference U1 (at -17.145 -10.16) (layer F.SilkS))
    (fp_text value Teensy-LC (at 0 10.16) (layer F.Fab))
    (fp_text user Vin (at -16.51 -5.08 90) (layer F.SilkS))
    (fp_text user GND (at -13.83 -2.695 90) (layer F.SilkS))
    (fp_text user Vusb (at -13.97 1.27 90) (layer F.SilkS))
    (fp_text user 3V3 (at -11.43 -5.08 90) (layer F.SilkS))
    (fp_text user 23 (at -8.89 -3.175 90) (layer F.SilkS))
    (fp_text user 22 (at -6.35 -3.175 270) (layer F.SilkS))
    (fp_text user 21 (at -3.81 -3.175 90) (layer F.SilkS))
    (fp_text user 20 (at -1.27 -5.08 90) (layer F.SilkS))
    (fp_text user 19 (at 1.27 -5.08 90) (layer F.SilkS))
    (fp_text user 18 (at 3.81 -5.08 90) (layer F.SilkS))
    (fp_text user 17 (at 6.35 -5.08 90) (layer F.SilkS))
    (fp_text user 16 (at 8.89 -5.08 90) (layer F.SilkS))
    (fp_text user 15 (at 11.43 -5.08 90) (layer F.SilkS))
    (fp_text user 14 (at 13.97 -5.08 90) (layer F.SilkS))
    (fp_text user 2 (at -8.89 5.08 90) (layer F.SilkS))
    (fp_text user 7 (at 3.81 5.08 90) (layer F.SilkS))
    (fp_text user 6 (at 1.27 5.08 90) (layer F.SilkS))
    (fp_text user 4 (at -3.81 5.08 90) (layer F.SilkS))
    (fp_text user 10 (at 11.43 5.08 90) (layer F.SilkS))
    (fp_text user 5 (at -1.27 5.08 90) (layer F.SilkS))
    (fp_text user 8 (at 6.35 5.08 90) (layer F.SilkS))
    (fp_text user 3 (at -6.35 5.08 270) (layer F.SilkS))
    (fp_text user 9 (at 8.89 5.08 90) (layer F.SilkS))
    (fp_text user 11 (at 13.97 5.08 90) (layer F.SilkS))
    (fp_text user 1 (at -11.43 5.08 90) (layer F.SilkS))
    (fp_text user 0 (at -13.97 5.08 90) (layer F.SilkS))
    (fp_text user Aref (at -8.89 1.27 90) (layer F.SilkS))
    (fp_text user 24 (at -6.35 0.635 90) (layer F.SilkS))
    (fp_text user 25 (at -3.81 0.635 90) (layer F.SilkS))
    (fp_text user Prg (at 13.97 -2.54) (layer F.SilkS))
    (fp_text user GND (at 13.97 0) (layer F.SilkS))
    (fp_text user 3V3 (at 13.97 2.54) (layer F.SilkS))
    (fp_text user GND (at -16.51 5.08 90) (layer F.SilkS))
    (pad 1 thru_hole roundrect (at -16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 thru_hole circle (at -13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 37 thru_hole circle (at -3.81 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 36 thru_hole circle (at -6.35 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 35 thru_hole circle (at -8.89 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 34 thru_hole circle (at -13.97 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 33 thru_hole circle (at -16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 32 thru_hole circle (at -13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 31 thru_hole circle (at -11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 30 thru_hole circle (at -8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 29 thru_hole circle (at -6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 28 thru_hole circle (at -3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 27 thru_hole circle (at -1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 26 thru_hole circle (at 1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 SCL))
    (pad 25 thru_hole circle (at 3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 SDA))
    (pad 24 thru_hole circle (at 6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at 8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at 11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 21 thru_hole circle (at 13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 16.51 5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 16.51 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at 16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 16.51 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 18 thru_hole circle (at 16.51 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at 16.51 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x14_P2.54mm_Vertical.wrl
      (offset (xyz 16.5 7.62 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x14_P2.54mm_Vertical.wrl
      (offset (xyz 16.5 -7.62 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 144.145 79.375 135)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at -3.592102 0 135) (layer F.SilkS))
    (fp_text value "0.1 u" (at 0 1.65 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 135) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 135) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:DFN-6-1EP_3x3mm_P1mm_EP1.5x2.4mm (layer F.Cu) (tedit 5EB0C96A)
    (at 125.048 82.588)
    (descr "DFN, 6 Pin (https://www.silabs.com/documents/public/data-sheets/Si7020-A20.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "DFN DFN_QFN")
    (attr smd)
    (fp_text reference S3 (at 1.317 -2.578) (layer F.SilkS))
    (fp_text value Si7021-A20 (at 0 2.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 6 smd roundrect (at 1.65 -1) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 SCL))
    (pad 5 smd roundrect (at 1.65 0) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (pad 4 smd roundrect (at 1.65 1) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -1.65 1) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -1.65 0) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.65 -1) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 SDA))
    (pad "" smd roundrect (at 0.375 0.6) (size 0.6 0.97) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.375 -0.6) (size 0.6 0.97) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.375 0.6) (size 0.6 0.97) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.375 -0.6) (size 0.6 0.97) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at 0 0) (size 1.5 2.4) (layers F.Cu F.Mask) (roundrect_rratio 0.166667)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-6-1EP_3x3mm_P1mm_EP1.5x2.4mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 125.984 85.344 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 3.429 -0.381) (layer F.SilkS))
    (fp_text value "0.1 u" (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad locked (layer F.Cu) (tedit 56D1B4CB)
    (at 169.7 72.39)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad locked (layer F.Cu) (tedit 56D1B4CB)
    (at 155.3 72.39)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_1.00mm:PinHeader_1x06_P1.00mm_Vertical (layer F.Cu) (tedit 5EB0CF07)
    (at 160 90 90)
    (descr "Through hole straight pin header, 1x06, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x06 1.00mm single row")
    (fp_text reference S41 (at 0 8.91 180) (layer F.SilkS))
    (fp_text value TOF10120 (at 0 6.56 90) (layer F.Fab))
    (fp_text user %R (at 0 2.5) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 5 90) (size 1.05 0.65) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 SCL))
    (pad 5 thru_hole oval (at 0 4 90) (size 1.05 0.65) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 SDA))
    (pad 4 thru_hole oval (at 0 3 90) (size 1.05 0.65) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 /TxD))
    (pad 3 thru_hole oval (at 0 2 90) (size 1.05 0.65) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 /RxD))
    (pad 2 thru_hole oval (at 0 1 90) (size 1.05 0.65) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.05 0.65) (drill 0.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x06_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 149.225 88.9 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 4.445 0 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 SCL))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 146.05 88.9 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 4.445 0 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 SDA))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric_Pad1.42x2.65mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 126.492 88.9 180)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 10u (at 0 2.279999 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "WPSA 6915 Temperature Screening\nCriterion Manufacturing\n20200504 Rev A" (at 174.625 78.74) (layer B.SilkS))
  (gr_text SDA (at 156.21 90.805 90) (layer F.SilkS))
  (gr_text SCL (at 153.67 90.805 90) (layer F.SilkS))
  (gr_line (start 119.38 68.58) (end 177.8 68.58) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 119.38 114.3) (end 119.38 68.58) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 177.8 114.3) (end 119.38 114.3) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 177.8 68.58) (end 177.8 114.3) (layer Edge.Cuts) (width 0.254))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 1))
    (polygon
      (pts
        (xy 120.396 69.596) (xy 176.784 69.596) (xy 176.784 113.284) (xy 120.396 113.284)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 1))
    (polygon
      (pts
        (xy 120.396 69.596) (xy 176.784 69.596) (xy 176.784 113.284) (xy 120.396 113.284)
      )
    )
  )
)
