(kicad_pcb (version 20171130) (host pcbnew "(5.0.1)-3")
  (general
    (thickness 1.6)
    (drawings 19)
    (tracks 437)
    (zones 0)
    (modules 25)
    (nets 122)
  )
  (page A)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad26)")
  (net 2 "Net-(U1-Pad28)")
  (net 3 "Net-(U1-Pad29)")
  (net 4 "Net-(U1-Pad36)")
  (net 5 "Net-(U1-Pad37)")
  (net 6 "Net-(U1-Pad12)")
  (net 7 "Net-(U1-Pad38)")
  (net 8 "Net-(U1-Pad52)")
  (net 9 "Net-(U1-Pad63)")
  (net 10 "Net-(U1-Pad64)")
  (net 11 "Net-(U1-Pad65)")
  (net 12 "Net-(U1-Pad66)")
  (net 13 "Net-(U1-Pad67)")
  (net 14 "Net-(U1-Pad68)")
  (net 15 "Net-(U1-Pad69)")
  (net 16 "Net-(U1-Pad70)")
  (net 17 "Net-(U1-Pad71)")
  (net 18 "Net-(U1-Pad72)")
  (net 19 "Net-(U1-Pad73)")
  (net 20 "Net-(U1-Pad74)")
  (net 21 "Net-(U1-Pad75)")
  (net 22 "Net-(U1-Pad76)")
  (net 23 "Net-(U1-Pad77)")
  (net 24 "Net-(U1-Pad78)")
  (net 25 "Net-(U1-Pad79)")
  (net 26 "Net-(U1-Pad80)")
  (net 27 "Net-(U1-Pad81)")
  (net 28 "Net-(U1-Pad82)")
  (net 29 "Net-(U1-Pad83)")
  (net 30 "Net-(U1-Pad84)")
  (net 31 "Net-(U1-Pad85)")
  (net 32 "Net-(U1-Pad86)")
  (net 33 "Net-(U2-Pad14)")
  (net 34 "Net-(S1-Pad2)")
  (net 35 "Net-(S1-Pad4)")
  (net 36 ATT_DATA)
  (net 37 Band5)
  (net 38 Band3)
  (net 39 ATT_CLK)
  (net 40 ATT_LE)
  (net 41 MISO)
  (net 42 Band4)
  (net 43 Band2)
  (net 44 Band1)
  (net 45 TFT_RST)
  (net 46 GND)
  (net 47 B1)
  (net 48 B2)
  (net 49 B3)
  (net 50 B4)
  (net 51 B7)
  (net 52 B5)
  (net 53 MCLK)
  (net 54 BCLK)
  (net 55 "Net-(SW2-PadE1)")
  (net 56 MOSI)
  (net 57 "Net-(SW2-PadA1)")
  (net 58 "Net-(SW2-PadB1)")
  (net 59 /Backlight)
  (net 60 "Net-(SW1-PadB1)")
  (net 61 "Net-(SW1-PadA1)")
  (net 62 "Net-(SW1-PadE1)")
  (net 63 RX)
  (net 64 SCLK)
  (net 65 VOL)
  (net 66 SDA)
  (net 67 SCL)
  (net 68 TFT_DC)
  (net 69 TFT_CS)
  (net 70 TX)
  (net 71 LRCLK)
  (net 72 +3V3)
  (net 73 "Net-(SW1-PadMH1)")
  (net 74 "Net-(SW1-PadMH2)")
  (net 75 "Net-(SW2-PadMH2)")
  (net 76 "Net-(SW2-PadMH1)")
  (net 77 "Net-(SW3-PadMH1)")
  (net 78 "Net-(SW3-PadMH2)")
  (net 79 "Net-(S2-Pad2)")
  (net 80 "Net-(S2-Pad4)")
  (net 81 "Net-(S3-Pad4)")
  (net 82 "Net-(S3-Pad2)")
  (net 83 "Net-(S4-Pad2)")
  (net 84 "Net-(S4-Pad4)")
  (net 85 "Net-(R3-Pad2)")
  (net 86 "Net-(R1-Pad2)")
  (net 87 +5V)
  (net 88 "Net-(R1-Pad1)")
  (net 89 "Net-(R3-Pad1)")
  (net 90 "Net-(S7-Pad2)")
  (net 91 "Net-(S7-Pad4)")
  (net 92 T_CS)
  (net 93 "Net-(Q1-Pad1)")
  (net 94 "Net-(Q1-Pad3)")
  (net 95 "Net-(R7-Pad2)")
  (net 96 "Net-(U2-Pad15)")
  (net 97 "Net-(U2-Pad16)")
  (net 98 "Net-(U2-Pad17)")
  (net 99 "Net-(U2-Pad18)")
  (net 100 PWR)
  (net 101 "Net-(S5-Pad2)")
  (net 102 "Net-(S5-Pad4)")
  (net 103 "Net-(BAT1-Pad1)")
  (net 104 "Net-(J2-Pad2)")
  (net 105 "Net-(J2-Pad6)")
  (net 106 "Net-(J2-Pad10)")
  (net 107 "Net-(J2-Pad1)")
  (net 108 "Net-(J2-Pad7)")
  (net 109 "Net-(J2-Pad11)")
  (net 110 "Net-(J2-Pad13)")
  (net 111 "Net-(J1-Pad3)")
  (net 112 "Net-(J1-Pad5)")
  (net 113 "Net-(J1-Pad7)")
  (net 114 "Net-(J1-Pad9)")
  (net 115 "Net-(J1-Pad2)")
  (net 116 "Net-(J1-Pad4)")
  (net 117 "Net-(J1-Pad6)")
  (net 118 "Net-(J1-Pad8)")
  (net 119 "Net-(J1-Pad10)")
  (net 120 "Net-(J1-Pad12)")
  (net 121 "Net-(J1-Pad14)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /Backlight)
    (add_net ATT_CLK)
    (add_net ATT_DATA)
    (add_net ATT_LE)
    (add_net B1)
    (add_net B2)
    (add_net B3)
    (add_net B4)
    (add_net B5)
    (add_net B7)
    (add_net BCLK)
    (add_net Band1)
    (add_net Band2)
    (add_net Band3)
    (add_net Band4)
    (add_net Band5)
    (add_net GND)
    (add_net LRCLK)
    (add_net MCLK)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(BAT1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(S1-Pad2)")
    (add_net "Net-(S1-Pad4)")
    (add_net "Net-(S2-Pad2)")
    (add_net "Net-(S2-Pad4)")
    (add_net "Net-(S3-Pad2)")
    (add_net "Net-(S3-Pad4)")
    (add_net "Net-(S4-Pad2)")
    (add_net "Net-(S4-Pad4)")
    (add_net "Net-(S5-Pad2)")
    (add_net "Net-(S5-Pad4)")
    (add_net "Net-(S7-Pad2)")
    (add_net "Net-(S7-Pad4)")
    (add_net "Net-(SW1-PadA1)")
    (add_net "Net-(SW1-PadB1)")
    (add_net "Net-(SW1-PadE1)")
    (add_net "Net-(SW1-PadMH1)")
    (add_net "Net-(SW1-PadMH2)")
    (add_net "Net-(SW2-PadA1)")
    (add_net "Net-(SW2-PadB1)")
    (add_net "Net-(SW2-PadE1)")
    (add_net "Net-(SW2-PadMH1)")
    (add_net "Net-(SW2-PadMH2)")
    (add_net "Net-(SW3-PadMH1)")
    (add_net "Net-(SW3-PadMH2)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad52)")
    (add_net "Net-(U1-Pad63)")
    (add_net "Net-(U1-Pad64)")
    (add_net "Net-(U1-Pad65)")
    (add_net "Net-(U1-Pad66)")
    (add_net "Net-(U1-Pad67)")
    (add_net "Net-(U1-Pad68)")
    (add_net "Net-(U1-Pad69)")
    (add_net "Net-(U1-Pad70)")
    (add_net "Net-(U1-Pad71)")
    (add_net "Net-(U1-Pad72)")
    (add_net "Net-(U1-Pad73)")
    (add_net "Net-(U1-Pad74)")
    (add_net "Net-(U1-Pad75)")
    (add_net "Net-(U1-Pad76)")
    (add_net "Net-(U1-Pad77)")
    (add_net "Net-(U1-Pad78)")
    (add_net "Net-(U1-Pad79)")
    (add_net "Net-(U1-Pad80)")
    (add_net "Net-(U1-Pad81)")
    (add_net "Net-(U1-Pad82)")
    (add_net "Net-(U1-Pad83)")
    (add_net "Net-(U1-Pad84)")
    (add_net "Net-(U1-Pad85)")
    (add_net "Net-(U1-Pad86)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net PWR)
    (add_net RX)
    (add_net SCL)
    (add_net SCLK)
    (add_net SDA)
    (add_net TFT_CS)
    (add_net TFT_DC)
    (add_net TFT_RST)
    (add_net TX)
    (add_net T_CS)
    (add_net VOL)
  )
  (module Teensy_Accessories:ILI9341_TOUCH (layer F.Cu) (tedit 5BF03917)
    (at 81.064 84.042)
    (descr "CR2013-MI2120 ILI9341 LCD Breakout http://pan.baidu.com/s/11Y990")
    (tags "CR2013-MI2120 ILI9341 LCD Breakout")
    (fp_text reference U2 (at -3.34 -7.08) (layer F.SilkS))
    (fp_text value ILI9341_TOUCH (at 4 43) (layer F.Fab))
    (fp_text user %R (at 44 17.5) (layer F.Fab))
    (pad 14 thru_hole circle (at 0 33.02) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(U2-Pad14)"))
    (pad 13 thru_hole circle (at 0 30.48) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 41 MISO))
    (pad 12 thru_hole circle (at 0 27.94) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 56 MOSI))
    (pad 11 thru_hole circle (at 0 25.4) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 92 T_CS))
    (pad 10 thru_hole circle (at 0 22.86) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 64 SCLK))
    (pad "" thru_hole circle (at 4.92 38.51) (size 4 4) (drill 2.7) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 81 38.51) (size 4 4) (drill 2.7) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 81 -5.49) (size 4 4) (drill 2.7) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 4.92 -5.49) (size 4 4) (drill 2.7) (layers *.Cu *.Mask))
    (pad 18 thru_hole circle (at 81 20.32) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 99 "Net-(U2-Pad18)"))
    (pad 17 thru_hole circle (at 81 17.78) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 98 "Net-(U2-Pad17)"))
    (pad 16 thru_hole circle (at 81 15.24) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 97 "Net-(U2-Pad16)"))
    (pad 15 thru_hole rect (at 81 12.7) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 96 "Net-(U2-Pad15)"))
    (pad 9 thru_hole circle (at 0 20.32) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 41 MISO))
    (pad 8 thru_hole circle (at 0 17.78) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 95 "Net-(R7-Pad2)"))
    (pad 7 thru_hole circle (at 0 15.24) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 64 SCLK))
    (pad 6 thru_hole circle (at 0 12.7) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 56 MOSI))
    (pad 5 thru_hole circle (at 0 10.16) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 68 TFT_DC))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 45 TFT_RST))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 69 TFT_CS))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 46 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 87 +5V))
    (model "C:/Users/Louis McCarthy/Dropbox/tft_320x240_touch.stp"
      (offset (xyz 41 -16.5 1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical_SMD_Pin1Left locked (layer B.Cu) (tedit 59FED5CC)
    (at 111.76 120 270)
    (descr "surface-mounted straight pin header, 1x14, 2.54mm pitch, single row, style 1 (pin 1 left)")
    (tags "Surface mounted pin header SMD 1x14 2.54mm single row style1 pin1 left")
    (attr smd)
    (fp_text reference J1 (at 0 18.84 270) (layer B.SilkS))
    (fp_text value Conn_01x14_Male (at 0 -18.84 270) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 14 smd rect (at 1.655 -16.51 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 121 "Net-(J1-Pad14)"))
    (pad 12 smd rect (at 1.655 -11.43 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 120 "Net-(J1-Pad12)"))
    (pad 10 smd rect (at 1.655 -6.35 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 119 "Net-(J1-Pad10)"))
    (pad 8 smd rect (at 1.655 -1.27 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 118 "Net-(J1-Pad8)"))
    (pad 6 smd rect (at 1.655 3.81 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 117 "Net-(J1-Pad6)"))
    (pad 4 smd rect (at 1.655 8.89 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 116 "Net-(J1-Pad4)"))
    (pad 2 smd rect (at 1.655 13.97 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 115 "Net-(J1-Pad2)"))
    (pad 13 smd rect (at -1.655 -13.97 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 53 MCLK))
    (pad 11 smd rect (at -1.655 -8.89 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 54 BCLK))
    (pad 9 smd rect (at -1.655 -3.81 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 114 "Net-(J1-Pad9)"))
    (pad 7 smd rect (at -1.655 1.27 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 113 "Net-(J1-Pad7)"))
    (pad 5 smd rect (at -1.655 6.35 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 112 "Net-(J1-Pad5)"))
    (pad 3 smd rect (at -1.655 11.43 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 111 "Net-(J1-Pad3)"))
    (pad 1 smd rect (at -1.655 16.51 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 46 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x14_P2.54mm_Vertical_SMD_Pin1Left.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical_SMD_Pin1Left locked (layer B.Cu) (tedit 59FED5CC)
    (at 111.76 104.76 270)
    (descr "surface-mounted straight pin header, 1x14, 2.54mm pitch, single row, style 1 (pin 1 left)")
    (tags "Surface mounted pin header SMD 1x14 2.54mm single row style1 pin1 left")
    (attr smd)
    (fp_text reference J2 (at 0 18.84 270) (layer B.SilkS))
    (fp_text value Conn_01x14_Male (at 0 -18.84 270) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.655 16.51 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 107 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at -1.655 11.43 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 72 +3V3))
    (pad 5 smd rect (at -1.655 6.35 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 70 TX))
    (pad 7 smd rect (at -1.655 1.27 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 108 "Net-(J2-Pad7)"))
    (pad 9 smd rect (at -1.655 -3.81 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 66 SDA))
    (pad 11 smd rect (at -1.655 -8.89 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 109 "Net-(J2-Pad11)"))
    (pad 13 smd rect (at -1.655 -13.97 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 110 "Net-(J2-Pad13)"))
    (pad 2 smd rect (at 1.655 13.97 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 104 "Net-(J2-Pad2)"))
    (pad 4 smd rect (at 1.655 8.89 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 71 LRCLK))
    (pad 6 smd rect (at 1.655 3.81 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 105 "Net-(J2-Pad6)"))
    (pad 8 smd rect (at 1.655 -1.27 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 67 SCL))
    (pad 10 smd rect (at 1.655 -6.35 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 106 "Net-(J2-Pad10)"))
    (pad 12 smd rect (at 1.655 -11.43 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 65 VOL))
    (pad 14 smd rect (at 1.655 -16.51 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 63 RX))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x14_P2.54mm_Vertical_SMD_Pin1Left.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Left (layer B.Cu) (tedit 59FED5CC)
    (at 136.144 105.283)
    (descr "surface-mounted straight pin header, 1x04, 2.54mm pitch, single row, style 1 (pin 1 left)")
    (tags "Surface mounted pin header SMD 1x04 2.54mm single row style1 pin1 left")
    (attr smd)
    (fp_text reference J3 (at 0 6.14) (layer B.SilkS))
    (fp_text value Conn_01x04_Male (at 0 -6.14) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 smd rect (at -1.655 3.81) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 87 +5V))
    (pad 3 smd rect (at -1.655 -1.27) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 66 SDA))
    (pad 2 smd rect (at 1.655 1.27) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 67 SCL))
    (pad 4 smd rect (at 1.655 -3.81) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 46 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Left.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Teensy_Accessories:Teensy35_36_SMD (layer B.Cu) (tedit 5BF0C578)
    (at 124.714 87.122)
    (fp_text reference U1 (at -32.131 -9.144) (layer B.SilkS))
    (fp_text value Teensy3.6 (at 0 -12.7) (layer B.Fab))
    (pad 30 smd rect (at 29.21 5.97 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 47 B1))
    (pad 52 smd rect (at -26.67 5.97 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(U1-Pad52)"))
    (pad 48 smd rect (at -16.51 5.97 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 69 TFT_CS))
    (pad 40 smd rect (at 3.81 5.97 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 63 RX))
    (pad 50 smd rect (at -21.59 5.97 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 71 LRCLK))
    (pad 46 smd rect (at -11.43 5.97 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 67 SCL))
    (pad 32 smd rect (at 24.13 5.97 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 49 B3))
    (pad 53 smd rect (at -29.21 9.27 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 87 +5V))
    (pad 49 smd rect (at -19.05 9.27 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 70 TX))
    (pad 47 smd rect (at -13.97 9.27 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 68 TFT_DC))
    (pad 36 smd rect (at 13.97 5.97 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(U1-Pad36)"))
    (pad 43 smd rect (at -3.81 9.27 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 85 "Net-(R3-Pad2)"))
    (pad 41 smd rect (at 1.27 9.27 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 64 SCLK))
    (pad 35 smd rect (at 16.51 9.27 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 52 B5))
    (pad 33 smd rect (at 21.59 9.27 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 50 B4))
    (pad 31 smd rect (at 26.67 9.27 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 48 B2))
    (pad 45 smd rect (at -8.89 9.27 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 66 SDA))
    (pad 37 smd rect (at 11.43 9.27 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(U1-Pad37)"))
    (pad 38 smd rect (at 8.89 5.97 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(U1-Pad38)"))
    (pad 34 smd rect (at 19.05 5.97 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 51 B7))
    (pad 51 smd rect (at -24.13 9.27 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 72 +3V3))
    (pad 39 smd rect (at 6.35 9.27 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 46 GND))
    (pad 44 smd rect (at -6.35 5.97 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 86 "Net-(R1-Pad2)"))
    (pad 42 smd rect (at -1.27 5.97 270) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 65 VOL))
    (pad 18 smd rect (at 13.97 -5.969 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 37 Band5))
    (pad 17 smd rect (at 11.43 -9.279 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 36 ATT_DATA))
    (pad 22 smd rect (at 24.13 -5.969 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 43 Band2))
    (pad 2 smd rect (at -26.67 -5.969 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(SW1-PadE1)"))
    (pad 5 smd rect (at -19.05 -9.279 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 59 /Backlight))
    (pad 4 smd rect (at -21.59 -5.969 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(SW1-PadB1)"))
    (pad 20 smd rect (at 19.05 -5.969 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 39 ATT_CLK))
    (pad 23 smd rect (at 26.67 -9.279 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 44 Band1))
    (pad 14 smd rect (at 3.81 -5.969 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 41 MISO))
    (pad 13 smd rect (at 1.27 -9.279 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 53 MCLK))
    (pad 10 smd rect (at -6.35 -5.969 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(SW2-PadE1)"))
    (pad 3 smd rect (at -24.13 -9.279 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(SW1-PadA1)"))
    (pad 12 smd rect (at -1.27 -5.969 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(U1-Pad12)"))
    (pad 21 smd rect (at 21.59 -9.279 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 42 Band4))
    (pad 7 smd rect (at -13.97 -9.279 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(SW2-PadA1)"))
    (pad 6 smd rect (at -16.51 -5.969 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(SW2-PadB1)"))
    (pad 19 smd rect (at 16.51 -9.279 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 38 Band3))
    (pad 24 smd rect (at 29.21 -5.969 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 45 TFT_RST))
    (pad 1 smd rect (at -29.21 -9.279 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 46 GND))
    (pad 9 smd rect (at -8.89 -9.279 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 56 MOSI))
    (pad 8 smd rect (at -11.43 -5.969 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 92 T_CS))
    (pad 11 smd rect (at -3.81 -9.279 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 54 BCLK))
    (pad 16 smd rect (at 8.89 -5.969 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 40 ATT_LE))
    (pad 15 smd rect (at 6.35 -9.279 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 100 PWR))
    (pad 25 thru_hole circle (at 16.51 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 103 "Net-(BAT1-Pad1)"))
    (pad 26 thru_hole circle (at 16.51 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(U1-Pad26)"))
    (pad 27 thru_hole circle (at 16.51 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 46 GND))
    (pad 28 thru_hole circle (at 16.51 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad28)"))
    (pad 29 thru_hole circle (at 16.51 5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad29)"))
    (pad 63 thru_hole circle (at -13.97 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "Net-(U1-Pad63)"))
    (pad 64 thru_hole circle (at -11.43 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "Net-(U1-Pad64)"))
    (pad 65 thru_hole circle (at -8.89 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 "Net-(U1-Pad65)"))
    (pad 66 thru_hole circle (at -6.35 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(U1-Pad66)"))
    (pad 67 thru_hole circle (at 8.89 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad67)"))
    (pad 68 thru_hole circle (at 11.43 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 "Net-(U1-Pad68)"))
    (pad 69 thru_hole circle (at 13.97 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(U1-Pad69)"))
    (pad 70 thru_hole circle (at 19.05 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 "Net-(U1-Pad70)"))
    (pad 71 thru_hole circle (at 21.59 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad71)"))
    (pad 72 thru_hole circle (at 24.13 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 18 "Net-(U1-Pad72)"))
    (pad 73 thru_hole circle (at 26.67 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 "Net-(U1-Pad73)"))
    (pad 74 thru_hole circle (at 29.21 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 20 "Net-(U1-Pad74)"))
    (pad 75 thru_hole circle (at 29.21 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 "Net-(U1-Pad75)"))
    (pad 76 thru_hole circle (at 26.67 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 "Net-(U1-Pad76)"))
    (pad 77 thru_hole circle (at 24.13 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 23 "Net-(U1-Pad77)"))
    (pad 78 thru_hole circle (at 21.59 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 24 "Net-(U1-Pad78)"))
    (pad 79 thru_hole circle (at 19.05 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 "Net-(U1-Pad79)"))
    (pad 80 thru_hole circle (at 13.97 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 26 "Net-(U1-Pad80)"))
    (pad 81 thru_hole circle (at 11.43 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 27 "Net-(U1-Pad81)"))
    (pad 82 thru_hole circle (at 8.89 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 28 "Net-(U1-Pad82)"))
    (pad 83 thru_hole circle (at -6.35 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad83)"))
    (pad 84 thru_hole circle (at -8.89 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 30 "Net-(U1-Pad84)"))
    (pad 85 thru_hole circle (at -11.43 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 31 "Net-(U1-Pad85)"))
    (pad 86 thru_hole circle (at -13.97 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 32 "Net-(U1-Pad86)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x24_P2.54mm_Vertical_SMD_Pin1Left.step
      (offset (xyz 0 -7.6 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x24_P2.54mm_Vertical_SMD_Pin1Right.step
      (offset (xyz 0 7.6 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model "C:/Users/Louis McCarthy/Dropbox/Teensy 3_6.STEP"
      (offset (xyz 30.5 -9 5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Teensy_Accessories:EM14A0D(AXIAL)" (layer F.Cu) (tedit 5BF0362B)
    (at 181.864 99.822 90)
    (descr "EM14A0D(AXIAL)")
    (tags Switch)
    (fp_text reference SW4 (at 8.255 6.25 180) (layer F.SilkS))
    (fp_text value EM14A0D-C24-L064S (at -0.34 0.043 90) (layer F.SilkS) hide)
    (pad 8 thru_hole circle (at 7.305 0 180) (size 2.78 2.78) (drill 1.83) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole circle (at -7.305 0 180) (size 2.78 2.78) (drill 1.83) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole circle (at 3.175 6.25 180) (size 1.05 1.05) (drill 0.64) (layers *.Cu *.Mask F.SilkS)
      (net 89 "Net-(R3-Pad1)"))
    (pad 5 thru_hole circle (at 1.905 6.25 180) (size 1.05 1.05) (drill 0.64) (layers *.Cu *.Mask F.SilkS)
      (net 87 +5V))
    (pad 4 thru_hole circle (at 0.635 6.25 180) (size 1.05 1.05) (drill 0.64) (layers *.Cu *.Mask F.SilkS)
      (net 52 B5))
    (pad 3 thru_hole circle (at -0.635 6.25 180) (size 1.05 1.05) (drill 0.64) (layers *.Cu *.Mask F.SilkS)
      (net 46 GND))
    (pad 2 thru_hole circle (at -1.905 6.25 180) (size 1.05 1.05) (drill 0.64) (layers *.Cu *.Mask F.SilkS)
      (net 88 "Net-(R1-Pad1)"))
    (pad 1 thru_hole circle (at -3.175 6.25 180) (size 1.05 1.05) (drill 0.64) (layers *.Cu *.Mask F.SilkS)
      (net 46 GND))
    (model "C:/Users/Louis McCarthy/Downloads/EM14AXD-B28-L.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Teensy_Accessories:EN12HS22AF20 (layer F.Cu) (tedit 5BF02DEB)
    (at 173.864 108.084)
    (descr EN12-HS22AF20-1)
    (tags "Undefined or Miscellaneous")
    (fp_text reference SW3 (at -4.27 -15.12) (layer F.SilkS))
    (fp_text value EN12-HS22AF20 (at 2.5 -7.25) (layer F.SilkS) hide)
    (pad A1 thru_hole circle (at 0 0 90) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 86 "Net-(R1-Pad2)"))
    (pad B1 thru_hole circle (at 5 0 90) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(R3-Pad2)"))
    (pad C1 thru_hole circle (at 2.5 0 90) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 46 GND))
    (pad D1 thru_hole circle (at 0 -14.5 90) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 46 GND))
    (pad E1 thru_hole circle (at 5 -14.5 90) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 52 B5))
    (pad MH1 thru_hole circle (at -3 -7.5 90) (size 4.667 4.667) (drill 3.1113) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(SW3-PadMH1)"))
    (pad MH2 thru_hole circle (at 8 -7.5 90) (size 4.667 4.667) (drill 3.1113) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(SW3-PadMH2)"))
    (model "C:/Users/Louis McCarthy/Downloads/EN12-HS.stp"
      (offset (xyz 8 0.9 4.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module Teensy_Accessories:EN12HS22AF20 (layer F.Cu) (tedit 5BF02DEB)
    (at 66.754 123.832)
    (descr EN12-HS22AF20-1)
    (tags "Undefined or Miscellaneous")
    (fp_text reference SW2 (at -4.27 0.12) (layer F.SilkS))
    (fp_text value EN12-HS22AF20 (at 2.5 -7.25) (layer F.SilkS) hide)
    (pad A1 thru_hole circle (at 0 0 90) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(SW2-PadA1)"))
    (pad B1 thru_hole circle (at 5 0 90) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(SW2-PadB1)"))
    (pad C1 thru_hole circle (at 2.5 0 90) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 46 GND))
    (pad D1 thru_hole circle (at 0 -14.5 90) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 46 GND))
    (pad E1 thru_hole circle (at 5 -14.5 90) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(SW2-PadE1)"))
    (pad MH1 thru_hole circle (at -3 -7.5 90) (size 4.667 4.667) (drill 3.1113) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(SW2-PadMH1)"))
    (pad MH2 thru_hole circle (at 8 -7.5 90) (size 4.667 4.667) (drill 3.1113) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(SW2-PadMH2)"))
    (model "C:/Users/Louis McCarthy/Downloads/EN12-HS.stp"
      (offset (xyz 8 0.9 4.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module Teensy_Accessories:EN12HS22AF20 (layer F.Cu) (tedit 5BF02DEB)
    (at 66.754 104.902)
    (descr EN12-HS22AF20-1)
    (tags "Undefined or Miscellaneous")
    (fp_text reference SW1 (at -4.27 -15.24) (layer F.SilkS))
    (fp_text value EN12-HS22AF20 (at 2.5 -7.25) (layer F.SilkS) hide)
    (pad MH2 thru_hole circle (at 8 -7.5 90) (size 4.667 4.667) (drill 3.1113) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(SW1-PadMH2)"))
    (pad MH1 thru_hole circle (at -3 -7.5 90) (size 4.667 4.667) (drill 3.1113) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(SW1-PadMH1)"))
    (pad E1 thru_hole circle (at 5 -14.5 90) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(SW1-PadE1)"))
    (pad D1 thru_hole circle (at 0 -14.5 90) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 46 GND))
    (pad C1 thru_hole circle (at 2.5 0 90) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 46 GND))
    (pad B1 thru_hole circle (at 5 0 90) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(SW1-PadB1)"))
    (pad A1 thru_hole circle (at 0 0 90) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(SW1-PadA1)"))
    (model "C:/Users/Louis McCarthy/Downloads/EN12-HS.stp"
      (offset (xyz 8 0.9 4.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module Teensy_Accessories:B3F1002 (layer F.Cu) (tedit 5BF02B29)
    (at 68.834 80.772)
    (descr B3F1002)
    (tags Switch)
    (fp_text reference S5 (at -5.08 0) (layer F.SilkS))
    (fp_text value B3F-1000 (at -0.384 -0.083) (layer F.SilkS) hide)
    (pad 4 thru_hole circle (at -3.25 -2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(S5-Pad4)"))
    (pad 3 thru_hole circle (at 3.25 -2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 46 GND))
    (pad 2 thru_hole circle (at -3.25 2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(S5-Pad2)"))
    (pad 1 thru_hole circle (at 3.25 2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 100 PWR))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H4.3mm.wrl
      (offset (xyz -3.15 2.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Teensy_Accessories:B3F1002 (layer F.Cu) (tedit 5BF02B29)
    (at 192.024 121.412)
    (descr B3F1002)
    (tags Switch)
    (fp_text reference S7 (at 0 -5.08) (layer F.SilkS))
    (fp_text value B3F-1000 (at -0.384 -0.083) (layer F.SilkS) hide)
    (pad 4 thru_hole circle (at -3.25 -2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(S7-Pad4)"))
    (pad 3 thru_hole circle (at 3.25 -2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 46 GND))
    (pad 2 thru_hole circle (at -3.25 2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 90 "Net-(S7-Pad2)"))
    (pad 1 thru_hole circle (at 3.25 2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 51 B7))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H4.3mm.wrl
      (offset (xyz -3.15 2.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Teensy_Accessories:B3F1002 (layer F.Cu) (tedit 5BF02B29)
    (at 181.154 121.412)
    (descr B3F1002)
    (tags Switch)
    (fp_text reference S3 (at -0.384 -5.08) (layer F.SilkS))
    (fp_text value B3F-1000 (at -0.384 -0.083) (layer F.SilkS) hide)
    (pad 4 thru_hole circle (at -3.25 -2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(S3-Pad4)"))
    (pad 3 thru_hole circle (at 3.25 -2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 46 GND))
    (pad 2 thru_hole circle (at -3.25 2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(S3-Pad2)"))
    (pad 1 thru_hole circle (at 3.25 2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 49 B3))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H4.3mm.wrl
      (offset (xyz -3.15 2.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Teensy_Accessories:B3F1002 (layer F.Cu) (tedit 5BF02B29)
    (at 192.584 79.502)
    (descr B3F1002)
    (tags Switch)
    (fp_text reference S2 (at -0.384 5.08) (layer F.SilkS))
    (fp_text value B3F-1000 (at -0.384 -0.083) (layer F.SilkS) hide)
    (pad 4 thru_hole circle (at -3.25 -2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(S2-Pad4)"))
    (pad 3 thru_hole circle (at 3.25 -2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 46 GND))
    (pad 2 thru_hole circle (at -3.25 2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(S2-Pad2)"))
    (pad 1 thru_hole circle (at 3.25 2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 48 B2))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H4.3mm.wrl
      (offset (xyz -3.15 2.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Teensy_Accessories:B3F1002 (layer F.Cu) (tedit 5BF02B29)
    (at 170.434 79.502)
    (descr B3F1002)
    (tags Switch)
    (fp_text reference S1 (at 0 5.08) (layer F.SilkS))
    (fp_text value B3F-1000 (at -0.384 -0.083) (layer F.SilkS) hide)
    (pad 4 thru_hole circle (at -3.25 -2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(S1-Pad4)"))
    (pad 3 thru_hole circle (at 3.25 -2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 46 GND))
    (pad 2 thru_hole circle (at -3.25 2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(S1-Pad2)"))
    (pad 1 thru_hole circle (at 3.25 2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 47 B1))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H4.3mm.wrl
      (offset (xyz -3.15 2.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Teensy_Accessories:B3F1002 (layer F.Cu) (tedit 5BF02B29)
    (at 170.434 121.412)
    (descr B3F1002)
    (tags Switch)
    (fp_text reference S4 (at 0 -5.08) (layer F.SilkS))
    (fp_text value B3F-1000 (at -0.384 -0.083) (layer F.SilkS) hide)
    (pad 4 thru_hole circle (at -3.25 -2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(S4-Pad4)"))
    (pad 3 thru_hole circle (at 3.25 -2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 46 GND))
    (pad 2 thru_hole circle (at -3.25 2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(S4-Pad2)"))
    (pad 1 thru_hole circle (at 3.25 2.25 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 50 B4))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H4.3mm.wrl
      (offset (xyz -3.15 2.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Teensy_Accessories:SOT95P285X120-3N (layer B.Cu) (tedit 5BF028F1)
    (at 87.884 109.982)
    (descr PG-SC59-3-5)
    (tags "Undefined or Miscellaneous")
    (attr smd)
    (fp_text reference Q2 (at 1.27 2.54) (layer B.SilkS))
    (fp_text value BSR802N_L6327 (at 0 0) (layer B.SilkS) hide)
    (pad 3 smd rect (at 1.3 0 270) (size 0.55 1.2) (layers B.Cu B.Paste B.Mask)
      (net 93 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1.3 -0.95 270) (size 0.55 1.2) (layers B.Cu B.Paste B.Mask)
      (net 46 GND))
    (pad 1 smd rect (at -1.3 0.95 270) (size 0.55 1.2) (layers B.Cu B.Paste B.Mask)
      (net 59 /Backlight))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Teensy_Accessories:SOT95P237X112-3N (layer B.Cu) (tedit 5BF02859)
    (at 87.884 106.172)
    (descr "SOT-23 (TO-236)")
    (tags "MOSFET (P-Channel)")
    (attr smd)
    (fp_text reference Q1 (at 1.27 -2.54) (layer B.SilkS))
    (fp_text value SI2371EDS-T1-GE3 (at 0 0) (layer B.SilkS) hide)
    (pad 3 smd rect (at 1.05 0 270) (size 0.6 1.3) (layers B.Cu B.Paste B.Mask)
      (net 94 "Net-(Q1-Pad3)"))
    (pad 2 smd rect (at -1.05 -0.95 270) (size 0.6 1.3) (layers B.Cu B.Paste B.Mask)
      (net 87 +5V))
    (pad 1 smd rect (at -1.05 0.95 270) (size 0.6 1.3) (layers B.Cu B.Paste B.Mask)
      (net 93 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:BATHLD001 (layer B.Cu) (tedit 5BDBB0FB)
    (at 152.019 111.379 90)
    (descr BAT-HLD-001)
    (tags "Undefined or Miscellaneous")
    (attr smd)
    (fp_text reference BAT1 (at -8.001 -8.509 90) (layer B.SilkS))
    (fp_text value BAT-HLD-001 (at 0 0 90) (layer B.SilkS) hide)
    (pad 3 smd circle (at 0 0) (size 17.8 17.8) (layers B.Cu B.Paste B.Mask)
      (net 46 GND))
    (pad 2 smd rect (at -11.45 0 90) (size 2.5 5.1) (layers B.Cu B.Paste B.Mask)
      (net 103 "Net-(BAT1-Pad1)"))
    (pad 1 smd rect (at 11.45 0 90) (size 2.5 5.1) (layers B.Cu B.Paste B.Mask)
      (net 103 "Net-(BAT1-Pad1)"))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 84.074 106.172 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 -1.27 90) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 +5V))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 93 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 84.074 102.362 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 -1.27 90) (layer B.SilkS))
    (fp_text value 100R (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 95 "Net-(R7-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 94 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 84.074 109.982 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 1.43 270) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 /Backlight))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 46 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 192.024 100.203 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -2.794 0 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 46 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 192.024 96.647)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 2.794 0) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 192.024 98.171 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at -2.794 -0.127 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 46 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 192.024 101.727)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 2.794 0) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "©2018 Louis McCarthy" (at 181.102 88.265) (layer F.SilkS))
  (gr_text "Version 1.0\n11/2018" (at 189.357 112.014) (layer F.SilkS))
  (gr_text "Teensy AV" (at 173.863 112.141) (layer F.SilkS))
  (gr_text "Version 1.0\n11/2018" (at 181.61 81.407) (layer B.SilkS))
  (gr_text "©2018 Louis McCarthy" (at 181.737 112.903) (layer B.SilkS))
  (gr_text "Teensy AV" (at 181.61 77.216) (layer B.SilkS))
  (gr_text +5V (at 131.445 109.22 90) (layer B.SilkS))
  (gr_text SDA (at 131.572 104.013 90) (layer B.SilkS))
  (gr_text GND (at 141.097 101.473 90) (layer B.SilkS))
  (gr_text SCL (at 140.97 106.68 90) (layer B.SilkS))
  (gr_text USB (at 91.694 86.868 90) (layer B.SilkS))
  (gr_text AC97 (at 111.76 100.457) (layer B.SilkS))
  (gr_text "Vol. Knob" (at 123.444 124.714) (layer B.SilkS))
  (gr_text "HP Jack" (at 98.806 124.714) (layer B.SilkS))
  (gr_text "Audio Board \"Face Down\"" (at 112.141 112.268) (layer B.SilkS))
  (gr_line (start 59.944 126.492) (end 59.944 74.422) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 198.374 126.492) (end 59.944 126.492) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 198.374 74.422) (end 198.374 126.492) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 59.944 74.422) (end 198.374 74.422) (layer Edge.Cuts) (width 0.15))
  (zone (net 46) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59.944 74.422) (xy 198.374 74.422) (xy 198.374 126.492) (xy 59.944 126.492)
      )
    )
  )
)
