(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(RV1-Pad1)")
  (net 3 "Net-(R1-Pad1)")
  (net 4 "Net-(R3-Pad1)")
  (net 5 "/TRI")
  (net 6 "+BATT")
  (net 7 "+3V3")
  (net 8 "Net-(C3-Pad2)")
  (net 9 "Net-(C4-Pad2)")
  (net 10 "Net-(C4-Pad1)")
  (net 11 "Net-(R2-Pad2)")
  (net 12 "Net-(L1-Pad1)")
  (net 13 "Net-(L2-Pad1)")
  (net 14 "Net-(Q1-Pad1)")
  (net 15 "Net-(Q1-Pad3)")
  (net 16 "Net-(R4-Pad1)")
  (net 17 "Net-(R6-Pad1)")
  (net 18 "Net-(R7-Pad1)")
  (net 19 "Net-(R11-Pad1)")
  (net 20 "Net-(R14-Pad1)")
  (net 21 "Net-(R16-Pad1)")
  (net 22 "unconnected-(U1-Pad4)")
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 25 45 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "DK" "445-12758-1-ND")
    (property "Field4" "C28323")
    (property "PART#" "CGA4J3X7R1E105M125AB")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at -2.25 0) (layer "F.SilkS"))
    (fp_text value "1µF" (at 0 1.68 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "+BATT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 32 45 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "DK" "445-12758-1-ND")
    (property "Field4" "C28323")
    (property "PART#" "CGA4J3X7R1E105M125AB")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at -2.25 0) (layer "F.SilkS"))
    (fp_text value "1µF" (at 0 1.68 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 38 35.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "DK" "445-2323-1-ND")
    (property "Field4" "C113851")
    (property "PART#" "C2012C0G2A332J125AA")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 2.75 0) (layer "F.SilkS"))
    (fp_text value "3.3nF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/TRI") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5B36C52B)
    (at 50 49.05 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "DK" "445-1418-1-ND")
    (property "Field4" "C49678")
    (property "PART#" "C2012X7R2A104K125AA")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at -3 0 180) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C4-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_PH_B2B-PH-SM4-TB_1x02-1MP_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 5B78AD87)
    (at 58 52 -90)
    (descr "JST PH series connector, B2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH side entry")
    (property "DK" "455-2872-1-ND")
    (property "Field4" "C160352")
    (property "PART#" "B2B-PH-SM4-TBT(LF)(SN)")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J3" (at 3.5 2.4 180) (layer "F.SilkS"))
    (fp_text value "PH" (at 0 4.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0.5 270) (size 1 5.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C4-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0.5 270) (size 1 5.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C4-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "MP" smd roundrect (at 3.4 -1.75 270) (size 1.6 3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 1 "GND") (pinfunction "MountPin") (pintype "passive"))
    (pad "MP" smd roundrect (at -3.4 -1.75 270) (size 1.6 3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 1 "GND") (pinfunction "MountPin") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_B2B-PH-SM4-TB_1x02-1MP_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 45.75 35.5 180)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "DK" "2N7002-FDICT-ND")
    (property "Field4" "C8545")
    (property "PART#" "2N7002-7-F")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at 2 1.5) (layer "F.SilkS"))
    (fp_text value "2N7002" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(Q1-Pad1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(Q1-Pad3)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 34 50 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "DK" "CRCW080547K0FKEAC")
    (property "Field4" "C17713")
    (property "PART#" "541-4137-1-ND")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 2.5 0.25) (layer "F.SilkS"))
    (fp_text value "47k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 3 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 6 "+BATT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 34 48)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "DK" "CRCW080547K0FKEAC")
    (property "Field4" "C17713")
    (property "PART#" "541-4137-1-ND")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at -2.5 0.25) (layer "F.SilkS"))
    (fp_text value "47k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 11 "Net-(R2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 38 48 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "DK" "541-4135-1-ND")
    (property "Field4" "C17514")
    (property "PART#" "CRCW08051M00FKEAC")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at -2.75 0) (layer "F.SilkS"))
    (fp_text value "1M" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(R3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 3 "Net-(R1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 38 46 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "DK" "541-4135-1-ND")
    (property "Field4" "C17514")
    (property "PART#" "CRCW08051M00FKEAC")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 2.75 0) (layer "F.SilkS"))
    (fp_text value "1M" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 16 "Net-(R4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 11 "Net-(R2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 38 44)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "DK" "RMCF0805FT22M0CT-ND ")
    (property "Field4" "C34719")
    (property "PART#" "RMCF0805FT22M0")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at -2.75 0) (layer "F.SilkS"))
    (fp_text value "22M" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 16 "Net-(R4-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 38 50 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "DK" "RMCF0805FT22M0CT-ND ")
    (property "Field4" "C34719")
    (property "PART#" "RMCF0805FT22M0")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at -2.75 0) (layer "F.SilkS"))
    (fp_text value "22M" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 17 "Net-(R6-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(R3-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 38 39.5 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "DK" "CRCW080547K0FKEAC")
    (property "Field4" "C17713")
    (property "PART#" "541-4137-1-ND")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 2.75 0) (layer "F.SilkS"))
    (fp_text value "47k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 18 "Net-(R7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 17 "Net-(R6-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 38 41.5)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "DK" "CRCW080547K0FKEAC")
    (property "Field4" "C17713")
    (property "PART#" "541-4137-1-ND")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at -2.75 0) (layer "F.SilkS"))
    (fp_text value "47k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 18 "Net-(R7-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 38 37.5 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "DK" "541-4318-1-ND")
    (property "Field4" "C149504")
    (property "PART#" "CRCW0805100KFKEB")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at 2.75 0) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 8 "Net-(C3-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 17 "Net-(R6-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 50 39)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "DK" "CRCW080547K0FKEAC")
    (property "Field4" "C17713")
    (property "PART#" "541-4137-1-ND")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 3.25 0) (layer "F.SilkS"))
    (fp_text value "47k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 19 "Net-(R11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 7 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 50 41 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "DK" "CRCW080547K0FKEAC")
    (property "Field4" "C17713")
    (property "PART#" "541-4137-1-ND")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at -3.25 0) (layer "F.SilkS"))
    (fp_text value "47k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 19 "Net-(R11-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 50 37)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "DK" "541-4318-1-ND")
    (property "Field4" "C149504")
    (property "PART#" "CRCW0805100KFKEB")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at 3.25 0) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 14 "Net-(Q1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 19 "Net-(R11-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 50 45)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "DK" "CRCW080547K0FKEAC")
    (property "Field4" "C17713")
    (property "PART#" "541-4137-1-ND")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at 3.25 0) (layer "F.SilkS"))
    (fp_text value "47k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 20 "Net-(R14-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 7 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 50 43 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "DK" "CRCW080547K0FKEAC")
    (property "Field4" "C17713")
    (property "PART#" "541-4137-1-ND")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at -3.25 0) (layer "F.SilkS"))
    (fp_text value "47k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 20 "Net-(R14-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 50 47.1)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "DK" "541-1.00KCCT-ND")
    (property "Field4" "C17513")
    (property "PART#" "CRCW08051K00FKEA")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at 3.25 0) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 21 "Net-(R16-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 14 "Net-(Q1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 28.8625 45)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "DK" "505-ADP122AUJZ-3.3-R7CT-ND")
    (property "Field4" "C143910")
    (property "PART#" "ADP122AUJZ-3.3-R7")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -2.4) (layer "F.SilkS"))
    (fp_text value "ADP122-3.3" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "+BATT") (pinfunction "IN") (pintype "power_in"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(R2-Pad2)") (pinfunction "EN") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "unconnected-(U1-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "+3V3") (pinfunction "OUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 44 42)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "DK" "AD8534ARZ-ND")
    (property "PART#" "AD8534ARZ")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at -2 -5.28) (layer "F.SilkS"))
    (fp_text value "AD8534" (at 0 5.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/TRI") (pintype "output"))
    (pad "2" smd roundrect (at -2.475 -2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C3-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 -1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(R7-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 0) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "+3V3") (pinfunction "V+") (pintype "power_in"))
    (pad "5" smd roundrect (at -2.475 1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(R4-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at -2.475 2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(R3-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "7" smd roundrect (at -2.475 3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(R6-Pad1)") (pintype "output"))
    (pad "8" smd roundrect (at 2.475 3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(L2-Pad1)") (pintype "output"))
    (pad "9" smd roundrect (at 2.475 2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(R16-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "10" smd roundrect (at 2.475 1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(R14-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "11" smd roundrect (at 2.475 0) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "12" smd roundrect (at 2.475 -1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(R11-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "13" smd roundrect (at 2.475 -2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/TRI") (pinfunction "-") (pintype "input"))
    (pad "14" smd roundrect (at 2.475 -3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(Q1-Pad1)") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_PH_B2B-PH-SM4-TB_1x02-1MP_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 5B78AD87)
    (at 28 52 90)
    (descr "JST PH series connector, B2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH side entry")
    (property "DK" "455-2872-1-ND")
    (property "Field4" "C160352")
    (property "PART#" "B2B-PH-SM4-TBT(LF)(SN)")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J2" (at 4.5 1.75 180) (layer "F.SilkS"))
    (fp_text value "PH" (at 0 4.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0.5 90) (size 1 5.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(RV1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0.5 90) (size 1 5.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(R2-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "MP" smd roundrect (at 3.4 -1.75 90) (size 1.6 3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 1 "GND") (pinfunction "MountPin") (pintype "passive"))
    (pad "MP" smd roundrect (at -3.4 -1.75 90) (size 1.6 3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 1 "GND") (pinfunction "MountPin") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_B2B-PH-SM4-TB_1x02-1MP_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 38 33.5 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "DK" "CRCW080547K0FKEAC")
    (property "Field4" "C17713")
    (property "PART#" "541-4137-1-ND")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 3.25 0) (layer "F.SilkS"))
    (fp_text value "47k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 15 "Net-(Q1-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 8 "Net-(C3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_PH_B2B-PH-SM4-TB_1x02-1MP_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 5B78AD87)
    (at 28 37 90)
    (descr "JST PH series connector, B2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH side entry")
    (property "DK" "455-2872-1-ND")
    (property "Field4" "C160352")
    (property "PART#" "B2B-PH-SM4-TBT(LF)(SN)")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at 3 2.5 180) (layer "F.SilkS"))
    (fp_text value "PH" (at 0 4.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0.5 90) (size 1 5.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "+BATT") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0.5 90) (size 1 5.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "MP" smd roundrect (at 3.4 -1.75 90) (size 1.6 3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 1 "GND") (pinfunction "MountPin") (pintype "passive"))
    (pad "MP" smd roundrect (at -3.4 -1.75 90) (size 1.6 3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 1 "GND") (pinfunction "MountPin") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_B2B-PH-SM4-TB_1x02-1MP_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 50 34.75 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "DK" "541-1.00CCCT-ND")
    (property "Field4" "C25271")
    (property "PART#" "CRCW08051R00FKEA")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R17" (at -3.3375 0 180) (layer "F.SilkS"))
    (fp_text value "1Ω" (at 0 1.65 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 12 "Net-(L1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 14 "Net-(Q1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 60 35)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -0.1) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Potentiometer_SMD:Potentiometer_Bourns_3314G_Vertical" (layer "F.Cu")
    (tedit 5A81E1D7)
    (at 44 54 -90)
    (descr "Potentiometer, vertical, Bourns 3314G, http://www.bourns.com/docs/Product-Datasheets/3314.pdf")
    (tags "Potentiometer vertical Bourns 3314G")
    (property "DK" "3314G-102ECT-ND")
    (property "Field4" "C3975231")
    (property "PART#" "3314G-1-102E")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "RV2" (at 1.5 -5.25 180) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 0 4.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.7 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.15 -2.75 270) (size 1.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(R16-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 0 2.75 270) (size 2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(L2-Pad1)") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at -1.15 -2.75 270) (size 1.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(L2-Pad1)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3314G_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 50 51 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "DK" "445-1418-1-ND")
    (property "Field4" "C49678")
    (property "PART#" "C2012X7R2A104K125AA")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at -3 0) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_1008_2520Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 46 49)
    (descr "Inductor SMD 1008 (2520 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://ecsxtal.com/store/pdf/ECS-MPI2520-SMD-POWER-INDUCTOR.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "DK" "490-15886-1-ND")
    (property "Field4" "C711113")
    (property "PART#" "LQH2HPN101MGRL")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "L2" (at -2.2 1.8) (layer "F.SilkS"))
    (fp_text value "100µH" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.075 0) (size 1.25 2.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 13 "Net-(L2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.075 0) (size 1.25 2.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 9 "Net-(C4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1008_2520Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_SMD:Potentiometer_Bourns_3314G_Vertical" (layer "F.Cu")
    (tedit 5A81E1D7)
    (at 36 54 -90)
    (descr "Potentiometer, vertical, Bourns 3314G, http://www.bourns.com/docs/Product-Datasheets/3314.pdf")
    (tags "Potentiometer vertical Bourns 3314G")
    (property "DK" "3314G-102ECT-ND")
    (property "Field4" "C3975231")
    (property "PART#" "3314G-1-102E")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "RV1" (at 1.75 5) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 0 4.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.7 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.15 -2.75 270) (size 1.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(RV1-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 0 2.75 270) (size 2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(RV1-Pad1)") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at -1.15 -2.75 270) (size 1.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(R1-Pad1)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3314G_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_1008_2520Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 56.75 45.25 -90)
    (descr "Inductor SMD 1008 (2520 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://ecsxtal.com/store/pdf/ECS-MPI2520-SMD-POWER-INDUCTOR.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "DK" "490-15886-1-ND")
    (property "Field4" "C711113")
    (property "PART#" "LQH2HPN101MGRL")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "L1" (at -3 0 180) (layer "F.SilkS"))
    (fp_text value "100µH" (at 0 2.05 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.075 0 270) (size 1.25 2.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 12 "Net-(L1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.075 0 270) (size 1.25 2.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 10 "Net-(C4-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1008_2520Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 50 53 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "DK" "445-1418-1-ND")
    (property "Field4" "C49678")
    (property "PART#" "C2012X7R2A104K125AA")
    (property "Sheetfile" "Beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at -3 0) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 63 57) (end 23 32) (layer "Edge.Cuts") (width 0.05) (fill none))
  (gr_text "+IN-" (at 24.75 51.75 -90) (layer "B.SilkS"))
  (gr_text "OUT 8Ω" (at 60.25 51.75 -90) (layer "B.SilkS"))
  (gr_text "U1=ADP122AUJZ-3.3\nU2=AD8534ARZ\nRVx=1kΩ 3314G\nLx=LQH2HPN101MGRL\nQ1=2N7002\nJx=B2B-PH-SM4-TB\nA=1Ω\nB=1kΩ\nC=47kΩ\nD=100kΩ\nE=1MΩ\nF=22MΩ\nW=3.3nF\nX=100nF\nY=1µF\n" (at 56.8 44.4) (layer "B.SilkS"))
  (gr_text "+BAT-" (at 24.25 37 -90) (layer "B.SilkS"))
  (gr_text "HACKADAY\nOP AMP ANORAK" (at 36.25 53.75) (layer "B.SilkS"))
  (gr_text "X" (at 48.1 49.1) (layer "F.SilkS"))
  (gr_text "E" (at 42.4 48) (layer "F.SilkS"))
  (gr_text "C" (at 35.9 48.1) (layer "F.SilkS"))
  (gr_text "Y" (at 33.3 45) (layer "F.SilkS"))
  (gr_text "1K" (at 35.9 53.8) (layer "F.SilkS"))
  (gr_text "D" (at 48.1 37) (layer "F.SilkS"))
  (gr_text "A" (at 48.1 35) (layer "F.SilkS"))
  (gr_text "1K" (at 44.1 54.2) (layer "F.SilkS"))
  (gr_text "X" (at 48.1 51.1) (layer "F.SilkS"))
  (gr_text "C" (at 35.9 50.1) (layer "F.SilkS"))
  (gr_text "BEEPER" (at 56.5 36.5 270) (layer "F.SilkS"))
  (gr_text "C" (at 39.9 41.5) (layer "F.SilkS"))
  (gr_text "B" (at 48.1 47.1) (layer "F.SilkS"))
  (gr_text "DFB" (at 44 45.75) (layer "F.SilkS"))
  (gr_text "Y" (at 26.3 46.2) (layer "F.SilkS"))
  (gr_text "D" (at 40 33.5) (layer "F.SilkS"))
  (gr_text "C" (at 48 45.1) (layer "F.SilkS"))
  (gr_text "C" (at 48.1 41) (layer "F.SilkS"))
  (gr_text "C" (at 48.1 43.1) (layer "F.SilkS"))
  (gr_text "AD8534" (at 43.75 41.25 270) (layer "F.SilkS"))
  (gr_text "X" (at 48.1 53) (layer "F.SilkS"))
  (gr_text "+BAT-" (at 32.75 37.25 90) (layer "F.SilkS"))
  (gr_text "+IN-" (at 24.75 52 90) (layer "F.SilkS"))
  (gr_text "F" (at 39.9 44.1) (layer "F.SilkS"))
  (gr_text "C" (at 48.1 39.1) (layer "F.SilkS"))
  (gr_text "E" (at 39.9 46) (layer "F.SilkS"))
  (gr_text "JRG©2023" (at 61 42.5 270) (layer "F.SilkS"))
  (gr_text "F" (at 42.4 50) (layer "F.SilkS"))
  (gr_text "W" (at 40.1 35.6) (layer "F.SilkS"))
  (gr_text "C" (at 40 39.6) (layer "F.SilkS"))
  (gr_text "D" (at 39.9 37.6) (layer "F.SilkS"))
  (zone (net 6) (net_name "+BATT") (layer "F.Cu") (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29.2 43)
        (xy 28.2 44)
        (xy 25 44)
        (xy 25 43.6)
        (xy 25.9 42.7)
        (xy 27.2 42.7)
        (xy 27.9 42)
        (xy 27.9 38.2)
        (xy 29.2 38.2)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 63 57)
        (xy 23 57)
        (xy 23 32)
        (xy 63 32)
      )
    )
  )
  (zone (net 7) (net_name "+3V3") (layer "F.Cu") (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 41.5 42)
        (xy 41.5 42.5)
        (xy 40.5 43.5)
        (xy 35.5 43.5)
        (xy 34.5 44.5)
        (xy 29.75 44.5)
        (xy 29.5 44.25)
        (xy 29.5 43.5)
        (xy 30.25 42.75)
        (xy 33 42.75)
        (xy 34.25 41.5)
        (xy 41 41.5)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 63 57)
        (xy 23 57)
        (xy 23 32)
        (xy 63 32)
      )
    )
  )
)
