(kicad_pcb (version 4) (host pcbnew 4.0.4+dfsg1-stable)
  (general
    (links 69)
    (no_connects 0)
    (area 64.186999 47.422999 115.137001 72.592001)
    (thickness 1.6)
    (drawings 174)
    (tracks 322)
    (zones 0)
    (modules 57)
    (nets 44)
  )
  (page USLetter portrait)
  (title_block
    (title "Pinguino 4550 SMD")
    (date 2016-12-21)
    (rev 1A)
    (company Rootdevel)
    (comment 1 Hackerspace)
    (comment 2 fAnDrEs)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3048)
    (user_trace_width 0.3048)
    (user_trace_width 0.381)
    (user_trace_width 0.4318)
    (user_trace_width 0.508)
    (user_trace_width 0.6096)
    (user_trace_width 0.8128)
    (trace_clearance 0.508)
    (zone_clearance 0.3302)
    (zone_45_only no)
    (trace_min 0.3048)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.381)
    (via_min_drill 0.3302)
    (user_via 0.508 0.3302)
    (user_via 0.8128 0.508)
    (user_via 1.016 0.4064)
    (user_via 1.2192 0.8128)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.5 2)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 100 60)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory PCB))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /OSC0)
  (net 3 /OSC1)
  (net 4 VCC)
  (net 5 /VUSB)
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(D2-Pad1)")
  (net 8 /D-)
  (net 9 /D+)
  (net 10 /PIN0/SDA)
  (net 11 /PIN1/SCL)
  (net 12 /PIN15/A2)
  (net 13 /PIN2)
  (net 14 /PIN16/A3)
  (net 15 /PIN3)
  (net 16 /PIN17/A4)
  (net 17 /PIN4)
  (net 18 /PIN18/A5)
  (net 19 /PIN5)
  (net 20 /PIN19/A6)
  (net 21 /PIN6)
  (net 22 /PIN20/A7)
  (net 23 /PIN7)
  (net 24 /PIN21)
  (net 25 /PIN8/TX)
  (net 26 /PIN22)
  (net 27 /PIN9/RX)
  (net 28 /PIN23)
  (net 29 /PIN10)
  (net 30 /PIN24)
  (net 31 /PIN11/PWM)
  (net 32 /PIN25)
  (net 33 /PIN12/PWM)
  (net 34 /PIN26)
  (net 35 /PIN13/A0)
  (net 36 /PIN27)
  (net 37 /PIN14/A1)
  (net 38 /PIN28)
  (net 39 /ICSP-VPP)
  (net 40 /ICSP_PGD)
  (net 41 /ICSP_PGC)
  (net 42 /RA4)
  (net 43 /MCLR)
  (net_class Default "This is the default net class."
    (clearance 0.508)
    (trace_width 0.3048)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /D+)
    (add_net /D-)
    (add_net /ICSP-VPP)
    (add_net /ICSP_PGC)
    (add_net /ICSP_PGD)
    (add_net /MCLR)
    (add_net /OSC0)
    (add_net /OSC1)
    (add_net /PIN0/SDA)
    (add_net /PIN1/SCL)
    (add_net /PIN10)
    (add_net /PIN11/PWM)
    (add_net /PIN12/PWM)
    (add_net /PIN13/A0)
    (add_net /PIN14/A1)
    (add_net /PIN15/A2)
    (add_net /PIN16/A3)
    (add_net /PIN17/A4)
    (add_net /PIN18/A5)
    (add_net /PIN19/A6)
    (add_net /PIN2)
    (add_net /PIN20/A7)
    (add_net /PIN21)
    (add_net /PIN22)
    (add_net /PIN23)
    (add_net /PIN24)
    (add_net /PIN25)
    (add_net /PIN26)
    (add_net /PIN27)
    (add_net /PIN28)
    (add_net /PIN3)
    (add_net /PIN4)
    (add_net /PIN5)
    (add_net /PIN6)
    (add_net /PIN7)
    (add_net /PIN8/TX)
    (add_net /PIN9/RX)
    (add_net /RA4)
    (add_net /VUSB)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net VCC)
  )
  (net_class Power ""
    (clearance 0.3048)
    (trace_width 0.4318)
    (via_dia 1.397)
    (via_drill 1.016)
    (uvia_dia 1.016)
    (uvia_drill 0.254)
  )
  (module LOGO (layer B.Cu) (tedit 0)
    (at 66.9036 59.9948 270)
    (fp_text reference G*** (at 0 -2.65176 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 2.65176 270) (layer B.SilkS) hide)
  )
  (module LOGO (layer F.Cu) (tedit 0)
    (at 86.3346 58.7502 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 58ACBEAD)
    (at 66.802 67.4116)
    (fp_text reference M2 (at 0.0762 1.9558) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_2mmDrill (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.99898) (layers *.Cu *.Mask F.SilkS))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 58ACBEBB)
    (at 66.802 52.5018)
    (fp_text reference M2 (at 0.0762 1.9558) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_2mmDrill (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.99898) (layers *.Cu *.Mask F.SilkS))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 58ACBEC3)
    (at 112.268 69.723)
    (fp_text reference M2 (at 0.0762 1.9558) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_2mmDrill (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.99898) (layers *.Cu *.Mask F.SilkS))
  )
  (module Housings_QFP:TQFP-44_10x10mm_Pitch0.8mm (layer B.Cu) (tedit 5861E595)
    (at 91 60)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U1 (at 0 7.45) (layer B.SilkS) hide)
    (fp_text value "PIC18(L)F4550-I/PT" (at 0 -7.45) (layer B.Fab))
    (pad 1 smd rect (at -5.7 4) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 27 /PIN9/RX))
    (pad 2 smd rect (at -5.7 3.2) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 32 /PIN25))
    (pad 3 smd rect (at -5.7 2.4) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 34 /PIN26))
    (pad 4 smd rect (at -5.7 1.6) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 36 /PIN27))
    (pad 5 smd rect (at -5.7 0.8) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 38 /PIN28))
    (pad 6 smd rect (at -5.7 0) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -5.7 -0.8) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 4 VCC))
    (pad 8 smd rect (at -5.7 -1.6) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 10 /PIN0/SDA))
    (pad 9 smd rect (at -5.7 -2.4) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 11 /PIN1/SCL))
    (pad 10 smd rect (at -5.7 -3.2) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 13 /PIN2))
    (pad 11 smd rect (at -5.7 -4) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 15 /PIN3))
    (pad 12 smd rect (at -4 -5.7 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 41 /ICSP_PGC))
    (pad 13 smd rect (at -3.2 -5.7 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 40 /ICSP_PGD))
    (pad 14 smd rect (at -2.4 -5.7 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 17 /PIN4))
    (pad 15 smd rect (at -1.6 -5.7 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 19 /PIN5))
    (pad 16 smd rect (at -0.8 -5.7 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 21 /PIN6))
    (pad 17 smd rect (at 0 -5.7 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 23 /PIN7))
    (pad 18 smd rect (at 0.8 -5.7 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 43 /MCLR))
    (pad 19 smd rect (at 1.6 -5.7 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 35 /PIN13/A0))
    (pad 20 smd rect (at 2.4 -5.7 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 37 /PIN14/A1))
    (pad 21 smd rect (at 3.2 -5.7 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 12 /PIN15/A2))
    (pad 22 smd rect (at 4 -5.7 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 14 /PIN16/A3))
    (pad 23 smd rect (at 5.7 -4) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 16 /PIN17/A4))
    (pad 24 smd rect (at 5.7 -3.2) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 42 /RA4))
    (pad 25 smd rect (at 5.7 -2.4) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 18 /PIN18/A5))
    (pad 26 smd rect (at 5.7 -1.6) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 20 /PIN19/A6))
    (pad 27 smd rect (at 5.7 -0.8) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 22 /PIN20/A7))
    (pad 28 smd rect (at 5.7 0) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 4 VCC))
    (pad 29 smd rect (at 5.7 0.8) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 30 smd rect (at 5.7 1.6) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 3 /OSC1))
    (pad 31 smd rect (at 5.7 2.4) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 /OSC0))
    (pad 32 smd rect (at 5.7 3.2) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 29 /PIN10))
    (pad 33 smd rect (at 5.7 4) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 39 /ICSP-VPP))
    (pad 34 smd rect (at 4 5.7 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 35 smd rect (at 3.2 5.7 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 31 /PIN11/PWM))
    (pad 36 smd rect (at 2.4 5.7 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 33 /PIN12/PWM))
    (pad 37 smd rect (at 1.6 5.7 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 5 /VUSB))
    (pad 38 smd rect (at 0.8 5.7 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 24 /PIN21))
    (pad 39 smd rect (at 0 5.7 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 26 /PIN22))
    (pad 40 smd rect (at -0.8 5.7 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 28 /PIN23))
    (pad 41 smd rect (at -1.6 5.7 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 30 /PIN24))
    (pad 42 smd rect (at -2.4 5.7 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 8 /D-))
    (pad 43 smd rect (at -3.2 5.7 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 9 /D+))
    (pad 44 smd rect (at -4 5.7 270) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 25 /PIN8/TX))
    (model Housings_QFP.3dshapes/TQFP-44_10x10mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FB86)
    (at 78.994 70.485)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P21 (at 0 -2.949999) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /PIN8/TX))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58ACC226)
    (at 73.5062 58.5724)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at -0.0014 0.0043) (layer B.SilkS))
    (fp_text value 22uF (at -2.7065 -0.2751 90) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 /OSC0) (clearance 0.508))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58ACC21E)
    (at 73.509 61.3664)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at -0.0268 0.0297) (layer B.SilkS))
    (fp_text value 22uF (at -2.6176 0.0678 90) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 /OSC1) (clearance 0.508))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58ACC20E)
    (at 73.509 64.1688)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at -0.0014 0.0043) (layer B.SilkS))
    (fp_text value 100nF (at 0.1256 1.7823) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 VCC) (clearance 0.508))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58ACC233)
    (at 73.509 55.7868 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at 0.0014 -0.0043 180) (layer B.SilkS))
    (fp_text value 220nF (at 0 1.397 180) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 5 /VUSB) (clearance 0.508))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206 (layer B.Cu) (tedit 58ACC5F1)
    (at 106.86034 56.7436 180)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D1 (at 0.0306 0.7214 180) (layer B.SilkS))
    (fp_text value Run (at -2.89306 0.0508 270) (layer B.SilkS))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 4 VCC) (clearance 0.508))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D1-Pad1)") (clearance 0.508))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer B.Cu) (tedit 58ACC5CC)
    (at 106.86034 63.2968 180)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D2 (at 0.0433 0.7214 180) (layer B.SilkS))
    (fp_text value Power (at -2.91846 -0.0508 450) (layer B.SilkS))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 4 VCC) (clearance 0.508))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D2-Pad1)") (clearance 0.508))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connect:USB_Mini-B (layer F.Cu) (tedit 58609E1F)
    (at 69 60)
    (descr "USB Mini-B 5-pin SMD connector")
    (tags "USB USB_B USB_Mini connector")
    (attr smd)
    (fp_text reference P1 (at 0 6.90118) (layer F.SilkS) hide)
    (fp_text value uUSB (at -1.563 -0.183 90) (layer F.Fab))
    (pad 1 smd rect (at 3.44932 -1.6002) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 2 smd rect (at 3.44932 -0.8001) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 8 /D-))
    (pad 3 smd rect (at 3.44932 0) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 9 /D+))
    (pad 4 smd rect (at 3.44932 0.8001) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 3.44932 1.6002) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 3.35026 -4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.14884 -4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 3.35026 4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.14884 4.45008) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 0.8509 -2.19964) (size 0.89916 0.89916) (drill 0.89916) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0.8509 2.19964) (size 0.89916 0.89916) (drill 0.89916) (layers *.Cu *.Mask F.SilkS))
    (model Connect.3dshapes/USB_Mini_B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 58ACB267)
    (at 101.854 57.404 90)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P2 (at 0 -3 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 VCC) (clearance 0.508))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 58630140)
    (at 101.854 62.484)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P3 (at 0 -2.739999) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 58ACB253)
    (at 101.854 59.944 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P4 (at 0 -2.349999 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 VCC) (clearance 0.508))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 58630146)
    (at 101.854 65.024)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P5 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FDBC)
    (at 68.834 49.403)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P7 (at 0 -2.939999) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /PIN1/SCL))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FB02)
    (at 96.774 49.403)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P8 (at 0 -3) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /PIN15/A2))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FDB7)
    (at 71.374 49.403)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P9 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /PIN2))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FB08)
    (at 99.314 49.403)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P10 (at 0 -3) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /PIN16/A3))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FDC2)
    (at 73.914 49.403)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P11 (at 0 -3) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /PIN3))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FB0D)
    (at 101.854 49.403)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P12 (at 0 -2.549999) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /PIN17/A4))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FA9F)
    (at 81.534 49.403)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P13 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /PIN4))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FB15)
    (at 101.854 52.324 90)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P14 (at 0 -3.139999 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /PIN18/A5))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FAB2)
    (at 84.074 49.403)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P15 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /PIN5))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FB2F)
    (at 101.854 54.864 90)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P16 (at 0.036666 -2.549999 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /PIN19/A6))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FABA)
    (at 86.614 49.403)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P17 (at 0.246666 -2.749999) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /PIN6))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FB21)
    (at 101.854 70.485)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P18 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /PIN20/A7))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FAC0)
    (at 89.154 49.403)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P19 (at 0.456666 -2.339999) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /PIN7))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FB51)
    (at 89.154 70.485)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P20 (at 0 -2.749999) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /PIN21))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FB75)
    (at 86.614 70.485)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P22 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /PIN22))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FB8B)
    (at 76.454 70.485)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P23 (at 0 -2.549999) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /PIN9/RX))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FB5C)
    (at 84.074 70.485)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P24 (at 0 -3) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /PIN23))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FB34)
    (at 99.314 70.485)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P25 (at 0.036666 -2.949999) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /PIN10))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FB62)
    (at 81.534 70.485)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P26 (at 0 -3.149999) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /PIN24))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FB41)
    (at 94.234 70.485)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P27 (at 0 -2.749999) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /PIN11/PWM))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FDD5)
    (at 73.914 70.485)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P28 (at 0 -3) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /PIN25))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FB4C)
    (at 91.694 70.485)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P29 (at 0 -2.549999) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /PIN12/PWM))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FB68)
    (at 71.374 70.485)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P30 (at 0 -3) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /PIN26))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FAC6)
    (at 91.694 49.403)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P31 (at 0.036666 -3.149999) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /PIN13/A0))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FB7A)
    (at 68.834 70.485)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P32 (at 0 -3) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /PIN27))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FAFB)
    (at 94.234 49.403)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P33 (at 0 -2.949999) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /PIN14/A1))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FB7F)
    (at 66.294 70.485)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P34 (at 0 -2.749999) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /PIN28))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FB3C)
    (at 96.774 70.485)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P35 (at 0 -2.549999) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /ICSP-VPP))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FA94)
    (at 78.994 49.403)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P36 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /ICSP_PGD))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FDAF)
    (at 76.454 49.403)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P37 (at 0 -2.949999) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /ICSP_PGC))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58ACC292)
    (at 106.8346 53.594)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at -0.0387 -0.4801) (layer B.SilkS))
    (fp_text value 470 (at 0.0121 0.6375) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 42 /RA4) (clearance 0.508))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D1-Pad1)") (clearance 0.508))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58ACC26C)
    (at 106.833 60.0939)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at -0.026 -0.5309) (layer B.SilkS))
    (fp_text value 10k (at -0.0006 0.4851) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VCC))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 43 /MCLR) (clearance 0.508))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58ACC264)
    (at 106.8346 66.294 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0.026 0.4039 180) (layer B.SilkS))
    (fp_text value 470 (at 0.026 -0.6121 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D2-Pad1)") (clearance 0.508))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_REED_CT05-XXXX-G1 (layer B.Cu) (tedit 58ACC2A2)
    (at 112.011 59.9999 90)
    (descr "Coto Technologies SPST Reed Switch CT05-XXXX-G1")
    (tags "Coto Reed SPST Switch")
    (attr smd)
    (fp_text reference SW1 (at 0.0051 -1.0638 90) (layer B.SilkS))
    (fp_text value Reset (at 0.0559 0.003 90) (layer B.Fab))
    (pad 2 smd rect (at 4.275 0 90) (size 2.5 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -4.275 0 90) (size 2.5 2) (layers B.Cu B.Paste B.Mask)
      (net 43 /MCLR) (clearance 0.508))
    (model Buttons_Switches_SMD.3dshapes/SW_SMD_1181.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Crystal SMD:Crystal_SMD_5032_2Pads" (layer B.Cu) (tedit 58ACC24E)
    (at 78.063 59.9218 90)
    (descr "Ceramic SMD crystal, 5.0x3.2mm, 2 Pads")
    (tags "crystal oscillator quartz SMD SMT 5032")
    (attr smd)
    (fp_text reference Y1 (at 0.073 -0.0039 90) (layer B.SilkS))
    (fp_text value Crystal (at -0.104806 0.974 90) (layer B.Fab))
    (pad 1 smd rect (at -2.05 0 90) (size 2 2.4) (layers B.Cu B.Paste B.Mask)
      (net 3 /OSC1))
    (pad 2 smd rect (at 2.05 0 90) (size 2 2.4) (layers B.Cu B.Paste B.Mask)
      (net 2 /OSC0) (clearance 0.508))
    (model Crystals.3dshapes/Crystal_SMD_5032_2Pads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5862FDCC)
    (at 66.294 49.403)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P6 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /PIN0/SDA))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 586302CF)
    (at 101.854 67.564)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P38 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:c_elec_6.3x5.3 (layer F.Cu) (tedit 55725E31)
    (at 78.3844 59.98718 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.3")
    (attr smd)
    (fp_text reference C5 (at -3.92938 2.2352 360) (layer F.SilkS))
    (fp_text value 10-100uF (at 0 4.445 270) (layer F.Fab))
    (pad 1 smd rect (at 2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 2 smd rect (at -2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/c_elec_6.3x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 58ACBE28)
    (at 112.268 50.292)
    (fp_text reference M2 (at 0.0762 1.9558) (layer F.SilkS))
    (fp_text value SolderWirePad_single_2mmDrill (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.99898) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text 19|A6 (at 103.9622 54.864 90) (layer B.SilkS))
  (dimension 25.019 (width 0.3) (layer Dwgs.User)
    (gr_text "0,9850 in" (at 60.88 60.0075 270) (layer Dwgs.User))
    (feature1 (pts (xy 64.262 72.517) (xy 59.53 72.517)))
    (feature2 (pts (xy 64.262 47.498) (xy 59.53 47.498)))
    (crossbar (pts (xy 62.23 47.498) (xy 62.23 72.517)))
    (arrow1a (pts (xy 62.23 72.517) (xy 61.643579 71.390496)))
    (arrow1b (pts (xy 62.23 72.517) (xy 62.816421 71.390496)))
    (arrow2a (pts (xy 62.23 47.498) (xy 61.643579 48.624504)))
    (arrow2b (pts (xy 62.23 47.498) (xy 62.816421 48.624504)))
  )
  (dimension 50.8 (width 0.3) (layer Dwgs.User)
    (gr_text "2,0000 in" (at 89.662 44.370001) (layer Dwgs.User))
    (feature1 (pts (xy 64.262 47.498) (xy 64.262 43.020001)))
    (feature2 (pts (xy 115.062 47.498) (xy 115.062 43.020001)))
    (crossbar (pts (xy 115.062 45.720001) (xy 64.262 45.720001)))
    (arrow1a (pts (xy 64.262 45.720001) (xy 65.388504 45.13358)))
    (arrow1b (pts (xy 64.262 45.720001) (xy 65.388504 46.306422)))
    (arrow2a (pts (xy 115.062 45.720001) (xy 113.935496 45.13358)))
    (arrow2b (pts (xy 115.062 45.720001) (xy 113.935496 46.306422)))
  )
  (gr_text "Pinguino 4550 SMD" (at 108.077 60.071 90) (layer F.SilkS))
  (gr_text Rootdevel.co (at 113.7158 60.1218 90) (layer F.SilkS))
  (gr_text "9\nRX" (at 76.454 67.8942) (layer B.SilkS))
  (gr_text "8\nTX" (at 79.0702 67.8942) (layer B.SilkS))
  (gr_text "11\nPWM" (at 94.2594 67.8434) (layer B.SilkS))
  (gr_text "12\nPWM" (at 91.7448 67.8434) (layer B.SilkS))
  (gr_text 28 (at 65.278 68.9356) (layer B.SilkS))
  (gr_text GND (at 104.0892 67.564 90) (layer B.SilkS))
  (gr_text GND (at 104.0892 65.024 90) (layer B.SilkS))
  (gr_text GND (at 104.0892 62.484 90) (layer B.SilkS))
  (gr_text 5V (at 103.9622 59.8678 90) (layer B.SilkS))
  (gr_text 5V (at 103.9622 57.4294 90) (layer B.SilkS))
  (gr_text "18\nA5" (at 104.5972 52.07 90) (layer B.SilkS))
  (gr_text "20\nA7" (at 104.5972 70.612 90) (layer B.SilkS))
  (gr_text "17\nA4" (at 104.5972 49.2252 90) (layer B.SilkS))
  (gr_text 10 (at 99.3394 68.4784) (layer B.SilkS))
  (gr_text VPP (at 96.8756 68.453) (layer B.SilkS))
  (gr_text 21 (at 89.154 68.4784) (layer B.SilkS))
  (gr_text 22 (at 86.614 68.4784) (layer B.SilkS))
  (gr_text 23 (at 84.074 68.4784) (layer B.SilkS))
  (gr_text 24 (at 81.534 68.4784) (layer B.SilkS))
  (gr_text 25 (at 73.914 68.4784) (layer B.SilkS))
  (gr_text 26 (at 71.374 68.4784) (layer B.SilkS))
  (gr_text 27 (at 68.834 68.4784) (layer B.SilkS))
  (gr_text "16\nA3" (at 99.06 52.0954) (layer B.SilkS))
  (gr_text "15\nA2" (at 96.52 52.0954) (layer B.SilkS))
  (gr_text "14\nA1" (at 94.234 52.0954) (layer B.SilkS))
  (gr_text "13\nA0" (at 91.6178 52.0954) (layer B.SilkS))
  (gr_text PGD (at 78.9686 51.6382) (layer B.SilkS))
  (gr_text PGC (at 76.454 51.6382) (layer B.SilkS))
  (gr_text "0\nSDA" (at 65.5066 50.927 270) (layer B.SilkS))
  (gr_text 1 (at 68.834 51.6128) (layer B.SilkS))
  (gr_text 7 (at 89.0016 51.6128) (layer B.SilkS))
  (gr_text 6 (at 86.4616 51.6128) (layer B.SilkS))
  (gr_text 5 (at 83.947 51.6128) (layer B.SilkS))
  (gr_text 4 (at 81.3816 51.6128) (layer B.SilkS))
  (gr_text 3 (at 73.914 51.6128) (layer B.SilkS))
  (gr_text 2 (at 71.2978 51.6128) (layer B.SilkS))
  (gr_text "20\nA7" (at 105.0798 70.5612 90) (layer F.SilkS))
  (gr_text "19\nA6" (at 105.0798 55.1434 90) (layer F.SilkS))
  (gr_text "18\nA5" (at 105.0798 52.5018 90) (layer F.SilkS))
  (gr_text "17\nA4" (at 105.0798 49.53 90) (layer F.SilkS))
  (gr_text "16\nA3" (at 98.9076 52.6796) (layer F.SilkS))
  (gr_text "15\nA2" (at 96.4438 52.6796) (layer F.SilkS))
  (gr_text "14\nA1" (at 93.9546 52.6796) (layer F.SilkS))
  (gr_text "13\nA0" (at 91.44 52.6796) (layer F.SilkS))
  (gr_text "9\nRX" (at 76.1492 67.5894) (layer F.SilkS))
  (gr_text "8\nTX" (at 78.6892 67.5894) (layer F.SilkS))
  (gr_text 10 (at 99.0854 68.0466) (layer F.SilkS))
  (gr_text "11\nPWM" (at 93.9546 67.6148) (layer F.SilkS))
  (gr_text VPP (at 96.52 67.9704) (layer F.SilkS))
  (gr_text "12\nPWM" (at 91.4146 67.6148) (layer F.SilkS))
  (gr_text 21 (at 88.8238 68.0466) (layer F.SilkS))
  (gr_text 22 (at 86.2838 68.0466) (layer F.SilkS))
  (gr_text 23 (at 83.7438 68.0466) (layer F.SilkS))
  (gr_text 24 (at 81.3054 68.0466) (layer F.SilkS))
  (gr_text 25 (at 73.6346 68.0466) (layer F.SilkS))
  (gr_text 26 (at 71.0946 68.0466) (layer F.SilkS))
  (gr_text 27 (at 68.8086 68.0974) (layer F.SilkS))
  (gr_text 28 (at 64.9986 67.945 90) (layer F.SilkS))
  (gr_text GND (at 104.521 67.4878 90) (layer F.SilkS))
  (gr_text GND (at 104.521 64.9732 90) (layer F.SilkS))
  (gr_text GND (at 104.521 62.4332 90) (layer F.SilkS))
  (gr_text 5V (at 104.5718 59.9948 90) (layer F.SilkS))
  (gr_text 5V (at 104.5718 57.5056 90) (layer F.SilkS))
  (gr_text 0|SDA (at 64.9224 52.3494 90) (layer F.SilkS))
  (gr_text PGD (at 78.7146 51.8414) (layer F.SilkS))
  (gr_text PGC (at 76.1492 51.8414) (layer F.SilkS))
  (gr_text 7 (at 88.9254 52.197) (layer F.SilkS))
  (gr_text 6 (at 86.3346 52.197) (layer F.SilkS))
  (gr_text 5 (at 83.82 52.197) (layer F.SilkS))
  (gr_text 4 (at 81.28 52.197) (layer F.SilkS))
  (gr_text 3 (at 73.66 52.197) (layer F.SilkS))
  (gr_text 2 (at 71.1962 52.197) (layer F.SilkS))
  (gr_text "SCL\n1" (at 68.9102 52.0446) (layer F.SilkS))
  (gr_line (start 64.262 72.517) (end 64.262 47.498) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.062 72.517) (end 64.262 72.517) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.062 47.498) (end 115.062 72.517) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 64.262 47.498) (end 115.062 47.498) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3302))
    (min_thickness 0.3048)
    (fill yes (arc_segments 16) (thermal_gap 0.3048) (thermal_bridge_width 0.381) (smoothing fillet))
    (polygon
      (pts
        (xy 64.3382 47.5742) (xy 114.9858 47.5742) (xy 114.9858 72.4408) (xy 64.3382 72.4408)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.381) (smoothing fillet))
    (polygon
      (pts
        (xy 114.9858 72.4408) (xy 64.3382 72.4408) (xy 64.3382 47.5742) (xy 114.9858 47.5742)
      )
    )
  )
)
