(kicad_pcb (version 20171130) (host pcbnew 5.1.7-a382d34a8~87~ubuntu20.04.1)
  (general
    (thickness 1.6)
    (drawings 59)
    (tracks 133)
    (zones 0)
    (modules 6)
    (nets 32)
  )
  (page USLetter)
  (title_block
    (date 2020-11-02)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.18)
    (user_trace_width 0.16)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (trace_clearance 0.16)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.16)
    (via_size 0.4)
    (via_drill 0.25)
    (via_min_size 0.4)
    (via_min_drill 0.25)
    (uvia_size 0.4)
    (uvia_drill 0.25)
    (uvias_allowed no)
    (uvia_min_size 0.4)
    (uvia_min_drill 0.25)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2)
    (pad_drill 2)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 127 101.6)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /D3)
  (net 2 /A12)
  (net 3 /D4)
  (net 4 /A7)
  (net 5 /D5)
  (net 6 /A6)
  (net 7 /D6)
  (net 8 /A5)
  (net 9 /D7)
  (net 10 /A4)
  (net 11 /~CS_OUT)
  (net 12 /A3)
  (net 13 /A10)
  (net 14 /A2)
  (net 15 /~OE)
  (net 16 /A1)
  (net 17 /A11)
  (net 18 /A0)
  (net 19 /A9)
  (net 20 /D0)
  (net 21 /A8)
  (net 22 /D1)
  (net 23 /A13)
  (net 24 /D2)
  (net 25 /A14)
  (net 26 /GND)
  (net 27 /VCC)
  (net 28 /~CS_IN)
  (net 29 /~WE)
  (net 30 /A14_~WE)
  (net 31 /NC_A14)
  (net_class Default "This is the default net class."
    (clearance 0.16)
    (trace_width 0.18)
    (via_dia 0.4)
    (via_drill 0.25)
    (uvia_dia 0.4)
    (uvia_drill 0.25)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A14_~WE)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /GND)
    (add_net /NC_A14)
    (add_net /VCC)
    (add_net /~CS_IN)
    (add_net /~CS_OUT)
    (add_net /~OE)
    (add_net /~WE)
  )
  (module 000_LOCAL:PinHeader_1x04_P2.00mm_Horizontal (layer F.Cu) (tedit 5F9FCD4A)
    (at 130 111.4 270)
    (descr "Through hole angled pin header, 1x04, 2.00mm pitch, 4.2mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.00mm single row")
    (fp_text reference JP2 (at 3.1 -2 90) (layer F.SilkS) hide)
    (fp_text value Jumper_4_Bridged23 (at 3.1 8 90) (layer F.Fab))
    (fp_text user %R (at 2.25 3) (layer F.Fab))
    (pad 4 thru_hole circle (at 0 6 270) (size 1.35 1.35) (drill 0.75) (layers *.Cu *.Mask)
      (net 31 /NC_A14))
    (pad 3 thru_hole circle (at 0 4 270) (size 1.35 1.35) (drill 0.75) (layers *.Cu *.Mask)
      (net 25 /A14))
    (pad 2 thru_hole circle (at 0 2 270) (size 1.35 1.35) (drill 0.75) (layers *.Cu *.Mask)
      (net 30 /A14_~WE))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.35 1.35) (drill 0.75) (layers *.Cu *.Mask)
      (net 29 /~WE))
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/PinHeader_1x04_P2.00mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:DIP28_0.6_pcb_sil_pins (layer F.Cu) (tedit 5E4383E0)
    (at 127 101.6)
    (descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (fp_text reference J1 (at -4.445 -16.51) (layer F.SilkS) hide)
    (fp_text value "27C256 DIP LEGS" (at 0 18.84) (layer F.Fab))
    (fp_text user %R (at 0.27 3.12) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 -17.11) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad 1 thru_hole roundrect (at -7.62 -16.51) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 31 /NC_A14))
    (pad 15 thru_hole circle (at 7.62 16.51) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 1 /D3))
    (pad 2 thru_hole circle (at -7.62 -13.97) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 2 /A12))
    (pad 16 thru_hole circle (at 7.62 13.97) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 3 /D4))
    (pad 3 thru_hole circle (at -7.62 -11.43) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 4 /A7))
    (pad 17 thru_hole circle (at 7.62 11.43) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 5 /D5))
    (pad 4 thru_hole circle (at -7.62 -8.89) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 6 /A6))
    (pad 18 thru_hole circle (at 7.62 8.89) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 7 /D6))
    (pad 5 thru_hole circle (at -7.62 -6.35) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 8 /A5))
    (pad 19 thru_hole circle (at 7.62 6.35) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 9 /D7))
    (pad 6 thru_hole circle (at -7.62 -3.81) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 10 /A4))
    (pad 20 thru_hole circle (at 7.62 3.81) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 11 /~CS_OUT))
    (pad 7 thru_hole circle (at -7.62 -1.27) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 12 /A3))
    (pad 21 thru_hole circle (at 7.62 1.27) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 13 /A10))
    (pad 8 thru_hole circle (at -7.62 1.27) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 14 /A2))
    (pad 22 thru_hole circle (at 7.62 -1.27) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 15 /~OE))
    (pad 9 thru_hole circle (at -7.62 3.81) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 16 /A1))
    (pad 23 thru_hole circle (at 7.62 -3.81) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 17 /A11))
    (pad 10 thru_hole circle (at -7.62 6.35) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 18 /A0))
    (pad 24 thru_hole circle (at 7.62 -6.35) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 19 /A9))
    (pad 11 thru_hole circle (at -7.62 8.89) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 20 /D0))
    (pad 25 thru_hole circle (at 7.62 -8.89) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 21 /A8))
    (pad 12 thru_hole circle (at -7.62 11.43) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 22 /D1))
    (pad 26 thru_hole circle (at 7.62 -11.43) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 23 /A13))
    (pad 13 thru_hole circle (at -7.62 13.97) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 24 /D2))
    (pad 27 thru_hole circle (at 7.62 -13.97) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 30 /A14_~WE))
    (pad 14 thru_hole circle (at -7.62 16.51) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 26 /GND))
    (pad 28 thru_hole circle (at 7.62 -16.51) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask)
      (net 27 /VCC))
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 16.51 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 13.97 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 11.43 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 8.890000000000001 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 6.35 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 3.81 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 1.27 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 -1.27 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 -3.81 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 -6.35 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 -8.890000000000001 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 -11.43 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 -13.97 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 -16.51 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 -16.51 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 -13.97 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 -11.43 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 -8.890000000000001 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 -6.35 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 -3.81 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 -1.27 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 1.27 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 3.81 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 6.35 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 8.890000000000001 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 11.43 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 13.97 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 16.51 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:R_0805 (layer F.Cu) (tedit 5F9E65BE)
    (at 129.495 91.335 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -0.005 -0.015 -90 unlocked) (layer F.SilkS))
    (fp_text value 47K (at 0 1.75) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 29 /~WE))
    (pad 2 smd roundrect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 27 /VCC))
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:R_0805 (layer F.Cu) (tedit 5F9E65BE)
    (at 124.495 91.335 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -0.005 -0.015 270 unlocked) (layer F.SilkS))
    (fp_text value 47K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 28 /~CS_IN))
    (pad 2 smd roundrect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 27 /VCC))
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:SOIC28W (layer F.Cu) (tedit 5E621A1B)
    (at 127 101.6)
    (descr "28-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -10.05) (layer F.SilkS) hide)
    (fp_text value 28C256 (at -0.0003 -0.0002 -90) (layer F.SilkS))
    (fp_text user %R (at -0.01 1.61) (layer F.Fab))
    (pad 28 smd roundrect (at 4.7 -8.255) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 /VCC))
    (pad 27 smd roundrect (at 4.7 -6.985) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /~WE))
    (pad 26 smd roundrect (at 4.7 -5.715) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /A13))
    (pad 25 smd roundrect (at 4.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /A8))
    (pad 24 smd roundrect (at 4.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /A9))
    (pad 23 smd roundrect (at 4.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /A11))
    (pad 22 smd roundrect (at 4.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /~OE))
    (pad 21 smd roundrect (at 4.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /A10))
    (pad 20 smd roundrect (at 4.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /~CS_IN))
    (pad 19 smd roundrect (at 4.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /D7))
    (pad 18 smd roundrect (at 4.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /D6))
    (pad 17 smd roundrect (at 4.7 5.715) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /D5))
    (pad 16 smd roundrect (at 4.7 6.985) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /D4))
    (pad 15 smd roundrect (at 4.7 8.255) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /D3))
    (pad 14 smd roundrect (at -4.7 8.255) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 /GND))
    (pad 13 smd roundrect (at -4.7 6.985) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /D2))
    (pad 12 smd roundrect (at -4.7 5.715) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /D1))
    (pad 11 smd roundrect (at -4.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /D0))
    (pad 10 smd roundrect (at -4.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /A0))
    (pad 9 smd roundrect (at -4.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /A1))
    (pad 8 smd roundrect (at -4.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /A2))
    (pad 7 smd roundrect (at -4.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /A3))
    (pad 6 smd roundrect (at -4.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /A4))
    (pad 5 smd roundrect (at -4.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /A5))
    (pad 4 smd roundrect (at -4.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /A6))
    (pad 3 smd roundrect (at -4.7 -5.715) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /A7))
    (pad 2 smd roundrect (at -4.7 -6.985) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /A12))
    (pad 1 smd roundrect (at -4.7 -8.255) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /A14))
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/SOIC28W.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:Pin_Header_Angled_1x02_Pitch2.54mm (layer F.Cu) (tedit 5E349946)
    (at 132.715 88.9 180)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference JP1 (at 4.385 -2.27 180) (layer F.SilkS) hide)
    (fp_text value "~CS~ breakout (REX TP1)" (at 4.385 4.81 180) (layer F.Fab))
    (fp_text user %R (at 2.77 1.27 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.914) (layers *.Cu *.Mask)
      (net 28 /~CS_IN))
    (pad 2 thru_hole circle (at 0 2.54 180) (size 1.4 1.4) (drill 0.914) (layers *.Cu *.Mask)
      (net 11 /~CS_OUT))
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/PinHeader_1x02_P2.54mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text RUN (at 126.95 116.65 -90) (layer F.SilkS))
  (gr_text "To program:\n  Set jumpers to PROGRAM.\n  Put board in programmer.\n  Set programmer for 28C256." (at 127 84.6 90) (layer B.SilkS))
  (gr_text "REX main rom: ~CS~ OUT to REX TP1\nNo REX: ~CS~ OUT to ~CS~ IN" (at 121.7 84.5 -270) (layer B.SilkS))
  (gr_text PROGRAM (at 127 115.4) (layer B.SilkS))
  (gr_text RUN (at 127 109.7) (layer B.SilkS))
  (gr_text tandy.wiki/FlexROM_102 (at 133.2865 101.6 -90) (layer F.SilkS))
  (gr_line (start 118.775 118.715) (end 118.775 84.495) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135.215 84.495) (end 135.215 118.715) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 118.775 84.495) (end 135.215 84.495) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 118.775 118.715) (end 135.215 118.715) (layer Edge.Cuts) (width 0.05))
  (gr_text "R1,R2: 47k" (at 132.316 90.505 90) (layer B.SilkS))
  (gr_text "TANDY MODEL 102 MAIN ROM" (at 120.7135 101.6 -90) (layer F.SilkS))
  (gr_text "~CS~ (to REX)" (at 124.95 87.65) (layer F.SilkS))
  (gr_text OUT (at 121.295 86.355) (layer F.SilkS))
  (gr_text IN (at 121.375 88.905) (layer F.SilkS))
  (gr_text "Legs: TE 1544210" (at 133.205 90.505 90) (layer B.SilkS))
)
