(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 20)
    (tracks 33)
    (zones 0)
    (modules 7)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 3)
    (user_trace_width 0.5)
    (user_trace_width 2.5)
    (user_trace_width 3)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 6 3.2)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 10 10)
    (pad_drill 4.2)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./"))
  )
  (net 0 "")
  (net 1 /Enable)
  (net 2 /ComMonGND)
  (net 3 /TActMon)
  (net 4 /TSetMon)
  (net 5 /PowerV+)
  (net 6 GND)
  (net 7 /TExtSP)
  (net 8 /TExtSPGND)
  (net 9 /Therm+)
  (net 10 /Therm-)
  (net 11 /TEC+)
  (net 12 /TEC-)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ComMonGND)
    (add_net /Enable)
    (add_net /PowerV+)
    (add_net /TActMon)
    (add_net /TEC+)
    (add_net /TEC-)
    (add_net /TExtSP)
    (add_net /TExtSPGND)
    (add_net /TSetMon)
    (add_net /Therm+)
    (add_net /Therm-)
    (add_net GND)
  )
  (module MyFootprints:PTC5000TEC (layer F.Cu) (tedit 5DFA5F31)
    (at 108 116)
    (fp_text reference PTC5000TEC1 (at 22 -3) (layer F.SilkS))
    (fp_text value Conn_01x12_Female (at 0 -0.5) (layer F.Fab))
    (pad 12 thru_hole circle (at 43.56 0) (size 3 3) (drill 1.7) (layers *.Cu *.Mask)
      (net 7 /TExtSP))
    (pad 11 thru_hole circle (at 39.6 0) (size 3 3) (drill 1.7) (layers *.Cu *.Mask)
      (net 8 /TExtSPGND))
    (pad 10 thru_hole circle (at 35.64 0) (size 3 3) (drill 1.7) (layers *.Cu *.Mask)
      (net 9 /Therm+))
    (pad 9 thru_hole circle (at 31.68 0) (size 3 3) (drill 1.7) (layers *.Cu *.Mask)
      (net 10 /Therm-))
    (pad 8 thru_hole circle (at 27.72 0) (size 3 3) (drill 1.7) (layers *.Cu *.Mask)
      (net 5 /PowerV+))
    (pad 7 thru_hole circle (at 23.76 0 90) (size 3 3) (drill 1.7) (layers *.Cu *.Mask)
      (net 6 GND) (zone_connect 1) (thermal_width 0.75) (thermal_gap 0.5))
    (pad 6 thru_hole circle (at 19.8 0) (size 3 3) (drill 1.7) (layers *.Cu *.Mask)
      (net 11 /TEC+))
    (pad 5 thru_hole circle (at 15.84 0 90) (size 3 3) (drill 1.7) (layers *.Cu *.Mask)
      (net 12 /TEC-))
    (pad 4 thru_hole circle (at 11.88 0) (size 3 3) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 /Enable))
    (pad 3 thru_hole circle (at 7.92 0) (size 3 3) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 /ComMonGND))
    (pad 2 thru_hole circle (at 3.96 0) (size 3 3) (drill 1.7) (layers *.Cu *.Mask)
      (net 3 /TActMon))
    (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.7) (layers *.Cu *.Mask)
      (net 4 /TSetMon))
    (pad 13 thru_hole circle (at 4.26 -20.88) (size 10 10) (drill 4.2) (layers *.Cu *.Mask)
      (net 6 GND) (zone_connect 2))
    (pad 14 thru_hole circle (at 39.82 -20.88) (size 10 10) (drill 4.2) (layers *.Cu *.Mask)
      (net 6 GND) (zone_connect 2))
  )
  (module MyFootprints:QLMLogo (layer F.Cu) (tedit 0)
    (at 130 96)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 5B78013E)
    (at 140 126)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference Therm2 (at 1.27 4.12) (layer B.SilkS))
    (fp_text value Conn_01x02_Male (at 1.27 -4.08) (layer B.Fab))
    (fp_text user %R (at 1.27 2.22) (layer B.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 /Therm+))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 10 /Therm-))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 5B78013E)
    (at 148 126)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference TExtSP1 (at 1.27 4.12) (layer B.SilkS))
    (fp_text value Conn_01x02_Male (at 1.27 -4.08) (layer B.Fab))
    (fp_text user %R (at 1.27 2.22) (layer B.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 /TExtSP))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 8 /TExtSPGND))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 5B78013E)
    (at 124 126)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference TEC2 (at 1.27 4.12) (layer B.SilkS))
    (fp_text value Conn_01x02_Male (at 1.27 -4.08) (layer B.Fab))
    (fp_text user %R (at 1.27 2.22) (layer B.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 /TEC+))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 12 /TEC-))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 5DF3C4EA)
    (at 132 126)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference Power1 (at 1.27 4.12) (layer B.SilkS))
    (fp_text value Conn_01x02_Male (at 1.27 -4.08) (layer B.Fab))
    (fp_text user %R (at 1.27 2.22) (layer B.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 /PowerV+))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.144)
      (net 6 GND) (zone_connect 1) (thermal_width 0.75) (thermal_gap 0.5))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer B.Cu) (tedit 5B78013E)
    (at 110.38 126)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference MonitorPins1 (at 3.81 4.12) (layer B.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 -4.08) (layer B.Fab))
    (fp_text user %R (at 3.81 2.22) (layer B.Fab))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 /ComMonGND))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 /Enable))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 /TActMon))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 4 /TSetMon))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "TExtSP GND" (at 149.5 132) (layer B.SilkS))
  (gr_text "GND Enbl TAct TSet" (at 113.5 132) (layer B.SilkS))
  (gr_line (start 156 56) (end 104 56) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 156 142) (end 156 56) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 104 142) (end 156 142) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 104 56) (end 104 142) (layer Edge.Cuts) (width 0.05))
  (gr_text GND (at 131.5 132) (layer B.SilkS))
  (gr_text V+ (at 135.5 132) (layer B.SilkS))
  (gr_text + (at 127 132) (layer B.SilkS))
  (gr_text - (at 123 132) (layer B.SilkS))
  (gr_text 12 (at 152 113) (layer F.SilkS))
  (gr_text 1 (at 108 113) (layer F.SilkS))
  (zone (net 6) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104 56) (xy 156 56) (xy 156 142) (xy 104 142)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104 56) (xy 156 56) (xy 156 142) (xy 104 142)
      )
    )
  )
)
