(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 0.2)
    (drawings 29)
    (tracks 144)
    (zones 0)
    (modules 32)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.05)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.9 0.8)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad3)")
  (net 2 "Net-(U1-Pad1)")
  (net 3 "Net-(J2-Pad2)")
  (net 4 "Net-(J2-Pad3)")
  (net 5 "Net-(J2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad3)")
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer B.Cu) (tedit 622022A1)
    (at 112.07 110.2 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference J2 (at 1.27 3.56 180) (layer B.SilkS) hide)
    (fp_text value Conn_VDG (at 1.27 -2.79 180) (layer B.Fab) hide)
    (fp_text user %R (at 1.27 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at 2.54 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 1.27 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (offset (xyz 0 0 0.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer B.Cu) (tedit 622022A1)
    (at 108.47 110.2 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference J2 (at 1.27 3.56 180) (layer B.SilkS) hide)
    (fp_text value Conn_VDG (at 1.27 -2.79 180) (layer B.Fab) hide)
    (fp_text user %R (at 1.27 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at 2.54 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 1.27 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (offset (xyz 0 0 0.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer B.Cu) (tedit 622022A1)
    (at 104.87 110.2 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference J2 (at 1.27 3.56 180) (layer B.SilkS) hide)
    (fp_text value Conn_VDG (at 1.27 -2.79 180) (layer B.Fab) hide)
    (fp_text user %R (at 1.27 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at 2.54 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 1.27 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (offset (xyz 0 0 0.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer B.Cu) (tedit 622022A1)
    (at 101.27 110.2 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference J2 (at 1.27 3.56 180) (layer B.SilkS) hide)
    (fp_text value Conn_VDG (at 1.27 -2.79 180) (layer B.Fab) hide)
    (fp_text user %R (at 1.27 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at 2.54 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 1.27 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (offset (xyz 0 0 0.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer B.Cu) (tedit 622022A1)
    (at 112.07 106.8 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference J2 (at 1.27 3.56 180) (layer B.SilkS) hide)
    (fp_text value Conn_VDG (at 1.27 -2.79 180) (layer B.Fab) hide)
    (fp_text user %R (at 1.27 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at 2.54 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 1.27 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (offset (xyz 0 0 0.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer B.Cu) (tedit 622022A1)
    (at 108.47 106.8 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference J2 (at 1.27 3.56 180) (layer B.SilkS) hide)
    (fp_text value Conn_VDG (at 1.27 -2.79 180) (layer B.Fab) hide)
    (fp_text user %R (at 1.27 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at 2.54 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 1.27 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (offset (xyz 0 0 0.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer B.Cu) (tedit 622022A1)
    (at 104.87 106.8 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference J2 (at 1.27 3.56 180) (layer B.SilkS) hide)
    (fp_text value Conn_VDG (at 1.27 -2.79 180) (layer B.Fab) hide)
    (fp_text user %R (at 1.27 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at 2.54 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 1.27 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (offset (xyz 0 0 0.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer B.Cu) (tedit 622022A1)
    (at 101.27 106.8 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference J2 (at 1.27 3.56 180) (layer B.SilkS) hide)
    (fp_text value Conn_VDG (at 1.27 -2.79 180) (layer B.Fab) hide)
    (fp_text user %R (at 1.27 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at 2.54 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 1.27 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (offset (xyz 0 0 0.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer B.Cu) (tedit 622022A1)
    (at 112.07 103.4 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference J2 (at 1.27 3.56 180) (layer B.SilkS) hide)
    (fp_text value Conn_VDG (at 1.27 -2.79 180) (layer B.Fab) hide)
    (fp_text user %R (at 1.27 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at 2.54 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 1.27 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (offset (xyz 0 0 0.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer B.Cu) (tedit 622022A1)
    (at 108.47 103.4 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference J2 (at 1.27 3.56 180) (layer B.SilkS) hide)
    (fp_text value Conn_VDG (at 1.27 -2.79 180) (layer B.Fab) hide)
    (fp_text user %R (at 1.27 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at 2.54 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 1.27 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (offset (xyz 0 0 0.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer B.Cu) (tedit 622022A1)
    (at 104.87 103.4 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference J2 (at 1.27 3.56 180) (layer B.SilkS) hide)
    (fp_text value Conn_VDG (at 1.27 -2.79 180) (layer B.Fab) hide)
    (fp_text user %R (at 1.27 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at 2.54 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 1.27 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (offset (xyz 0 0 0.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer B.Cu) (tedit 622022A1)
    (at 101.27 103.4 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference J2 (at 1.27 3.56 180) (layer B.SilkS) hide)
    (fp_text value Conn_VDG (at 1.27 -2.79 180) (layer B.Fab) hide)
    (fp_text user %R (at 1.27 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at 2.54 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 1.27 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (offset (xyz 0 0 0.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer B.Cu) (tedit 622022A1)
    (at 112.07 100 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference J2 (at 1.27 3.56 180) (layer B.SilkS) hide)
    (fp_text value Conn_VDG (at 1.27 -2.79 180) (layer B.Fab) hide)
    (fp_text user %R (at 1.27 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at 2.54 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 1.27 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (offset (xyz 0 0 0.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer B.Cu) (tedit 622022A1)
    (at 108.47 100 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference J2 (at 1.27 3.56 180) (layer B.SilkS) hide)
    (fp_text value Conn_VDG (at 1.27 -2.79 180) (layer B.Fab) hide)
    (fp_text user %R (at 1.27 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at 2.54 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 1.27 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (offset (xyz 0 0 0.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer B.Cu) (tedit 622022A1)
    (at 104.87 100 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference J2 (at 1.27 3.56 180) (layer B.SilkS) hide)
    (fp_text value Conn_VDG (at 1.27 -2.79 180) (layer B.Fab) hide)
    (fp_text user %R (at 1.27 0 180) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at 2.54 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 1.27 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (offset (xyz 0 0 0.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 6220299B)
    (at 110.8 110.2)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value ATtiny4-TS (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad1)"))
    (pad 2 smd roundrect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J2-Pad3)"))
    (pad 3 smd roundrect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(U1-Pad3)"))
    (pad 4 smd roundrect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J2-Pad2)"))
    (pad 6 smd roundrect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (pad 5 smd roundrect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 6220299B)
    (at 107.2 110.2)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value ATtiny4-TS (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad1)"))
    (pad 2 smd roundrect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J2-Pad3)"))
    (pad 3 smd roundrect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(U1-Pad3)"))
    (pad 4 smd roundrect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J2-Pad2)"))
    (pad 6 smd roundrect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (pad 5 smd roundrect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 6220299B)
    (at 103.6 110.2)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value ATtiny4-TS (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad1)"))
    (pad 2 smd roundrect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J2-Pad3)"))
    (pad 3 smd roundrect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(U1-Pad3)"))
    (pad 4 smd roundrect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J2-Pad2)"))
    (pad 6 smd roundrect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (pad 5 smd roundrect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 6220299B)
    (at 100 110.2)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value ATtiny4-TS (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad1)"))
    (pad 2 smd roundrect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J2-Pad3)"))
    (pad 3 smd roundrect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(U1-Pad3)"))
    (pad 4 smd roundrect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J2-Pad2)"))
    (pad 6 smd roundrect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (pad 5 smd roundrect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 6220299B)
    (at 110.8 106.8)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value ATtiny4-TS (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad1)"))
    (pad 2 smd roundrect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J2-Pad3)"))
    (pad 3 smd roundrect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(U1-Pad3)"))
    (pad 4 smd roundrect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J2-Pad2)"))
    (pad 6 smd roundrect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (pad 5 smd roundrect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 6220299B)
    (at 107.2 106.8)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value ATtiny4-TS (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad1)"))
    (pad 2 smd roundrect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J2-Pad3)"))
    (pad 3 smd roundrect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(U1-Pad3)"))
    (pad 4 smd roundrect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J2-Pad2)"))
    (pad 6 smd roundrect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (pad 5 smd roundrect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 6220299B)
    (at 103.6 106.8)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value ATtiny4-TS (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad1)"))
    (pad 2 smd roundrect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J2-Pad3)"))
    (pad 3 smd roundrect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(U1-Pad3)"))
    (pad 4 smd roundrect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J2-Pad2)"))
    (pad 6 smd roundrect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (pad 5 smd roundrect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 6220299B)
    (at 100 106.8)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value ATtiny4-TS (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad1)"))
    (pad 2 smd roundrect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J2-Pad3)"))
    (pad 3 smd roundrect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(U1-Pad3)"))
    (pad 4 smd roundrect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J2-Pad2)"))
    (pad 6 smd roundrect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (pad 5 smd roundrect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 6220299B)
    (at 110.8 103.4)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value ATtiny4-TS (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad1)"))
    (pad 2 smd roundrect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J2-Pad3)"))
    (pad 3 smd roundrect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(U1-Pad3)"))
    (pad 4 smd roundrect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J2-Pad2)"))
    (pad 6 smd roundrect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (pad 5 smd roundrect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 6220299B)
    (at 107.2 103.4)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value ATtiny4-TS (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad1)"))
    (pad 2 smd roundrect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J2-Pad3)"))
    (pad 3 smd roundrect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(U1-Pad3)"))
    (pad 4 smd roundrect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J2-Pad2)"))
    (pad 6 smd roundrect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (pad 5 smd roundrect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 6220299B)
    (at 103.6 103.4)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value ATtiny4-TS (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad1)"))
    (pad 2 smd roundrect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J2-Pad3)"))
    (pad 3 smd roundrect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(U1-Pad3)"))
    (pad 4 smd roundrect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J2-Pad2)"))
    (pad 6 smd roundrect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (pad 5 smd roundrect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 6220299B)
    (at 100 103.4)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value ATtiny4-TS (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad1)"))
    (pad 2 smd roundrect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J2-Pad3)"))
    (pad 3 smd roundrect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(U1-Pad3)"))
    (pad 4 smd roundrect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J2-Pad2)"))
    (pad 6 smd roundrect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (pad 5 smd roundrect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 6220299B)
    (at 110.8 100)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value ATtiny4-TS (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad1)"))
    (pad 2 smd roundrect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J2-Pad3)"))
    (pad 3 smd roundrect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(U1-Pad3)"))
    (pad 4 smd roundrect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J2-Pad2)"))
    (pad 6 smd roundrect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (pad 5 smd roundrect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 6220299B)
    (at 107.2 100)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value ATtiny4-TS (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad1)"))
    (pad 2 smd roundrect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J2-Pad3)"))
    (pad 3 smd roundrect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(U1-Pad3)"))
    (pad 4 smd roundrect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J2-Pad2)"))
    (pad 6 smd roundrect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (pad 5 smd roundrect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 6220299B)
    (at 103.6 100)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value ATtiny4-TS (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad1)"))
    (pad 2 smd roundrect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J2-Pad3)"))
    (pad 3 smd roundrect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(U1-Pad3)"))
    (pad 4 smd roundrect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J2-Pad2)"))
    (pad 6 smd roundrect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (pad 5 smd roundrect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 6220299B)
    (at 100 100)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value ATtiny4-TS (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 5 smd roundrect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (pad 6 smd roundrect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)"))
    (pad 4 smd roundrect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J2-Pad2)"))
    (pad 3 smd roundrect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(U1-Pad3)"))
    (pad 2 smd roundrect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J2-Pad3)"))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer B.Cu) (tedit 622022A1)
    (at 101.27 100 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference J2 (at 1.27 3.56 180) (layer B.SilkS) hide)
    (fp_text value Conn_VDG (at 1.27 -2.79 180) (layer B.Fab) hide)
    (fp_text user %R (at 1.27 0 180) (layer B.Fab) hide)
    (pad 2 smd rect (at 1.27 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (pad 3 smd rect (at 2.54 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad3)"))
    (pad 1 smd rect (at 0 0 180) (size 0.75 3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (offset (xyz 0 0 0.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (gr_line (start 112.6 98.3) (end 98.2 98.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 112.6 111.9) (end 112.6 98.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 112.6 111.9) (end 98.2 111.9) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 101.8 110.9) (end 101.8 109) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 105.4 110.9) (end 105.4 109) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 109 110.9) (end 109 109) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 109 108) (end 109 105.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 105.4 108) (end 105.4 105.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 101.8 108) (end 101.8 105.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 109 104.6) (end 109 102.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 105.4 104.6) (end 105.4 102.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 101.8 104.6) (end 101.8 102.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102.3 108.5) (end 104.9 108.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102.3 105.1) (end 104.9 105.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 111.6 108.5) (end 109.5 108.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 111.6 105.1) (end 109.5 105.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 105.9 108.5) (end 108.5 108.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 105.9 105.1) (end 108.5 105.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 99.2 108.5) (end 101.3 108.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 99.2 105.1) (end 101.3 105.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 111.6 101.7) (end 109.5 101.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 99.2 101.7) (end 101.3 101.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 105.9 101.7) (end 108.5 101.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 112.6 101.7) (end 112.6 98.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 109 99.3) (end 109 101.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 105.4 99.3) (end 105.4 101.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102.3 101.7) (end 104.9 101.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 98.2 111.9) (end 98.2 98.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 101.8 99.3) (end 101.8 101.2) (layer Edge.Cuts) (width 0.05))
)
