(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-2~bpo8+1-stable)
  (general
    (links 10)
    (no_connects 1)
    (area 44.399999 24.714999 59.740001 52.120001)
    (thickness 1.6)
    (drawings 15)
    (tracks 11)
    (zones 0)
    (modules 4)
    (nets 6)
  )
  (page A3)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.3048)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFBF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /LED)
  (net 2 /PWM)
  (net 3 GND)
  (net 4 VCC)
  (net 5 "Net-(R1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.3048)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /PWM)
    (add_net GND)
    (add_net "Net-(R1-Pad1)")
    (add_net VCC)
  )
  (net_class HIGHPWR ""
    (clearance 0.254)
    (trace_width 0.8128)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /LED)
  )
  (module TO263-5 (layer F.Cu) (tedit 583097D1)
    (at 52.07 41.91)
    (attr smd)
    (fp_text reference U1 (at 0 -3.81) (layer F.SilkS))
    (fp_text value CAT4101 (at 0 -7.62) (layer F.SilkS))
    (pad 2 smd rect (at -1.69926 0) (size 1.143 2.286) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 3 smd rect (at 0 -10.795) (size 10.80008 9.99998) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at 1.69926 0) (size 1.143 2.286) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(R1-Pad1)"))
    (pad 3 smd rect (at 0 0) (size 1.143 2.286) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -3.40106 0) (size 1.143 2.286) (layers F.Cu F.Paste F.Mask)
      (net 2 /PWM))
    (pad 5 smd rect (at 3.40106 0) (size 1.143 2.286) (layers F.Cu F.Paste F.Mask)
      (net 1 /LED))
  )
  (module SM0603 (layer F.Cu) (tedit 581E743B)
    (at 53.975 45.085 270)
    (attr smd)
    (fp_text reference R1 (at 0 0 270) (layer F.SilkS))
    (fp_text value 549R (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 581F2B86)
    (at 50.8 44.45 180)
    (attr smd)
    (fp_text reference C1 (at 0 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SIL-5 (layer F.Cu) (tedit 583095F3)
    (at 53.34 49.53)
    (descr "Connecteur 5 pins")
    (tags "CONN DEV")
    (fp_text reference P1 (at -6.35 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN_5 (at 0 -2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 /PWM))
    (pad 2 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 3 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 VCC))
    (pad 4 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 5 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 /LED))
  )
  (gr_text "1A LED Driver" (at 52.07 25.4) (layer F.SilkS))
  (gr_text - (at 54.61 46.99) (layer F.SilkS))
  (gr_text - (at 49.53 46.99) (layer F.SilkS))
  (gr_text + (at 52.07 46.99) (layer F.SilkS))
  (gr_text LED (at 57.15 46.99 270) (layer F.SilkS))
  (gr_text PWM (at 46.99 46.99 270) (layer F.SilkS))
  (gr_line (start 44.45 24.765) (end 44.45 52.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 45.085 24.765) (end 44.45 24.765) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 59.69 24.765) (end 45.085 24.765) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 59.69 52.07) (end 59.69 24.765) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 44.45 52.07) (end 59.69 52.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 47.625 29.845) (end 47.625 35.56) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 56.515 29.845) (end 56.515 35.56) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 56.515 35.56) (end 47.625 35.56) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 47.625 29.845) (end 56.515 29.845) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59.69 52.07) (xy 44.45 52.07) (xy 44.45 24.765) (xy 59.69 24.765) (xy 59.69 52.07)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59.69 52.07) (xy 44.45 52.07) (xy 44.45 24.765) (xy 59.69 24.765)
      )
    )
  )
)
