(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen") (color "White"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Purple") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Purple") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen") (color "White"))
      (copper_finish "ENIG")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (net 0 "")
  (net 1 "+3V3")
  (net 2 "GND")
  (net 3 "/VCC_B")
  (net 4 "/GPIO_5V0_01")
  (net 5 "/GPIO_5V0_02")
  (net 6 "/GPIO_5V0_03")
  (net 7 "Net-(D5-Pad1)")
  (net 8 "/GPIO_5V0_04")
  (net 9 "/GPIO_5V0_05")
  (net 10 "/GPIO_5V0_06")
  (net 11 "Net-(D9-Pad1)")
  (net 12 "/GPIO_5V0_07")
  (net 13 "/GPIO_5V0_08")
  (net 14 "/GPIO_5V0_09")
  (net 15 "/GPIO_5V0_10")
  (net 16 "Net-(D14-Pad1)")
  (net 17 "/GPIO_5V0_11")
  (net 18 "/GPIO_5V0_12")
  (net 19 "/GPIO_3V3_01")
  (net 20 "/GPIO_3V3_02")
  (net 21 "/GPIO_3V3_03")
  (net 22 "/GPIO_3V3_04")
  (net 23 "/GPIO_3V3_05")
  (net 24 "/GPIO_3V3_06")
  (net 25 "/GPIO_3V3_07")
  (net 26 "/GPIO_3V3_08")
  (net 27 "/GPIO_3V3_09")
  (net 28 "/GPIO_3V3_10")
  (net 29 "/GPIO_3V3_11")
  (net 30 "/GPIO_3V3_OE")
  (net 31 "/OE")
  (net 32 "/GPIO_3V3_12")
  (net 33 "Net-(U1-Pad7)")
  (net 34 "Net-(U1-Pad8)")
  (net 35 "Net-(U1-Pad9)")
  (net 36 "Net-(U1-Pad10)")
  (net 37 "Net-(U2-Pad7)")
  (net 38 "Net-(U2-Pad8)")
  (net 39 "Net-(U2-Pad9)")
  (net 40 "Net-(U2-Pad10)")
  (net 41 "Net-(U3-Pad7)")
  (net 42 "Net-(U3-Pad8)")
  (net 43 "Net-(U3-Pad9)")
  (net 44 "Net-(U3-Pad10)")
  (net 45 "/VCC_B_IN")
  (net 46 "Net-(Q2-Pad1)")
  (net 47 "Net-(Q2-Pad2)")
  (net 48 "Net-(R18-Pad2)")
  (net 49 "Net-(R19-Pad2)")
  (net 50 "Net-(R21-Pad2)")
  (net 51 "unconnected-(U7-Pad6)")
  (net 52 "Net-(Q1-Pad2)")
  (net 53 "Net-(Q1-Pad3)")
  (net 54 "Net-(Q1-Pad5)")
  (net 55 "Net-(Q1-Pad6)")
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 120.65 78.232)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at -0.508 1.016) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(D5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(Q1-Pad6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SON:USON-10_2.5x1.0mm_P0.5mm" (layer "F.Cu")
    (tedit 5A02F1D8)
    (at 121.666 100.838)
    (descr "USON-10 2.5x1.0mm_ Pitch 0.5mm http://www.ti.com/lit/ds/symlink/tpd4e02b04.pdf")
    (tags "USON-10 2.5x1.0mm Pitch 0.5mm")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U5" (at 0.01829 -2.5) (layer "F.SilkS"))
    (fp_text value "ESD224" (at 0.01829 2.5) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.385 -1 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "Net-(U2-Pad10)") (pinfunction "IO1_C") (pintype "passive"))
    (pad "2" smd rect (at -0.385 -0.5 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "Net-(U2-Pad9)") (pinfunction "IO2_C") (pintype "passive"))
    (pad "3" smd rect (at -0.385 0 270) (size 0.4 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "G") (pintype "passive"))
    (pad "4" smd rect (at -0.385 0.5 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(U2-Pad8)") (pinfunction "IO3_C") (pintype "passive"))
    (pad "5" smd rect (at -0.385 1 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(U2-Pad7)") (pinfunction "IO4_C") (pintype "passive"))
    (pad "6" smd rect (at 0.385 1 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/GPIO_5V0_08") (pinfunction "IO4_S") (pintype "passive"))
    (pad "7" smd rect (at 0.385 0.5 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/GPIO_5V0_07") (pinfunction "IO3_S") (pintype "passive"))
    (pad "8" smd rect (at 0.385 0 270) (size 0.4 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "G") (pintype "passive"))
    (pad "9" smd rect (at 0.385 -0.5 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/GPIO_5V0_06") (pinfunction "IO2_S") (pintype "passive"))
    (pad "10" smd rect (at 0.385 -1 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/GPIO_5V0_05") (pinfunction "IO1_S") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SON.3dshapes/USON-10_2.5x1.0mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock_TE-Connectivity:TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 5B1EC513)
    (at 133.1468 109.7788)
    (descr "Terminal Block TE 282834-2, 2 pins, pitch 2.54mm, size 5.54x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-2 pitch 2.54mm size 5.54x6.5mm^2 drill 1.1mm pad 2.1mm")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 5.588 -3.1242) (layer "F.SilkS"))
    (fp_text value "VCC_B" (at 5.5118 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 1.27 2) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 45 "/VCC_B_IN") (pinfunction "Pin_1") (pintype "power_out"))
    (pad "2" thru_hole circle (at 2.54 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock_TE-Connectivity.3dshapes/TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 118.364 98.298 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at -0.107836 1.27 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/VCC_B") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 123.2154 106.4514 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R18" (at -2.0828 0 270) (layer "F.SilkS"))
    (fp_text value "1.5M" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "/VCC_B_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(R18-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 122.1486 104.0384)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "VCC_B" (at 1.1938 -3.1242 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 3 "/VCC_B") (pinfunction "1") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" (layer "F.Cu")
    (tedit 56DDBCCA)
    (at 134.6708 77.8764)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "delta_lib:SIA906EDJ-T1-GE3" (layer "F.Cu")
    (tedit 0)
    (at 128.2192 108.217843 180)
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (clearance 0.1524)
    (attr through_hole)
    (fp_text reference "Q2" (at 0 2.122043) (layer "F.SilkS"))
    (fp_text value "SIA906EDJ" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "*" (at -0.035 2.25) (layer "F.SilkS") hide)
    (fp_text user "0.023in/0.584mm" (at -1.0922 2.8575) (layer "Cmts.User"))
    (fp_text user "0.086in/2.184mm" (at 0 -3.4925) (layer "Cmts.User"))
    (fp_text user "0.013in/0.33mm" (at 4.1402 -0.649986) (layer "Cmts.User"))
    (fp_text user "0.026in/0.65mm" (at -4.1402 -0.324993) (layer "Cmts.User"))
    (fp_text user "0.028in/0.711mm" (at 3.4925 0) (layer "Cmts.User"))
    (fp_text user "0.041in/1.041mm" (at 0 4.1275) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.0922 -0.649986 180) (size 0.5842 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "Net-(Q2-Pad1)") (pinfunction "S") (pintype "passive"))
    (pad "2" smd rect (at -1.0922 0 180) (size 0.5842 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "Net-(Q2-Pad2)") (pinfunction "G") (pintype "input"))
    (pad "3" smd rect (at -1.0922 0.649986 180) (size 0.5842 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/VCC_B") (pinfunction "D") (pintype "passive"))
    (pad "4" smd rect (at 1.0922 0.649986 180) (size 0.5842 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "Net-(Q2-Pad1)") (pinfunction "S") (pintype "passive"))
    (pad "5" smd rect (at 1.0922 0 180) (size 0.5842 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "Net-(Q2-Pad2)") (pinfunction "G") (pintype "input"))
    (pad "6" smd rect (at 1.0922 -0.649986 180) (size 0.5842 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/VCC_B_IN") (pinfunction "D") (pintype "passive"))
    (pad "7" smd rect (at 0 -0.516 180) (size 1.0414 0.7112) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/VCC_B_IN") (pinfunction "D") (pintype "passive"))
    (pad "8" smd rect (at 0 0.516 180) (size 1.0414 0.7112) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/VCC_B") (pinfunction "D") (pintype "passive") (clearance 0.1524))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 118.364 84.3 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 0 1.27 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/VCC_B") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 120.65 75.9715 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D5" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "VCC_A" (at -0.7365 1.778 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(D5-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/VCC_B") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 119.507 104.267 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R22" (at 1.397 0 180) (layer "F.SilkS"))
    (fp_text value "12K" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/OE") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "delta_lib:X1SON" (layer "F.Cu")
    (tedit 0)
    (at 130.6068 108.3818 -90)
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at -1.0668 -0.0254 unlocked) (layer "F.SilkS"))
    (fp_text value "TPD1E1B04" (at -0.005 1.1875 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.35 0 270) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1666666667)
      (net 2 "GND") (pinfunction "A1") (pintype "passive") (solder_mask_margin 0.07))
    (pad "2" smd roundrect (at 0.35 0 270) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1666666667)
      (net 45 "/VCC_B_IN") (pinfunction "A2") (pintype "passive") (solder_mask_margin 0.07))
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124.204 78.232)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at 0.002 1.016) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(D9-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 116.078 80.01)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP2" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "3V3_SDR" (at 2.54 -0.254 270) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 1 "+3V3") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (tedit 5B391E66)
    (at 117.348 111.079047)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP2" (at 0 -1.8) (layer "F.SilkS") hide)
    (fp_text value "GPIO_12" (at 0 -2.032) (layer "F.SilkS"))
    (pad "1" smd custom (at -0.65 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 30 "/GPIO_3V3_OE") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 32 "/GPIO_3V3_12") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "Package_SON:USON-10_2.5x1.0mm_P0.5mm" (layer "F.Cu")
    (tedit 5A02F1D8)
    (at 121.666 86.868)
    (descr "USON-10 2.5x1.0mm_ Pitch 0.5mm http://www.ti.com/lit/ds/symlink/tpd4e02b04.pdf")
    (tags "USON-10 2.5x1.0mm Pitch 0.5mm")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U6" (at 0.01829 -2.5) (layer "F.SilkS"))
    (fp_text value "ESD224" (at 0.01829 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.385 -1 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(U3-Pad10)") (pinfunction "IO1_C") (pintype "passive"))
    (pad "2" smd rect (at -0.385 -0.5 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "Net-(U3-Pad9)") (pinfunction "IO2_C") (pintype "passive"))
    (pad "3" smd rect (at -0.385 0 270) (size 0.4 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "G") (pintype "passive"))
    (pad "4" smd rect (at -0.385 0.5 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "Net-(U3-Pad8)") (pinfunction "IO3_C") (pintype "passive"))
    (pad "5" smd rect (at -0.385 1 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(U3-Pad7)") (pinfunction "IO4_C") (pintype "passive"))
    (pad "6" smd rect (at 0.385 1 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/GPIO_5V0_12") (pinfunction "IO4_S") (pintype "passive"))
    (pad "7" smd rect (at 0.385 0.5 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/GPIO_5V0_11") (pinfunction "IO3_S") (pintype "passive"))
    (pad "8" smd rect (at 0.385 0 270) (size 0.4 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "G") (pintype "passive"))
    (pad "9" smd rect (at 0.385 -0.5 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/GPIO_5V0_10") (pinfunction "IO2_S") (pintype "passive"))
    (pad "10" smd rect (at 0.385 -1 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/GPIO_5V0_09") (pinfunction "IO1_S") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SON.3dshapes/USON-10_2.5x1.0mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 128.016 78.232)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at 0 1.016) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(D14-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(Q1-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "delta_lib:SIA906EDJ-T1-GE3" (layer "F.Cu")
    (tedit 0)
    (at 122.1232 80.8736 90)
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (clearance 0.1524)
    (attr through_hole)
    (fp_text reference "Q1" (at -0.0254 2.1844 90) (layer "F.SilkS"))
    (fp_text value "SIA906EDJ" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text user "*" (at -0.035 2.25 90) (layer "F.SilkS") hide)
    (fp_text user "0.028in/0.711mm" (at 3.4925 0 90) (layer "Cmts.User"))
    (fp_text user "0.041in/1.041mm" (at 0 4.1275 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.013in/0.33mm" (at 4.1402 -0.649986 90) (layer "Cmts.User"))
    (fp_text user "0.086in/2.184mm" (at 0 -3.4925 90) (layer "Cmts.User"))
    (fp_text user "0.026in/0.65mm" (at -4.1402 -0.324993 90) (layer "Cmts.User"))
    (fp_text user "0.023in/0.584mm" (at -1.0922 2.8575 90) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.0922 -0.649986 90) (size 0.5842 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "S") (pintype "passive"))
    (pad "2" smd rect (at -1.0922 0 90) (size 0.5842 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "Net-(Q1-Pad2)") (pinfunction "G") (pintype "input"))
    (pad "3" smd rect (at -1.0922 0.649986 90) (size 0.5842 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "Net-(Q1-Pad3)") (pinfunction "D") (pintype "passive"))
    (pad "4" smd rect (at 1.0922 0.649986 90) (size 0.5842 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "S") (pintype "passive"))
    (pad "5" smd rect (at 1.0922 0 90) (size 0.5842 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "Net-(Q1-Pad5)") (pinfunction "G") (pintype "input"))
    (pad "6" smd rect (at 1.0922 -0.649986 90) (size 0.5842 0.3302) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "Net-(Q1-Pad6)") (pinfunction "D") (pintype "passive"))
    (pad "7" smd rect (at 0 -0.516 90) (size 1.0414 0.7112) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "Net-(Q1-Pad6)") (pinfunction "D") (pintype "passive"))
    (pad "8" smd rect (at 0 0.516 90) (size 1.0414 0.7112) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "Net-(Q1-Pad3)") (pinfunction "D") (pintype "passive"))
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (tedit 5C745321)
    (at 117.348 106.68)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
    (tags "net tie solder jumper bridged")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP1" (at 0 -1.8) (layer "F.SilkS") hide)
    (fp_text value "OE" (at 0 -2.032) (layer "F.SilkS"))
    (pad "1" smd custom (at -1.3 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 30 "/GPIO_3V3_OE") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0.55 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.55 -0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd rect (at 0 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 31 "/OE") (pinfunction "C") (pintype "passive"))
    (pad "3" smd custom (at 1.3 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 1 "+3V3") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0 0.75)
            (xy -0.55 0.75)
            (xy -0.55 -0.75)
            (xy 0 -0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 117.094 91.186 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.16 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 128.016 75.946 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D14" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "OE" (at 0.508 1.778 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(D14-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/VCC_B") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 120.7262 110.8202 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R20" (at 0 1.2192 90) (layer "F.SilkS"))
    (fp_text value "288K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(R19-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 120.9802 108.2802 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R19" (at -1.3208 -0.0508 180) (layer "F.SilkS"))
    (fp_text value "12K" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(R18-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(R19-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "delta_lib:Texas_R_PUQFN-N12" (layer "F.Cu")
    (tedit 5A0AA2C1)
    (at 117.856 100.838)
    (descr "Texas_R_PUQFN-N12 http://www.ti.com/lit/ds/symlink/txb0104.pdf")
    (tags "Texas_R_PUQFN-N12")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at -0.0508 2.159) (layer "F.SilkS"))
    (fp_text value "TXB0104RUT" (at 0.25 2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.65 -0.8 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3V3") (pinfunction "VCCA") (pintype "power_in") (solder_mask_margin 0.05))
    (pad "1" smd rect (at -0.425 -0.975) (size 0.15 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3V3") (pinfunction "VCCA") (pintype "power_in") (solder_mask_margin 0.05))
    (pad "2" smd rect (at -0.65 -0.4 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/GPIO_3V3_05") (pinfunction "A1") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "3" smd rect (at -0.65 0 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "/GPIO_3V3_06") (pinfunction "A2") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "4" smd rect (at -0.65 0.4 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "/GPIO_3V3_07") (pinfunction "A3") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "5" smd rect (at -0.65 0.8 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/GPIO_3V3_08") (pinfunction "A4") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "6" smd rect (at 0 0.8 270) (size 0.6 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.05))
    (pad "7" smd rect (at 0.65 0.8 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(U2-Pad7)") (pinfunction "B4") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "8" smd rect (at 0.65 0.4 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(U2-Pad8)") (pinfunction "B3") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "9" smd rect (at 0.65 0 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "Net-(U2-Pad9)") (pinfunction "B2") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "10" smd rect (at 0.65 -0.4 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "Net-(U2-Pad10)") (pinfunction "B1") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "11" smd rect (at 0.65 -0.8 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/VCC_B") (pinfunction "VCCB") (pintype "power_in") (solder_mask_margin 0.05))
    (pad "12" smd rect (at 0 -0.8 270) (size 0.6 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/OE") (pinfunction "OE") (pintype "input") (solder_mask_margin 0.05))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_R_PUQFN-N12.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 117.094 84.328 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.16 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 124.206 75.946 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D9" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "VCC_B" (at -0.762 1.778 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(D9-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/VCC_B") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "delta_lib:DSUB-15_Male_L717SDA15PA4CH4F" (layer "F.Cu")
    (tedit 59FEDEE2)
    (at 101.559743 93.728597 -90)
    (descr "15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 9.9mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 11.32mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "15-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 9.9mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -18.620797 -14.111857) (layer "F.SilkS"))
    (fp_text value "SDR_CONN" (at -1.272597 1.991743 90) (layer "F.Fab"))
    (pad "0" thru_hole circle (at -16.65 -9.5 270) (size 4 4) (drill 3.05) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "PAD") (pintype "passive"))
    (pad "0" thru_hole circle (at 16.65 -9.5 270) (size 4 4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "PAD") (pintype "passive"))
    (pad "1" thru_hole rect (at -9.695 -10.92 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+3V3") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -6.925 -10.92 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/GPIO_3V3_01") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -4.155 -10.92 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/GPIO_3V3_02") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -1.385 -10.92 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/GPIO_3V3_03") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at 1.385 -10.92 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/GPIO_3V3_04") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at 4.155 -10.92 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 23 "/GPIO_3V3_05") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at 6.925 -10.92 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 24 "/GPIO_3V3_06") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at 9.695 -10.92 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 25 "/GPIO_3V3_07") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at -8.31 -8.31 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 26 "/GPIO_3V3_08") (pinfunction "P9") (pintype "passive"))
    (pad "10" thru_hole circle (at -5.54 -8.31 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 27 "/GPIO_3V3_09") (pinfunction "P10") (pintype "passive"))
    (pad "11" thru_hole circle (at -2.77 -8.31 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 28 "/GPIO_3V3_10") (pinfunction "P111") (pintype "passive"))
    (pad "12" thru_hole circle (at 0 -8.31 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 29 "/GPIO_3V3_11") (pinfunction "P12") (pintype "passive"))
    (pad "13" thru_hole circle (at 2.77 -8.31 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 30 "/GPIO_3V3_OE") (pinfunction "P13") (pintype "passive"))
    (pad "14" thru_hole circle (at 5.54 -8.31 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "P14") (pintype "passive"))
    (pad "15" thru_hole circle (at 8.31 -8.31 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "P15") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-15_Male_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm.wrl"
      (offset (xyz -9.56 11 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 120.3198 79.8322 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at -2.0066 -0.0254 90) (layer "F.SilkS"))
    (fp_text value "33" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/OE") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(Q1-Pad5)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical" (layer "F.Cu")
    (tedit 5B78AD87)
    (at 126.492 85.852 -90)
    (descr "JST SH series connector, BM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH side entry")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J5" (at 0 -3.3 90) (layer "F.SilkS") hide)
    (fp_text value "12-09" (at 0 -3.81 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -0.25 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5 1.325 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/GPIO_5V0_09") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at -0.5 1.325 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/GPIO_5V0_10") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at 0.5 1.325 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/GPIO_5V0_11") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at 1.5 1.325 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/GPIO_5V0_12") (pinfunction "Pin_4") (pintype "passive"))
    (pad "MP" smd roundrect (at -2.8 -1.2 270) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pinfunction "MP") (pintype "passive"))
    (pad "MP" smd roundrect (at 2.8 -1.2 270) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pinfunction "MP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 118.364 91.186 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0 1.27 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/VCC_B") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 122.174 83.1342)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 1.6002 0 90) (layer "F.SilkS"))
    (fp_text value "33" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(Q1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.5mm_EP1.65x2.38mm" (layer "F.Cu")
    (tedit 5E99EE6D)
    (at 123.825 109.2454)
    (descr "DFN, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/4320fb.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "DFN NoLead")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U7" (at 0 2.6162) (layer "F.SilkS"))
    (fp_text value "LTC4367CDD" (at 0 2.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd roundrect (at 0 0) (size 1.33 1.92) (layers "F.Paste") (roundrect_rratio 0.1879699248))
    (pad "1" smd roundrect (at -1.45 -0.75) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "/VCC_B_IN") (pinfunction "Vin") (pintype "power_in"))
    (pad "2" smd roundrect (at -1.45 -0.25) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(R18-Pad2)") (pinfunction "UV") (pintype "input"))
    (pad "3" smd roundrect (at -1.45 0.25) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(R19-Pad2)") (pinfunction "OV") (pintype "input"))
    (pad "4" smd roundrect (at -1.45 0.75) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd roundrect (at 1.45 0.75) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(R21-Pad2)") (pinfunction "~{SHDN}") (pintype "input"))
    (pad "6" smd roundrect (at 1.45 0.25) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "unconnected-(U7-Pad6)") (pinfunction "~{FAULT}") (pintype "open_collector+no_connect"))
    (pad "7" smd roundrect (at 1.45 -0.25) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/VCC_B") (pinfunction "Vout") (pintype "input"))
    (pad "8" smd roundrect (at 1.45 -0.75) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(Q2-Pad2)") (pinfunction "GATE") (pintype "output"))
    (pad "9" smd rect (at 0 0) (size 1.65 2.38) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-8-1EP_3x3mm_P0.5mm_EP1.65x2.38mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "delta_lib:Texas_R_PUQFN-N12" (layer "F.Cu")
    (tedit 5A0AA2C1)
    (at 117.856 93.726)
    (descr "Texas_R_PUQFN-N12 http://www.ti.com/lit/ds/symlink/txb0104.pdf")
    (tags "Texas_R_PUQFN-N12")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0.0254 2.1336) (layer "F.SilkS"))
    (fp_text value "TXB0104RUT" (at 0.25 2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.425 -0.975) (size 0.15 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3V3") (pinfunction "VCCA") (pintype "power_in") (solder_mask_margin 0.05))
    (pad "1" smd rect (at -0.65 -0.8 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3V3") (pinfunction "VCCA") (pintype "power_in") (solder_mask_margin 0.05))
    (pad "2" smd rect (at -0.65 -0.4 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/GPIO_3V3_01") (pinfunction "A1") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "3" smd rect (at -0.65 0 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/GPIO_3V3_02") (pinfunction "A2") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "4" smd rect (at -0.65 0.4 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/GPIO_3V3_03") (pinfunction "A3") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "5" smd rect (at -0.65 0.8 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/GPIO_3V3_04") (pinfunction "A4") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "6" smd rect (at 0 0.8 270) (size 0.6 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.05))
    (pad "7" smd rect (at 0.65 0.8 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "Net-(U1-Pad7)") (pinfunction "B4") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "8" smd rect (at 0.65 0.4 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(U1-Pad8)") (pinfunction "B3") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "9" smd rect (at 0.65 0 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "Net-(U1-Pad9)") (pinfunction "B2") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "10" smd rect (at 0.65 -0.4 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "Net-(U1-Pad10)") (pinfunction "B1") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "11" smd rect (at 0.65 -0.8 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/VCC_B") (pinfunction "VCCB") (pintype "power_in") (solder_mask_margin 0.05))
    (pad "12" smd rect (at 0 -0.8 270) (size 0.6 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/OE") (pinfunction "OE") (pintype "input") (solder_mask_margin 0.05))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_R_PUQFN-N12.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "delta_lib:Texas_R_PUQFN-N12" (layer "F.Cu")
    (tedit 5A0AA2C1)
    (at 117.841 86.868)
    (descr "Texas_R_PUQFN-N12 http://www.ti.com/lit/ds/symlink/txb0104.pdf")
    (tags "Texas_R_PUQFN-N12")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at -0.0358 2.1336) (layer "F.SilkS"))
    (fp_text value "TXB0104RUT" (at 0.25 2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.425 -0.975) (size 0.15 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3V3") (pinfunction "VCCA") (pintype "power_in") (solder_mask_margin 0.05))
    (pad "1" smd rect (at -0.65 -0.8 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3V3") (pinfunction "VCCA") (pintype "power_in") (solder_mask_margin 0.05))
    (pad "2" smd rect (at -0.65 -0.4 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/GPIO_3V3_09") (pinfunction "A1") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "3" smd rect (at -0.65 0 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/GPIO_3V3_10") (pinfunction "A2") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "4" smd rect (at -0.65 0.4 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/GPIO_3V3_11") (pinfunction "A3") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "5" smd rect (at -0.65 0.8 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/GPIO_3V3_12") (pinfunction "A4") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "6" smd rect (at 0 0.8 270) (size 0.6 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.05))
    (pad "7" smd rect (at 0.65 0.8 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(U3-Pad7)") (pinfunction "B4") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "8" smd rect (at 0.65 0.4 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "Net-(U3-Pad8)") (pinfunction "B3") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "9" smd rect (at 0.65 0 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "Net-(U3-Pad9)") (pinfunction "B2") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "10" smd rect (at 0.65 -0.4 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(U3-Pad10)") (pinfunction "B1") (pintype "tri_state") (solder_mask_margin 0.05))
    (pad "11" smd rect (at 0.65 -0.8 270) (size 0.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/VCC_B") (pinfunction "VCCB") (pintype "power_in") (solder_mask_margin 0.05))
    (pad "12" smd rect (at 0 -0.8 270) (size 0.6 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/OE") (pinfunction "OE") (pintype "input") (solder_mask_margin 0.05))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_R_PUQFN-N12.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 117.094 98.298 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.16 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical" (layer "F.Cu")
    (tedit 5B78AD87)
    (at 126.492 101.6 -90)
    (descr "JST SH series connector, BM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH side entry")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J4" (at 0 -3.3 90) (layer "F.SilkS") hide)
    (fp_text value "08-05" (at 0 -3.81 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -0.25 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5 1.325 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/GPIO_5V0_05") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at -0.5 1.325 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/GPIO_5V0_06") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at 0.5 1.325 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/GPIO_5V0_07") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at 1.5 1.325 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/GPIO_5V0_08") (pinfunction "Pin_4") (pintype "passive"))
    (pad "MP" smd roundrect (at 2.8 -1.2 270) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pinfunction "MP") (pintype "passive"))
    (pad "MP" smd roundrect (at -2.8 -1.2 270) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pinfunction "MP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SON:USON-10_2.5x1.0mm_P0.5mm" (layer "F.Cu")
    (tedit 5A02F1D8)
    (at 121.666 93.726)
    (descr "USON-10 2.5x1.0mm_ Pitch 0.5mm http://www.ti.com/lit/ds/symlink/tpd4e02b04.pdf")
    (tags "USON-10 2.5x1.0mm Pitch 0.5mm")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U4" (at 0.01829 -2.5) (layer "F.SilkS"))
    (fp_text value "ESD224" (at 0.01829 2.5) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.385 -1 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "Net-(U1-Pad10)") (pinfunction "IO1_C") (pintype "passive"))
    (pad "2" smd rect (at -0.385 -0.5 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "Net-(U1-Pad9)") (pinfunction "IO2_C") (pintype "passive"))
    (pad "3" smd rect (at -0.385 0 270) (size 0.4 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "G") (pintype "passive"))
    (pad "4" smd rect (at -0.385 0.5 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(U1-Pad8)") (pinfunction "IO3_C") (pintype "passive"))
    (pad "5" smd rect (at -0.385 1 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "Net-(U1-Pad7)") (pinfunction "IO4_C") (pintype "passive"))
    (pad "6" smd rect (at 0.385 1 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/GPIO_5V0_04") (pinfunction "IO4_S") (pintype "passive"))
    (pad "7" smd rect (at 0.385 0.5 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/GPIO_5V0_03") (pinfunction "IO3_S") (pintype "passive"))
    (pad "8" smd rect (at 0.385 0 270) (size 0.4 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "G") (pintype "passive"))
    (pad "9" smd rect (at 0.385 -0.5 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/GPIO_5V0_02") (pinfunction "IO2_S") (pintype "passive"))
    (pad "10" smd rect (at 0.385 -1 270) (size 0.3 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/GPIO_5V0_01") (pinfunction "IO1_S") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SON.3dshapes/USON-10_2.5x1.0mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical" (layer "F.Cu")
    (tedit 5B78AD87)
    (at 126.492 93.726 -90)
    (descr "JST SH series connector, BM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH side entry")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J3" (at 0 -3.3 90) (layer "F.SilkS") hide)
    (fp_text value "04-01" (at 0 -3.81 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -0.25 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5 1.325 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/GPIO_5V0_01") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at -0.5 1.325 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/GPIO_5V0_02") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at 0.5 1.325 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/GPIO_5V0_03") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at 1.5 1.325 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/GPIO_5V0_04") (pinfunction "Pin_4") (pintype "passive"))
    (pad "MP" smd roundrect (at 2.8 -1.2 270) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pinfunction "MP") (pintype "passive"))
    (pad "MP" smd roundrect (at -2.8 -1.2 270) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pinfunction "MP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 128.1938 110.617 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sdr_switch_interface.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R21" (at -2.4892 0.3048 90) (layer "F.SilkS"))
    (fp_text value "510K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "/VCC_B_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(R21-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "aps_radar_lib:delta_logo" (layer "B.Cu")
    (tedit 0)
    (at 121.285 93.6752 -90)
    (attr through_hole)
    (fp_text reference "G***" (at 0 0 90) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0 90) (layer "B.SilkS") hide)
  )
  (gr_line (start 101.346 74.93) (end 101.346 112.522) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 139.7 112.522) (mid 139.40242 113.24042) (end 138.684 113.538) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 138.67678 73.92122) (mid 139.3952 74.2188) (end 139.69278 74.93722) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 139.69278 74.93722) (end 139.7 112.522) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 101.346 74.93) (mid 101.64358 74.21158) (end 102.362 73.914) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 138.684 113.538) (end 102.362 113.538) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 138.67678 73.92122) (end 102.362 73.914) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 102.362 113.538) (mid 101.64358 113.24042) (end 101.346 112.522) (layer "Edge.Cuts") (width 0.1))
  (gr_text "X310 GPIO Interface  |  " (at 130.5052 89.3826 90) (layer "B.SilkS"))
  (gr_text "Rev. 1.1" (at 130.5052 105.918 90) (layer "B.SilkS"))
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.634 84.328)
        (xy 115.8748 84.328)
        (xy 115.8748 83.4136)
        (xy 116.6368 82.6008)
        (xy 118.8212 82.6008)
        (xy 119.634 83.4136)
      )
    )
  )
  (zone (net 3) (net_name "/VCC_B") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.7 73.914)
        (xy 139.7 113.538)
        (xy 101.2952 113.538)
        (xy 101.2952 73.8632)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.6378 110.3884)
        (xy 124.9172 110.6932)
        (xy 124.9172 111.633)
        (xy 121.9708 111.633)
        (xy 121.285 112.0394)
        (xy 120.269 112.0394)
        (xy 120.269 111.0488)
        (xy 120.6754 111.0488)
        (xy 121.9962 109.7534)
        (xy 123.0122 109.7534)
        (xy 123.0122 108.0516)
        (xy 123.5964 106.9594)
        (xy 124.6378 106.9594)
      )
    )
  )
  (zone (net 1) (net_name "+3V3") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.5004 93.0148)
        (xy 116.8908 93.0148)
        (xy 116.7892 92.8116)
        (xy 116.7892 91.3892)
        (xy 117.5004 91.3892)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.634 91.186)
        (xy 115.8748 91.186)
        (xy 115.8748 90.2716)
        (xy 116.6368 89.4588)
        (xy 118.8212 89.4588)
        (xy 119.634 90.2716)
      )
    )
  )
  (zone (net 1) (net_name "+3V3") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.3988 86.1568)
        (xy 116.7892 86.1568)
        (xy 116.6876 85.9536)
        (xy 116.6876 84.5312)
        (xy 117.3988 84.5312)
      )
    )
  )
  (zone (net 1) (net_name "+3V3") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.4496 100.1268)
        (xy 116.84 100.1268)
        (xy 116.7384 99.9236)
        (xy 116.7384 98.5012)
        (xy 117.4496 98.5012)
      )
    )
  )
  (zone (net 45) (net_name "/VCC_B_IN") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.7902 110.1344)
        (xy 126.7206 110.1344)
        (xy 126.7206 109.4486)
        (xy 126.7206 108.3056)
        (xy 128.905 108.3056)
        (xy 129.921 108.5342)
        (xy 134.4168 108.5342)
        (xy 134.4168 113.5126)
        (xy 119.504215 113.514258)
        (xy 119.529615 105.386258)
        (xy 124.7902 105.3846)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.634 98.298)
        (xy 115.8748 98.298)
        (xy 115.8748 97.3836)
        (xy 116.6368 96.5708)
        (xy 118.8212 96.5708)
        (xy 119.634 97.3836)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.7 73.914)
        (xy 139.7 113.538)
        (xy 101.2952 113.538)
        (xy 101.2952 73.8632)
      )
    )
  )
)
