(kicad_pcb (version 20171130) (host pcbnew 5.1.7-1.fc32)
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 129)
    (zones 0)
    (modules 10)
    (nets 18)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.381)
    (via_min_size 0.6858)
    (via_min_drill 0.381)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed yes)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 132.08 68.58)
    (grid_origin 105.41 34.29)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/tmp/Test"))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad9)")
  (net 2 "Net-(J1-Pad8)")
  (net 3 "Net-(J1-Pad7)")
  (net 4 "Net-(J1-Pad6)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad4)")
  (net 7 "Net-(J1-Pad3)")
  (net 8 "Net-(J1-Pad1)")
  (net 9 "Net-(J3-Pad9)")
  (net 10 "Net-(J3-Pad8)")
  (net 11 "Net-(J3-Pad7)")
  (net 12 "Net-(J3-Pad6)")
  (net 13 "Net-(J3-Pad5)")
  (net 14 "Net-(J3-Pad4)")
  (net 15 "Net-(J3-Pad3)")
  (net 16 "Net-(J3-Pad1)")
  (net 17 GNDD)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.381)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(J3-Pad9)")
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 0.508)
    (via_dia 0.9906)
    (via_drill 0.381)
    (uvia_dia 0.9906)
    (uvia_drill 0.381)
    (add_net GNDD)
  )
  (module MouserLib:HDRV10W43P254_2X5_1270X508X599P (layer B.Cu) (tedit 5F8EBAB5)
    (at 174.9552 64.8716)
    (descr 823-22-010-10-004101)
    (tags Connector)
    (fp_text reference J4 (at -0.508 -2.286) (layer F.SilkS) hide)
    (fp_text value 823-22-010-10-004101 (at 0 0) (layer B.SilkS) hide)
    (fp_text user %R (at 10.668 5.334) (layer F.Fab) hide)
    (pad 10 thru_hole circle (at 10.16 2.54) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask)
      (net 17 GNDD))
    (pad 9 thru_hole circle (at 10.16 0) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask)
      (net 9 "Net-(J3-Pad9)"))
    (pad 8 thru_hole circle (at 7.62 2.54) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask)
      (net 10 "Net-(J3-Pad8)"))
    (pad 7 thru_hole circle (at 7.62 0) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad7)"))
    (pad 6 thru_hole circle (at 5.08 2.54) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad6)"))
    (pad 5 thru_hole circle (at 5.08 0) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask)
      (net 13 "Net-(J3-Pad5)"))
    (pad 4 thru_hole circle (at 2.54 2.54) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask)
      (net 14 "Net-(J3-Pad4)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask)
      (net 15 "Net-(J3-Pad3)"))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask)
      (net 17 GNDD))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask)
      (net 16 "Net-(J3-Pad1)"))
    (model Z:\KicadLibraries\SamacSys_Parts.3dshapes\823-22-010-10-004101.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MouserLib:HDRV10W43P254_2X5_1270X508X599P (layer B.Cu) (tedit 5F8EB98E)
    (at 142.24 68.58 180)
    (descr 823-22-010-10-004101)
    (tags Connector)
    (fp_text reference J2 (at 10.668 5.08) (layer F.SilkS) hide)
    (fp_text value 823-22-010-10-004101 (at 0 0) (layer B.SilkS) hide)
    (fp_text user %R (at -0.508 -2.54) (layer F.Fab) hide)
    (pad 10 thru_hole circle (at 10.16 2.54 180) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask)
      (net 17 GNDD))
    (pad 9 thru_hole circle (at 10.16 0 180) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad9)"))
    (pad 8 thru_hole circle (at 7.62 2.54 180) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad8)"))
    (pad 7 thru_hole circle (at 7.62 0 180) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad7)"))
    (pad 6 thru_hole circle (at 5.08 2.54 180) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad6)"))
    (pad 5 thru_hole circle (at 5.08 0 180) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 4 thru_hole circle (at 2.54 2.54 180) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad4)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 0 2.54 180) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask)
      (net 17 GNDD))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad1)"))
    (model Z:\KicadLibraries\SamacSys_Parts.3dshapes\823-22-010-10-004101.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MouserLib:51461314 (layer F.Cu) (tedit 0)
    (at 223.012 59.69 90)
    (descr 5-146131-4-1)
    (tags Connector)
    (attr smd)
    (fp_text reference J3 (at -8.636 3.556 90) (layer F.SilkS) hide)
    (fp_text value 5-146131-4 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -5.08 2.605 90) (size 1.27 3.56) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at -5.08 -2.605 90) (size 1.27 3.56) (layers F.Cu F.Paste F.Mask)
      (net 17 GNDD))
    (pad 3 smd rect (at -2.54 2.605 90) (size 1.27 3.56) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J3-Pad3)"))
    (pad 4 smd rect (at -2.54 -2.605 90) (size 1.27 3.56) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J3-Pad4)"))
    (pad 5 smd rect (at 0 2.605 90) (size 1.27 3.56) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J3-Pad5)"))
    (pad 6 smd rect (at 0 -2.605 90) (size 1.27 3.56) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J3-Pad6)"))
    (pad 7 smd rect (at 2.54 2.605 90) (size 1.27 3.56) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J3-Pad7)"))
    (pad 8 smd rect (at 2.54 -2.605 90) (size 1.27 3.56) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J3-Pad8)"))
    (pad 9 smd rect (at 5.08 2.605 90) (size 1.27 3.56) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J3-Pad9)"))
    (pad 10 smd rect (at 5.08 -2.605 90) (size 1.27 3.56) (layers F.Cu F.Paste F.Mask)
      (net 17 GNDD))
    (model Z:\KicadLibraries\SamacSys_Parts.3dshapes\5-146131-4.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MouserLib:51461314 (layer F.Cu) (tedit 0)
    (at 223.012 44.831 90)
    (descr 5-146131-4-1)
    (tags Connector)
    (attr smd)
    (fp_text reference J1 (at -8.382 3.048 90) (layer F.SilkS) hide)
    (fp_text value 5-146131-4 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -5.08 2.605 90) (size 1.27 3.56) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -5.08 -2.605 90) (size 1.27 3.56) (layers F.Cu F.Paste F.Mask)
      (net 17 GNDD))
    (pad 3 smd rect (at -2.54 2.605 90) (size 1.27 3.56) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at -2.54 -2.605 90) (size 1.27 3.56) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at 0 2.605 90) (size 1.27 3.56) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at 0 -2.605 90) (size 1.27 3.56) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad6)"))
    (pad 7 smd rect (at 2.54 2.605 90) (size 1.27 3.56) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad7)"))
    (pad 8 smd rect (at 2.54 -2.605 90) (size 1.27 3.56) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad8)"))
    (pad 9 smd rect (at 5.08 2.605 90) (size 1.27 3.56) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad9)"))
    (pad 10 smd rect (at 5.08 -2.605 90) (size 1.27 3.56) (layers F.Cu F.Paste F.Mask)
      (net 17 GNDD))
    (model Z:\KicadLibraries\SamacSys_Parts.3dshapes\5-146131-4.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 233.172 36.83)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 233.172 69.85)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 203.2 68.58)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 109.22 68.58)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 203.2 38.1)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 109.22 38.1)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (gr_text P1 (at 226.7712 67.0306 90) (layer F.SilkS))
  (gr_text P1 (at 226.7712 52.1716 90) (layer F.SilkS))
  (gr_text ESP32 (at 232.2322 59.7916 90) (layer F.SilkS))
  (gr_text FPGA (at 232.2322 45.1866 90) (layer F.SilkS))
  (gr_text "CPC2.4 Programming board\n(c)2020 intelligent.toasters@gmail.com\nhttps://intelligenttoasters.blog" (at 158.3182 51.1556) (layer F.SilkS))
  (gr_poly (pts (xy 237.49 73.914) (xy 104.394 73.914) (xy 104.394 32.766) (xy 237.49 32.766)) (layer Edge.Cuts) (width 0.1))
  (zone (net 17) (net_name GNDD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 237.49 73.914) (xy 104.394 73.914) (xy 104.394 32.766) (xy 237.49 32.766)
      )
    )
  )
  (zone (net 17) (net_name GNDD) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 237.49 73.914) (xy 104.394 73.914) (xy 104.394 32.766) (xy 237.49 32.766)
      )
    )
  )
)
