(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 80)
    (no_connects 0)
    (area 132.004999 41.834999 193.115001 142.315001)
    (thickness 1.6)
    (drawings 73)
    (tracks 314)
    (zones 0)
    (modules 46)
    (nets 55)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4)
    (user_trace_width 0.8)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.50012 3.50012)
    (pad_drill 2.6)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(CON1-Pad3)")
  (net 4 323F)
  (net 5 "Net-(D1-Pad1)")
  (net 6 323E)
  (net 7 "Net-(D2-Pad1)")
  (net 8 323D)
  (net 9 "Net-(D3-Pad1)")
  (net 10 324G)
  (net 11 "Net-(D4-Pad1)")
  (net 12 324F)
  (net 13 "Net-(D5-Pad1)")
  (net 14 G323G2)
  (net 15 "Net-(D6-Pad1)")
  (net 16 G323G1)
  (net 17 "Net-(D7-Pad1)")
  (net 18 G323F)
  (net 19 "Net-(D8-Pad1)")
  (net 20 G323E)
  (net 21 "Net-(D9-Pad1)")
  (net 22 G323D)
  (net 23 "Net-(D10-Pad1)")
  (net 24 316)
  (net 25 "Net-(D11-Pad1)")
  (net 26 355)
  (net 27 "Net-(D12-Pad1)")
  (net 28 320)
  (net 29 "Net-(D13-Pad1)")
  (net 30 319)
  (net 31 "Net-(D14-Pad1)")
  (net 32 318)
  (net 33 "Net-(D15-Pad1)")
  (net 34 "Net-(D16-Pad1)")
  (net 35 /324C)
  (net 36 /323C)
  (net 37 /G323C)
  (net 38 "Net-(P1-Pad6)")
  (net 39 "Net-(P5-Pad1)")
  (net 40 "Net-(P5-Pad10)")
  (net 41 "Net-(P5-Pad2)")
  (net 42 "Net-(P5-Pad3)")
  (net 43 "Net-(P5-Pad12)")
  (net 44 "Net-(P5-Pad4)")
  (net 45 "Net-(P5-Pad15)")
  (net 46 "Net-(P5-Pad6)")
  (net 47 "Net-(P5-Pad17)")
  (net 48 "Net-(P5-Pad8)")
  (net 49 "Net-(P5-Pad9)")
  (net 50 /316C)
  (net 51 /355C)
  (net 52 /319F)
  (net 53 /320F)
  (net 54 /318F)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /316C)
    (add_net /318F)
    (add_net /319F)
    (add_net /320F)
    (add_net /323C)
    (add_net /324C)
    (add_net /355C)
    (add_net /G323C)
    (add_net 316)
    (add_net 318)
    (add_net 319)
    (add_net 320)
    (add_net 323D)
    (add_net 323E)
    (add_net 323F)
    (add_net 324F)
    (add_net 324G)
    (add_net 355)
    (add_net G323D)
    (add_net G323E)
    (add_net G323F)
    (add_net G323G1)
    (add_net G323G2)
    (add_net GND)
    (add_net "Net-(CON1-Pad3)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D11-Pad1)")
    (add_net "Net-(D12-Pad1)")
    (add_net "Net-(D13-Pad1)")
    (add_net "Net-(D14-Pad1)")
    (add_net "Net-(D15-Pad1)")
    (add_net "Net-(D16-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D9-Pad1)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P5-Pad10)")
    (add_net "Net-(P5-Pad12)")
    (add_net "Net-(P5-Pad15)")
    (add_net "Net-(P5-Pad17)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P5-Pad3)")
    (add_net "Net-(P5-Pad4)")
    (add_net "Net-(P5-Pad6)")
    (add_net "Net-(P5-Pad8)")
    (add_net "Net-(P5-Pad9)")
    (add_net VCC)
  )
  (module Connect:BARREL_JACK (layer F.Cu) (tedit 5956844D)
    (at 186.69 49.53 270)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference CON1 (at -5.842 7.747 360) (layer F.SilkS))
    (fp_text value BARREL_JACK (at 0 -5.99948 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 6.20014 0 270) (size 3.50012 3.50012) (drill 2.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole rect (at 0.20066 0 270) (size 3.50012 3.50012) (drill 2.6) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at 3.2004 4.699 270) (size 3.50012 3.50012) (drill 2.6) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(CON1-Pad3)"))
    (model Connect.3dshapes/JACK_ALIM.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 59566547)
    (at 177.8 115.57 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 324F (at 0 1.651 360) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 12 324F))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 59566549)
    (at 171.958 115.57 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D2 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 324G (at 0 1.651 360) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 10 324G))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 59566543)
    (at 151.892 135.382 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D3 (at 2.54 0 450) (layer F.SilkS))
    (fp_text value G323D (at 0 1.651 360) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 22 G323D))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D3-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 59566541)
    (at 158.242 135.382 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D4 (at 2.54 0 450) (layer F.SilkS))
    (fp_text value G323E (at 0 1.651 360) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 20 G323E))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D4-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 5956653B)
    (at 164.592 135.382 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D5 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value G323F (at 0 1.651 360) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 18 G323F))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D5-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 5956653A)
    (at 170.942 135.382 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D6 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value G324G1 (at 0 1.651 360) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 16 G323G1))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D6-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 59566538)
    (at 177.292 135.382 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D7 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value G323G2 (at 0 1.651 360) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 14 G323G2))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D7-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 595665CE)
    (at 177.546 74.676 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D8 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 318 (at -0.0635 1.7145 360) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 32 318))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D8-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 595665D3)
    (at 177.546 84.836 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D9 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 319 (at -0.0635 1.7145 360) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 30 319))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D9-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 595665D7)
    (at 177.546 94.996 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D10 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 320 (at -0.0635 1.7145 360) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 28 320))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D10-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 595665E2)
    (at 177.546 105.156 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D11 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 355 (at -0.0635 1.7145 360) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 26 355))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D11-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 595660F6)
    (at 177.546 64.516 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D12 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 316 (at 0 1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 24 316))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D12-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 595660FB)
    (at 165.862 124.968 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D13 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 323D (at 0 1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 8 323D))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D13-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 595660FD)
    (at 171.958 124.968 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D14 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 323E (at 0 1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 6 323E))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D14-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 595660FF)
    (at 177.8 124.968 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D15 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 323F (at 0 1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 323F))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D15-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 59568459)
    (at 176.53 53.34 270)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D16 (at 0 1.651 450) (layer F.SilkS))
    (fp_text value PWR (at 0 1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 1 smd rect (at -1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D16-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Connector_Microfit3_Header_02x09_Angled_43045-180x (layer F.Cu) (tedit 55BBA990)
    (at 138.43 50.165 180)
    (descr "Microfit3 02x09 heder angled 43045-1800")
    (tags "Microfit 02x09 angled 3mm pitch")
    (fp_text reference P5 (at -11 11 180) (layer F.SilkS))
    (fp_text value "MODULE GPIO (G)" (at -12 -6.604 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(P5-Pad1)"))
    (pad 10 thru_hole circle (at 0 -3 180) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(P5-Pad10)"))
    (pad 11 thru_hole circle (at -3 -3 180) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 10 324G))
    (pad 2 thru_hole circle (at -3 0 180) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(P5-Pad2)"))
    (pad 3 thru_hole circle (at -6 0 180) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(P5-Pad3)"))
    (pad 12 thru_hole circle (at -6 -3 180) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(P5-Pad12)"))
    (pad 13 thru_hole circle (at -9 -3 180) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 24 316))
    (pad 4 thru_hole circle (at -9 0 180) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(P5-Pad4)"))
    (pad 5 thru_hole circle (at -12 0 180) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 16 G323G1))
    (pad 14 thru_hole circle (at -12 -3 180) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 14 G323G2))
    (pad "" np_thru_hole circle (at -2.1 4.32 180) (size 3.1 3.1) (drill 3.1) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole circle (at -15 -3 180) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(P5-Pad15)"))
    (pad 6 thru_hole circle (at -15 0 180) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(P5-Pad6)"))
    (pad 7 thru_hole circle (at -18 0 180) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 32 318))
    (pad 16 thru_hole circle (at -18 -3 180) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 26 355))
    (pad 17 thru_hole circle (at -21 -3 180) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(P5-Pad17)"))
    (pad 8 thru_hole circle (at -21 0 180) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(P5-Pad8)"))
    (pad 18 thru_hole circle (at -24 -3 180) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 28 320))
    (pad 9 thru_hole circle (at -24 0 180) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(P5-Pad9)"))
    (pad "" np_thru_hole circle (at -21.8 4.32 180) (size 3.1 3.1) (drill 3.1) (layers *.Cu *.Mask F.SilkS))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5956605D)
    (at 177.8 118.364)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 300Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 595660CD)
    (at 171.958 118.364)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 300Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59566128)
    (at 151.892 138.176)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 300Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59566126)
    (at 158.242 138.176)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 300Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59566124)
    (at 164.592 138.176)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 300Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59566120)
    (at 170.942 138.176)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 300Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D6-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5956611E)
    (at 177.292 138.176)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 300Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D7-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5956611C)
    (at 177.546 77.47)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 300Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D8-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59566118)
    (at 177.546 87.63)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 300Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D9-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59566116)
    (at 177.546 97.79)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 300Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D10-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59566114)
    (at 177.546 107.95)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 300Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D11-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5956610E)
    (at 177.546 67.31)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 300Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D12-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5956610B)
    (at 165.862 127.762)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 300Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D13-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59566109)
    (at 171.958 127.762)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 300Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D14-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59566107)
    (at 177.8 127.762)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 300Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D15-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59568455)
    (at 177.8 48.26)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 0 -1.651 180) (layer F.SilkS))
    (fp_text value 300Ω (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D16-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_SMALL (layer F.Cu) (tedit 59566972)
    (at 186.69 116.84 180)
    (fp_text reference SW1 (at 0 -0.762 180) (layer F.SilkS))
    (fp_text value 324 (at 0 -5.08 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /324C))
    (pad 1 thru_hole circle (at -3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at -3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /324C))
    (model Buttons_Switches_ThroughHole.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2.5 2.5 2.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_SMALL (layer F.Cu) (tedit 5956696C)
    (at 186.69 127 180)
    (fp_text reference SW2 (at 0 -0.762 180) (layer F.SilkS))
    (fp_text value 323 (at 0 -5.08 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 /323C))
    (pad 1 thru_hole circle (at -3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at -3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 /323C))
    (model Buttons_Switches_ThroughHole.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2.5 2.5 2.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_SMALL (layer F.Cu) (tedit 59566957)
    (at 186.69 66.04 180)
    (fp_text reference SW3 (at 0 -0.762 180) (layer F.SilkS))
    (fp_text value 316 (at 0 -5.08 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 /316C))
    (pad 1 thru_hole circle (at -3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at -3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 /316C))
    (model Buttons_Switches_ThroughHole.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2.5 2.5 2.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_SMALL (layer F.Cu) (tedit 59566976)
    (at 186.69 106.68 180)
    (fp_text reference SW4 (at 0 -0.762 180) (layer F.SilkS))
    (fp_text value 355 (at 0 -5.08 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 /355C))
    (pad 1 thru_hole circle (at -3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at -3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 /355C))
    (model Buttons_Switches_ThroughHole.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2.5 2.5 2.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_SMALL (layer F.Cu) (tedit 5956696F)
    (at 186.69 137.16 180)
    (fp_text reference SW5 (at 0 -0.762 180) (layer F.SilkS))
    (fp_text value G323 (at 0 -5.08 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 /G323C))
    (pad 1 thru_hole circle (at -3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at -3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 /G323C))
    (model Buttons_Switches_ThroughHole.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2.5 2.5 2.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_SMALL (layer F.Cu) (tedit 59566968)
    (at 186.69 96.52 180)
    (fp_text reference SW6 (at 0 -0.762 180) (layer F.SilkS))
    (fp_text value 320 (at 0 -5.08 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 /320F))
    (pad 1 thru_hole circle (at -3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at -3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 /320F))
    (model Buttons_Switches_ThroughHole.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2.5 2.5 2.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_SMALL (layer F.Cu) (tedit 59566965)
    (at 186.69 86.36 180)
    (fp_text reference SW7 (at 0 -0.762 180) (layer F.SilkS))
    (fp_text value 319 (at 0 -5.08 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 /319F))
    (pad 1 thru_hole circle (at -3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at -3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 /319F))
    (model Buttons_Switches_ThroughHole.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2.5 2.5 2.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_SMALL (layer F.Cu) (tedit 5956695F)
    (at 186.69 76.2 180)
    (fp_text reference SW8 (at 0 -0.762 180) (layer F.SilkS))
    (fp_text value 318 (at 0 -5.08 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 /318F))
    (pad 1 thru_hole circle (at -3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at -3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 /318F))
    (model Buttons_Switches_ThroughHole.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2.5 2.5 2.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sockets_MOLEX_KK-System:Socket_MOLEX-KK-RM3-96mm_Lock_6pin_straight (layer F.Cu) (tedit 595669C5)
    (at 136.525 129.54 90)
    (descr "Socket, MOLEX, KK, RM 3.96mm, Lock, 6pin, straight,")
    (tags "Socket, MOLEX, KK, RM 3.96mm, Lock, 6pin, straight,")
    (fp_text reference P1 (at 12.6492 0 180) (layer F.SilkS))
    (fp_text value "TELEMATICS M1 (C)" (at -0.0508 6.35 90) (layer F.Fab))
    (pad 3 thru_hole oval (at -1.9812 0 90) (size 2.99974 5.00126) (drill 1.80086) (layers *.Cu *.Mask F.SilkS)
      (net 50 /316C))
    (pad 4 thru_hole oval (at 1.9812 0 90) (size 2.99974 5.00126) (drill 1.80086) (layers *.Cu *.Mask F.SilkS)
      (net 51 /355C))
    (pad 2 thru_hole oval (at -5.94106 0 90) (size 2.99974 5.00126) (drill 1.80086) (layers *.Cu *.Mask F.SilkS)
      (net 36 /323C))
    (pad 5 thru_hole oval (at 5.94106 0 90) (size 2.99974 5.00126) (drill 1.80086) (layers *.Cu *.Mask F.SilkS)
      (net 37 /G323C))
    (pad 1 thru_hole oval (at -9.90092 0 90) (size 2.99974 5.00126) (drill 1.80086) (layers *.Cu *.Mask F.SilkS)
      (net 35 /324C))
    (pad 6 thru_hole oval (at 9.90092 0 90) (size 2.99974 5.00126) (drill 1.80086) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(P1-Pad6)"))
  )
  (module Sockets_MOLEX_KK-System:Socket_MOLEX-KK-RM3-96mm_Lock_6pin_straight (layer F.Cu) (tedit 595669B9)
    (at 136.525 71.12 90)
    (descr "Socket, MOLEX, KK, RM 3.96mm, Lock, 6pin, straight,")
    (tags "Socket, MOLEX, KK, RM 3.96mm, Lock, 6pin, straight,")
    (fp_text reference P2 (at 12.7 0 180) (layer F.SilkS))
    (fp_text value "POWER CONTROL (F)" (at 0 6.35 90) (layer F.Fab))
    (pad 3 thru_hole oval (at -1.9812 0 90) (size 2.99974 5.00126) (drill 1.80086) (layers *.Cu *.Mask F.SilkS)
      (net 52 /319F))
    (pad 4 thru_hole oval (at 1.9812 0 90) (size 2.99974 5.00126) (drill 1.80086) (layers *.Cu *.Mask F.SilkS)
      (net 12 324F))
    (pad 2 thru_hole oval (at -5.94106 0 90) (size 2.99974 5.00126) (drill 1.80086) (layers *.Cu *.Mask F.SilkS)
      (net 53 /320F))
    (pad 5 thru_hole oval (at 5.94106 0 90) (size 2.99974 5.00126) (drill 1.80086) (layers *.Cu *.Mask F.SilkS)
      (net 54 /318F))
    (pad 1 thru_hole oval (at -9.90092 0 90) (size 2.99974 5.00126) (drill 1.80086) (layers *.Cu *.Mask F.SilkS)
      (net 4 323F))
    (pad 6 thru_hole oval (at 9.90092 0 90) (size 2.99974 5.00126) (drill 1.80086) (layers *.Cu *.Mask F.SilkS)
      (net 18 G323F))
  )
  (module Sockets_MOLEX_KK-System:Socket_MOLEX-KK-RM3-96mm_Lock_2pin_straight (layer F.Cu) (tedit 595669B6)
    (at 136.525 92.71 90)
    (descr "Socket, MOLEX, KK, RM 3.96mm, Lock, 2pin, straight,")
    (tags "Socket, MOLEX, KK, RM 3.96mm, Lock, 2pin, straight,")
    (fp_text reference P3 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value "MODEM POWER (E)" (at 1.2192 6.35 90) (layer F.Fab))
    (pad 1 thru_hole oval (at -1.9812 0 90) (size 2.99974 5.00126) (drill 1.80086) (layers *.Cu *.Mask F.SilkS)
      (net 8 323D))
    (pad 2 thru_hole oval (at 1.9812 0 90) (size 2.99974 5.00126) (drill 1.80086) (layers *.Cu *.Mask F.SilkS)
      (net 20 G323E))
  )
  (module Sockets_MOLEX_KK-System:Socket_MOLEX-KK-RM3-96mm_Lock_3pin_straight (layer F.Cu) (tedit 595669C1)
    (at 136.525 107.315 90)
    (descr "Socket, MOLEX, KK, RM 3.96mm, Lock, 3pin, straight,")
    (tags "Socket, MOLEX, KK, RM 3.96mm, Lock, 3pin, straight,")
    (fp_text reference P4 (at 6.2992 0 180) (layer F.SilkS))
    (fp_text value "MODULE POWER (D)" (at -0.0508 6.35 90) (layer F.Fab))
    (pad 1 thru_hole oval (at -3.95986 0 90) (size 2.99974 5.00126) (drill 1.80086) (layers *.Cu *.Mask F.SilkS)
      (net 6 323E))
    (pad 2 thru_hole oval (at 0 0 90) (size 2.99974 5.00126) (drill 1.80086) (layers *.Cu *.Mask F.SilkS)
      (net 22 G323D))
    (pad 3 thru_hole oval (at 3.95986 0 90) (size 2.99974 5.00126) (drill 1.80086) (layers *.Cu *.Mask F.SilkS)
      (net 30 319))
  )
  (gr_text GJS (at 186.563 137.414) (layer B.SilkS))
  (gr_text "© 2017 Tigercat Industries \n75397B Tester" (at 161.29 78.359) (layer B.SilkS))
  (gr_text F (at 177.8 113.284) (layer F.SilkS))
  (gr_text G (at 171.958 113.284) (layer F.SilkS))
  (gr_text F (at 177.8 122.936) (layer F.SilkS))
  (gr_text E (at 171.958 122.936) (layer F.SilkS))
  (gr_text D (at 165.862 122.936) (layer F.SilkS))
  (gr_text G2 (at 177.292 133.35) (layer F.SilkS))
  (gr_text G1 (at 170.942 133.35) (layer F.SilkS))
  (gr_text F (at 164.592 133.35) (layer F.SilkS))
  (gr_text E (at 158.242 133.35) (layer F.SilkS))
  (gr_text D (at 151.892 133.35) (layer F.SilkS))
  (gr_text "MODULE GPIO\n(G)" (at 150.495 57.785) (layer F.SilkS))
  (gr_text "TELEMATICS M1\n(C)" (at 144.78 128.905 90) (layer F.SilkS))
  (gr_text "MODULE PWR\n(D)" (at 144.78 107.95 90) (layer F.SilkS))
  (gr_text "MODEM PWR\n(E)" (at 144.78 92.71 90) (layer F.SilkS))
  (gr_text "POWER CONTROL\n(F)" (at 144.78 71.12 90) (layer F.SilkS))
  (gr_text 355 (at 171.45 106.68) (layer F.SilkS))
  (gr_text 324 (at 165.1 116.84) (layer F.SilkS))
  (gr_text G232 (at 152.4 130.81) (layer F.SilkS))
  (gr_text 323 (at 159.385 126.365) (layer F.SilkS))
  (gr_text 320 (at 171.45 96.52) (layer F.SilkS))
  (gr_text 319 (at 171.45 86.36) (layer F.SilkS))
  (gr_text 318 (at 171.45 76.2) (layer F.SilkS))
  (gr_text 316 (at 171.45 66.04) (layer F.SilkS))
  (gr_line (start 193.04 41.91) (end 193.04 142.24) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.08 41.91) (end 193.04 41.91) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.08 142.24) (end 132.08 41.91) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 193.04 142.24) (end 132.08 142.24) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193.04 142.24) (xy 132.08 142.24) (xy 132.08 41.91) (xy 193.04 41.91) (xy 193.04 142.24)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193.04 142.24) (xy 132.08 142.24) (xy 132.08 41.91) (xy 193.04 41.91) (xy 193.04 142.24)
      )
    )
  )
)
