(kicad_pcb (version 4) (host pcbnew 4.0.2-1.fc23-product)
  (general
    (links 0)
    (no_connects 0)
    (area 123.622999 54.534999 171.017001 100.151001)
    (thickness 1.6)
    (drawings 29)
    (tracks 59)
    (zones 0)
    (modules 15)
    (nets 38)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFE77F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad0)")
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J1-Pad17A)")
  (net 10 "Net-(J1-Pad3V1)")
  (net 11 "Net-(J1-PadG2)")
  (net 12 "Net-(J1-PadPGM)")
  (net 13 "Net-(J1-PadDAC)")
  (net 14 "Net-(J1-Pad16)")
  (net 15 "Net-(J1-Pad17)")
  (net 16 "Net-(J1-PadG3)")
  (net 17 "Net-(J1-Pad22)")
  (net 18 "Net-(J1-PadVIN)")
  (net 19 "Net-(J1-Pad21)")
  (net 20 "Net-(J1-Pad20)")
  (net 21 "Net-(J1-Pad23)")
  (net 22 "Net-(J1-Pad14)")
  (net 23 "Net-(J1-Pad15)")
  (net 24 /CS)
  (net 25 /RST)
  (net 26 /GND)
  (net 27 "Net-(J1-Pad9)")
  (net 28 "Net-(J1-Pad10)")
  (net 29 "Net-(J1-Pad11)")
  (net 30 "Net-(J1-Pad12)")
  (net 31 "Net-(J1-Pad13)")
  (net 32 /SDA)
  (net 33 /3.3V)
  (net 34 /VIN)
  (net 35 /SCK)
  (net 36 /3V0)
  (net 37 /SDO)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3.3V)
    (add_net /3V0)
    (add_net /CS)
    (add_net /GND)
    (add_net /RST)
    (add_net /SCK)
    (add_net /SDA)
    (add_net /SDO)
    (add_net /VIN)
    (add_net "Net-(J1-Pad0)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad17A)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad3V1)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J1-PadDAC)")
    (add_net "Net-(J1-PadG2)")
    (add_net "Net-(J1-PadG3)")
    (add_net "Net-(J1-PadPGM)")
    (add_net "Net-(J1-PadVIN)")
  )
  (module CHIP-DIPs:Symbol_OSHW-Logo_SilkScreen (layer B.Cu) (tedit 572EAEC9)
    (at 127.508 64.77 180)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 4.38912 180) (layer B.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 -6.56082 180) (layer B.Fab) hide)
  )
  (module Wickerlib:TEENSY-LC (layer F.Cu) (tedit 57379CE3)
    (at 153.136601 71.094601)
    (fp_text reference J1 (at -10.16 25.4 180) (layer F.SilkS))
    (fp_text value TEENSY-LC (at -2.54 20.32 180) (layer F.Fab))
    (fp_text user "TEENSY LC" (at 2.54 25.4) (layer F.SilkS))
    (pad G1 thru_hole circle (at -10.16 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /GND))
    (pad 0 thru_hole circle (at -10.16 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(J1-Pad0)"))
    (pad 1 thru_hole circle (at -10.16 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at -10.16 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at -10.16 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /RST))
    (pad 5 thru_hole circle (at -10.16 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at -10.16 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at -10.16 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at -10.16 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-Pad8)"))
    (pad 9 thru_hole circle (at -10.16 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(J1-Pad9)"))
    (pad 10 thru_hole circle (at -10.16 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(J1-Pad10)"))
    (pad 11 thru_hole circle (at -10.16 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(J1-Pad11)"))
    (pad 12 thru_hole circle (at -10.16 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(J1-Pad12)"))
    (pad 17A thru_hole circle (at -7.62 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad17A)"))
    (pad 3V1 thru_hole circle (at -5.08 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J1-Pad3V1)"))
    (pad G2 thru_hole circle (at -2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-PadG2)"))
    (pad PGM thru_hole circle (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J1-PadPGM)"))
    (pad DAC thru_hole circle (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J1-PadDAC)"))
    (pad 13 thru_hole circle (at 5.08 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(J1-Pad13)"))
    (pad 16 thru_hole circle (at 5.08 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J1-Pad16)"))
    (pad 3V2 thru_hole circle (at 5.08 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /VIN))
    (pad 18 thru_hole circle (at 5.08 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /SDA))
    (pad 17 thru_hole circle (at 5.08 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J1-Pad17)"))
    (pad G3 thru_hole circle (at 5.08 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J1-PadG3)"))
    (pad 22 thru_hole circle (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J1-Pad22)"))
    (pad VIN thru_hole circle (at 5.08 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J1-PadVIN)"))
    (pad 21 thru_hole circle (at 5.08 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J1-Pad21)"))
    (pad 20 thru_hole circle (at 5.08 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J1-Pad20)"))
    (pad 19 thru_hole circle (at 5.08 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /SCK))
    (pad 23 thru_hole circle (at 5.08 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J1-Pad23)"))
    (pad 14 thru_hole circle (at 5.08 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(J1-Pad14)"))
    (pad 15 thru_hole circle (at 5.08 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J1-Pad15)"))
  )
  (module Wickerlib:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 0)
    (at 168.656 68.834)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J2 (at 0 -5.1) (layer F.SilkS))
    (fp_text value OLED-I2C (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /SDA))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /SCK))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /RST))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /3.3V))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /VIN))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x07 (layer F.Cu) (tedit 0)
    (at 132.08 82.804 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J3 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value ADAFRUIT_BME280 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /VIN))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /3V0))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /GND))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /SCK))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /SDO))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /SDA))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /CS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x07.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:Symbol_OSHW-Logo_SilkScreen (layer F.Cu) (tedit 572EAEC9)
    (at 148.59 88.138 270)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 -4.38912 270) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082 270) (layer F.Fab) hide)
  )
  (module CHIP-DIPs:Symbol_OSHW-Logo_SilkScreen (layer F.Cu) (tedit 572EAEC9)
    (at 148.59 88.138 270)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 -4.38912 270) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082 270) (layer F.Fab) hide)
  )
  (module CHIP-DIPs:Symbol_OSHW-Logo_SilkScreen (layer F.Cu) (tedit 572EAEC9)
    (at 148.59 88.138 270)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 -4.38912 270) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082 270) (layer F.Fab) hide)
  )
  (module CHIP-DIPs:Symbol_OSHW-Logo_SilkScreen (layer F.Cu) (tedit 572EAEC9)
    (at 137.414 91.186 270)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 -4.38912 270) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082 270) (layer F.Fab) hide)
  )
  (module oshpark:logo-smaller (layer F.Cu) (tedit 0)
    (at 149.098 104.14 270)
    (fp_text reference G*** (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer F.SilkS) hide)
  )
  (module oshpark:logo-smaller (layer F.Cu) (tedit 0)
    (at 149.352 77.47 270)
    (fp_text reference G*** (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer F.SilkS) hide)
  )
  (module oshpark:logo-smaller (layer F.Cu) (tedit 0)
    (at 149.352 77.47 270)
    (fp_text reference G*** (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer F.SilkS) hide)
  )
  (module CHIP-DIPs:Symbol_OSHW-Logo_SilkScreen (layer B.Cu) (tedit 572EAEC9)
    (at 133.604 62.484)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 4.38912) (layer B.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 -6.56082) (layer B.Fab) hide)
  )
  (module CHIP-DIPs:Symbol_OSHW-Logo_SilkScreen (layer F.Cu) (tedit 572EAEC9)
    (at 133.604 62.484)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 -4.38912) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082) (layer F.Fab) hide)
  )
  (module CHIP-DIPs:Symbol_OSHW-Logo_SilkScreen (layer F.Cu) (tedit 572EAEC9)
    (at 133.604 62.484)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 -4.38912) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082) (layer F.Fab) hide)
  )
  (module teensyi2c:oshw-2in-silk (layer B.Cu) (tedit 0)
    (at 148.59 75.438 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (gr_text "drew@oshpark.com\n" (at 126.492 77.724 90) (layer B.SilkS))
  (gr_text "drew@oshpark.com\n" (at 151.384 98.298) (layer F.SilkS))
  (gr_text "DREW FUSTINI\n" (at 126.238 75.438 90) (layer F.SilkS))
  (gr_text "DREW FUSTINI\n" (at 153.924 69.85 270) (layer B.SilkS))
  (gr_text "drew@oshpark.com\n" (at 141.732 57.15 360) (layer F.SilkS))
  (gr_text "drew@oshpark.com\n" (at 151.384 98.806) (layer B.SilkS))
  (gr_text "DREW FUSTINI\n" (at 129.54 75.184 90) (layer B.SilkS))
  (gr_text "I2C OLED" (at 165.1 84.836) (layer F.Cu))
  (gr_text "I2C OLED" (at 165.1 84.836) (layer F.Mask))
  (gr_text BME280 (at 136.906 86.106) (layer F.Mask))
  (gr_text BME280 (at 136.906 86.106) (layer F.Cu))
  (gr_line (start 164.846 58.42) (end 150.368 54.61) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.942 66.294) (end 164.846 58.42) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.942 83.312) (end 170.942 66.294) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.56 100.076) (end 170.942 83.312) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.208 100.076) (end 162.814 100.076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.698 86.868) (end 140.208 100.076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.698 63.754) (end 123.698 86.868) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.826 54.61) (end 123.698 63.754) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.384 54.61) (end 131.826 54.61) (layer Edge.Cuts) (width 0.15))
)
