(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "+15V")
	(net 2 "-15V")
	(net 3 "GND")
	(net 4 "V1")
	(net 5 "unconnected-(J0-Pad1)")
	(net 6 "unconnected-(J0-Pad2)")
	(net 7 "unconnected-(J0-Pad35)")
	(net 8 "unconnected-(J0-Pad36)")
	(net 9 "V21")
	(net 10 "V22")
	(net 11 "V23")
	(net 12 "V24")
	(net 13 "V25")
	(net 14 "V26")
	(net 15 "V27")
	(net 16 "V28")
	(net 17 "V29")
	(net 18 "V30")
	(net 19 "V31")
	(net 20 "V32")
	(net 21 "G21")
	(net 22 "G22")
	(net 23 "G23")
	(net 24 "G24")
	(net 25 "G25")
	(net 26 "G26")
	(net 27 "G27")
	(net 28 "G28")
	(net 29 "G29")
	(net 30 "G30")
	(net 31 "G31")
	(net 32 "G32")
	(net 33 "unconnected-(J21-Pad13)")
	(net 34 "V18")
	(net 35 "V10")
	(net 36 "V9")
	(net 37 "V8")
	(net 38 "V3")
	(net 39 "V7")
	(net 40 "V14")
	(net 41 "V6")
	(net 42 "V11")
	(net 43 "V13")
	(net 44 "V16")
	(net 45 "V19")
	(net 46 "V17")
	(net 47 "V2")
	(net 48 "V15")
	(net 49 "V20")
	(net 50 "V12")
	(net 51 "V5")
	(net 52 "V4")
	(footprint "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 78.9 47.05)
		(descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J6"
			(at 0 -2.92 0)
			(layer "F.SilkS")
		)
		(property "Value" "4P4C"
			(at 0 10.42 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "4P4C* RJ9* RJ10* RJ22*")
		(sheetname "LEM2")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.099999 3.75 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.34 3.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "V6")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 119.539998 86.58)
		(descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J19"
			(at 0 -2.92 0)
			(layer "F.SilkS")
		)
		(property "Value" "4P4C"
			(at 0 10.42 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "4P4C* RJ9* RJ10* RJ22*")
		(sheetname "LEM4")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.099999 3.75 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.34 3.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "V19")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 92.446666 86.58)
		(descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J17"
			(at 0 -2.92 0)
			(layer "F.SilkS")
		)
		(property "Value" "4P4C"
			(at 0 10.42 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "4P4C* RJ9* RJ10* RJ22*")
		(sheetname "LEM3")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.099999 3.75 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.34 3.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "V17")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 138.43 74.84 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R15"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "50 Ohm"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "LEM5")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(J0-Pad2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "V15")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 92.446666 67.28)
		(descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J12"
			(at 0 -2.92 0)
			(layer "F.SilkS")
		)
		(property "Value" "4P4C"
			(at 0 10.42 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "4P4C* RJ9* RJ10* RJ22*")
		(sheetname "LEM3")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.099999 3.75 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.34 3.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "V12")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(J0-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 138.43 94.14 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R20"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "50 Ohm"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "LEM5")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "V20")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 119.539998 47.05)
		(descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J9"
			(at 0 -2.92 0)
			(layer "F.SilkS")
		)
		(property "Value" "4P4C"
			(at 0 10.42 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "4P4C* RJ9* RJ10* RJ22*")
		(sheetname "LEM4")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.099999 3.75 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.34 3.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "V9")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_6.4mm_M6_DIN965_Pad"
		(layer "F.Cu")
		(at 45.5 22.5)
		(descr "Mounting Hole 6.4mm, M6, DIN965")
		(tags "mounting hole 6.4mm m6 din965")
		(property "Reference" "H0"
			(at 0 -6.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 6.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_6.4mm_M6_DIN965_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 11 11)
			(drill 6.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(footprint "TerminalBlock:TerminalBlock_Altech_AK300-3_P5.00mm"
		(layer "F.Cu")
		(at 62.23 25.4 -90)
		(descr "Altech AK300 terminal block, pitch 5.0mm, 45 degree angled, see http://www.mouser.com/ds/2/16/PCBMETRC-24178.pdf")
		(tags "Altech AK300 terminal block pitch 5.0mm")
		(property "Reference" "J_power1"
			(at 5 -7.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 4.95 7.3 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TerminalBlock:TerminalBlock_Altech_AK300-3_P5.00mm"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "5_Lems")
		(sheetfile "5_Lems.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5 -1.999999 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.98 3.96)
			(drill 1.32)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+15V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0 270)
			(size 1.98 3.96)
			(drill 1.32)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 10 0 270)
			(size 1.98 3.96)
			(drill 1.32)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_Altech_AK300-3_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 133.086664 47.05)
		(descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J10"
			(at 0 -2.92 0)
			(layer "F.SilkS")
		)
		(property "Value" "4P4C"
			(at 0 10.42 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "4P4C* RJ9* RJ10* RJ22*")
		(sheetname "LEM5")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.099999 3.75 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.34 3.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "V10")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 92.446666 26.73)
		(descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J2"
			(at 0 -2.92 0)
			(layer "F.SilkS")
		)
		(property "Value" "4P4C"
			(at 0 10.42 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "4P4C* RJ9* RJ10* RJ22*")
		(sheetname "LEM3")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.099999 3.75 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.34 3.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "V2")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 111.336665 34.29 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R3"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "50 Ohm"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "LEM1")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 138.43 34.29 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R5"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "50 Ohm"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "LEM5")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "V5")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 84.243333 54.61 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R6"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "50 Ohm"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "LEM2")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "V6")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 97.789999 54.61 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R7"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "50 Ohm"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "LEM3")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "V7")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 105.993332 67.28)
		(descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J13"
			(at 0 -2.92 0)
			(layer "F.SilkS")
		)
		(property "Value" "4P4C"
			(at 0 10.42 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "4P4C* RJ9* RJ10* RJ22*")
		(sheetname "LEM1")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.099999 3.75 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.34 3.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "V13")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(J0-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 84.243333 74.84 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R11"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "50 Ohm"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "LEM2")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(J0-Pad2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "V11")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 124.883331 34.29 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R4"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "50 Ohm"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "LEM4")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "V4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 92.446666 47.05)
		(descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J7"
			(at 0 -2.92 0)
			(layer "F.SilkS")
		)
		(property "Value" "4P4C"
			(at 0 10.42 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "4P4C* RJ9* RJ10* RJ22*")
		(sheetname "LEM3")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.099999 3.75 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.34 3.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "V7")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 138.43 54.61 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R10"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "50 Ohm"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "LEM5")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "V10")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock:TerminalBlock_Altech_AK300-3_P5.00mm"
		(layer "F.Cu")
		(at 62.23 45.72 -90)
		(descr "Altech AK300 terminal block, pitch 5.0mm, 45 degree angled, see http://www.mouser.com/ds/2/16/PCBMETRC-24178.pdf")
		(tags "Altech AK300 terminal block pitch 5.0mm")
		(property "Reference" "J_power2"
			(at 5 -7.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 4.95 7.3 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TerminalBlock:TerminalBlock_Altech_AK300-3_P5.00mm"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "5_Lems1")
		(sheetfile "5_Lems.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5 -1.999999 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.98 3.96)
			(drill 1.32)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+15V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0 270)
			(size 1.98 3.96)
			(drill 1.32)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 10 0 270)
			(size 1.98 3.96)
			(drill 1.32)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_Altech_AK300-3_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_6.4mm_M6_DIN965_Pad"
		(layer "F.Cu")
		(at 154 117)
		(descr "Mounting Hole 6.4mm, M6, DIN965")
		(tags "mounting hole 6.4mm m6 din965")
		(property "Reference" "H0"
			(at 0 -6.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 6.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_6.4mm_M6_DIN965_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 11 11)
			(drill 6.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(footprint "SCSI_Molex:TE_1761028-4"
		(layer "F.Cu")
		(at 155.046756 71 90)
		(property "Reference" "J0"
			(at -29.5066 -6.48637 90)
			(layer "F.SilkS")
		)
		(property "Value" "1761028-4"
			(at -24.53434 8.135745 90)
			(layer "F.Fab")
		)
		(property "Footprint" "SCSI_Molex:TE_1761028-4"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "\n68 Position Receptacle Connector SCSI+, VHDCI Through Hole, Right Angle Solder\n"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 225.48 -80.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/71430-0101/Molex/view-part/?ref=eda"
			(at 225.48 -80.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Molex"
			(at 225.48 -80.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "6.41 mm"
			(at 225.48 -80.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Molex"
			(at 225.48 -80.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "71430-0101"
			(at 225.48 -80.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "N"
			(at 225.48 -80.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "None"
			(at 225.48 -80.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 225.48 -80.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 225.48 -80.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/71430-0101/Molex/view-part/?ref=snap"
			(at 225.48 -80.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Bias-Current-LEM.kicad_sch")
		(attr through_hole)
		(fp_text user "PCB EDGE"
			(at 22.4 6.72 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -28.955 0 90)
			(size 2.77 2.77)
			(drill 2.77)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 28.955 0 90)
			(size 2.77 2.77)
			(drill 2.77)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole rect
			(at 20.955 -1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 19.685 -3.8 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(J0-Pad2)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at 18.415 -1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "V1")
			(pinfunction "3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at 17.145 -3.8 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "V2")
			(pinfunction "4")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 15.875 -1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "V3")
			(pinfunction "5")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 14.605 -3.8 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "V4")
			(pinfunction "6")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "7" thru_hole circle
			(at 13.335 -1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "V5")
			(pinfunction "7")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "8" thru_hole circle
			(at 12.065 -3.8 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "V6")
			(pinfunction "8")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "9" thru_hole circle
			(at 10.795 -1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "V7")
			(pinfunction "9")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "10" thru_hole circle
			(at 9.525 -3.8 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "V8")
			(pinfunction "10")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "11" thru_hole circle
			(at 8.255 -1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "V9")
			(pinfunction "11")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "12" thru_hole circle
			(at 6.985 -3.8 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "V10")
			(pinfunction "12")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "13" thru_hole circle
			(at 5.715 -1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "V11")
			(pinfunction "13")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "14" thru_hole circle
			(at 4.445 -3.8 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "V12")
			(pinfunction "14")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "15" thru_hole circle
			(at 3.175 -1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "V13")
			(pinfunction "15")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "16" thru_hole circle
			(at 1.905 -3.8 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "V14")
			(pinfunction "16")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "17" thru_hole circle
			(at 0.635 -1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "V15")
			(pinfunction "17")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "18" thru_hole circle
			(at -0.635 -3.8 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "V16")
			(pinfunction "18")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "19" thru_hole circle
			(at -1.905 -1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "V17")
			(pinfunction "19")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "20" thru_hole circle
			(at -3.175 -3.8 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "V18")
			(pinfunction "20")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "21" thru_hole circle
			(at -4.445 -1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "V19")
			(pinfunction "21")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "22" thru_hole circle
			(at -5.715 -3.81 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "V20")
			(pinfunction "22")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "23" thru_hole circle
			(at -6.985 -1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "V21")
			(pinfunction "23")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "24" thru_hole circle
			(at -8.255 -3.8 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "V22")
			(pinfunction "24")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "25" thru_hole circle
			(at -9.525 -1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "V23")
			(pinfunction "25")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "26" thru_hole circle
			(at -10.795 -3.8 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "V24")
			(pinfunction "26")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "27" thru_hole circle
			(at -12.065 -1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "V25")
			(pinfunction "27")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "28" thru_hole circle
			(at -13.335 -3.8 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "V26")
			(pinfunction "28")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "29" thru_hole circle
			(at -14.605 -1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "V27")
			(pinfunction "29")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "30" thru_hole circle
			(at -15.875 -3.8 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "V28")
			(pinfunction "30")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "31" thru_hole circle
			(at -17.145 -1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "V29")
			(pinfunction "31")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "32" thru_hole circle
			(at -18.415 -3.8 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "V30")
			(pinfunction "32")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "33" thru_hole circle
			(at -19.685 -1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "V31")
			(pinfunction "33")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "34" thru_hole circle
			(at -20.955 -3.8 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "V32")
			(pinfunction "34")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "35" thru_hole circle
			(at 20.955 1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "unconnected-(J0-Pad35)")
			(pinfunction "35")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "36" thru_hole circle
			(at 19.685 0 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "unconnected-(J0-Pad36)")
			(pinfunction "36")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "37" thru_hole circle
			(at 18.415 1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pinfunction "37")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "38" thru_hole circle
			(at 17.145 0 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pinfunction "38")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "39" thru_hole circle
			(at 15.875 1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pinfunction "39")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "40" thru_hole circle
			(at 14.605 0 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pinfunction "40")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "41" thru_hole circle
			(at 13.335 1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pinfunction "41")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "42" thru_hole circle
			(at 12.065 0 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pinfunction "42")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "43" thru_hole circle
			(at 10.795 1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pinfunction "43")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "44" thru_hole circle
			(at 9.525 0 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pinfunction "44")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "45" thru_hole circle
			(at 8.255 1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pinfunction "45")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "46" thru_hole circle
			(at 6.985 0 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pinfunction "46")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "47" thru_hole circle
			(at 5.715 1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(J0-Pad2)")
			(pinfunction "47")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "48" thru_hole circle
			(at 4.445 0 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(J0-Pad2)")
			(pinfunction "48")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "49" thru_hole circle
			(at 3.175 1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(J0-Pad2)")
			(pinfunction "49")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "50" thru_hole circle
			(at 1.905 0 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(J0-Pad2)")
			(pinfunction "50")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "51" thru_hole circle
			(at 0.635 1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(J0-Pad2)")
			(pinfunction "51")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "52" thru_hole circle
			(at -0.635 0 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pinfunction "52")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "53" thru_hole circle
			(at -1.905 1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pinfunction "53")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "54" thru_hole circle
			(at -3.175 0 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pinfunction "54")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "55" thru_hole circle
			(at -4.445 1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pinfunction "55")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "56" thru_hole circle
			(at -5.715 -0.01 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pinfunction "56")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "57" thru_hole circle
			(at -6.985 1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "G21")
			(pinfunction "57")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "58" thru_hole circle
			(at -8.255 0 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "G22")
			(pinfunction "58")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "59" thru_hole circle
			(at -9.525 1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "G23")
			(pinfunction "59")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "60" thru_hole circle
			(at -10.795 0 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "G24")
			(pinfunction "60")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "61" thru_hole circle
			(at -12.065 1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "G25")
			(pinfunction "61")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "62" thru_hole circle
			(at -13.335 0 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "G26")
			(pinfunction "62")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "63" thru_hole circle
			(at -14.605 1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "G27")
			(pinfunction "63")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "64" thru_hole circle
			(at -15.875 0 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "G28")
			(pinfunction "64")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "65" thru_hole circle
			(at -17.145 1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "G29")
			(pinfunction "65")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "66" thru_hole circle
			(at -18.415 0 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "G30")
			(pinfunction "66")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "67" thru_hole circle
			(at -19.685 1.9 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "G31")
			(pinfunction "67")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "68" thru_hole circle
			(at -20.955 0 90)
			(size 1.368 1.368)
			(drill 0.86)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "G32")
			(pinfunction "68")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
	)
	(footprint "MountingHole:MountingHole_6.4mm_M6_DIN965_Pad"
		(layer "F.Cu")
		(at 46.5 116.5)
		(descr "Mounting Hole 6.4mm, M6, DIN965")
		(tags "mounting hole 6.4mm m6 din965")
		(property "Reference" "H0"
			(at 0 -6.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 6.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_6.4mm_M6_DIN965_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 11 11)
			(drill 6.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 111.336665 74.84 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R13"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "50 Ohm"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "LEM1")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(J0-Pad2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "V13")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 133.086664 86.58)
		(descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J20"
			(at 0 -2.92 0)
			(layer "F.SilkS")
		)
		(property "Value" "4P4C"
			(at 0 10.42 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "4P4C* RJ9* RJ10* RJ22*")
		(sheetname "LEM5")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.099999 3.75 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.34 3.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "V20")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 78.9 26.73)
		(descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J1"
			(at 0 -2.92 0)
			(layer "F.SilkS")
		)
		(property "Value" "4P4C"
			(at 0 10.42 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "4P4C* RJ9* RJ10* RJ22*")
		(sheetname "LEM2")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.099999 3.75 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.34 3.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "V1")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 97.789999 74.84 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R12"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "50 Ohm"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "LEM3")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(J0-Pad2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "V12")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 78.9 86.58)
		(descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J16"
			(at 0 -2.92 0)
			(layer "F.SilkS")
		)
		(property "Value" "4P4C"
			(at 0 10.42 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "4P4C* RJ9* RJ10* RJ22*")
		(sheetname "LEM2")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.099999 3.75 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.34 3.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "V16")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 133.086664 67.28)
		(descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J15"
			(at 0 -2.92 0)
			(layer "F.SilkS")
		)
		(property "Value" "4P4C"
			(at 0 10.42 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "4P4C* RJ9* RJ10* RJ22*")
		(sheetname "LEM5")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.099999 3.75 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.34 3.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "V15")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(J0-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 105.993332 26.73)
		(descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J3"
			(at 0 -2.92 0)
			(layer "F.SilkS")
		)
		(property "Value" "4P4C"
			(at 0 10.42 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "4P4C* RJ9* RJ10* RJ22*")
		(sheetname "LEM1")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.099999 3.75 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.34 3.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "V3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 84.243333 34.29 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "50 Ohm"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "LEM2")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "V1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 97.789999 34.29 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "50 Ohm"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "LEM3")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "V2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock:TerminalBlock_Altech_AK300-3_P5.00mm"
		(layer "F.Cu")
		(at 62.23 65.95 -90)
		(descr "Altech AK300 terminal block, pitch 5.0mm, 45 degree angled, see http://www.mouser.com/ds/2/16/PCBMETRC-24178.pdf")
		(tags "Altech AK300 terminal block pitch 5.0mm")
		(property "Reference" "J_power3"
			(at 5 -7.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 4.95 7.3 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TerminalBlock:TerminalBlock_Altech_AK300-3_P5.00mm"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "5_Lems2")
		(sheetfile "5_Lems.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5 -1.999999 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.98 3.96)
			(drill 1.32)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+15V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0 270)
			(size 1.98 3.96)
			(drill 1.32)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 10 0 270)
			(size 1.98 3.96)
			(drill 1.32)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(J0-Pad2)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_Altech_AK300-3_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 105.993332 86.58)
		(descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J18"
			(at 0 -2.92 0)
			(layer "F.SilkS")
		)
		(property "Value" "4P4C"
			(at 0 10.42 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "4P4C* RJ9* RJ10* RJ22*")
		(sheetname "LEM1")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.099999 3.75 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.34 3.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "V18")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 84.243333 94.14 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R16"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "50 Ohm"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "LEM2")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "V16")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 105.993332 47.05)
		(descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J8"
			(at 0 -2.92 0)
			(layer "F.SilkS")
		)
		(property "Value" "4P4C"
			(at 0 10.42 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "4P4C* RJ9* RJ10* RJ22*")
		(sheetname "LEM1")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.099999 3.75 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.34 3.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "V8")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Dsub:DSUB-25_Male_Vertical_P2.77x2.84mm_MountingHoles"
		(layer "F.Cu")
		(at 90.64 109.07)
		(descr "25-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
		(tags "25-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 47.1mm")
		(property "Reference" "J21"
			(at 16.62 -5.89 0)
			(layer "F.SilkS")
		)
		(property "Value" "DB25_Plug_MountingHoles"
			(at 16.62 8.73 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_Dsub:DSUB-25_Male_Vertical_P2.77x2.84mm_MountingHoles"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" " ~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DSUB*Male*")
		(sheetname "Root")
		(sheetfile "Bias-Current-LEM.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 16.62 1.42 0)
			(layer "F.Fab")
		)
		(pad "0" thru_hole circle
			(at -6.93 1.42)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "0" thru_hole circle
			(at 40.17 1.42)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "V21")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.77 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "V22")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 5.54 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "V23")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 8.31 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "V24")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 11.08 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "V25")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 13.85 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "V26")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 16.62 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "V27")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 19.39 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "V28")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 22.16 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "V29")
			(pinfunction "9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 24.93 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "V30")
			(pinfunction "10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 27.7 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "V31")
			(pinfunction "11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 30.47 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "V32")
			(pinfunction "12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 33.24 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "unconnected-(J21-Pad13)")
			(pinfunction "13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 1.385 2.84)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "G21")
			(pinfunction "P14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at 4.155 2.84)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "G22")
			(pinfunction "P15")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at 6.925 2.84)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "G23")
			(pinfunction "P16")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at 9.695 2.84)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "G24")
			(pinfunction "P17")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at 12.465 2.84)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "G25")
			(pinfunction "P18")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at 15.235 2.84)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "G26")
			(pinfunction "P19")
			(pintype "passive")
		)
		(pad "20" thru_hole circle
			(at 18.005 2.84)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "G27")
			(pinfunction "P20")
			(pintype "passive")
		)
		(pad "21" thru_hole circle
			(at 20.775 2.84)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "G28")
			(pinfunction "P21")
			(pintype "passive")
		)
		(pad "22" thru_hole circle
			(at 23.545 2.84)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "G29")
			(pinfunction "P22")
			(pintype "passive")
		)
		(pad "23" thru_hole circle
			(at 26.315 2.84)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "G30")
			(pinfunction "P23")
			(pintype "passive")
		)
		(pad "24" thru_hole circle
			(at 29.085 2.84)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "G31")
			(pinfunction "P24")
			(pintype "passive")
		)
		(pad "25" thru_hole circle
			(at 31.855 2.84)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "G32")
			(pinfunction "P25")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-25_Male_Vertical_P2.77x2.84mm_MountingHoles.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 124.883331 74.84 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R14"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "50 Ohm"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "LEM4")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(J0-Pad2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "V14")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 124.883331 94.14 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R19"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "50 Ohm"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "LEM4")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "V19")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 124.883331 54.61 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R9"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "50 Ohm"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "LEM4")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "V9")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 133.086664 26.73)
		(descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J5"
			(at 0 -2.92 0)
			(layer "F.SilkS")
		)
		(property "Value" "4P4C"
			(at 0 10.42 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "4P4C* RJ9* RJ10* RJ22*")
		(sheetname "LEM5")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.099999 3.75 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.34 3.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "V5")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 119.539998 26.73)
		(descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J4"
			(at 0 -2.92 0)
			(layer "F.SilkS")
		)
		(property "Value" "4P4C"
			(at 0 10.42 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "4P4C* RJ9* RJ10* RJ22*")
		(sheetname "LEM4")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.099999 3.75 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.34 3.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "V4")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 111.336665 94.14 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R18"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "50 Ohm"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "LEM1")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "V18")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_6.4mm_M6_DIN965_Pad"
		(layer "F.Cu")
		(at 154 22.5)
		(descr "Mounting Hole 6.4mm, M6, DIN965")
		(tags "mounting hole 6.4mm m6 din965")
		(property "Reference" "H0"
			(at 0 -6.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 6.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_6.4mm_M6_DIN965_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "Bias-Current-LEM.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 11 11)
			(drill 6.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(footprint "TerminalBlock:TerminalBlock_Altech_AK300-3_P5.00mm"
		(layer "F.Cu")
		(at 62.23 85.25 -90)
		(descr "Altech AK300 terminal block, pitch 5.0mm, 45 degree angled, see http://www.mouser.com/ds/2/16/PCBMETRC-24178.pdf")
		(tags "Altech AK300 terminal block pitch 5.0mm")
		(property "Reference" "J_power4"
			(at 5 -7.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 4.95 7.3 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TerminalBlock:TerminalBlock_Altech_AK300-3_P5.00mm"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "5_Lems3")
		(sheetfile "5_Lems.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5 -1.999999 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.98 3.96)
			(drill 1.32)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+15V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0 270)
			(size 1.98 3.96)
			(drill 1.32)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 10 0 270)
			(size 1.98 3.96)
			(drill 1.32)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_Altech_AK300-3_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 119.539998 67.28)
		(descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J14"
			(at 0 -2.92 0)
			(layer "F.SilkS")
		)
		(property "Value" "4P4C"
			(at 0 10.42 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "4P4C* RJ9* RJ10* RJ22*")
		(sheetname "LEM4")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.099999 3.75 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.34 3.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "V14")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(J0-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Wham:wham-logo-kicad_2"
		(layer "F.Cu")
		(at 46 85.5 90)
		(property "Reference" "G***"
			(at 0 -8.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0 -10.25 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "Wham:wham-logo-kicad_2"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 111.336665 54.61 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R8"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "50 Ohm"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "LEM1")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "V8")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 78.9 67.28)
		(descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J11"
			(at 0 -2.92 0)
			(layer "F.SilkS")
		)
		(property "Value" "4P4C"
			(at 0 10.42 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "4P4C* RJ9* RJ10* RJ22*")
		(sheetname "LEM2")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.099999 3.75 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -1.34 3.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-15V")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "V11")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.5)
			(size 2.2 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(J0-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 97.789999 94.14 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R17"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "50 Ohm"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "LEM3")
		(sheetfile "LEM1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J0-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "V17")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 37.11598 15)
		(end 161.61598 125)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "End Ring ILEM\n11 Feb 2025\nL Grantz, T Qian"
		(at 49.5 68.5 90)
		(layer "F.SilkS")
	)
	(zone
		(net 3)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 37.5 15.5) (xy 37.5 124.5) (xy 161 124.5) (xy 161 15.5)
			)
		)
	)
)
