(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 0.1916)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen") (color "White"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "#808080D4") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (color "Polyimide") (thickness 0.1016) (material "Polyimide") (epsilon_r 3.2) (loss_tangent 0.004))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen") (color "#808080FF"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00210fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "output/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "/SCL")
  (net 3 "/SDA")
  (net 4 "/ANT")
  (net 5 "VDD")
  (net 6 "unconnected-(GS1-GS-Pad1)")
  (net 7 "Net-(D1-BK)")
  (net 8 "Net-(D1-GA)")
  (net 9 "/SWIO")
  (net 10 "/PZ+")
  (net 11 "/PZ-")
  (net 12 "/FD")
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 162.56 97.155)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "LCSC" "C14445")
    (property "MPN" "CL05A105KP5NNNC")
    (property "Sheetfile" "nfcwchsao.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 151.765 101.6 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "LCSC" "")
    (property "MPN" "")
    (property "Sheetfile" "nfcwchsao.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C2" (at 0 -2.032 90) (layer "F.SilkS") hide)
    (fp_text value "DNP" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/ANT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/ANT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprint:gs_logo_200mil" (layer "F.Cu")
    (at 159.385 88.9 90)
    (property "LCSC" "")
    (property "MPN" "")
    (property "Sheetfile" "nfcwchsao.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "GS1" (at 0 -3.175 90) (layer "F.SilkS") hide)
    (fp_text value "GS_logo" (at 0 -0.5 90) (layer "F.Fab"))
    (pad "1" smd custom (at 0 0 90) (size 5.08 5.08) (layers "F.Cu")
      (net 6 "unconnected-(GS1-GS-Pad1)") (pinfunction "GS") (pintype "unspecified") (zone_connect 0) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor circle))
      (primitives
      ))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 168.275 107.95 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "LCSC" "")
    (property "MPN" "")
    (property "Sheetfile" "nfcwchsao.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(D1-BK)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/SWIO") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 170.815 107.95 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "LCSC" "")
    (property "MPN" "")
    (property "Sheetfile" "nfcwchsao.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "2k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(D1-GA)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/FD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Buzzer_Beeper:Buzzer_Murata_PKLCS1212E" (layer "F.Cu")
    (at 159.385 88.9 90)
    (descr "Murata Buzzer https://www.murata.com/~/media/webrenewal/support/library/catalog/products/sound/p37e.ashx")
    (tags "Murata Buzzer Beeper")
    (property "Sheetfile" "nfcwchsao.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Crystal speaker/transducer")
    (property "ki_keywords" "crystal speaker ultrasonic transducer")
    (attr smd)
    (fp_text reference "LS1" (at 3.81 0 180) (layer "F.SilkS"))
    (fp_text value "Speaker_Crystal" (at 0 7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -5.6 0 90) (size 1.2 4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/PZ-") (pinfunction "1") (pintype "input"))
    (pad "2" smd rect (at 5.6 0 90) (size 1.2 4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/PZ+") (pinfunction "2") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Buzzer_Beeper.3dshapes/Buzzer_Murata_PKLCS1212E.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOP-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (at 163.195 101.6 -90)
    (descr "SOP, 8 Pin (http://www.macronix.com/Lists/Datasheet/Attachments/7534/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.6.pdf#page=79), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOP SO")
    (property "LCSC" "C5346354")
    (property "MPN" "CH32V003J4M6")
    (property "Sheetfile" "nfcwchsao.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 0 0 90) (layer "F.SilkS"))
    (fp_text value "CH32V003F4P6" (at -0.127 -29.083 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.625 -1.905 270) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/PZ+") (pinfunction "PA1_T1CH2_A1") (pintype "bidirectional"))
    (pad "2" smd roundrect (at -2.625 -0.635 270) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "3" smd roundrect (at -2.625 0.635 270) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/PZ-") (pinfunction "PA2_T1CH2N_A0") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -2.625 1.905 270) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "VDD") (pinfunction "VDD") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.625 1.905 270) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/SDA") (pinfunction "PC1_SDA") (pintype "bidirectional"))
    (pad "6" smd roundrect (at 2.625 0.635 270) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/SCL") (pinfunction "PC2_SCL") (pintype "bidirectional"))
    (pad "7" smd roundrect (at 2.625 -0.635 270) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/FD") (pinfunction "PC4_MCO_A2") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 2.625 -1.905 270) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/SWIO") (pinfunction "PD1_SWIO") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOP-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "custom:KiCad-Logo_8mm" (layer "F.Cu")
    (at 159.385 115.57)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -6.35) (layer "F.SilkS") hide)
    (fp_text value "KiCad-Logo_8mm" (at 0 7.62) (layer "F.Fab") hide)
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 168.27 99.075)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "LCSC" "")
    (property "MPN" "")
    (property "Sheetfile" "nfcwchsao.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 1.27 -2.33) (layer "F.SilkS") hide)
    (fp_text value "Conn_02x03_Odd_Even" (at 1.27 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "VDD") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "/SDA") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "/SCL") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "/SWIO") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "/FD") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 159.385 103.505 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "LCSC" "")
    (property "MPN" "")
    (property "Sheetfile" "nfcwchsao.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/SCL") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SO-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (at 155.575 101.6 90)
    (descr "SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SO SO")
    (property "LCSC" "C2905792")
    (property "MPN" "NT3H2211W0FT1X")
    (property "Sheetfile" "nfcwchsao.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "NFC/I2C EEPROM, SOIC-8/TSSOP-8/DFN-8")
    (property "ki_keywords" "NFC/I2C EEPROM")
    (attr smd)
    (fp_text reference "U1" (at 0 0 90) (layer "F.SilkS"))
    (fp_text value "NT3H2211" (at 0.127 37.846 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.575 -1.905 90) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/ANT") (pinfunction "LA") (pintype "input"))
    (pad "2" smd roundrect (at -2.575 -0.635 90) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "input"))
    (pad "3" smd roundrect (at -2.575 0.635 90) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "4" smd roundrect (at -2.575 1.905 90) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/FD") (pinfunction "FD") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.575 1.905 90) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "6" smd roundrect (at 2.575 0.635 90) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "VDD") (pinfunction "VCC") (pintype "input"))
    (pad "7" smd roundrect (at 2.575 -0.635 90) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "VDD") (pinfunction "VOUT") (pintype "input"))
    (pad "8" smd roundrect (at 2.575 -1.905 90) (size 1.75 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/ANT") (pinfunction "LB") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SO-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 159.385 99.695 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "LCSC" "")
    (property "MPN" "")
    (property "Sheetfile" "nfcwchsao.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/SDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "VDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "custom:LED_Cree-PLCC6_4.7x1.5mm_extended pads" (layer "F.Cu")
    (at 159.385 108.458)
    (descr "4.7mm x 1.5mm PLCC6 LED, http://www.cree.com/led-components/media/documents/1381-QLS6AFKW.pdf")
    (tags "LED Cree PLCC-6")
    (property "Sheetfile" "nfcwchsao.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED, 6 pin package")
    (property "ki_keywords" "LED RGB diode")
    (attr smd)
    (fp_text reference "D1" (at 0 1.8) (layer "F.SilkS") hide)
    (fp_text value "LED_RGB" (at 0 3.1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab"))
    (pad "1" smd rect (at -2.52 0.335) (size 1.66 0.63) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "VDD") (pinfunction "BA") (pintype "passive"))
    (pad "2" smd rect (at -1.21 -0.65) (size 0.4 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(D1-BK)") (pinfunction "BK") (pintype "passive"))
    (pad "3" smd rect (at -0.53 -0.65) (size 0.4 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(D1-BK)") (pinfunction "RA") (pintype "passive"))
    (pad "4" smd rect (at 0.53 -0.65) (size 0.4 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(D1-GA)") (pinfunction "RK") (pintype "passive"))
    (pad "5" smd rect (at 1.21 -0.65) (size 0.4 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(D1-GA)") (pinfunction "GA") (pintype "passive"))
    (pad "6" smd rect (at 2.52 0.335) (size 1.66 0.63) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GK") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_Cree-PLCC6_4.7x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 142.24 80.645) (mid 143.169936 78.399936) (end 145.415 77.47)
    (layer "Edge.Cuts"))
  (gr_arc (start 145.415 125.73) (mid 143.169936 124.800064) (end 142.24 122.555)
    (layer "Edge.Cuts"))
  (gr_arc (start 173.355 77.47) (mid 175.600064 78.399936) (end 176.53 80.645)
    (layer "Edge.Cuts"))
  (gr_line (start 176.53 80.645) (end 176.53 122.555)
    (layer "Edge.Cuts"))
  (gr_arc (start 176.53 122.555) (mid 175.600064 124.800064) (end 173.355 125.73)
    (layer "Edge.Cuts"))
  (gr_line (start 161.925 109.22) (end 156.845 109.22)
    (layer "Edge.Cuts"))
  (gr_arc (start 156.845 111.76) (mid 155.575 110.49) (end 156.845 109.22)
    (layer "Edge.Cuts"))
  (gr_line (start 156.845 111.76) (end 161.925 111.76)
    (layer "Edge.Cuts"))
  (gr_line (start 145.415 77.47) (end 173.355 77.47)
    (layer "Edge.Cuts"))
  (gr_line (start 142.24 122.555) (end 142.24 80.645)
    (layer "Edge.Cuts"))
  (gr_arc (start 161.925 109.22) (mid 163.195 110.49) (end 161.925 111.76)
    (layer "Edge.Cuts"))
  (gr_line (start 173.355 125.73) (end 145.415 125.73)
    (layer "Edge.Cuts"))
  (gr_text "Beeping\nBlinking\nBadge\nBuddy\n" (at 147.955 111.125 90) (layer "F.SilkS"))
  (gr_text "B4" (at 171.45 88.9 90) (layer "F.SilkS"))
  (gr_text "NTAG I2C Plus\nWCH32V003" (at 147.32 89.535 90) (layer "F.SilkS"))
)
