(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 98)
    (no_connects 0)
    (area 35.924999 61.924999 136.075001 134.075001)
    (thickness 1.6)
    (drawings 49)
    (tracks 466)
    (zones 0)
    (modules 22)
    (nets 36)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /5V)
  (net 2 /SCL0)
  (net 3 /~INT0)
  (net 4 /SDA0)
  (net 5 /GPIOG11)
  (net 6 /GPIOG6)
  (net 7 /GPIOG7)
  (net 8 /GPIOA0)
  (net 9 /GPIOA6)
  (net 10 /GPIOA2)
  (net 11 /GPIOA3)
  (net 12 /GPIOG8)
  (net 13 /GPIOG9)
  (net 14 /GPIOC0)
  (net 15 /GPIOC1)
  (net 16 /GPIOA1)
  (net 17 /GPIOC2)
  (net 18 /GPIOC3)
  (net 19 /~RESET0)
  (net 20 /RX)
  (net 21 /TX)
  (net 22 /I2S0-SDIN)
  (net 23 /I2S0-SDOUT)
  (net 24 /I2S0-BCK)
  (net 25 /I2S0-LRCK)
  (net 26 /GPIOA17)
  (net 27 /GPIOL11)
  (net 28 /USB2-D-)
  (net 29 /USB2-D+)
  (net 30 /USB1-D-)
  (net 31 /USB1-D+)
  (net 32 /3.3V)
  (net 33 /3.3V-I2C)
  (net 34 GNDREF)
  (net 35 /ALT-3.3V)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3.3V)
    (add_net /3.3V-I2C)
    (add_net /5V)
    (add_net /ALT-3.3V)
    (add_net /GPIOA0)
    (add_net /GPIOA1)
    (add_net /GPIOA17)
    (add_net /GPIOA2)
    (add_net /GPIOA3)
    (add_net /GPIOA6)
    (add_net /GPIOC0)
    (add_net /GPIOC1)
    (add_net /GPIOC2)
    (add_net /GPIOC3)
    (add_net /GPIOG11)
    (add_net /GPIOG6)
    (add_net /GPIOG7)
    (add_net /GPIOG8)
    (add_net /GPIOG9)
    (add_net /GPIOL11)
    (add_net /I2S0-BCK)
    (add_net /I2S0-LRCK)
    (add_net /I2S0-SDIN)
    (add_net /I2S0-SDOUT)
    (add_net /RX)
    (add_net /SCL0)
    (add_net /SDA0)
    (add_net /TX)
    (add_net /USB1-D+)
    (add_net /USB1-D-)
    (add_net /USB2-D+)
    (add_net /USB2-D-)
    (add_net /~INT0)
    (add_net /~RESET0)
    (add_net GNDREF)
  )
  (module w_conn_strip:vasch_strip_4x2 (layer F.Cu) (tedit 5A9C570D)
    (at 74.84 127 180)
    (descr "Box header 4x2pin 2.54mm")
    (tags "CONN DEV")
    (fp_text reference P2 (at -7.71 5.715 180) (layer F.SilkS))
    (fp_text value MY_CONN_I2C (at 0 5.7 180) (layer F.SilkS) hide)
    (pad 8 thru_hole oval (at 3.81 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 34 GNDREF))
    (pad 7 thru_hole oval (at 3.81 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 34 GNDREF))
    (pad 1 thru_hole rect (at -3.81 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 33 /3.3V-I2C))
    (pad 2 thru_hole oval (at -3.81 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 1 /5V))
    (pad 3 thru_hole oval (at -1.27 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 2 /SCL0))
    (pad 4 thru_hole oval (at -1.27 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 3 /~INT0))
    (pad 5 thru_hole oval (at 1.27 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 4 /SDA0))
    (pad 6 thru_hole oval (at 1.27 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 19 /~RESET0))
    (model walter/conn_strip/vasch_strip_4x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_strip:vasch_strip_4x2 (layer F.Cu) (tedit 5A9C5703)
    (at 54.61 69.215)
    (descr "Box header 4x2pin 2.54mm")
    (tags "CONN DEV")
    (fp_text reference P4 (at -7.62 5.715) (layer F.SilkS))
    (fp_text value MY_CONN_I2C (at 0 5.7) (layer F.SilkS) hide)
    (pad 8 thru_hole oval (at 3.81 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 34 GNDREF))
    (pad 7 thru_hole oval (at 3.81 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 34 GNDREF))
    (pad 1 thru_hole rect (at -3.81 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 33 /3.3V-I2C))
    (pad 2 thru_hole oval (at -3.81 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 1 /5V))
    (pad 3 thru_hole oval (at -1.27 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 2 /SCL0))
    (pad 4 thru_hole oval (at -1.27 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 3 /~INT0))
    (pad 5 thru_hole oval (at 1.27 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 4 /SDA0))
    (pad 6 thru_hole oval (at 1.27 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 19 /~RESET0))
    (model walter/conn_strip/vasch_strip_4x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Main:MECH_NPTH_M3 (layer F.Cu) (tedit 579B0774)
    (at 41 68)
    (fp_text reference MP1 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value MECH_NPTH_M3 (at 0 -2.8) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.6) (layers *.Cu *.Mask F.SilkS))
  )
  (module Main:MECH_NPTH_M3 (layer F.Cu) (tedit 579B0774)
    (at 131 68)
    (fp_text reference MP2 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value MECH_NPTH_M3 (at 0 -2.8) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.6) (layers *.Cu *.Mask F.SilkS))
  )
  (module Main:MECH_NPTH_M3 (layer F.Cu) (tedit 579B0774)
    (at 131 128)
    (fp_text reference MP3 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value MECH_NPTH_M3 (at 0 -2.8) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.6) (layers *.Cu *.Mask F.SilkS))
  )
  (module Main:MECH_NPTH_M3 (layer F.Cu) (tedit 579B0774)
    (at 41 128)
    (fp_text reference MP4 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value MECH_NPTH_M3 (at 0 -2.8) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.6) (layers *.Cu *.Mask F.SilkS))
  )
  (module w_conn_strip:vasch_strip_4x2 (layer F.Cu) (tedit 5A9C5715)
    (at 54.52 127 180)
    (descr "Box header 4x2pin 2.54mm")
    (tags "CONN DEV")
    (fp_text reference P1 (at -7.71 5.715 180) (layer F.SilkS))
    (fp_text value MY_CONN_I2C (at 0 5.7 180) (layer F.SilkS) hide)
    (pad 8 thru_hole oval (at 3.81 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 34 GNDREF))
    (pad 7 thru_hole oval (at 3.81 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 34 GNDREF))
    (pad 1 thru_hole rect (at -3.81 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 33 /3.3V-I2C))
    (pad 2 thru_hole oval (at -3.81 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 1 /5V))
    (pad 3 thru_hole oval (at -1.27 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 2 /SCL0))
    (pad 4 thru_hole oval (at -1.27 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 3 /~INT0))
    (pad 5 thru_hole oval (at 1.27 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 4 /SDA0))
    (pad 6 thru_hole oval (at 1.27 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 19 /~RESET0))
    (model walter/conn_strip/vasch_strip_4x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_strip:vasch_strip_4x2 (layer F.Cu) (tedit 5A9C5707)
    (at 74.93 69.215)
    (descr "Box header 4x2pin 2.54mm")
    (tags "CONN DEV")
    (fp_text reference P3 (at -7.62 5.715) (layer F.SilkS))
    (fp_text value MY_CONN_I2C (at 0 5.7) (layer F.SilkS) hide)
    (pad 8 thru_hole oval (at 3.81 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 34 GNDREF))
    (pad 7 thru_hole oval (at 3.81 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 34 GNDREF))
    (pad 1 thru_hole rect (at -3.81 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 33 /3.3V-I2C))
    (pad 2 thru_hole oval (at -3.81 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 1 /5V))
    (pad 3 thru_hole oval (at -1.27 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 2 /SCL0))
    (pad 4 thru_hole oval (at -1.27 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 3 /~INT0))
    (pad 5 thru_hole oval (at 1.27 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 4 /SDA0))
    (pad 6 thru_hole oval (at 1.27 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 19 /~RESET0))
    (model walter/conn_strip/vasch_strip_4x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_pt-1,5:pt_1,5-2-3,5-h (layer F.Cu) (tedit 5A64B54D)
    (at 88.9 126.365)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P6 (at 1.905 -5.08) (layer F.SilkS))
    (fp_text value CONN_2 (at 0 -5) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at -1.75 -0.7) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 34 GNDREF))
    (pad 1 thru_hole rect (at 1.75 -0.7) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 /5V))
    (model walter/conn_pt-1_5/pt_1,5-2-3,5-h.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_pt-1,5:pt_1,5-2-3,5-h (layer F.Cu) (tedit 5A64B549)
    (at 88.9 69.85 180)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P7 (at -1.905 -5.08 180) (layer F.SilkS))
    (fp_text value CONN_2 (at 0 -5 180) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at -1.75 -0.7 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 35 /ALT-3.3V))
    (pad 1 thru_hole rect (at 1.75 -0.7 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 34 GNDREF))
    (model walter/conn_pt-1_5/pt_1,5-2-3,5-h.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A63BBA7)
    (at 85.979 84.455 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP1 (at 2.159 2.54 270) (layer F.SilkS))
    (fp_text value Jumper_NC_Dual (at 0 7.41 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /3.3V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /3.3V-I2C))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /ALT-3.3V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "0 My FriendlyARM:NanoPi-NEO" (layer F.Cu) (tedit 5A9B2758)
    (at 62.23 98.425)
    (fp_text reference M2 (at 0.3175 18) (layer F.SilkS))
    (fp_text value NanoPi-NEO (at 0 8.89 180) (layer F.SilkS))
    (fp_text user CONSOLE (at -16.3195 2.794 90) (layer F.SilkS))
    (fp_text user RX (at -15.4305 1.016 90) (layer F.SilkS))
    (fp_text user TX (at -15.4305 2.413 90) (layer F.SilkS))
    (fp_text user 5 (at -15.4305 3.556 90) (layer F.SilkS))
    (fp_text user G (at -15.4305 4.445 90) (layer F.SilkS))
    (fp_text user U2- (at -16.1925 -3.81 90) (layer F.SilkS))
    (fp_text user U2+ (at -16.1925 -6.35 90) (layer F.SilkS))
    (fp_text user U1- (at -16.1925 -8.89 90) (layer F.SilkS))
    (fp_text user U1+ (at -16.1925 -11.43 90) (layer F.SilkS))
    (fp_text user 5V0 (at -16.1925 -13.97 90) (layer F.SilkS))
    (fp_text user CLK (at 13.0175 13.97 90) (layer F.SilkS))
    (fp_text user MISO (at 13.0175 11.43 90) (layer F.SilkS))
    (fp_text user MOSI (at 13.0175 8.89 90) (layer F.SilkS))
    (fp_text user X (at 13.0175 6.35 90) (layer F.SilkS))
    (fp_text user PA3 (at 13.0175 3.81 90) (layer F.SilkS))
    (fp_text user PA2 (at 13.0175 1.27 90) (layer F.SilkS))
    (fp_text user PA0 (at 13.0175 -1.27 90) (layer F.SilkS))
    (fp_text user GND (at 13.0175 -3.81 90) (layer F.SilkS))
    (fp_text user PG11 (at 13.0175 -6.35 90) (layer F.SilkS))
    (fp_text user SCL (at 13.0175 -8.89 90) (layer F.SilkS))
    (fp_text user SDA (at 13.0175 -11.43 90) (layer F.SilkS))
    (fp_text user CS (at 14.2875 13.97 90) (layer F.SilkS))
    (fp_text user PA1 (at 14.2875 11.43 90) (layer F.SilkS))
    (fp_text user GND (at 14.2875 8.89 90) (layer F.SilkS))
    (fp_text user PG9 (at 14.2875 6.35 90) (layer F.SilkS))
    (fp_text user PG8 (at 14.2875 3.81 90) (layer F.SilkS))
    (fp_text user GND (at 14.2875 1.27 90) (layer F.SilkS))
    (fp_text user PA6 (at 14.2875 -1.27 90) (layer F.SilkS))
    (fp_text user PG7 (at 14.2875 -3.81 90) (layer F.SilkS))
    (fp_text user PG6 (at 14.2875 -6.35 90) (layer F.SilkS))
    (fp_text user X (at 14.2875 -8.89 90) (layer F.SilkS))
    (fp_text user 5V (at 14.2875 -11.43 90) (layer F.SilkS))
    (fp_text user 5V (at 14.2875 -13.97 90) (layer F.SilkS))
    (fp_text user 3VO (at 13.0175 -13.97 90) (layer F.SilkS))
    (pad 40 thru_hole circle (at -15.875 6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /RX))
    (pad 39 thru_hole circle (at -15.875 8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /TX))
    (pad 38 thru_hole circle (at -15.875 11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /5V))
    (pad 37 thru_hole circle (at -15.875 13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 GNDREF))
    (pad 36 thru_hole circle (at -18.415 13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 GNDREF))
    (pad 35 thru_hole circle (at -18.415 11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /I2S0-SDIN))
    (pad 34 thru_hole circle (at -18.415 8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /I2S0-SDOUT))
    (pad 33 thru_hole circle (at -18.415 6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /I2S0-BCK))
    (pad 32 thru_hole circle (at -18.415 3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /I2S0-LRCK))
    (pad 31 thru_hole circle (at -18.415 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /GPIOA17))
    (pad 30 thru_hole circle (at -18.415 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /GPIOL11))
    (pad 29 thru_hole circle (at -18.415 -3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /USB2-D-))
    (pad 28 thru_hole circle (at -18.415 -6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /USB2-D+))
    (pad 27 thru_hole circle (at -18.415 -8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /USB1-D-))
    (pad 26 thru_hole circle (at -18.415 -11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /USB1-D+))
    (pad 24 thru_hole circle (at 19.05 13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /GPIOC3))
    (pad 22 thru_hole circle (at 19.05 11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /GPIOA1))
    (pad 20 thru_hole circle (at 19.05 8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 GNDREF))
    (pad 18 thru_hole circle (at 19.05 6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /GPIOG9))
    (pad 16 thru_hole circle (at 19.05 3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /GPIOG8))
    (pad 14 thru_hole circle (at 19.05 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 GNDREF))
    (pad 12 thru_hole circle (at 19.05 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GPIOA6))
    (pad 10 thru_hole circle (at 19.05 -3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /GPIOG7))
    (pad 8 thru_hole circle (at 19.05 -6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /GPIOG6))
    (pad 6 thru_hole circle (at 19.05 -8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 19.05 -11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /5V))
    (pad 25 thru_hole circle (at -18.415 -13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /5V))
    (pad 23 thru_hole circle (at 16.51 13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /GPIOC2))
    (pad 21 thru_hole circle (at 16.51 11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /GPIOC1))
    (pad 1 thru_hole circle (at 16.51 -13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /3.3V))
    (pad "" np_thru_hole circle (at -17.3825 17.7) (size 4 4) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 18.0175 17.7) (size 4 4) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 18.0175 -17.7) (size 4 4) (drill 3.2) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 19.05 -13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /5V))
    (pad 3 thru_hole circle (at 16.51 -11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /SDA0))
    (pad 5 thru_hole circle (at 16.51 -8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /SCL0))
    (pad 7 thru_hole circle (at 16.51 -6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /GPIOG11))
    (pad 9 thru_hole circle (at 16.51 -3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 GNDREF))
    (pad 11 thru_hole circle (at 16.51 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /GPIOA0))
    (pad 13 thru_hole circle (at 16.51 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /GPIOA2))
    (pad 15 thru_hole circle (at 16.51 3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /GPIOA3))
    (pad 17 thru_hole circle (at 16.51 6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 16.51 8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /GPIOC0))
    (pad "" np_thru_hole circle (at -17.3825 -17.7) (size 4 4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module "0 My FriendlyARM:NanoPi-NEO-mirrored" (layer F.Cu) (tedit 5A9B2052)
    (at 109.22 98.425)
    (fp_text reference M1 (at 0.3175 18) (layer F.SilkS))
    (fp_text value NanoPi-NEO (at 0.6175 -0.1) (layer F.SilkS))
    (fp_text user CONSOLE (at 16.9545 2.794 270) (layer F.SilkS))
    (fp_text user RX (at 16.0655 1.016 270) (layer F.SilkS))
    (fp_text user TX (at 16.0655 2.413 270) (layer F.SilkS))
    (fp_text user 5 (at 16.0655 3.556 270) (layer F.SilkS))
    (fp_text user G (at 16.0655 4.445 270) (layer F.SilkS))
    (fp_text user U2- (at 16.8275 -3.81 270) (layer F.SilkS))
    (fp_text user U2+ (at 16.8275 -6.35 270) (layer F.SilkS))
    (fp_text user U1- (at 16.8275 -8.89 270) (layer F.SilkS))
    (fp_text user U1+ (at 16.8275 -11.43 270) (layer F.SilkS))
    (fp_text user 5V0 (at 16.8275 -13.97 270) (layer F.SilkS))
    (fp_text user CLK (at -12.3825 13.97 270) (layer F.SilkS))
    (fp_text user MISO (at -12.3825 11.43 270) (layer F.SilkS))
    (fp_text user MOSI (at -12.3825 8.89 270) (layer F.SilkS))
    (fp_text user X (at -12.3825 6.35 90) (layer F.SilkS))
    (fp_text user PA3 (at -12.3825 3.81 270) (layer F.SilkS))
    (fp_text user PA2 (at -12.3825 1.27 270) (layer F.SilkS))
    (fp_text user PA0 (at -12.3825 -1.27 270) (layer F.SilkS))
    (fp_text user GND (at -12.3825 -3.81 270) (layer F.SilkS))
    (fp_text user PG11 (at -12.3825 -6.35 270) (layer F.SilkS))
    (fp_text user SCL (at -12.3825 -8.89 270) (layer F.SilkS))
    (fp_text user SDA (at -12.3825 -11.43 270) (layer F.SilkS))
    (fp_text user CS (at -13.6525 13.97 270) (layer F.SilkS))
    (fp_text user PA1 (at -13.6525 11.43 270) (layer F.SilkS))
    (fp_text user GND (at -13.6525 8.89 270) (layer F.SilkS))
    (fp_text user PG9 (at -13.6525 6.35 270) (layer F.SilkS))
    (fp_text user PG8 (at -13.6525 3.81 270) (layer F.SilkS))
    (fp_text user GND (at -13.6525 1.27 270) (layer F.SilkS))
    (fp_text user PA6 (at -13.6525 -1.27 270) (layer F.SilkS))
    (fp_text user PG7 (at -13.6525 -3.81 270) (layer F.SilkS))
    (fp_text user PG6 (at -13.6525 -6.35 270) (layer F.SilkS))
    (fp_text user X (at -13.6525 -8.89 90) (layer F.SilkS))
    (fp_text user 5V (at -13.6525 -11.43 270) (layer F.SilkS))
    (fp_text user 5V (at -13.6525 -13.97 270) (layer F.SilkS))
    (fp_text user 3VO (at -12.3825 -13.97 270) (layer F.SilkS))
    (pad 40 thru_hole circle (at 16.51 6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /RX))
    (pad 39 thru_hole circle (at 16.51 8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /TX))
    (pad 38 thru_hole circle (at 16.51 11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /5V))
    (pad 37 thru_hole circle (at 16.51 13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 GNDREF))
    (pad 36 thru_hole circle (at 19.05 13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 GNDREF))
    (pad 35 thru_hole circle (at 19.05 11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /I2S0-SDIN))
    (pad 34 thru_hole circle (at 19.05 8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /I2S0-SDOUT))
    (pad 33 thru_hole circle (at 19.05 6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /I2S0-BCK))
    (pad 32 thru_hole circle (at 19.05 3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /I2S0-LRCK))
    (pad 31 thru_hole circle (at 19.05 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /GPIOA17))
    (pad 30 thru_hole circle (at 19.05 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /GPIOL11))
    (pad 29 thru_hole circle (at 19.05 -3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /USB2-D-))
    (pad 28 thru_hole circle (at 19.05 -6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /USB2-D+))
    (pad 27 thru_hole circle (at 19.05 -8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /USB1-D-))
    (pad 26 thru_hole circle (at 19.05 -11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /USB1-D+))
    (pad 24 thru_hole circle (at -18.415 13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /GPIOC3))
    (pad 22 thru_hole circle (at -18.415 11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /GPIOA1))
    (pad 20 thru_hole circle (at -18.415 8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 GNDREF))
    (pad 18 thru_hole circle (at -18.415 6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /GPIOG9))
    (pad 16 thru_hole circle (at -18.415 3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /GPIOG8))
    (pad 14 thru_hole circle (at -18.415 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 GNDREF))
    (pad 12 thru_hole circle (at -18.415 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GPIOA6))
    (pad 10 thru_hole circle (at -18.415 -3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /GPIOG7))
    (pad 8 thru_hole circle (at -18.415 -6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /GPIOG6))
    (pad 6 thru_hole circle (at -18.415 -8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -18.415 -11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /5V))
    (pad 25 thru_hole circle (at 19.05 -13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /5V))
    (pad 23 thru_hole circle (at -15.875 13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /GPIOC2))
    (pad 21 thru_hole circle (at -15.875 11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /GPIOC1))
    (pad 1 thru_hole circle (at -15.875 -13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /3.3V))
    (pad "" np_thru_hole circle (at 18.0175 17.7) (size 4 4) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -17.3825 17.7) (size 4 4) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -17.3825 -17.7) (size 4 4) (drill 3.2) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -18.415 -13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /5V))
    (pad 3 thru_hole circle (at -15.875 -11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /SDA0))
    (pad 5 thru_hole circle (at -15.875 -8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /SCL0))
    (pad 7 thru_hole circle (at -15.875 -6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /GPIOG11))
    (pad 9 thru_hole circle (at -15.875 -3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 GNDREF))
    (pad 11 thru_hole circle (at -15.875 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /GPIOA0))
    (pad 13 thru_hole circle (at -15.875 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /GPIOA2))
    (pad 15 thru_hole circle (at -15.875 3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /GPIOA3))
    (pad 17 thru_hole circle (at -15.875 6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at -15.875 8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /GPIOC0))
    (pad "" np_thru_hole circle (at 18.0175 -17.7) (size 4 4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Connectors_JST:JST_XH_S04B-XH-A_04x2.50mm_Angled (layer F.Cu) (tedit 58EAE850)
    (at 120.65 81.28 180)
    (descr "JST XH series connector, S04B-XH-A, side entry type, through hole")
    (tags "connector jst xh tht side horizontal angled 2.50mm")
    (fp_text reference P5 (at 3.75 -3.5 180) (layer F.SilkS))
    (fp_text value CONN_4 (at 3.75 10.3 180) (layer F.Fab))
    (fp_text user %R (at 3.75 2.25 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 34 GNDREF))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 /5V))
    (pad 3 thru_hole circle (at 5 0 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 21 /TX))
    (pad 4 thru_hole circle (at 7.5 0 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 20 /RX))
    (model Connectors_JST.3dshapes/JST_XH_S04B-XH-A_04x2.50mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_strip_4-90 (layer F.Cu) (tedit 0)
    (at 102.235 81.28 180)
    (descr "Pin strip 4pin 90")
    (tags "CONN DEV")
    (fp_text reference P8 (at 0 -2.159 180) (layer F.SilkS))
    (fp_text value CONN_4 (at 0.254 -3.556 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -3.81 0 180) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 34 GNDREF))
    (pad 2 thru_hole oval (at -1.27 0 180) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 /5V))
    (pad 3 thru_hole oval (at 1.27 0 180) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 21 /TX))
    (pad 4 thru_hole oval (at 3.81 0 180) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 20 /RX))
    (model walter/pin_strip/pin_strip_4-90.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A9C57F8)
    (at 71.755 96.52 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference "R1 100" (at 5.08 -2.31 180) (layer F.SilkS))
    (fp_text value 100 (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /GPIOA6))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /~INT0))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A9C5806)
    (at 71.755 92.075 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference "R2 10K" (at 5.08 2.159 180) (layer F.SilkS))
    (fp_text value 10K (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /3.3V))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /~INT0))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A9C5800)
    (at 61.595 100.965)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference "R3 100" (at 5.08 -6.604) (layer F.SilkS))
    (fp_text value 100 (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /~RESET0))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /GPIOG8))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A9C5810)
    (at 61.595 86.36)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference "R4 4.7K" (at 5.08 -1.905) (layer F.SilkS))
    (fp_text value 4.7K (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /3.3V))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /SCL0))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A9C5818)
    (at 61.595 82.55)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference "R5 4.7K" (at 5.08 -2.159) (layer F.SilkS))
    (fp_text value 4.7K (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /3.3V))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /SDA0))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_logo:Logo_silk_CC-BY-NC-SA_10x3.6mm (layer F.Cu) (tedit 0)
    (at 124.46 122.555)
    (descr "CC BY-NC-SA logo, 10x3.6mm")
    (fp_text reference LIC1 (at 0.3 -1.4) (layer F.SilkS) hide)
    (fp_text value CC-BY-NC-SA-icon (at 0.3 0.5) (layer F.SilkS) hide)
  )
  (module Symbols:KiCad-Logo2_8mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 109.22 106.68 180)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo2_8mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (gr_text "(3V)	" (at 114.554 67.945) (layer F.SilkS))
  (gr_text "(3V)	" (at 99.949 67.945) (layer F.SilkS))
  (gr_text I2C (at 53.34 74.93) (layer F.SilkS))
  (gr_text I2C (at 73.66 74.93) (layer F.SilkS))
  (gr_text I2C (at 73.66 121.285) (layer F.SilkS))
  (gr_text I2C (at 53.34 121.285) (layer F.SilkS))
  (gr_text "GND	" (at 120.65 64.77 90) (layer F.SilkS))
  (gr_text 5V (at 118.11 65.405 90) (layer F.SilkS))
  (gr_text TX (at 115.57 65.405 90) (layer F.SilkS))
  (gr_text RX (at 113.03 65.405 90) (layer F.SilkS))
  (gr_text SCL (at 55.245 86.36) (layer F.SilkS))
  (gr_text SDA (at 55.245 82.55) (layer F.SilkS))
  (gr_text ~RESET (at 55.245 100.965) (layer F.SilkS))
  (gr_text ~INT (at 55.245 94.615) (layer F.SilkS))
  (gr_text "GND	" (at 106.045 64.77 90) (layer F.SilkS))
  (gr_text 5V (at 103.505 65.405 90) (layer F.SilkS))
  (gr_text Peripherals (at 62.23 109.22) (layer F.SilkS))
  (gr_text NEO (at 85.725 87.63) (layer F.SilkS))
  (gr_text Alt (at 85.725 76.2) (layer F.SilkS))
  (gr_text "I2C 3.3V SRC ->" (at 85.725 99.695 90) (layer F.SilkS))
  (gr_text TX (at 100.965 65.405 90) (layer F.SilkS))
  (gr_text RX (at 98.425 65.405 90) (layer F.SilkS))
  (gr_text "NanoPi NEO\nAdapter" (at 108.585 129.54) (layer F.SilkS))
  (gr_text v3 (at 118.745 130.81) (layer F.SilkS))
  (gr_text by (at 108.585 123.19) (layer F.SilkS))
  (gr_text jeditekunum (at 108.585 125.095) (layer F.SilkS))
  (gr_text "Alt 3.3V" (at 94.615 69.85 90) (layer F.SilkS))
  (gr_text + (at 90.805 131.445) (layer F.SilkS))
  (gr_text - (at 86.995 131.445) (layer F.SilkS))
  (gr_text 5V (at 94.615 126.365) (layer F.SilkS))
  (gr_text + (at 91.44 64.77) (layer F.SilkS))
  (gr_text - (at 86.995 64.77) (layer F.SilkS))
  (gr_line (start 37 62) (end 135 62) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 37 134) (end 135 134) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 100 (width 0.3) (layer Cmts.User)
    (gr_text "100.000 mm" (at 86 53.65) (layer Cmts.User))
    (feature1 (pts (xy 136 64) (xy 136 52.3)))
    (feature2 (pts (xy 36 64) (xy 36 52.3)))
    (crossbar (pts (xy 36 55) (xy 136 55)))
    (arrow1a (pts (xy 136 55) (xy 134.873496 55.586421)))
    (arrow1b (pts (xy 136 55) (xy 134.873496 54.413579)))
    (arrow2a (pts (xy 36 55) (xy 37.126504 55.586421)))
    (arrow2b (pts (xy 36 55) (xy 37.126504 54.413579)))
  )
  (gr_arc (start 135 133) (end 136 133) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 135 63) (end 135 62) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136 133) (end 136 63) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 37 63) (end 36 63) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 37 133) (end 37 134) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 60 (width 0.3) (layer Cmts.User)
    (gr_text "60.000 mm" (at 31 98 90) (layer Cmts.User))
    (feature1 (pts (xy 40 68) (xy 29.3 68)))
    (feature2 (pts (xy 40 128) (xy 29.3 128)))
    (crossbar (pts (xy 32 128) (xy 32 68)))
    (arrow1a (pts (xy 32 68) (xy 32.586421 69.126504)))
    (arrow1b (pts (xy 32 68) (xy 31.413579 69.126504)))
    (arrow2a (pts (xy 32 128) (xy 32.586421 126.873496)))
    (arrow2b (pts (xy 32 128) (xy 31.413579 126.873496)))
  )
  (gr_line (start 36 63) (end 36 133) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 72 (width 0.3) (layer Cmts.User)
    (gr_text "72.000 mm" (at 26.65 98 90) (layer Cmts.User))
    (feature1 (pts (xy 33 62) (xy 25.3 62)))
    (feature2 (pts (xy 33 134) (xy 25.3 134)))
    (crossbar (pts (xy 28 134) (xy 28 62)))
    (arrow1a (pts (xy 28 62) (xy 28.586421 63.126504)))
    (arrow1b (pts (xy 28 62) (xy 27.413579 63.126504)))
    (arrow2a (pts (xy 28 134) (xy 28.586421 132.873496)))
    (arrow2b (pts (xy 28 134) (xy 27.413579 132.873496)))
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136 134) (xy 36 134) (xy 36 62) (xy 136 62)
      )
    )
    (polygon
      (pts        (xy 38 63) (xy 38 133) (xy 95 133) (xy 95 121) (xy 124 121)
        (xy 124 133) (xy 134 133) (xy 134 63) (xy 124 63) (xy 124 63.3)
        (xy 95 63.3) (xy 95 63)
      )
    )
  )
)
