(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (grid_origin 89 117)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/HS")
  (net 2 "GND")
  (net 3 "Net-(D3-Pad2)")
  (net 4 "Net-(J1-Pad1)")
  (net 5 "Net-(J2-Pad1)")
  (net 6 "Net-(H1-Pad1)")
  (net 7 "Net-(J3-Pad1)")
  (net 8 "unconnected-(J6-PadS1)")
  (net 9 "unconnected-(J6-PadS2)")
  (net 10 "unconnected-(J8-PadS1)")
  (net 11 "unconnected-(J8-PadS2)")
  (net 12 "unconnected-(J9-PadS1)")
  (net 13 "unconnected-(J9-PadS2)")
  (net 14 "Net-(C2-Pad1)")
  (net 15 "unconnected-(J7-PadS1)")
  (net 16 "unconnected-(J7-PadS2)")
  (net 17 "Net-(PS1-Pad3)")
  (net 18 "unconnected-(PS1-Pad6)")
  (net 19 "/-12V")
  (net 20 "/+12V")
  (net 21 "Net-(C1-Pad1)")
  (net 22 "Net-(C3-Pad2)")
  (net 23 "Net-(C3-Pad1)")
  (footprint "MountingHole:MountingHole_4.3mm_M4_Pad_Via" (layer "F.Cu")
    (tedit 56DDBFD7)
    (at 129 106.5)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (zone_connect 2)
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -5.3) (layer "F.SilkS"))
    (fp_text value "C-" (at 6 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -3.225 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 -3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 3.225 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 59 67)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "XT60PW-F:AMASS_XT60PW-F" (layer "F.Cu")
    (tedit 62CE43DE)
    (at 153.75 79 90)
    (property "MANUFACTURER" "AMASS")
    (property "MAXIMUM_PACKAGE_HEIGHT" "8.4 mm")
    (property "PARTREV" "V1.2")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (zone_connect 2)
    (attr through_hole)
    (fp_text reference "J7" (at 0 5.75 180) (layer "F.SilkS"))
    (fp_text value "XT60PW-F" (at 1.14 16.385 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3.6 0 90) (size 3.716 3.716) (drill 2.7) (layers *.Cu *.Mask)
      (net 1 "/HS") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole circle (at -3.6 0 90) (size 3.716 3.716) (drill 2.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "-") (pintype "passive"))
    (pad "S1" thru_hole oval (at -6.75 6 90) (size 1.3 2.6) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 15 "unconnected-(J7-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S2" thru_hole oval (at 6.75 6 90) (size 1.3 2.6) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 16 "unconnected-(J7-PadS2)") (pinfunction "SHIELD") (pintype "passive"))
    (model "D:/Documents/KiCad/6.0/footprints/XT60PW-F.pretty/XT60PW-F.step"
      (offset (xyz 0 -15.5 4))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 100.75 138)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "XT60PW-F:AMASS_XT60PW-F" (layer "F.Cu")
    (tedit 62CE43DE)
    (at 65.25 79 -90)
    (property "MANUFACTURER" "AMASS")
    (property "MAXIMUM_PACKAGE_HEIGHT" "8.4 mm")
    (property "PARTREV" "V1.2")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (zone_connect 2)
    (attr through_hole)
    (fp_text reference "J6" (at 0 6.25) (layer "F.SilkS"))
    (fp_text value "XT60PW-F" (at 1.14 16.385 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3.6 0 270) (size 3.716 3.716) (drill 2.7) (layers *.Cu *.Mask)
      (net 1 "/HS") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole circle (at -3.6 0 270) (size 3.716 3.716) (drill 2.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "-") (pintype "passive"))
    (pad "S1" thru_hole oval (at -6.75 6 270) (size 1.3 2.6) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 8 "unconnected-(J6-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S2" thru_hole oval (at 6.75 6 270) (size 1.3 2.6) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 9 "unconnected-(J6-PadS2)") (pinfunction "SHIELD") (pintype "passive"))
    (model "D:/Documents/KiCad/6.0/footprints/XT60PW-F.pretty/XT60PW-F.step"
      (offset (xyz 0 -15.5 4))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 100.75 126)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140 81 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 3.5 1.5 180) (layer "F.SilkS"))
    (fp_text value "4.7μF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(C3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4_Pad_Via" (layer "F.Cu")
    (tedit 56DDBFD7)
    (at 129 119.5)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -5.3) (layer "F.SilkS"))
    (fp_text value "B-" (at 6 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask)
      (net 6 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -3.225 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 3.225 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 -3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140 66.5 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "1000pF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 23 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 20 "/+12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 160 138)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 102.5 109.5)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "0.22μF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 21 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "/HS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "XT60PW-F:AMASS_XT60PW-M" locked (layer "F.Cu")
    (tedit 63016512)
    (at 159.5 126 -90)
    (property "MANUFACTURER" "AMASS")
    (property "MAXIMUM_PACKAGE_HEIGHT" "8.4 mm")
    (property "PARTREV" "V1.2")
    (property "STANDARD" "Manufacturer recommendations")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 0 -180) (layer "F.SilkS"))
    (fp_text value "XT60PW-M" (at 0.9054 -12.0434 -270) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 3.6 6 270) (size 3.716 3.716) (drill 2.7) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -3.6 6 270) (size 3.716 3.716) (drill 2.7) (layers *.Cu *.Mask)
      (net 6 "Net-(H1-Pad1)") (pinfunction "-") (pintype "passive"))
    (pad "S1" thru_hole oval locked (at 6.75 0 270) (size 1.2 2.4) (drill oval 0.6 1.7) (layers *.Cu *.Mask))
    (pad "S2" thru_hole oval locked (at -6.75 0 270) (size 1.2 2.4) (drill oval 0.6 1.7) (layers *.Cu *.Mask))
    (model "D:/Documents/KiCad/6.0/footprints/XT60PW-M.pretty/XT60PW-M.step"
      (offset (xyz 0 9.3 4))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (footprint "SamacSys_Parts:LPS6235123MRC" (layer "F.Cu")
    (tedit 0)
    (at 144.5 88 180)
    (descr "LPS6235-123MRC-1")
    (tags "Inductor")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "L2" (at 0 -5.5) (layer "F.SilkS"))
    (fp_text value "12μF" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.15 0 180) (size 2.3 6.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 2.15 0 180) (size 2.3 6.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(C3-Pad2)") (pinfunction "2") (pintype "passive"))
  )
  (footprint "XT60PW-F:AMASS_XT60PW-F" (layer "F.Cu")
    (tedit 62CE43DE)
    (at 65.25 97.2375 -90)
    (property "MANUFACTURER" "AMASS")
    (property "MAXIMUM_PACKAGE_HEIGHT" "8.4 mm")
    (property "PARTREV" "V1.2")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (zone_connect 2)
    (attr through_hole)
    (fp_text reference "J9" (at -0.2375 6.25) (layer "F.SilkS"))
    (fp_text value "XT60PW-F" (at 1.14 16.385 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3.6 0 270) (size 3.716 3.716) (drill 2.7) (layers *.Cu *.Mask)
      (net 1 "/HS") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole circle (at -3.6 0 270) (size 3.716 3.716) (drill 2.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "-") (pintype "passive"))
    (pad "S1" thru_hole oval (at -6.75 6 270) (size 1.3 2.6) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 12 "unconnected-(J9-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S2" thru_hole oval (at 6.75 6 270) (size 1.3 2.6) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 13 "unconnected-(J9-PadS2)") (pinfunction "SHIELD") (pintype "passive"))
    (model "D:/Documents/KiCad/6.0/footprints/XT60PW-F.pretty/XT60PW-F.step"
      (offset (xyz 0 -15.5 4))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "SamacSys_Parts:2MS6T1B3M2QES" (layer "F.Cu")
    (tedit 0)
    (at 146 99 90)
    (descr "2MS6T1B3M2QES-3")
    (tags "Switch")
    (property "Description" "Toggle Switches SPST OFF-ON")
    (property "Height" "23.63")
    (property "Manufacturer_Name" "Dailywell")
    (property "Manufacturer_Part_Number" "2MS6T1B3M2QES")
    (property "Mouser Part Number" "118-2MS6T1B3M2QES")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Dailywell/2MS6T1B3M2QES?qs=B6kkDfuK7%2FCLnLIcqzvQEQ%3D%3D")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "S1" (at 0 -2.123 90) (layer "F.SilkS"))
    (fp_text value "2MS6T1B3M2QES" (at 0 -2.123 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.123 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 0 -5.08 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 17 "Net-(PS1-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "D:\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\2MS6T1B3M2QES.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 118.25 138)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "SamacSys_Parts:LPS6235123MRC" (layer "F.Cu")
    (tedit 0)
    (at 147 68.5 180)
    (descr "LPS6235-123MRC-1")
    (tags "Inductor")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "L1" (at -6 1) (layer "F.SilkS"))
    (fp_text value "12μF" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.15 0 180) (size 2.3 6.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(C2-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 2.15 0 180) (size 2.3 6.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(C3-Pad1)") (pinfunction "2") (pintype "passive"))
  )
  (footprint "XT60PW-F:AMASS_XT60-F" (layer "F.Cu")
    (tedit 6303BD90)
    (at 154.5 110.5)
    (property "MANUFACTURER" "AMASS")
    (property "PARTREV" "1.2")
    (property "STANDARD" "IPC-7251")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (zone_connect 2)
    (attr through_hole)
    (fp_text reference "J5" (at -4.92842 -5.03849) (layer "F.SilkS"))
    (fp_text value "XT60-F" (at -0.48032 4.968395) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 3.6 0) (size 5.516 5.516) (drill 4.5) (layers *.Cu *.Mask)
      (net 1 "/HS") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole circle (at -3.6 0) (size 5.516 5.516) (drill 4.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "-") (pintype "passive"))
    (model "D:/Documents/KiCad/6.0/footprints/XT60.pretty/XT60-F.step"
      (offset (xyz 1.5 0 8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (footprint "SamacSys_Parts:JTL6048S15" (layer "F.Cu")
    (tedit 0)
    (at 133.86 70.38 -90)
    (descr "JTL6048S15-4")
    (tags "Undefined or Miscellaneous")
    (property "Description" "XP POWER - JTL6048S15 - DC-DC CONVERTER, 15V, 4A")
    (property "Height" "12")
    (property "Manufacturer_Name" "XP POWER")
    (property "Manufacturer_Part_Number" "JTL6048S15")
    (property "Mouser Part Number" "209-JTL6048S15")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/XP-Power/JTL6048S15?qs=w%2Fv1CP2dgqpuhtR6ox8pSA%3D%3D")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (zone_connect 2)
    (attr through_hole)
    (fp_text reference "PS1" (at 7.62 22.86 -90) (layer "F.SilkS"))
    (fp_text value "JTL6048S15" (at 7.62 22.86 -90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 7.62 22.86 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 23 "Net-(C3-Pad1)") (pinfunction "+VIN") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5.08 0 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 22 "Net-(C3-Pad2)") (pinfunction "-VIN") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 15.24 0 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "Net-(PS1-Pad3)") (pinfunction "REMOTE_ON/OFF") (pintype "passive"))
    (pad "4" thru_hole circle locked (at -2.54 45.72 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 20 "/+12V") (pinfunction "+VOUT") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 7.62 45.72 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 19 "/-12V") (pinfunction "-VOUT") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 17.78 45.72 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 "unconnected-(PS1-Pad6)") (pinfunction "TRIM") (pintype "passive"))
    (model "D:\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\JTL6048S15.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 160 67)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "SamacSys_Parts:AK3066CY" (layer "F.Cu")
    (tedit 0)
    (at 98.5 102 180)
    (descr "AK3-066C-Y-1")
    (tags "TVS Diode (Bi-directional)")
    (property "Description" "ESD Suppressors / TVS Diodes TVS DIODE AXIAL")
    (property "Height" "11")
    (property "Manufacturer_Name" "LITTELFUSE")
    (property "Manufacturer_Part_Number" "AK3-066C-Y")
    (property "Mouser Part Number" "576-AK3-066C-Y")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Littelfuse/AK3-066C-Y?qs=P1JMDcb91o7SsHSLqUW48g%3D%3D")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (zone_connect 2)
    (attr through_hole)
    (fp_text reference "D1" (at 12.074 0 180) (layer "F.SilkS"))
    (fp_text value "AK3-066C-Y" (at 12.074 0 180) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 12.074 0 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 2.205 2.205) (drill 1.47) (layers *.Cu *.Mask)
      (net 1 "/HS") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 24.15 0 180) (size 2.205 2.205) (drill 1.47) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
  )
  (footprint "B2B-XH-A_LF__SN_:JST_B2B-XH-A(LF)(SN)" (layer "F.Cu")
    (tedit 62CEDF5E)
    (at 80 85.5 90)
    (property "AVAILABILITY" "In Stock")
    (property "DESCRIPTION" "Connector Header Through Hole 2 position 0.098 (2.50mm)")
    (property "MF" "JST Sales")
    (property "MP" "B2B-XH-A(LF)(SN)")
    (property "PACKAGE" "None")
    (property "PRICE" "None")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (zone_connect 2)
    (attr through_hole)
    (fp_text reference "J4" (at -5 0 180) (layer "F.SilkS"))
    (fp_text value "B2B-XH-A(LF)(SN)" (at 8.75 4.11 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 1.25 0 90) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/+12V") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -1.25 0 90) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/-12V") (pinfunction "2") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 59 138)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140 76 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at -1.5 -2.5 180) (layer "F.SilkS"))
    (fp_text value "470pF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 23 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 19 "/-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SamacSys_Parts:DIOM7959X262N" (layer "F.Cu")
    (tedit 0)
    (at 79.5 70 -90)
    (descr "SMDJ")
    (tags "TVS Diode (Uni-directional)")
    (property "Description" "TVS Diode Single Uni-Dir 17V 3KW 2-Pin SMC T/R")
    (property "Height" "2.62")
    (property "Manufacturer_Name" "LITTELFUSE")
    (property "Manufacturer_Part_Number" "SMDJ17A")
    (property "Mouser Part Number" "")
    (property "Mouser Price/Stock" "")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at 0 0) (layer "F.SilkS"))
    (fp_text value "SMDJ17A" (at 0 0 -90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -3.5 0 270) (size 2.2 3.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/+12V") (pintype "power_in"))
    (pad "2" smd rect locked (at 3.5 0 270) (size 2.2 3.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/-12V") (pintype "power_in"))
    (model "D:\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\SMDJ17A.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 118.25 126)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "XT60PW-F:AMASS_XT60PW-M" (layer "F.Cu")
    (tedit 63016512)
    (at 59.5 126 90)
    (property "MANUFACTURER" "AMASS")
    (property "MAXIMUM_PACKAGE_HEIGHT" "8.4 mm")
    (property "PARTREV" "V1.2")
    (property "STANDARD" "Manufacturer recommendations")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (zone_connect 2)
    (attr through_hole)
    (fp_text reference "J2" (at 0 0 180) (layer "F.SilkS"))
    (fp_text value "XT60PW-M" (at 0.9054 -12.0434 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 3.6 6 90) (size 3.716 3.716) (drill 2.7) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)") (pinfunction "+") (pintype "passive") (zone_connect 2))
    (pad "2" thru_hole circle (at -3.6 6 90) (size 3.716 3.716) (drill 2.7) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)") (pinfunction "-") (pintype "passive") (zone_connect 2))
    (pad "S1" thru_hole oval (at 6.75 0 90) (size 1.2 2.4) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad "S2" thru_hole oval (at -6.75 0 90) (size 1.2 2.4) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (zone_connect 2))
    (model "D:/Documents/KiCad/6.0/footprints/XT60PW-M.pretty/XT60PW-M.step"
      (offset (xyz 0 9.3 4))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 81 78)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "1000pF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 19 "/-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "benbokser:FT Power Switch" locked (layer "F.Cu")
    (tedit 0)
    (at 109.5 112.5 90)
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (zone_connect 2)
    (attr through_hole)
    (fp_text reference "SW1" (at -7.5 0 unlocked) (layer "F.SilkS"))
    (fp_text value "FT_Power_Switch" (at 0 4.445 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 8.89 2.54 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at -3 0 90) (size 3 5.5) (drill oval 1.3 4) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole roundrect locked (at 3 0 90) (size 3 5.5) (drill oval 1.3 4) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 "/HS") (pintype "passive"))
    (model "D:/Documents/KiCad/6.0/footprints/benbokser.pretty/MINI POWER SWITCH.STEP"
      (offset (xyz 1.9 -0.4 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (footprint "SamacSys_Parts:CAPC3225X270N" (layer "F.Cu")
    (tedit 0)
    (at 146.5 80.5 -90)
    (descr "325")
    (tags "Capacitor")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -3 180) (layer "F.SilkS"))
    (fp_text value "4.7μF" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.35 0 270) (size 1.22 2.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.35 0 270) (size 1.22 2.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "D:\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\HMK325C7475KM-PE.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 118.5 107 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at -2.95625 0) (layer "F.SilkS"))
    (fp_text value "22kΩ" (at 0 -2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(D3-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "/HS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_2512_6332Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 101.5 116.5 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (zone_connect 1)
    (attr smd)
    (fp_text reference "R3" (at 0 -2.62) (layer "F.SilkS"))
    (fp_text value "290Ω" (at 0 2.62) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.9625 0 180) (size 1.225 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.204082)
      (net 5 "Net-(J2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.9625 0 180) (size 1.225 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.204082)
      (net 21 "Net-(C1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 118.5 104.5)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D3" (at 2.95625 0) (layer "F.SilkS"))
    (fp_text value "LED" (at -0.05 -2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(D3-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "benbokser:AC03000003600JAC00" (layer "F.Cu")
    (tedit 0)
    (at 79 129.5 90)
    (descr "B12")
    (tags "Resistor")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (zone_connect 2)
    (attr through_hole)
    (fp_text reference "R1" (at 10 0 90) (layer "F.SilkS"))
    (fp_text value "360Ω" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 20 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 1 "/HS") (pintype "passive"))
    (model "D:/Documents/KiCad/6.0/footprints/benbokser.pretty/AC03000003600JAC00.STEP"
      (offset (xyz 10 0 2.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "XT60PW-F:AMASS_XT60PW-F" (layer "F.Cu")
    (tedit 62CE43DE)
    (at 153.75 97.2625 90)
    (property "MANUFACTURER" "AMASS")
    (property "MAXIMUM_PACKAGE_HEIGHT" "8.4 mm")
    (property "PARTREV" "V1.2")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (zone_connect 2)
    (attr through_hole)
    (fp_text reference "J8" (at 0.2625 5.75 180) (layer "F.SilkS"))
    (fp_text value "XT60PW-F" (at 1.14 16.385 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3.6 0 90) (size 3.716 3.716) (drill 2.7) (layers *.Cu *.Mask)
      (net 1 "/HS") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole circle (at -3.6 0 90) (size 3.716 3.716) (drill 2.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "-") (pintype "passive"))
    (pad "S1" thru_hole oval (at -6.75 6 90) (size 1.3 2.6) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 10 "unconnected-(J8-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S2" thru_hole oval (at 6.75 6 90) (size 1.3 2.6) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 11 "unconnected-(J8-PadS2)") (pinfunction "SHIELD") (pintype "passive"))
    (model "D:/Documents/KiCad/6.0/footprints/XT60PW-F.pretty/XT60PW-F.step"
      (offset (xyz 0 -15.5 4))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "B2B-XH-A_LF__SN_:JST_B2B-XH-A(LF)(SN)" (layer "F.Cu")
    (tedit 62CEDF5E)
    (at 87 124 -90)
    (property "AVAILABILITY" "In Stock")
    (property "DESCRIPTION" "Connector Header Through Hole 2 position 0.098 (2.50mm)")
    (property "MF" "JST Sales")
    (property "MP" "B2B-XH-A(LF)(SN)")
    (property "PACKAGE" "None")
    (property "PRICE" "None")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -5 0 90) (layer "F.SilkS"))
    (fp_text value "B2B-XH-A(LF)(SN)" (at 7.5 0 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 1.25 0 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -1.25 0 270) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)") (pinfunction "2") (pintype "passive"))
  )
  (footprint "SamacSys_Parts:FUSC3216X123N" (layer "F.Cu")
    (tedit 0)
    (at 147.5 76 180)
    (descr "SF-1206s4")
    (tags "Fuse")
    (property "Description" "BOURNS - SF-1206S1000W-2 - Fuse, Surface Mount, Wire Core, 10 A, SinglFuse SF-1206SxxxW Series, 32 V, Slow Blow, 1206")
    (property "Height" "1.23")
    (property "Manufacturer_Name" "Bourns")
    (property "Manufacturer_Part_Number" "SF-1206S1000W-2")
    (property "Mouser Part Number" "652-SF-1206S1000W-2")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Bourns/SF-1206S1000W-2?qs=fAHHVMwC%252BbilUMcZCwppRg%3D%3D")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F1" (at -1.5 2 180) (layer "F.SilkS"))
    (fp_text value "SF-1206S1000W-2" (at 0 0 180) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.285 0 180) (size 1.55 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/HS") (pintype "passive"))
    (pad "2" smd rect locked (at 1.285 0 180) (size 1.55 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(C2-Pad1)") (pintype "passive"))
    (model "D:\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\SF-1206S1000W-2.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect locked (start 55 63) (end 164 142) (layer "Edge.Cuts") (width 0.2) (fill none))
  (gr_text "Bokser\nhopper-power-dist rev02\n08-29-22\nREx Lab\n" (at 102.5 100.5) (layer "F.SilkS"))
  (zone (net 4) (net_name "Net-(J1-Pad1)") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 75 133)
        (xy 144 133)
        (xy 150 127)
        (xy 164 127)
        (xy 164 142)
        (xy 55 142)
        (xy 55 127)
        (xy 69 127)
      )
    )
  )
  (zone (net 5) (net_name "Net-(J2-Pad1)") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 114 132)
        (xy 75.5 132)
        (xy 69.5 126)
        (xy 55 126)
        (xy 55 116.5)
        (xy 94.5 116.5)
        (xy 98 113)
        (xy 114 113)
      )
    )
  )
  (zone (net 20) (net_name "/+12V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128 89.5)
        (xy 125.5 92)
        (xy 76.5 92)
        (xy 74 89.5)
        (xy 74 63)
        (xy 128 63)
      )
    )
  )
  (zone (net 1) (net_name "/HS") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 70.5 92.5)
        (xy 73.5 95.5)
        (xy 128.5 95.5)
        (xy 131.5 92.5)
        (xy 131.5 63)
        (xy 164 63)
        (xy 163.993115 115.5)
        (xy 143.5 115.5)
        (xy 140 112)
        (xy 97.5 112)
        (xy 94 115.5)
        (xy 55 115.5)
        (xy 55 63)
        (xy 70.5 63)
      )
    )
  )
  (zone (net 6) (net_name "Net-(H1-Pad1)") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 143 116.5)
        (xy 164 116.5)
        (xy 164 126)
        (xy 149.5 126)
        (xy 143.5 132)
        (xy 115 132)
        (xy 115 113)
        (xy 139.5 113)
      )
    )
  )
  (zone (net 19) (net_name "/-12V") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128 89.5)
        (xy 125.5 92)
        (xy 76.5 92)
        (xy 74 89.5)
        (xy 74 63)
        (xy 128 63)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 70.5 92.5)
        (xy 73.5 95.5)
        (xy 128.5 95.5)
        (xy 131.5 92.5)
        (xy 131.5 63)
        (xy 164 63)
        (xy 164 115.5)
        (xy 143.5 115.5)
        (xy 140 112)
        (xy 97.5 112)
        (xy 94 115.5)
        (xy 55 115.5)
        (xy 55 63)
        (xy 70.5 63)
      )
    )
  )
)
