(kicad_pcb (version 20171130) (host pcbnew "(5.1.6-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 62)
    (zones 0)
    (modules 5)
    (nets 25)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 "Net-(U1-Pad2)")
  (net 3 GND)
  (net 4 "Net-(U1-Pad5)")
  (net 5 CLK)
  (net 6 "Net-(U2-Pad5)")
  (net 7 "Net-(U2-Pad2)")
  (net 8 "Net-(U4-Pad2)")
  (net 9 "Net-(U3-Pad2)")
  (net 10 "Net-(U3-Pad5)")
  (net 11 "Net-(U4-Pad5)")
  (net 12 "Net-(U5-Pad11)")
  (net 13 "Net-(U5-Pad12)")
  (net 14 "Net-(U5-Pad13)")
  (net 15 "Net-(U5-Pad4)")
  (net 16 "Net-(U5-Pad14)")
  (net 17 "Net-(U5-Pad15)")
  (net 18 "Net-(U5-Pad6)")
  (net 19 "Net-(U5-Pad16)")
  (net 20 "Net-(U5-Pad17)")
  (net 21 "Net-(U5-Pad18)")
  (net 22 "Net-(U5-Pad19)")
  (net 23 "Net-(U5-Pad20)")
  (net 24 CIPO)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net CIPO)
    (add_net CLK)
    (add_net GND)
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U4-Pad2)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U5-Pad11)")
    (add_net "Net-(U5-Pad12)")
    (add_net "Net-(U5-Pad13)")
    (add_net "Net-(U5-Pad14)")
    (add_net "Net-(U5-Pad15)")
    (add_net "Net-(U5-Pad16)")
    (add_net "Net-(U5-Pad17)")
    (add_net "Net-(U5-Pad18)")
    (add_net "Net-(U5-Pad19)")
    (add_net "Net-(U5-Pad20)")
    (add_net "Net-(U5-Pad4)")
    (add_net "Net-(U5-Pad6)")
  )
  (module TEMPSENSE:FT232H-socket (layer F.Cu) (tedit 5F0C98CD)
    (at 317.5 205.74)
    (descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U5 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value FT232H (at 3.81 25.19) (layer F.Fab))
    (fp_text user %R (at 3.81 11.43) (layer F.Fab))
    (pad 20 thru_hole oval (at 20.32 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(U5-Pad20)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(U4-Pad5)"))
    (pad 19 thru_hole oval (at 20.32 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(U5-Pad19)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(U3-Pad5)"))
    (pad 18 thru_hole oval (at 20.32 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(U5-Pad18)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(U2-Pad5)"))
    (pad 17 thru_hole oval (at 20.32 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(U5-Pad17)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad5)"))
    (pad 16 thru_hole oval (at 20.32 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(U5-Pad16)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(U5-Pad6)"))
    (pad 15 thru_hole oval (at 20.32 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(U5-Pad15)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 CIPO))
    (pad 14 thru_hole oval (at 20.32 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(U5-Pad14)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(U5-Pad4)"))
    (pad 13 thru_hole oval (at 20.32 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(U5-Pad13)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 CLK))
    (pad 12 thru_hole oval (at 20.32 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(U5-Pad12)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 11 thru_hole oval (at 20.32 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(U5-Pad11)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-20_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TEMPSENSE:Max-31855-board (layer F.Cu) (tedit 5F0C9454)
    (at 309.88 238.76 180)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference U2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value MAX31855 (at 0 15.03) (layer F.Fab))
    (fp_text user V (at 2.54 0) (layer F.SilkS))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 CLK))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(U2-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 CIPO))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(U2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TEMPSENSE:Max-31855-board (layer F.Cu) (tedit 5F0C9454)
    (at 309.88 218.44 180)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference U1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value MAX31855 (at 0 15.03) (layer F.Fab))
    (fp_text user V (at 2.54 0) (layer F.SilkS))
    (fp_text user %R (at 0 6.35 180) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 CLK))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 CIPO))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TEMPSENSE:Max-31855-board (layer F.Cu) (tedit 5F0C9454)
    (at 345.44 226.06)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference U3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value MAX31855 (at 0 15.03) (layer F.Fab))
    (fp_text user V (at 2.54 0) (layer F.SilkS))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 CLK))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(U3-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 CIPO))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(U3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TEMPSENSE:Max-31855-board (layer F.Cu) (tedit 5F0C9454)
    (at 345.44 205.74)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference U4 (at 0 -2.33) (layer F.SilkS))
    (fp_text value MAX31855 (at 0 15.03) (layer F.Fab))
    (fp_text user V (at 2.54 0) (layer F.SilkS))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 CLK))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(U4-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 CIPO))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(U4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Licensed under CERN-OHL-P v2" (at 327.66 241.3) (layer F.SilkS))
  (gr_text "TEMPSENSE v0.2" (at 327.66 238.76) (layer F.SilkS))
  (gr_circle (center 336.55 237.49) (end 335.28 236.22) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 318.77 237.49) (end 320.04 236.22) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 350.52 201.93) (end 303.53 201.93) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 350.52 242.57) (end 350.52 201.93) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 303.53 242.57) (end 350.52 242.57) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 303.53 201.93) (end 303.53 242.57) (layer Edge.Cuts) (width 0.05))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 350.52 242.57) (xy 303.53 242.57) (xy 303.53 201.93) (xy 350.52 201.93)
      )
    )
  )
  (zone (net 1) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 350.52 242.57) (xy 303.53 242.57) (xy 303.53 201.93) (xy 350.52 201.93)
      )
    )
  )
)
