(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (footprint "Library:TestPoint_Pad_0.5mmx3mm" (layer "F.Cu")
    (at 98 48.9)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_0.5x3.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 99.1 48.9)
    (fp_text reference "" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 93.4 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 101.3 48.9)
    (fp_text reference "" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 86.7 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_0.5mmx3mm" (layer "F.Cu")
    (at 85.4 48.9)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_0.5x3.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 103.5 48.9)
    (fp_text reference "" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 77.7 48.9)
    (fp_text reference "" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 86.5 48.9)
    (fp_text reference "" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 85.3 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 106.8 48.9)
    (fp_text reference "" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 99.7 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 83.9 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 105.7 48.9)
    (fp_text reference "" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 98.3 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 75.5 48.9)
    (fp_text reference "" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 88.8 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 83.2 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 88.1 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 86 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_0.5mmx3mm" (layer "F.Cu")
    (at 95.8 48.9)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_0.5x3.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_0.5mmx3mm" (layer "F.Cu")
    (at 74.4 48.9)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_0.5x3.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 96.9 48.9)
    (fp_text reference "" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 89.5 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 95.5 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 90.6 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_0.5mmx3mm" (layer "F.Cu")
    (at 83.2 48.9)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_0.5x3.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_0.5mmx3mm" (layer "F.Cu")
    (at 76.6 48.9)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_0.5x3.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 84.6 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 84.3 48.9)
    (fp_text reference "" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 81.8 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 94.8 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_0.5mmx3mm" (layer "F.Cu")
    (at 104.6 48.9)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_0.5x3.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 94.1 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 87.4 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 73.3 48.9)
    (fp_text reference "" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 82.1 48.9)
    (fp_text reference "" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 79.9 48.9)
    (fp_text reference "" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 92.7 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 91.3 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 97.6 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_0.5mmx3mm" (layer "F.Cu")
    (at 78.8 48.9)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_0.5x3.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 92.5 48.9)
    (fp_text reference "" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 81.1 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 99 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 82.5 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 92 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_0.5mmx3mm" (layer "F.Cu")
    (at 87.6 48.9)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_0.5x3.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_0.5mmx3mm" (layer "F.Cu")
    (at 100.2 48.9)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_0.5x3.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_0.5mmx3mm" (layer "F.Cu")
    (at 93.6 48.9)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_0.5x3.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_0.5mmx3mm" (layer "F.Cu")
    (at 102.4 48.9)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_0.5x3.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:screw_hole" (layer "F.Cu")
    (at 90.05 48)
    (descr "solder Pin_ with flat with hole, hole diameter 1.3mm, length 11.3mm, width 2.8mm")
    (tags "solder Pin_ with flat fork")
    (attr through_hole)
    (fp_text reference "REF**" (at 0 2.25) (layer "F.SilkS") hide)
    (fp_text value "screw_hole" (at 0 -2.05) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.3mm_L11.3mm_W2.8mm_Flat.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:TestPoint_Pad_0.5mmx3mm" (layer "F.Cu")
    (at 81 48.9)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_0.5x3.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 96.9 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 94.7 48.9)
    (fp_text reference "" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0 0) (size 0.5 3) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 80.4 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Library:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 96.2 41.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint_Pad_1.0x1.0mm" (at 0 1.55) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 0) (size 0.2 2) (layers "F.Cu" "F.Mask"))
  )
  (gr_line (start 80 40) (end 100 40)
    (layer "Edge.Cuts"))
  (gr_line (start 100 40) (end 107.5 47)
    (layer "Edge.Cuts"))
  (gr_line (start 107.6 47) (end 100.1 40)
    (layer "Edge.Cuts"))
  (gr_line (start 72.5 47) (end 80 40)
    (layer "Edge.Cuts"))
  (gr_line (start 107.5 51) (end 107.5 47)
    (layer "Edge.Cuts"))
  (gr_line (start 72.5 51) (end 72.5 47)
    (layer "Edge.Cuts"))
  (gr_line (start 72.5 51) (end 107.5 51)
    (layer "Edge.Cuts"))
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 71 35)
        (xy 109 35)
        (xy 109 54)
        (xy 71 54)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 71 35)
        (xy 109 35)
        (xy 109 54)
        (xy 71 54)
      )
    )
  )
)
