<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0.635" y1="2.54" x2="2.41770625" y2="2.54" width="0" layer="20"/>
<wire x1="2.41770625" y1="2.54" x2="2.653540625" y2="2.49458125" width="0" layer="20" curve="-21.801567"/>
<wire x1="2.653540625" y1="2.49458125" x2="8.77645625" y2="0.04541875" width="0" layer="20"/>
<wire x1="8.77645625" y1="0.04541875" x2="9.012290625" y2="0" width="0" layer="20" curve="21.801357"/>
<wire x1="9.012290625" y1="0" x2="17.145" y2="0" width="0" layer="20"/>
<wire x1="17.145" y1="0" x2="17.78" y2="0.635" width="0" layer="20" curve="90"/>
<wire x1="17.78" y1="0.635" x2="17.78" y2="12.065" width="0" layer="20"/>
<wire x1="17.78" y1="12.065" x2="17.145" y2="12.7" width="0" layer="20" curve="90"/>
<wire x1="17.145" y1="12.7" x2="9.012290625" y2="12.7" width="0" layer="20"/>
<wire x1="9.012290625" y1="12.7" x2="8.77645625" y2="12.65458125" width="0" layer="20" curve="21.801567"/>
<wire x1="8.77645625" y1="12.65458125" x2="2.65354375" y2="10.20541875" width="0" layer="20"/>
<wire x1="2.65354375" y1="10.20541875" x2="2.417709375" y2="10.16" width="0" layer="20" curve="-21.801357"/>
<wire x1="2.417709375" y1="10.16" x2="0.635" y2="10.16" width="0" layer="20"/>
<wire x1="0.635" y1="10.16" x2="0" y2="9.525" width="0" layer="20" curve="90"/>
<wire x1="0" y1="9.525" x2="0" y2="3.175" width="0" layer="20"/>
<wire x1="0" y1="3.175" x2="0.635" y2="2.54" width="0" layer="20" curve="90"/>
<text>(c) 2017</text>
<text>J-Link Adapter</text>
<text>Daniel Brown</text>
</plain>
<libraries>
<library name="0-Lantzer">
<packages>
<package name="KITPROG">
</package>
<package name="KITPROG127">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="0-Lantzer" package="KITPROG" value="KITPROG"/>
<element name="U$3" library="0-Lantzer" package="KITPROG127" value="KITPROG127">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="SWDIO">
<contactref element="U$3" pad="5"/>
<contactref element="U$2" pad="P$5"/>
</signal>
<signal name="SWDCLK">
<contactref element="U$3" pad="4"/>
<contactref element="U$2" pad="P$4"/>
</signal>
<signal name="!RESET">
<contactref element="U$3" pad="3"/>
<contactref element="U$2" pad="P$3"/>
</signal>
<signal name="GND">
<contactref element="U$3" pad="2"/>
<contactref element="U$2" pad="P$2"/>
</signal>
<signal name="3V3">
<contactref element="U$3" pad="1"/>
<contactref element="U$2" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
