<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="-7.62" y1="24.13" x2="-7.62" y2="-3.81" width="0.0254" layer="20"/>
<wire x1="-7.62" y1="-3.81" x2="11.43" y2="-3.81" width="0.0254" layer="20"/>
<wire x1="11.43" y1="-3.81" x2="11.43" y2="24.13" width="0.0254" layer="20"/>
<wire x1="11.43" y1="24.13" x2="-7.62" y2="24.13" width="0.0254" layer="20"/>
<text>ENC_breakout</text>
</plain>
<libraries>
<library name="mcu-accessories">
<packages>
<package name="ML08">
</package>
<package name="SPDT_BULKHEAD">
<description>Standard bulkhead switch, vertical mount</description>
</package>
<package name="PEC11R">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ENC" library="mcu-accessories" package="PEC11R" value="PEC11R">
<attribute name="NAME"/>
</element>
<element name="JP1" library="mcu-accessories" package="ML08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="mcu-accessories" package="SPDT_BULKHEAD" value="SPDT-VERT-BULK">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JP1" pad="1"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP1" pad="5"/>
<contactref element="JP1" pad="7"/>
<contactref element="ENC" pad="C"/>
<contactref element="ENC" pad="2"/>
<contactref element="SW1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="ENC" pad="1"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="ENC" pad="B"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="ENC" pad="A"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="N$1">
<contactref element="SW1" pad="TAP"/>
<contactref element="JP1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
