(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 24)
    (no_connects 0)
    (area 131.105 86.049523 157.705001 122.995)
    (thickness 1.6)
    (drawings 26)
    (tracks 73)
    (zones 0)
    (modules 9)
    (nets 20)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "MCRobbie v1.0.1.svg"))
  )
  (net 0 "")
  (net 1 "Net-(J0-Pad1)")
  (net 2 "Net-(J0-Pad2)")
  (net 3 "Net-(J0-Pad3)")
  (net 4 "Net-(J1-Pad1)")
  (net 5 "Net-(J1-Pad2)")
  (net 6 "Net-(J1-Pad3)")
  (net 7 "Net-(J2-Pad1)")
  (net 8 "Net-(J2-Pad2)")
  (net 9 "Net-(J2-Pad3)")
  (net 10 "Net-(J3-Pad1)")
  (net 11 "Net-(J3-Pad2)")
  (net 12 "Net-(J3-Pad3)")
  (net 13 "Net-(J4-Pad1)")
  (net 14 "Net-(J4-Pad2)")
  (net 15 "Net-(J5-Pad2)")
  (net 16 "Net-(J5-Pad3)")
  (net 17 GND)
  (net 18 +5V)
  (net 19 "Net-(J5-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(J0-Pad1)")
    (add_net "Net-(J0-Pad2)")
    (add_net "Net-(J0-Pad3)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad6)")
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 59456341)
    (at 151.13 96.52)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C1 (at 2.54 0) (layer F.SilkS))
    (fp_text value "" (at 2.5 2.31) (layer F.Fab))
    (fp_text user %R (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 +5V))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:PINHEAD1-3 (layer F.Cu) (tedit 594556F8)
    (at 135.89 90.17 270)
    (fp_text reference Motor0 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value Motor0 (at 2.54 3.81 270) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J0-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J0-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J0-Pad3)"))
  )
  (module Connectors:PINHEAD1-3 (layer F.Cu) (tedit 59455704)
    (at 135.89 99.06 270)
    (fp_text reference Motor1 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value Motor1 (at 2.54 3.81 270) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad3)"))
  )
  (module Connectors:PINHEAD1-3 (layer F.Cu) (tedit 59455714)
    (at 135.89 107.95 270)
    (fp_text reference Motor2 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value Motor2 (at 2.54 3.81 270) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad3)"))
  )
  (module Connectors:PINHEAD1-3 (layer F.Cu) (tedit 5945571F)
    (at 153.67 100.33 270)
    (fp_text reference Motor3 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value Motor3 (at 2.54 3.81 270) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad3)"))
  )
  (module Connectors:PINHEAD1-2 (layer F.Cu) (tedit 59455729)
    (at 153.67 110.49 270)
    (fp_text reference I2C (at 1.27 -2.54 270) (layer F.SilkS))
    (fp_text value I2C_Header (at 1.27 3.81 270) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J4-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J4-Pad2)"))
  )
  (module Connectors:PINHEAD1-6 (layer F.Cu) (tedit 59455D5E)
    (at 138.43 118.11)
    (fp_text reference ICSP (at 6.35 2.54) (layer F.SilkS))
    (fp_text value ICP_Header (at 6.35 3.81) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J5-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J5-Pad3)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 17 GND))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 18 +5V))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J5-Pad6)"))
  )
  (module Connectors:PINHEAD1-2 (layer F.Cu) (tedit 59455732)
    (at 153.67 90.17 270)
    (fp_text reference Power (at 1.27 -2.54 270) (layer F.SilkS))
    (fp_text value Power_Header (at 1.27 3.81 270) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 18 +5V))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 17 GND))
  )
  (module Housings_DIP:DIP-20_W7.62mm (layer F.Cu) (tedit 59455CEE)
    (at 140.97 90.17)
    (descr "20-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference PIC18F14K50 (at 3.81 12.7 90) (layer F.SilkS))
    (fp_text value PIC18F14K50 (at 3.81 25.25) (layer F.Fab))
    (fp_text user %R (at 3.81 11.43) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 +5V))
    (pad 11 thru_hole oval (at 7.62 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J4-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(J0-Pad1)"))
    (pad 12 thru_hole oval (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J0-Pad3)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J0-Pad2)"))
    (pad 13 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J4-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(J5-Pad6)"))
    (pad 14 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad3)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (pad 15 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad2)"))
    (pad 16 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J3-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad3)"))
    (pad 17 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad1)"))
    (pad 18 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J5-Pad2)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad2)"))
    (pad 19 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J5-Pad3)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad3)"))
    (pad 20 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 GND))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Copyright OokTech CC-BY-SA" (at 144.78 120.65) (layer B.SilkS))
  (gr_text - (at 154.94 96.52) (layer F.SilkS))
  (gr_text + (at 152.4 96.52) (layer F.SilkS))
  (gr_line (start 157.48 86.36) (end 132.08 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.48 121.92) (end 157.48 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.08 121.92) (end 157.48 121.92) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.08 86.36) (end 132.08 121.92) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Design by OokTech" (at 144.78 115.57) (layer B.SilkS))
  (gr_text ▲ (at 138.43 120.65) (layer F.SilkS))
  (gr_text "MCRobbie v.1.0.1\n2017" (at 144.78 101.6 90) (layer B.SilkS))
  (gr_text GND (at 151.13 92.71 90) (layer F.SilkS))
  (gr_text SCL (at 151.13 113.03 90) (layer F.SilkS))
  (gr_text SDA (at 151.13 110.49 90) (layer F.SilkS))
  (gr_text C (at 133.35 113.03 90) (layer F.SilkS))
  (gr_text C (at 133.35 104.14 90) (layer F.SilkS))
  (gr_text C (at 151.13 105.41 90) (layer F.SilkS))
  (gr_text D (at 151.13 102.87 90) (layer F.SilkS))
  (gr_text D (at 133.35 110.49 90) (layer F.SilkS))
  (gr_text D (at 133.35 101.6 90) (layer F.SilkS))
  (gr_text P (at 151.13 100.33 90) (layer F.SilkS))
  (gr_text P (at 133.35 107.95 90) (layer F.SilkS))
  (gr_text P (at 133.35 99.06 90) (layer F.SilkS))
  (gr_text C (at 133.35 95.25 90) (layer F.SilkS))
  (gr_text D (at 133.35 92.71 90) (layer F.SilkS))
  (gr_text P (at 133.35 90.17 90) (layer F.SilkS))
  (gr_text 5V (at 151.13 90.17 90) (layer F.SilkS))
  (zone (net 17) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.08 86.36) (xy 157.48 86.36) (xy 157.48 121.92) (xy 132.08 121.92)
      )
    )
  )
  (zone (net 17) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.08 86.36) (xy 157.48 86.36) (xy 157.48 121.92) (xy 132.08 121.92)
      )
    )
  )
)
