(kicad_pcb (version 20171130) (host pcbnew 5.1.6)
  (general
    (thickness 1.6)
    (drawings 88)
    (tracks 538)
    (zones 0)
    (modules 24)
    (nets 89)
  )
  (page A4)
  (title_block
    (date 2020-06-30)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1524)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.101)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /ROW_2)
  (net 2 /ROW_3)
  (net 3 /ROW_4)
  (net 4 /ROW_5)
  (net 5 /ROW_6)
  (net 6 /ROW_8)
  (net 7 /ROW_7)
  (net 8 /ROW_9)
  (net 9 "Net-(U1-PadRESET)")
  (net 10 "Net-(U1-PadPROG)")
  (net 11 "Net-(U1-PadGND3)")
  (net 12 "Net-(U1-PadVBAT)")
  (net 13 "Net-(U1-PadA22/DAC1)")
  (net 14 "Net-(U1-Pad21/DAC0)")
  (net 15 "Net-(U1-Pad39/A20)")
  (net 16 /ROW_ESC)
  (net 17 /ROW_F1)
  (net 18 /ROW_F2)
  (net 19 "Net-(U1-Pad35/A16)")
  (net 20 "Net-(U1-Pad34/A15)")
  (net 21 "Net-(U1-Pad33/A14)")
  (net 22 /ROW_1)
  (net 23 /ROW_EQL)
  (net 24 "Net-(U1-PadGND2)")
  (net 25 /3V3)
  (net 26 "Net-(U1-PadVIN)")
  (net 27 "Net-(U1-PadAGND)")
  (net 28 "Net-(U1-Pad3V3_LO)")
  (net 29 "Net-(U1-Pad13/SCK)")
  (net 30 /ROW_MIN)
  (net 31 /ROW_0)
  (net 32 GND)
  (net 33 /COL_3)
  (net 34 "Net-(J2-Pad10)")
  (net 35 /COL_4)
  (net 36 /COL_2)
  (net 37 /COL_1)
  (net 38 "Net-(J2-Pad5)")
  (net 39 /COL_0)
  (net 40 "Net-(J3-Pad12)")
  (net 41 "Net-(J3-Pad13)")
  (net 42 "Net-(J3-Pad9)")
  (net 43 /COL_5)
  (net 44 "Net-(J5-Pad10)")
  (net 45 "Net-(J5-Pad9)")
  (net 46 "Net-(J5-Pad7)")
  (net 47 "Net-(J5-Pad6)")
  (net 48 /COL_6)
  (net 49 "Net-(J6-Pad10)")
  (net 50 "Net-(J6-Pad9)")
  (net 51 "Net-(J6-Pad2)")
  (net 52 "Net-(J6-Pad1)")
  (net 53 "Net-(LED1-Pad1)")
  (net 54 "Net-(LED2-Pad1)")
  (net 55 "Net-(LED3-Pad1)")
  (net 56 "Net-(LED4-Pad1)")
  (net 57 /LED_CAPS_LOCK)
  (net 58 /LED_NUM_LOCK)
  (net 59 /LED_SCROLL_LOCK)
  (net 60 /LED_KEYPAD)
  (net 61 "Net-(U1-Pad36/A17)")
  (net 62 "Net-(U1-Pad32/A13)")
  (net 63 "Net-(U1-Pad31/A12)")
  (net 64 "Net-(U1-Pad30)")
  (net 65 "Net-(U1-Pad29)")
  (net 66 "Net-(U1-Pad28)")
  (net 67 "Net-(U1-Pad3V3)")
  (net 68 "Net-(J4-Pad2)")
  (net 69 "Net-(J4-Pad1)")
  (net 70 "Net-(J7-Pad11)")
  (net 71 "Net-(J7-Pad5)")
  (net 72 "Net-(J1-Pad12)")
  (net 73 "Net-(J1-Pad2)")
  (net 74 "Net-(J1-Pad13)")
  (net 75 "Net-(J1-Pad11)")
  (net 76 "Net-(J1-Pad1)")
  (net 77 "Net-(J8-Pad8)")
  (net 78 "Net-(J8-Pad4)")
  (net 79 "Net-(J8-Pad2)")
  (net 80 "Net-(J8-Pad7)")
  (net 81 "Net-(J8-Pad5)")
  (net 82 "Net-(J8-Pad3)")
  (net 83 "Net-(J8-Pad1)")
  (net 84 "Net-(J1-Pad10)")
  (net 85 "Net-(J1-Pad9)")
  (net 86 "Net-(JP2-Pad1)")
  (net 87 "Net-(JP3-Pad1)")
  (net 88 "Net-(JP1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3V3)
    (add_net /COL_0)
    (add_net /COL_1)
    (add_net /COL_2)
    (add_net /COL_3)
    (add_net /COL_4)
    (add_net /COL_5)
    (add_net /COL_6)
    (add_net /LED_CAPS_LOCK)
    (add_net /LED_KEYPAD)
    (add_net /LED_NUM_LOCK)
    (add_net /LED_SCROLL_LOCK)
    (add_net /ROW_0)
    (add_net /ROW_1)
    (add_net /ROW_2)
    (add_net /ROW_3)
    (add_net /ROW_4)
    (add_net /ROW_5)
    (add_net /ROW_6)
    (add_net /ROW_7)
    (add_net /ROW_8)
    (add_net /ROW_9)
    (add_net /ROW_EQL)
    (add_net /ROW_ESC)
    (add_net /ROW_F1)
    (add_net /ROW_F2)
    (add_net /ROW_MIN)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J3-Pad12)")
    (add_net "Net-(J3-Pad13)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J5-Pad10)")
    (add_net "Net-(J5-Pad6)")
    (add_net "Net-(J5-Pad7)")
    (add_net "Net-(J5-Pad9)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J6-Pad10)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J6-Pad9)")
    (add_net "Net-(J7-Pad11)")
    (add_net "Net-(J7-Pad5)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J8-Pad2)")
    (add_net "Net-(J8-Pad3)")
    (add_net "Net-(J8-Pad4)")
    (add_net "Net-(J8-Pad5)")
    (add_net "Net-(J8-Pad7)")
    (add_net "Net-(J8-Pad8)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(JP2-Pad1)")
    (add_net "Net-(JP3-Pad1)")
    (add_net "Net-(LED1-Pad1)")
    (add_net "Net-(LED2-Pad1)")
    (add_net "Net-(LED3-Pad1)")
    (add_net "Net-(LED4-Pad1)")
    (add_net "Net-(U1-Pad13/SCK)")
    (add_net "Net-(U1-Pad21/DAC0)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad31/A12)")
    (add_net "Net-(U1-Pad32/A13)")
    (add_net "Net-(U1-Pad33/A14)")
    (add_net "Net-(U1-Pad34/A15)")
    (add_net "Net-(U1-Pad35/A16)")
    (add_net "Net-(U1-Pad36/A17)")
    (add_net "Net-(U1-Pad39/A20)")
    (add_net "Net-(U1-Pad3V3)")
    (add_net "Net-(U1-Pad3V3_LO)")
    (add_net "Net-(U1-PadA22/DAC1)")
    (add_net "Net-(U1-PadAGND)")
    (add_net "Net-(U1-PadGND2)")
    (add_net "Net-(U1-PadGND3)")
    (add_net "Net-(U1-PadPROG)")
    (add_net "Net-(U1-PadRESET)")
    (add_net "Net-(U1-PadVBAT)")
    (add_net "Net-(U1-PadVIN)")
  )
  (module kinx:TEENSY_3.5_3.6 (layer B.Cu) (tedit 5EFACA97)
    (at 143.51 101.8236 180)
    (fp_text reference U1 (at -25.908 -8.255 270) (layer B.SilkS) hide)
    (fp_text value TEENSY_3.5/3.6 (at -11.775 -11.555) (layer B.SilkS) hide)
    (fp_text user "compat w/\nTEENSY++" (at 14.478 -0.0254 90 unlocked) (layer F.SilkS))
    (fp_text user "TEENSY\n3.5\n3.6\n4.1" (at 11.8872 -0.127 270 unlocked) (layer B.SilkS))
    (fp_text user "see soldr\ninstruct." (at 1.524 0.0254 90 unlocked) (layer F.SilkS))
    (fp_text user TEENSY++ (at 24.003 0.0762 270 unlocked) (layer B.SilkS))
    (fp_text user 23 (at -20.3708 10.5918 270 unlocked) (layer B.SilkS))
    (fp_text user 22 (at -17.8562 10.5918 270 unlocked) (layer B.SilkS))
    (fp_text user 21 (at -15.2654 10.5918 270 unlocked) (layer B.SilkS))
    (fp_text user 20 (at -12.7254 10.5918 270 unlocked) (layer B.SilkS))
    (fp_text user 19 (at -10.1854 10.5918 270 unlocked) (layer B.SilkS))
    (fp_text user 18 (at -7.6708 10.5918 270 unlocked) (layer B.SilkS))
    (fp_text user 17 (at -5.1308 10.5918 270 unlocked) (layer B.SilkS))
    (fp_text user 16 (at -2.6162 10.5918 270 unlocked) (layer B.SilkS))
    (fp_text user 15 (at 0 10.5918 270 unlocked) (layer B.SilkS))
    (fp_text user 14 (at 2.54 10.5918 270 unlocked) (layer B.SilkS))
    (fp_text user 26 (at 15.24 -10.8204 270 unlocked) (layer B.SilkS))
    (fp_text user 25 (at 12.7 -10.8204 270 unlocked) (layer B.SilkS))
    (fp_text user 24 (at 10.16 -10.8204 270 unlocked) (layer B.SilkS))
    (fp_text user 12 (at 4.953 -10.4394 270 unlocked) (layer B.SilkS))
    (fp_text user 11 (at 2.4384 -10.4444 270 unlocked) (layer B.SilkS))
    (fp_text user 10 (at -0.0762 -10.4902 270 unlocked) (layer B.SilkS))
    (fp_text user 9 (at -2.6162 -10.4902 270 unlocked) (layer B.SilkS))
    (fp_text user 8 (at -5.1308 -10.4902 270 unlocked) (layer B.SilkS))
    (fp_text user 7 (at -7.6962 -10.4902 270 unlocked) (layer B.SilkS))
    (fp_text user 6 (at -10.2108 -10.4902 270 unlocked) (layer B.SilkS))
    (fp_text user 5 (at -12.7254 -10.4902 270 unlocked) (layer B.SilkS))
    (fp_text user 4 (at -15.2654 -10.4902 270 unlocked) (layer B.SilkS))
    (fp_text user 3 (at -17.8054 -10.4902 270 unlocked) (layer B.SilkS))
    (fp_text user 2 (at -20.3454 -10.4902 270 unlocked) (layer B.SilkS))
    (fp_text user 1 (at -22.8854 -10.4902 270 unlocked) (layer B.SilkS))
    (fp_text user 0 (at -25.4254 -10.5156 270 unlocked) (layer B.SilkS))
    (fp_text user 14 (at 2.54 10.5918 90 unlocked) (layer F.SilkS))
    (fp_text user 15 (at 0 10.5918 90 unlocked) (layer F.SilkS))
    (fp_text user 16 (at -2.6162 10.5918 90 unlocked) (layer F.SilkS))
    (fp_text user 17 (at -5.1308 10.5918 90 unlocked) (layer F.SilkS))
    (fp_text user 18 (at -7.6708 10.5918 90 unlocked) (layer F.SilkS))
    (fp_text user 19 (at -10.1854 10.5918 90 unlocked) (layer F.SilkS))
    (fp_text user 20 (at -12.7254 10.5918 90 unlocked) (layer F.SilkS))
    (fp_text user 21 (at -15.2654 10.5918 90 unlocked) (layer F.SilkS))
    (fp_text user 22 (at -17.8562 10.5918 90 unlocked) (layer F.SilkS))
    (fp_text user 23 (at -20.3708 10.5918 90 unlocked) (layer F.SilkS))
    (fp_text user 26 (at 15.24 -10.8204 90 unlocked) (layer F.SilkS))
    (fp_text user 25 (at 12.7 -10.8204 90 unlocked) (layer F.SilkS))
    (fp_text user 12 (at 4.9784 -10.4394 90 unlocked) (layer F.SilkS))
    (fp_text user 11 (at 2.4384 -10.4648 90 unlocked) (layer F.SilkS))
    (fp_text user 10 (at -0.0762 -10.4902 90 unlocked) (layer F.SilkS))
    (fp_text user 9 (at -2.6162 -10.4902 90 unlocked) (layer F.SilkS))
    (fp_text user 8 (at -5.1308 -10.4902 90 unlocked) (layer F.SilkS))
    (fp_text user 7 (at -7.6962 -10.4902 90 unlocked) (layer F.SilkS))
    (fp_text user 6 (at -10.2108 -10.4902 90 unlocked) (layer F.SilkS))
    (fp_text user 5 (at -12.7254 -10.4902 90 unlocked) (layer F.SilkS))
    (fp_text user 4 (at -15.2654 -10.4902 90 unlocked) (layer F.SilkS))
    (fp_text user 3 (at -17.8054 -10.4902 90 unlocked) (layer F.SilkS))
    (fp_text user 2 (at -20.3454 -10.4902 90 unlocked) (layer F.SilkS))
    (fp_text user 1 (at -22.8854 -10.4902 90 unlocked) (layer F.SilkS))
    (fp_text user 24 (at 10.1854 -10.8204 90 unlocked) (layer F.SilkS))
    (fp_text user 0 (at -25.4254 -10.5156 90 unlocked) (layer F.SilkS))
    (fp_text user "TEENSY\nLC\n3.2\n4.0\n\n(only caps\nlock LED)" (at -10.4648 0.0254 270 unlocked) (layer B.SilkS))
    (pad RESET thru_hole circle (at 5.08 5.08 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 9 "Net-(U1-PadRESET)") (solder_mask_margin 0.0635))
    (pad PROG thru_hole circle (at 5.08 2.54 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 10 "Net-(U1-PadPROG)") (solder_mask_margin 0.0635))
    (pad GND3 thru_hole circle (at 5.08 0 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 11 "Net-(U1-PadGND3)") (solder_mask_margin 0.0635))
    (pad VBAT thru_hole circle (at 5.08 -5.08 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 12 "Net-(U1-PadVBAT)") (solder_mask_margin 0.0635))
    (pad 3V3_2 thru_hole circle (at 5.08 -2.54 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 25 /3V3) (solder_mask_margin 0.0635))
    (pad 3V3_2 thru_hole circle (at 20.32 -2.54 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 25 /3V3) (solder_mask_margin 0.0635))
    (pad GND3 thru_hole circle (at 20.32 0 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 11 "Net-(U1-PadGND3)") (solder_mask_margin 0.0635))
    (pad RESET thru_hole circle (at 20.32 2.54 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 9 "Net-(U1-PadRESET)") (solder_mask_margin 0.0635))
    (pad RESET thru_hole circle (at 17.78 5.08 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 9 "Net-(U1-PadRESET)") (solder_mask_margin 0.0635))
    (pad 3V3_2 thru_hole circle (at 17.78 -2.54 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 25 /3V3) (solder_mask_margin 0.0635))
    (pad PROG thru_hole circle (at 17.78 2.54 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 10 "Net-(U1-PadPROG)") (solder_mask_margin 0.0635))
    (pad GND3 thru_hole circle (at 17.78 0 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 11 "Net-(U1-PadGND3)") (solder_mask_margin 0.0635))
    (pad VBAT thru_hole circle (at 17.78 -5.08 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 12 "Net-(U1-PadVBAT)") (solder_mask_margin 0.0635))
    (pad A22/DAC1 thru_hole circle (at 10.16 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-PadA22/DAC1)") (solder_mask_margin 0.0635))
    (pad 21/DAC0 thru_hole circle (at 12.7 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 14 "Net-(U1-Pad21/DAC0)") (solder_mask_margin 0.0635))
    (pad 39/A20 thru_hole circle (at 15.24 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 15 "Net-(U1-Pad39/A20)") (solder_mask_margin 0.0635))
    (pad 38/A19 thru_hole circle (at 17.78 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 86 "Net-(JP2-Pad1)") (solder_mask_margin 0.0635))
    (pad 37/A18 thru_hole circle (at 20.32 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 87 "Net-(JP3-Pad1)") (solder_mask_margin 0.0635))
    (pad 36/A17 thru_hole circle (at 22.86 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 61 "Net-(U1-Pad36/A17)") (solder_mask_margin 0.0635))
    (pad 35/A16 thru_hole circle (at 25.4 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 19 "Net-(U1-Pad35/A16)") (solder_mask_margin 0.0635))
    (pad 34/A15 thru_hole circle (at 27.94 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 20 "Net-(U1-Pad34/A15)") (solder_mask_margin 0.0635))
    (pad 33/A14 thru_hole circle (at 30.48 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 21 "Net-(U1-Pad33/A14)") (solder_mask_margin 0.0635))
    (pad 32/A13 thru_hole circle (at 30.48 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 62 "Net-(U1-Pad32/A13)") (solder_mask_margin 0.0635))
    (pad 31/A12 thru_hole circle (at 27.94 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 63 "Net-(U1-Pad31/A12)") (solder_mask_margin 0.0635))
    (pad 30 thru_hole circle (at 25.4 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 64 "Net-(U1-Pad30)") (solder_mask_margin 0.0635))
    (pad 29 thru_hole circle (at 22.86 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 65 "Net-(U1-Pad29)") (solder_mask_margin 0.0635))
    (pad 28 thru_hole circle (at 20.32 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 66 "Net-(U1-Pad28)") (solder_mask_margin 0.0635))
    (pad 27 thru_hole circle (at 17.78 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 88 "Net-(JP1-Pad1)") (solder_mask_margin 0.0635))
    (pad 26 thru_hole circle (at 15.24 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 58 /LED_NUM_LOCK) (solder_mask_margin 0.0635))
    (pad 25 thru_hole circle (at 12.7 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 59 /LED_SCROLL_LOCK) (solder_mask_margin 0.0635))
    (pad 24 thru_hole circle (at 10.16 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 60 /LED_KEYPAD) (solder_mask_margin 0.0635))
    (pad GND2 thru_hole circle (at 7.62 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 24 "Net-(U1-PadGND2)") (solder_mask_margin 0.0635))
    (pad 3V3 thru_hole circle (at 7.62 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 67 "Net-(U1-Pad3V3)") (solder_mask_margin 0.0635))
    (pad VIN thru_hole circle (at -27.94 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 26 "Net-(U1-PadVIN)") (solder_mask_margin 0.0635))
    (pad GND thru_hole circle (at -27.94 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 32 GND) (solder_mask_margin 0.0635))
    (pad AGND thru_hole circle (at -25.4 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 27 "Net-(U1-PadAGND)") (solder_mask_margin 0.0635))
    (pad 3V3_LO thru_hole circle (at -22.86 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 28 "Net-(U1-Pad3V3_LO)") (solder_mask_margin 0.0635))
    (pad 0/RX thru_hole circle (at -25.4 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 31 /ROW_0) (solder_mask_margin 0.0635))
    (pad 23/A9 thru_hole circle (at -20.32 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 17 /ROW_F1) (solder_mask_margin 0.0635))
    (pad 22/A8 thru_hole circle (at -17.78 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 35 /COL_4) (solder_mask_margin 0.0635))
    (pad 21/A7 thru_hole circle (at -15.24 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 18 /ROW_F2) (solder_mask_margin 0.0635))
    (pad 20/A6 thru_hole circle (at -12.7 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 33 /COL_3) (solder_mask_margin 0.0635))
    (pad 19/A5/SCL thru_hole circle (at -10.16 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 43 /COL_5) (solder_mask_margin 0.0635))
    (pad 18/A4/SDA thru_hole circle (at -7.62 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 39 /COL_0) (solder_mask_margin 0.0635))
    (pad 17/A3 thru_hole circle (at -5.08 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 16 /ROW_ESC) (solder_mask_margin 0.0635))
    (pad 16/A2 thru_hole circle (at -2.54 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 4 /ROW_5) (solder_mask_margin 0.0635))
    (pad 15/A1 thru_hole circle (at 0 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 36 /COL_2) (solder_mask_margin 0.0635))
    (pad 14/A0 thru_hole circle (at 2.54 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 37 /COL_1) (solder_mask_margin 0.0635))
    (pad 13/SCK thru_hole circle (at 5.08 7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad13/SCK)") (solder_mask_margin 0.0635))
    (pad 12/MISO thru_hole circle (at 5.08 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 57 /LED_CAPS_LOCK) (solder_mask_margin 0.0635))
    (pad 11/MOSI thru_hole circle (at 2.54 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 2 /ROW_3) (solder_mask_margin 0.0635))
    (pad 10/CS thru_hole circle (at 0 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 1 /ROW_2) (solder_mask_margin 0.0635))
    (pad 9/CS thru_hole circle (at -2.54 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 22 /ROW_1) (solder_mask_margin 0.0635))
    (pad 8 thru_hole circle (at -5.08 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 23 /ROW_EQL) (solder_mask_margin 0.0635))
    (pad 7 thru_hole circle (at -7.62 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 3 /ROW_4) (solder_mask_margin 0.0635))
    (pad 6 thru_hole circle (at -10.16 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 48 /COL_6) (solder_mask_margin 0.0635))
    (pad 5 thru_hole circle (at -12.7 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 5 /ROW_6) (solder_mask_margin 0.0635))
    (pad 4/CANRX thru_hole circle (at -15.24 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 6 /ROW_8) (solder_mask_margin 0.0635))
    (pad 3/CANTX thru_hole circle (at -17.78 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 7 /ROW_7) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at -20.32 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 30 /ROW_MIN) (solder_mask_margin 0.0635))
    (pad 1/TX thru_hole circle (at -22.86 -7.62 180) (size 1.4478 1.4478) (drill 0.9652) (layers *.Cu *.Mask)
      (net 8 /ROW_9) (solder_mask_margin 0.0635))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm (layer F.Cu) (tedit 5A64794F)
    (at 133.35 97.536)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP3 (at 0 -1.8) (layer F.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd custom (at -0.725 0) (size 0.3 0.3) (layers F.Cu F.Mask)
      (net 87 "Net-(JP3-Pad1)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.5 -0.75) (xy 0.5 -0.75) (xy 1 0) (xy 0.5 0.75) (xy -0.5 0.75)
) (width 0))
      ))
    (pad 2 smd custom (at 0.725 0) (size 0.3 0.3) (layers F.Cu F.Mask)
      (net 36 /COL_2) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.65 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy -0.65 0.75) (xy -0.15 0)
) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm (layer F.Cu) (tedit 5A64794F)
    (at 133.387 101.727)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 0 -1.8) (layer F.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd custom (at -0.725 0) (size 0.3 0.3) (layers F.Cu F.Mask)
      (net 86 "Net-(JP2-Pad1)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.5 -0.75) (xy 0.5 -0.75) (xy 1 0) (xy 0.5 0.75) (xy -0.5 0.75)
) (width 0))
      ))
    (pad 2 smd custom (at 0.725 0) (size 0.3 0.3) (layers F.Cu F.Mask)
      (net 4 /ROW_5) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.65 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy -0.65 0.75) (xy -0.15 0)
) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm (layer F.Cu) (tedit 5A64794F)
    (at 133.387 106.426)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 -1.8) (layer F.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd custom (at -0.725 0) (size 0.3 0.3) (layers F.Cu F.Mask)
      (net 88 "Net-(JP1-Pad1)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.5 -0.75) (xy 0.5 -0.75) (xy 1 0) (xy 0.5 0.75) (xy -0.5 0.75)
) (width 0))
      ))
    (pad 2 smd custom (at 0.725 0) (size 0.3 0.3) (layers F.Cu F.Mask)
      (net 3 /ROW_4) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.65 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy -0.65 0.75) (xy -0.15 0)
) (width 0))
      ))
  )
  (module MountingHole:MountingHole_6mm (layer F.Cu) (tedit 56D1B4CB)
    (at 148.463 86.487)
    (descr "Mounting Hole 6mm, no annular")
    (tags "mounting hole 6mm no annular")
    (attr virtual)
    (fp_text reference H2 (at 0 -7) (layer F.SilkS) hide)
    (fp_text value "mounting pad" (at 0 7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 6 6) (drill 6) (layers *.Cu *.Mask))
  )
  (module kinx:39-53-2135 (layer B.Cu) (tedit 5EE5D146)
    (at 196.088 118.11 90)
    (descr "\"1.25 FPC CONN ASSY ZF 13\"")
    (fp_text reference J7 (at 11.811 -1.143 unlocked) (layer B.SilkS))
    (fp_text value RIGHT_13_DOWN (at 6.35 -5.08 270 unlocked) (layer B.SilkS))
    (pad 12 thru_hole circle (at 6.25 -1.65 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /ROW_9) (solder_mask_margin 0.0635))
    (pad 10 thru_hole circle (at 3.75 -1.65 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /COL_0) (solder_mask_margin 0.0635))
    (pad 8 thru_hole circle (at 1.25 -1.65 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /COL_2) (solder_mask_margin 0.0635))
    (pad 6 thru_hole circle (at -1.25 -1.65 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /ROW_MIN) (solder_mask_margin 0.0635))
    (pad 4 thru_hole circle (at -3.75 -1.65 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /COL_4) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at -6.25 -1.65 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /ROW_8) (solder_mask_margin 0.0635))
    (pad 13 thru_hole circle (at 7.5 0 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /ROW_0) (solder_mask_margin 0.0635))
    (pad 11 thru_hole circle (at 5 0 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 "Net-(J7-Pad11)") (solder_mask_margin 0.0635))
    (pad 9 thru_hole circle (at 2.5 0 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /COL_1) (solder_mask_margin 0.0635))
    (pad 7 thru_hole circle (at 0 0 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /COL_3) (solder_mask_margin 0.0635))
    (pad 5 thru_hole circle (at -2.5 0 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 "Net-(J7-Pad5)") (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at -5 0 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /ROW_7) (solder_mask_margin 0.0635))
    (pad 1 thru_hole circle (at -7.5 0 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /ROW_6) (solder_mask_margin 0.0635))
  )
  (module kinx:logo locked (layer B.Cu) (tedit 0)
    (at 165.1 77.216 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module kinx:logo locked (layer F.Cu) (tedit 0)
    (at 123.317 77.216)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module kinx:39-53-2135 (layer B.Cu) (tedit 5EE5D146)
    (at 101.346 117.602 270)
    (descr "\"1.25 FPC CONN ASSY ZF 13\"")
    (fp_text reference J2 (at -11.43 -1.397 unlocked) (layer B.SilkS))
    (fp_text value LEFT_13_LT (at -5.207 -5.08 90 unlocked) (layer B.SilkS))
    (pad 12 thru_hole circle (at 6.25 -1.65 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /COL_3) (solder_mask_margin 0.0635))
    (pad 10 thru_hole circle (at 3.75 -1.65 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad10)") (solder_mask_margin 0.0635))
    (pad 8 thru_hole circle (at 1.25 -1.65 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /ROW_EQL) (solder_mask_margin 0.0635))
    (pad 6 thru_hole circle (at -1.25 -1.65 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /ROW_2) (solder_mask_margin 0.0635))
    (pad 4 thru_hole circle (at -3.75 -1.65 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /ROW_3) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at -6.25 -1.65 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /ROW_5) (solder_mask_margin 0.0635))
    (pad 13 thru_hole circle (at 7.5 0 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /COL_4) (solder_mask_margin 0.0635))
    (pad 11 thru_hole circle (at 5 0 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /COL_2) (solder_mask_margin 0.0635))
    (pad 9 thru_hole circle (at 2.5 0 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /COL_1) (solder_mask_margin 0.0635))
    (pad 7 thru_hole circle (at 0 0 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /ROW_1) (solder_mask_margin 0.0635))
    (pad 5 thru_hole circle (at -2.5 0 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad5)") (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at -5 0 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /ROW_4) (solder_mask_margin 0.0635))
    (pad 1 thru_hole circle (at -7.5 0 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /COL_0) (solder_mask_margin 0.0635))
  )
  (module kinx:39-53-2135 (layer B.Cu) (tedit 5EE5D146)
    (at 104.521 74.549 270)
    (descr "\"1.25 FPC CONN ASSY ZF 13\"")
    (fp_text reference J3 (at 12.827 -1.27 unlocked) (layer B.SilkS))
    (fp_text value TOP_LEFT (at -4.064 -4.953 90 unlocked) (layer B.SilkS))
    (pad 12 thru_hole circle (at 6.25 -1.65 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(J3-Pad12)") (solder_mask_margin 0.0635))
    (pad 10 thru_hole circle (at 3.75 -1.65 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /ROW_F1) (solder_mask_margin 0.0635))
    (pad 8 thru_hole circle (at 1.25 -1.65 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /COL_1) (solder_mask_margin 0.0635))
    (pad 6 thru_hole circle (at -1.25 -1.65 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /ROW_F1) (solder_mask_margin 0.0635))
    (pad 4 thru_hole circle (at -3.75 -1.65 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /ROW_F2) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at -6.25 -1.65 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /ROW_ESC) (solder_mask_margin 0.0635))
    (pad 13 thru_hole circle (at 7.5 0 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(J3-Pad13)") (solder_mask_margin 0.0635))
    (pad 11 thru_hole circle (at 5 0 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /ROW_F2) (solder_mask_margin 0.0635))
    (pad 9 thru_hole circle (at 2.5 0 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(J3-Pad9)") (solder_mask_margin 0.0635))
    (pad 7 thru_hole circle (at 0 0 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /ROW_F2) (solder_mask_margin 0.0635))
    (pad 5 thru_hole circle (at -2.5 0 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /COL_2) (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at -5 0 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /ROW_F1) (solder_mask_margin 0.0635))
    (pad 1 thru_hole circle (at -7.5 0 270) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /COL_0) (solder_mask_margin 0.0635))
  )
  (module kinx:39-53-2135 (layer B.Cu) (tedit 5EE5D146)
    (at 192.532 76.073 90)
    (descr "\"1.25 FPC CONN ASSY ZF 13\"")
    (fp_text reference J4 (at -12.573 1.143 180) (layer B.SilkS))
    (fp_text value TOP_RIGHT (at -3.429 -4.953 270 unlocked) (layer B.SilkS))
    (pad 12 thru_hole circle (at 6.25 -1.65 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /ROW_F2) (solder_mask_margin 0.0635))
    (pad 10 thru_hole circle (at 3.75 -1.65 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /COL_5) (solder_mask_margin 0.0635))
    (pad 8 thru_hole circle (at 1.25 -1.65 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /COL_3) (solder_mask_margin 0.0635))
    (pad 6 thru_hole circle (at -1.25 -1.65 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /ROW_F1) (solder_mask_margin 0.0635))
    (pad 4 thru_hole circle (at -3.75 -1.65 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /ROW_F2) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at -6.25 -1.65 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 "Net-(J4-Pad2)") (solder_mask_margin 0.0635))
    (pad 13 thru_hole circle (at 7.5 0 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /ROW_F1) (solder_mask_margin 0.0635))
    (pad 11 thru_hole circle (at 5 0 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /COL_5) (solder_mask_margin 0.0635))
    (pad 9 thru_hole circle (at 2.5 0 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /ROW_ESC) (solder_mask_margin 0.0635))
    (pad 7 thru_hole circle (at 0 0 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /ROW_F2) (solder_mask_margin 0.0635))
    (pad 5 thru_hole circle (at -2.5 0 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /COL_4) (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at -5 0 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /ROW_F1) (solder_mask_margin 0.0635))
    (pad 1 thru_hole circle (at -7.5 0 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "Net-(J4-Pad1)") (solder_mask_margin 0.0635))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 121.412 141.097 90)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J5 (at -2.54 -22.987 180) (layer B.SilkS))
    (fp_text value THUMB_LEFT_BAK (at 7.874 -4.191 unlocked) (layer B.SilkS))
    (fp_text user %R (at 0 -11.43 180) (layer B.Fab))
    (pad 10 thru_hole oval (at 0 -22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J5-Pad10)"))
    (pad 9 thru_hole oval (at 0 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(J5-Pad9)"))
    (pad 8 thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /ROW_3))
    (pad 7 thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J5-Pad7)"))
    (pad 6 thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(J5-Pad6)"))
    (pad 5 thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /COL_5))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /COL_6))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /ROW_5))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /ROW_2))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /ROW_4))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 175.641 141.224 270)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J6 (at 2.794 -23.749 180) (layer B.SilkS))
    (fp_text value THUMB_RIGHT_SPC (at -8.001 -3.556 unlocked) (layer B.SilkS))
    (fp_text user %R (at 0 -11.43 180) (layer B.Fab))
    (pad 10 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(J6-Pad10)"))
    (pad 9 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(J6-Pad9)"))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /COL_5))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /COL_6))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /ROW_9))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /ROW_8))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /ROW_7))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /ROW_6))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(J6-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(J6-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 133.2511 144.0036 270)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference LED1 (at 0 -2.1309 90) (layer F.SilkS) hide)
    (fp_text value LEDSML1206 (at 0 1.82 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 25 /3V3))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 53 "Net-(LED1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 143.4511 144.0036 270)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference LED2 (at 0 -2.0909 90) (layer F.SilkS) hide)
    (fp_text value LEDSML1206 (at 0 1.82 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 25 /3V3))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 54 "Net-(LED2-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 153.5511 144.0036 270)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference LED3 (at 0 -2.0239 90) (layer F.SilkS) hide)
    (fp_text value LEDSML1206 (at 0 1.82 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 25 /3V3))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 55 "Net-(LED3-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 163.7511 144.0036 270)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference LED4 (at 0 -2.1109 90) (layer F.SilkS) hide)
    (fp_text value LEDSML1206 (at 0 1.82 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 25 /3V3))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 56 "Net-(LED4-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 133.2511 137.0036 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at -3.2726 -0.0989 180) (layer F.SilkS))
    (fp_text value 10K (at 0 -2.1309 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 53 "Net-(LED1-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 57 /LED_CAPS_LOCK))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 143.4511 137.0036 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -3.2726 0.0681 180) (layer F.SilkS))
    (fp_text value 10K (at 0 -2.0909 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 54 "Net-(LED2-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 58 /LED_NUM_LOCK))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 153.5511 137.0036 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -3.2726 0.0081 180) (layer F.SilkS))
    (fp_text value 10K (at 0 -2.1509 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 55 "Net-(LED3-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 59 /LED_SCROLL_LOCK))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 163.7511 137.0036 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at -3.2726 0.0481 180) (layer F.SilkS))
    (fp_text value 10K (at 0 -2.1109 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 56 "Net-(LED4-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 60 /LED_KEYPAD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 148.5011 118.0036)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference H1 (at 0 -5.3) (layer F.SilkS) hide)
    (fp_text value "mounting pad" (at 0 5.3) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask)
      (net 32 GND))
  )
  (module kinx:39-53-2135 (layer B.Cu) (tedit 5EE5D146)
    (at 184.658 136.906)
    (descr "\"1.25 FPC CONN ASSY ZF 13\"")
    (fp_text reference J1 (at 11.557 0.254 180) (layer B.SilkS))
    (fp_text value THUMB_RIGHT_SPC_KB600 (at -10.16 3.81 180) (layer B.Fab) hide)
    (pad 12 thru_hole circle (at 6.25 -1.65) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 "Net-(J1-Pad12)") (solder_mask_margin 0.0635))
    (pad 10 thru_hole circle (at 3.75 -1.65) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 "Net-(J1-Pad10)") (solder_mask_margin 0.0635))
    (pad 8 thru_hole circle (at 1.25 -1.65) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /COL_5) (solder_mask_margin 0.0635))
    (pad 6 thru_hole circle (at -1.25 -1.65) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /ROW_9) (solder_mask_margin 0.0635))
    (pad 4 thru_hole circle (at -3.75 -1.65) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /ROW_7) (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at -6.25 -1.65) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(J1-Pad2)") (solder_mask_margin 0.0635))
    (pad 13 thru_hole circle (at 7.5 0) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(J1-Pad13)") (solder_mask_margin 0.0635))
    (pad 11 thru_hole circle (at 5 0) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 "Net-(J1-Pad11)") (solder_mask_margin 0.0635))
    (pad 9 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 "Net-(J1-Pad9)") (solder_mask_margin 0.0635))
    (pad 7 thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /COL_6) (solder_mask_margin 0.0635))
    (pad 5 thru_hole circle (at -2.5 0) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /ROW_8) (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at -5 0) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /ROW_6) (solder_mask_margin 0.0635))
    (pad 1 thru_hole circle (at -7.5 0) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 "Net-(J1-Pad1)") (solder_mask_margin 0.0635))
  )
  (module kinx:39-53-2135 (layer B.Cu) (tedit 5EE5D146)
    (at 112.014 136.779)
    (descr "\"1.25 FPC CONN ASSY ZF 13\"")
    (fp_text reference J8 (at -12.827 0.254 180) (layer B.SilkS))
    (fp_text value THUMB_LEFT_BAK_KB600 (at -10.16 3.81 180) (layer B.Fab) hide)
    (pad 12 thru_hole circle (at 6.25 -1.65) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /ROW_2) (solder_mask_margin 0.0635))
    (pad 10 thru_hole circle (at 3.75 -1.65) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /COL_6) (solder_mask_margin 0.0635))
    (pad 8 thru_hole circle (at 1.25 -1.65) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 "Net-(J8-Pad8)") (solder_mask_margin 0.0635))
    (pad 6 thru_hole circle (at -1.25 -1.65) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /ROW_3) (solder_mask_margin 0.0635))
    (pad 4 thru_hole circle (at -3.75 -1.65) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 "Net-(J8-Pad4)") (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at -6.25 -1.65) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "Net-(J8-Pad2)") (solder_mask_margin 0.0635))
    (pad 13 thru_hole circle (at 7.5 0) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /ROW_4) (solder_mask_margin 0.0635))
    (pad 11 thru_hole circle (at 5 0) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /ROW_5) (solder_mask_margin 0.0635))
    (pad 9 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /COL_5) (solder_mask_margin 0.0635))
    (pad 7 thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(J8-Pad7)") (solder_mask_margin 0.0635))
    (pad 5 thru_hole circle (at -2.5 0) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 "Net-(J8-Pad5)") (solder_mask_margin 0.0635))
    (pad 3 thru_hole circle (at -5 0) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 "Net-(J8-Pad3)") (solder_mask_margin 0.0635))
    (pad 1 thru_hole circle (at -7.5 0) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 "Net-(J8-Pad1)") (solder_mask_margin 0.0635))
  )
  (gr_text x (at 145.923 95.631 90) (layer F.SilkS))
  (gr_text x (at 143.383 95.631 90) (layer F.SilkS))
  (gr_text x (at 151.003 107.95 90) (layer F.SilkS))
  (gr_text C (at 166.37 142.494 90) (layer F.SilkS))
  (gr_text A (at 166.37 146.05 90) (layer F.SilkS))
  (gr_text C (at 156.21 142.494 90) (layer F.SilkS))
  (gr_text A (at 156.21 146.05 90) (layer F.SilkS))
  (gr_text A (at 146.05 146.05 90) (layer F.SilkS))
  (gr_text C (at 146.05 142.494 90) (layer F.SilkS))
  (gr_text A (at 136.017 146.05 90) (layer F.SilkS))
  (gr_text C (at 136.017 142.494 90) (layer F.SilkS))
  (gr_line (start 105.918 110.617) (end 105.918 108.458) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.918 108.458) (end 110.49 108.458) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.49 108.458) (end 110.49 110.617) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.49 110.617) (end 105.918 110.617) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 191.008 108.458) (end 191.008 110.617) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.436 108.458) (end 191.008 108.458) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.436 110.617) (end 186.436 108.458) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 191.008 110.617) (end 186.436 110.617) (layer Edge.Cuts) (width 0.1))
  (gr_text "Molex\n39-53-2135" (at 96.774 117.221 90) (layer B.SilkS))
  (gr_text "Molex\n39-53-2135" (at 200.533 122.174 270) (layer B.SilkS))
  (gr_text "Molex\n39-53-2135" (at 197.231 75.311 270) (layer B.SilkS))
  (gr_text "Molex\n39-53-2135" (at 99.949 74.041 90) (layer B.SilkS))
  (gr_text v2020-06-30 (at 152.527 82.931) (layer F.SilkS))
  (gr_text https://github.com/kinx-project/kint (at 134.493 73.66) (layer F.SilkS))
  (gr_text "by https://michael.stapelberg.ch" (at 134.493 76.2) (layer F.SilkS))
  (gr_text "kinT keyboard controller" (at 134.493 70.358) (layer F.SilkS))
  (gr_text "Open Hardware: CC-BY-SA" (at 134.493 78.613) (layer F.SilkS))
  (gr_text "Open Hardware: CC-BY-SA" (at 154.94 77.343) (layer B.SilkS))
  (gr_text -or- (at 127.127 138.938) (layer B.SilkS))
  (gr_text KB500 (at 127 141.351) (layer B.SilkS))
  (gr_text KB600 (at 127 136.652) (layer B.SilkS))
  (gr_text -or- (at 170.307 138.938) (layer B.SilkS))
  (gr_text KB500 (at 170.18 141.351) (layer B.SilkS))
  (gr_text KB600 (at 170.18 136.652) (layer B.SilkS))
  (gr_text "kinT keyboard controller" (at 154.94 69.088) (layer B.SilkS))
  (gr_text v2020-06-30 (at 140.97 83.693) (layer B.SilkS))
  (gr_text "by https://michael.stapelberg.ch" (at 154.94 74.93) (layer B.SilkS))
  (gr_text https://github.com/kinx-project/kint (at 154.94 72.39) (layer B.SilkS))
  (gr_line (start 95.25 148.0036) (end 203.2 148.0036) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 203.2 148.0036) (end 203.2 62.0036) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 203.2 62.0036) (end 95.25 62.0036) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 95.25 62.0036) (end 95.25 148.0036) (layer Edge.Cuts) (width 0.05))
  (gr_text CAPS_LOCK (at 131.572 144.526 90) (layer F.SilkS))
  (gr_text NUM_LOCK (at 141.605 144.526 90) (layer F.SilkS))
  (gr_text SCROLL_LOCK (at 151.892 144.272 90) (layer F.SilkS))
  (gr_text KEYPAD (at 162.179 144.018 90) (layer F.SilkS))
  (zone (net 32) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.4564) (thermal_bridge_width 0.4564))
    (polygon
      (pts
        (xy 203.1163 147.2068) (xy 95.25 147.2068) (xy 95.25 62.8004) (xy 203.1163 62.8004)
      )
    )
  )
  (zone (net 32) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.4564) (thermal_bridge_width 0.4564))
    (polygon
      (pts
        (xy 203.1163 147.2068) (xy 95.25 147.2068) (xy 95.25 62.8004) (xy 203.1163 62.8004)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.365 129.286) (xy 171.196 129.286) (xy 171.196 134.747) (xy 126.365 134.747)
      )
    )
  )
)
