(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 219)
    (no_connects 0)
    (area 99.924999 71.924999 139.075001 88.075001)
    (thickness 1.6)
    (drawings 92)
    (tracks 606)
    (zones 0)
    (modules 104)
    (nets 54)
  )
  (page A4)
  (title_block
    (date 2018-06-04)
    (rev 0.8)
  )
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.1)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.4572)
    (via_min_drill 0.254)
    (uvia_size 0.5)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.4572)
    (uvia_min_drill 0.254)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.5 4)
    (pad_drill 1.2)
    (pad_to_mask_clearance 0.0381)
    (aux_axis_origin 0 0)
    (grid_origin 100 80)
    (visible_elements 7FFEFF7F)
    (pcbplotparams
      (layerselection 0x000c0_80000007)
      (usegerberextensions false)
      (excludeedgelayer false)
      (linewidth 0.050000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 2)
      (scaleselection 1)
      (outputdirectory PDF))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 +3V3)
  (net 5 "Net-(C5-Pad2)")
  (net 6 +5V)
  (net 7 "Net-(C16-Pad2)")
  (net 8 +1V8)
  (net 9 "Net-(C24-Pad2)")
  (net 10 "Net-(C25-Pad1)")
  (net 11 "Net-(C25-Pad2)")
  (net 12 "Net-(C29-Pad1)")
  (net 13 "Net-(C29-Pad2)")
  (net 14 "Net-(C32-Pad2)")
  (net 15 "Net-(C33-Pad1)")
  (net 16 "Net-(C33-Pad2)")
  (net 17 "Net-(C34-Pad2)")
  (net 18 "Net-(C35-Pad2)")
  (net 19 DP)
  (net 20 DM)
  (net 21 "Net-(D2-Pad2)")
  (net 22 RX)
  (net 23 TX)
  (net 24 SWDIO)
  (net 25 SWCLK)
  (net 26 SCL)
  (net 27 SDA)
  (net 28 DAC)
  (net 29 "Net-(R5-Pad2)")
  (net 30 MCLK)
  (net 31 SCK)
  (net 32 "Net-(R11-Pad1)")
  (net 33 LRCK)
  (net 34 /+5VDIG)
  (net 35 /+1V8OSC)
  (net 36 /+1V8VD)
  (net 37 /+1V8VA)
  (net 38 /+VP)
  (net 39 "Net-(R10-Pad2)")
  (net 40 "Net-(R12-Pad1)")
  (net 41 /+5VANA)
  (net 42 "Net-(U5-Pad2)")
  (net 43 PA15)
  (net 44 PA0)
  (net 45 "Net-(R13-Pad2)")
  (net 46 "Net-(C12-Pad1)")
  (net 47 "Net-(U12-Pad1)")
  (net 48 "Net-(C13-Pad1)")
  (net 49 "Net-(R2-Pad2)")
  (net 50 RST)
  (net 51 "Net-(R14-Pad2)")
  (net 52 "Net-(U9-Pad14)")
  (net 53 "Net-(U9-Pad16)")
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.5)
    (uvia_drill 0.254)
    (add_net +1V8)
    (add_net +3V3)
    (add_net +5V)
    (add_net /+1V8OSC)
    (add_net /+1V8VA)
    (add_net /+1V8VD)
    (add_net /+5VANA)
    (add_net /+5VDIG)
    (add_net /+VP)
    (add_net DAC)
    (add_net DM)
    (add_net DP)
    (add_net GND)
    (add_net LRCK)
    (add_net MCLK)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C16-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C24-Pad2)")
    (add_net "Net-(C25-Pad1)")
    (add_net "Net-(C25-Pad2)")
    (add_net "Net-(C29-Pad1)")
    (add_net "Net-(C29-Pad2)")
    (add_net "Net-(C32-Pad2)")
    (add_net "Net-(C33-Pad1)")
    (add_net "Net-(C33-Pad2)")
    (add_net "Net-(C34-Pad2)")
    (add_net "Net-(C35-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(U12-Pad1)")
    (add_net "Net-(U5-Pad2)")
    (add_net "Net-(U9-Pad14)")
    (add_net "Net-(U9-Pad16)")
    (add_net PA0)
    (add_net PA15)
    (add_net RST)
    (add_net RX)
    (add_net SCK)
    (add_net SCL)
    (add_net SDA)
    (add_net SWCLK)
    (add_net SWDIO)
    (add_net TX)
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 109.5377 73.9167)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 115.3416 76.6218)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 114.224 76.6599)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B20B550)
    (at 108.3185 78.9332)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 111.6078 84.953)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:Choke_SMD_LPS30 (layer B.Cu) (tedit 5ACA832D)
    (at 109.525 74.4628 180)
    (descr "SMD Power Inductors (NR series S type)")
    (tags "SMD inductor")
    (attr smd)
    (fp_text reference L2 (at 2.3622 9.144 450) (layer B.SilkS))
    (fp_text value "LPS3015 100u" (at 0 -2.4 180) (layer B.Fab))
    (pad 1 smd rect (at -1.2 0 180) (size 1.14 3.05) (layers B.Cu B.Paste B.Mask)
      (net 41 /+5VANA))
    (pad 2 smd rect (at 1.2 0 180) (size 1.14 3.05) (layers B.Cu B.Paste B.Mask)
      (net 6 +5V))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 105.7404 77.7394)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 104.9022 77.7394)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 129.6672 74.7676)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 137.0586 77.3711)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 108.2296 86.1976)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 132.131 73.65)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 136.322 82.794)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 116.3 84.9)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 106.096 73.523)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 101.27 76.444)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 101.27 78.476)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 129.2608 82.1964)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 128 79.873)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 126.289 77.46)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 125.527 76.051)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 115.367 75.301)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 118.923 79.619)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 118.8976 86.1228)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 125.2 84.4)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 137.9 86.9)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 136.031 85.846)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 137.9 75.428)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 135.687 73.396)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 101.27 81.27)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 58613494)
    (at 112.7 74.92 90)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference P1 (at 4.826 1.524 180) (layer F.SilkS))
    (fp_text value UART (at 1.8 0 180) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.27 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 0 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 22 RX))
    (pad 3 smd rect (at 0 1.27 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 23 TX))
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 58613494)
    (at 107.1374 84.0132 90)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (zone_connect 2)
    (attr smd)
    (fp_text reference P2 (at -6.858 1.905 180) (layer F.SilkS))
    (fp_text value SWD (at 1.8 0 180) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.27 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 smd rect (at 0 0 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 24 SWDIO) (zone_connect 2))
    (pad 3 smd rect (at 0 1.27 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 25 SWCLK) (zone_connect 2))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 101.27 83.048 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (zone_connect 2)
    (attr smd)
    (fp_text reference R1 (at 0 -5.715 90) (layer F.SilkS))
    (fp_text value 1M (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)") (zone_connect 2))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 123.114 82.6924 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 3.7592 -13.0048 180) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 125.7556 85.7658)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -0.6096 9.9822) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 /+1V8VD))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 128.7274 85.7912 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0.2794 -8.3058 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 /+1V8VD))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 109.779 75.936 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -7.366 0 270) (layer F.SilkS))
    (fp_text value 27 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at -0.145001 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 DAC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 120.066 78.095)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 5.334 -10.033) (layer F.SilkS))
    (fp_text value 1M (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C16-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B142FA1)
    (at 125.8572 81.651 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0.9652 -11.6586 180) (layer F.SilkS))
    (fp_text value 27 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 MCLK))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 111.7983 78.6157)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at -14.7955 9.3091) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 43 PA15))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 128.157 78.9205 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at -1.6626 -16.5735 180) (layer F.SilkS))
    (fp_text value 27 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 SCK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 119.939 83.556 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0.635 -10.0076 180) (layer F.SilkS))
    (fp_text value 27 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R12-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 LRCK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 112.5984 75.174 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C21 (at -7.2136 0.4318 270) (layer B.SilkS))
    (fp_text value 100u (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 -0.0016 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 41 /+5VANA))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_1206 (layer B.Cu) (tedit 58AA84B8)
    (at 108.5471 85.9944 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C7 (at 14.6304 5.0292 180) (layer B.SilkS))
    (fp_text value 100u (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at -0.0529 -0.1056 180) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 34 /+5VDIG))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_1206 (layer B.Cu) (tedit 5B142FF2)
    (at 114.986 75.174 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C20 (at -14.0462 -0.4826 270) (layer B.SilkS))
    (fp_text value 100u (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 -0.014 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 41 /+5VANA))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 116.0655 78.7935 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 9.2075 1.3335 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 PA0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 108.382 75.936 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at -12.0142 -3.7338 270) (layer F.SilkS))
    (fp_text value 27 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 DAC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R13-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:35RASMT2BHNTRX_Jack_no_holes (layer B.Cu) (tedit 5B158A41)
    (at 139 80 180)
    (descr "Headphones with microphone connector, 3.5mm, 4 pins.")
    (tags "3.5mm jack mic microphone phones headphones 4pins audio plug")
    (attr smd)
    (fp_text reference X2 (at -5.196 -0.127 180) (layer B.SilkS))
    (fp_text value JACK_35RASMT2BHNTRX (at 7.8 -5.9 180) (layer B.Fab))
    (fp_text user %R (at 7.3 0 180) (layer B.Fab))
    (pad 4 smd rect (at 11.7 -3.7 180) (size 2.9 2.5) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(U9-Pad14)"))
    (pad 1 smd rect (at 4.3 3.7 180) (size 2.4 2.5) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(U9-Pad16)"))
    (pad 5 smd rect (at 2.4 -3.7 180) (size 2.4 2.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 120.6248 82.6924 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -3.7592 -15.7988 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(C13-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 113.9065 77.841)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 2.9845 -12.954) (layer F.SilkS))
    (fp_text value 1k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 RST))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R14-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Button_P-TS1107GS (layer B.Cu) (tedit 5AFC7B2D)
    (at 119.5 80 180)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE7.pdf")
    (attr smd)
    (fp_text reference SW1 (at -3.3092 14.6812 180) (layer B.SilkS))
    (fp_text value P-TS1107GS (at 0 -3 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 3.75 0 180) (size 1.5 1.5) (layers B.Cu B.Paste B.Mask)
      (net 8 +1V8))
    (pad 1 smd rect (at -3.75 0 180) (size 1.5 1.5) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_EVQPE1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:QFN-40-1EP_5x5mm_Pitch0.4mm_Cirrus (layer F.Cu) (tedit 5B007751)
    (at 132.946 80.032 90)
    (descr "40-Lead Plastic Quad Flat, No Lead Package (MP) - 5x5 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.4")
    (zone_connect 2)
    (attr smd)
    (fp_text reference U9 (at 15.2466 6.8812 90) (layer F.SilkS))
    (fp_text value CS43131 (at 0 3.875 90) (layer F.Fab))
    (pad 1 smd oval (at -2.45 -1.8 90) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 26 SCL) (zone_connect 2))
    (pad 2 smd oval (at -2.45 -1.4 90) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 28 DAC) (zone_connect 2))
    (pad 3 smd oval (at -2.45 -1 90) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (zone_connect 2))
    (pad 4 smd oval (at -2.45 -0.6 90) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 36 /+1V8VD) (zone_connect 2))
    (pad 5 smd oval (at -2.45 -0.2 90) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C24-Pad2)") (zone_connect 2))
    (pad 6 smd oval (at -2.45 0.2 90) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C25-Pad2)") (zone_connect 2))
    (pad 7 smd oval (at -2.45 0.6 90) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 37 /+1V8VA) (zone_connect 2))
    (pad 8 smd oval (at -2.45 1 90) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 9 smd oval (at -2.45 1.4 90) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C25-Pad1)") (zone_connect 2))
    (pad 10 smd oval (at -2.45 1.8 90) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C33-Pad2)") (zone_connect 2))
    (pad 11 smd oval (at -1.8 2.45 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C33-Pad1)") (zone_connect 2))
    (pad 12 smd oval (at -1.4 2.45 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 13 smd oval (at -1 2.45 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 14 smd oval (at -0.6 2.45 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U9-Pad14)") (zone_connect 2))
    (pad 15 smd oval (at -0.2 2.45 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 16 smd oval (at 0.2 2.45 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U9-Pad16)") (zone_connect 2))
    (pad 17 smd oval (at 0.6 2.45 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 18 smd oval (at 1 2.45 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C35-Pad2)") (zone_connect 2))
    (pad 19 smd oval (at 1.4 2.45 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 20 smd oval (at 1.8 2.45 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C32-Pad2)") (zone_connect 2))
    (pad 21 smd oval (at 2.45 1.8 90) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C34-Pad2)") (zone_connect 2))
    (pad 22 smd oval (at 2.45 1.4 90) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 23 smd oval (at 2.45 1 90) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C29-Pad2)") (zone_connect 2))
    (pad 24 smd oval (at 2.45 0.6 90) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C29-Pad1)") (zone_connect 2))
    (pad 25 smd oval (at 2.45 0.2 90) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 37 /+1V8VA) (zone_connect 2))
    (pad 26 smd oval (at 2.45 -0.2 90) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 38 /+VP) (zone_connect 2))
    (pad 27 smd oval (at 2.45 -0.6 90) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (zone_connect 2))
    (pad 28 smd oval (at 2.45 -1 90) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R14-Pad2)") (zone_connect 2))
    (pad 29 smd oval (at 2.45 -1.4 90) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 30 smd oval (at 2.45 -1.8 90) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 31 smd oval (at 1.8 -2.45 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 36 /+1V8VD) (zone_connect 2))
    (pad 32 smd oval (at 1.4 -2.45 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 33 smd oval (at 1 -2.45 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (zone_connect 2))
    (pad 34 smd oval (at 0.6 -2.45 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R11-Pad1)") (zone_connect 2))
    (pad 35 smd oval (at 0.2 -2.45 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 36 smd oval (at -0.2 -2.45 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 37 smd oval (at -0.6 -2.45 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 30 MCLK) (zone_connect 2))
    (pad 38 smd oval (at -1 -2.45 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U5-Pad2)") (zone_connect 2))
    (pad 39 smd oval (at -1.4 -2.45 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 27 SDA) (zone_connect 2))
    (pad 40 smd oval (at -1.8 -2.45 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 41 smd rect (at 0.9 0.9 90) (size 1.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2) (zone_connect 2))
    (pad 41 smd rect (at 0.9 -0.9 90) (size 1.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2) (zone_connect 2))
    (pad 41 smd rect (at -0.9 0.9 90) (size 1.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2) (zone_connect 2))
    (pad 41 smd rect (at -0.9 -0.9 90) (size 1.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2) (zone_connect 2))
    (pad 41 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.Paste)
      (net 1 GND) (solder_paste_margin_ratio -0.2) (zone_connect 2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-40-1EP_5x5mm_Pitch0.4mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SOT-23-5 (layer B.Cu) (tedit 583F3A3F)
    (at 116.256 84.953 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at -13.208 -0.381 90) (layer B.SilkS))
    (fp_text value ADP151-3.3 (at 0 -2.9 90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 34 /+5VDIG))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 34 /+5VDIG))
    (pad 4 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SOT-23-5 (layer B.Cu) (tedit 583F3A3F)
    (at 112.7 84.953 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at -12.319 -2.54 90) (layer B.SilkS))
    (fp_text value ADP151-1.8 (at 0 -2.9 90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 34 /+5VDIG))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 34 /+5VDIG))
    (pad 4 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 8 +1V8))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SC-70-5 (layer F.Cu) (tedit 0)
    (at 122.86 78.73 90)
    (descr "SC70-5 SOT323-5")
    (attr smd)
    (fp_text reference U4 (at 8.89 1.905 90) (layer F.SilkS))
    (fp_text value NC7SZU04P5 (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -0.6604 1.016 90) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.6604 1.016 90) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 1.016 90) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C16-Pad2)"))
    (pad 4 smd rect (at 0.6604 -1.016 90) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C12-Pad1)"))
    (pad 5 smd rect (at -0.6604 -1.016 90) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 35 /+1V8OSC))
    (model TO_SOT_Packages_SMD.3dshapes/SC-70-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SC-70-5 (layer F.Cu) (tedit 0)
    (at 122.86 84.064 90)
    (descr "SC70-5 SOT323-5")
    (attr smd)
    (fp_text reference U5 (at -12.9032 -1.2192 90) (layer F.SilkS))
    (fp_text value NC7SZ04P5 (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -0.6604 1.016 90) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.6604 1.016 90) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 1.016 90) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U5-Pad2)"))
    (pad 4 smd rect (at 0.6604 -1.016 90) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R12-Pad1)"))
    (pad 5 smd rect (at -0.6604 -1.016 90) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 36 /+1V8VD))
    (model TO_SOT_Packages_SMD.3dshapes/SC-70-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SC-70-5 (layer F.Cu) (tedit 0)
    (at 122.86 81.27 270)
    (descr "SC70-5 SOT323-5")
    (attr smd)
    (fp_text reference U6 (at 12.7508 0.7112 270) (layer F.SilkS))
    (fp_text value NC7SZ04P5 (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -0.6604 1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.6604 1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C16-Pad2)"))
    (pad 4 smd rect (at 0.6604 -1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R10-Pad2)"))
    (pad 5 smd rect (at -0.6604 -1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 35 /+1V8OSC))
    (model TO_SOT_Packages_SMD.3dshapes/SC-70-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SOT-23-5 (layer B.Cu) (tedit 583F3A3F)
    (at 121.749778 85.08)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U7 (at -0.616978 14.2748) (layer B.SilkS))
    (fp_text value ADP151-1.8 (at 0 -2.9) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 41 /+5VANA))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 41 /+5VANA))
    (pad 4 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 36 /+1V8VD))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SOT-23-5 (layer B.Cu) (tedit 583F3A3F)
    (at 129.591 74.793)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U8 (at 1.651 -11.557) (layer B.SilkS))
    (fp_text value ADP151-3.3 (at 0 -2.9) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 41 /+5VANA))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 41 /+5VANA))
    (pad 4 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 38 /+VP))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SOT-23-5 (layer B.Cu) (tedit 583F3A3F)
    (at 120.701 76.063 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U10 (at -5.4102 12.4714 180) (layer B.SilkS))
    (fp_text value ADP151-1.8 (at 0 -2.9 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 38 /+VP))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 44 PA0))
    (pad 4 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 35 /+1V8OSC))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SOT-23-5 (layer B.Cu) (tedit 583F3A3F)
    (at 131.369 84.826)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U11 (at -0.381 11.938) (layer B.SilkS))
    (fp_text value ADP151-1.8 (at 0 -2.9) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 38 /+VP))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 38 /+VP))
    (pad 4 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 37 /+1V8VA))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SOT-23 (layer F.Cu) (tedit 5B142F67)
    (at 105.715 76.063 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U12 (at -0.381 7.239 180) (layer F.SilkS))
    (fp_text value MCP120-3.15 (at 0 2.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U12-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SOT-23 (layer F.Cu) (tedit 59E653E3)
    (at 102.54 80.0508 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D1 (at 5.588 0 180) (layer F.SilkS))
    (fp_text value TPD2E2U06-Q1 (at 0 2.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 DP))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 DM))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Choke_SMD_LPS30 (layer B.Cu) (tedit 5ACA832D)
    (at 108.3566 82.9718 180)
    (descr "SMD Power Inductors (NR series S type)")
    (tags "SMD inductor")
    (attr smd)
    (fp_text reference L1 (at 18.161 -0.4572 450) (layer B.SilkS))
    (fp_text value "LPS3015 100u" (at 0 -2.4 180) (layer B.Fab))
    (pad 1 smd rect (at -1.2 0 180) (size 1.14 3.05) (layers B.Cu B.Paste B.Mask)
      (net 34 /+5VDIG))
    (pad 2 smd rect (at 1.2 0 180) (size 1.14 3.05) (layers B.Cu B.Paste B.Mask)
      (net 6 +5V))
  )
  (module footprints:VIA-0.3mm (layer F.Cu) (tedit 5B143424)
    (at 104.306 83.556)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module footprints:LED_0603 (layer B.Cu) (tedit 5B1588BB)
    (at 113.335 80 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at -0.5715 15.3924 180) (layer B.SilkS))
    (fp_text value LED (at 0 -1.35 180) (layer B.Fab))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module footprints:Crystal_SMD_EuroQuartz_MJ-4pin_5.0x3.2mm (layer F.Cu) (tedit 5B15883A)
    (at 121.844 75.301 180)
    (descr "SMD Crystal EuroQuartz MJ series http://cdn-reichelt.de/documents/datenblatt/B400/MJ.pdf, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Q2 (at -1.1176 13.6398 180) (layer F.SilkS))
    (fp_text value 22.579MHz (at 0 2.8 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.85 1.15 180) (size 1.9 1.1) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 1.85 1.15 180) (size 1.9 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.85 -1.15 180) (size 1.9 1.1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C16-Pad2)"))
    (pad 4 smd rect (at -1.85 -1.15 180) (size 1.9 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_EuroQuartz_MJ-4pin_5.0x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Crystal_SMD_EuroQuartz_MT-4pin_3.2x2.5mm (layer F.Cu) (tedit 5B158C5D)
    (at 115.24 83.556 180)
    (descr "SMD Crystal EuroQuartz MT series http://cdn-reichelt.de/documents/datenblatt/B400/MT.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Q1 (at 0.9652 -12.5476 180) (layer F.SilkS))
    (fp_text value 8MHz (at 0 2.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0.9 180) (size 1.3 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad2)"))
    (pad 2 smd rect (at 1.1 0.9 180) (size 1.3 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 -0.9 180) (size 1.3 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 4 smd rect (at -1.1 -0.9 180) (size 1.3 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_EuroQuartz_MT-4pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 106.4008 86.1976)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -0.6008 4.9024) (layer F.SilkS))
    (fp_text value 4n7 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 129.2608 82.9464 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C39 (at 10.1536 -8.2392 270) (layer F.SilkS))
    (fp_text value 10p (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 28 DAC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer B.Cu) (tedit 5B218981)
    (at 118.8976 85.3728 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 9.2272 2.9976 270) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer B.Cu) (tedit 5B218981)
    (at 132.131 74.412 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C28 (at -14.912 -2.769 270) (layer B.SilkS))
    (fp_text value 22u (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 38 /+VP))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 119.939 84.826)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at -1.639 12.874) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 /+1V8VD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer B.Cu) (tedit 5B218981)
    (at 112.319 82.3495)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (zone_connect 2)
    (attr smd)
    (fp_text reference C9 (at -4.919 10.9505) (layer B.SilkS))
    (fp_text value 2.2u (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 +1V8) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer B.Cu) (tedit 5B218981)
    (at 124.289778 84.895624 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C18 (at 13.404376 -3.310222 270) (layer B.SilkS))
    (fp_text value 2.2u (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 36 /+1V8VD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer B.Cu) (tedit 5B218981)
    (at 118.034 76.444 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C36 (at 13.244 2.566 90) (layer B.SilkS))
    (fp_text value 2.2u (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 35 /+1V8OSC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer B.Cu) (tedit 5B218981)
    (at 134.036 85.08 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C37 (at 12.32 -0.564 270) (layer B.SilkS))
    (fp_text value 2.2u (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 37 /+1V8VA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 137.047 78.095 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C35 (at -3.795 -5.153 270) (layer F.SilkS))
    (fp_text value 2.2u (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C35-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 135.65 75.444 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C34 (at -6.244 0.05 270) (layer F.SilkS))
    (fp_text value 2.2u (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C34-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 137.25 82.75 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C33 (at 0.65 -7.85 270) (layer F.SilkS))
    (fp_text value 2.2u (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C33-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C33-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 137.047 75.444 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C32 (at -6.444 -0.853 270) (layer F.SilkS))
    (fp_text value 22u (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C29-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C32-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 133.999 85.858 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C31 (at -0.801 -7.642 180) (layer F.SilkS))
    (fp_text value 2.2u (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 37 /+1V8VA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 136.031 85.096 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C30 (at -7.304 5.969 90) (layer F.SilkS))
    (fp_text value 2.2u (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C25-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 134.253 75.444 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C29 (at -5.944 0.353 270) (layer F.SilkS))
    (fp_text value 22u (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C29-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C29-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 131.713 76.079)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C26 (at -0.313 -8.579) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 38 /+VP))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 133.999 84.334 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C25 (at -8.301 -5.566 180) (layer F.SilkS))
    (fp_text value 15u (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C25-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C25-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 131.967 85.096 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C24 (at -7.304 -0.667 90) (layer F.SilkS))
    (fp_text value 15u (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 37 /+1V8VA))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C24-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 131.713 74.682 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C23 (at 0.413 5.382 180) (layer F.SilkS))
    (fp_text value 2.2u (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 37 /+1V8VA))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 130.57 85.096 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C22 (at 7.304 -2.13 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 /+1V8VD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 128.157 77.476 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C19 (at 0.057 8.076 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 /+1V8VD))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 125.8572 80.2032 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C17 (at -2.7428 -11.4968 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 35 /+1V8OSC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 118.034 77.46 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 8.66 0.966 90) (layer F.SilkS))
    (fp_text value 10p (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C16-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 119.685 79.619)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 1.515 -10.819) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 35 /+1V8OSC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 125.527 75.301 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at -9.801 -2.873 270) (layer F.SilkS))
    (fp_text value 10p (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 113.843 79.492)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at -3.943 -8.792) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 105.3975 79.4412 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 7.5975 2.2412 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 +1V8))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer B.Cu) (tedit 5B218981)
    (at 115.24 82.3495)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (zone_connect 2)
    (attr smd)
    (fp_text reference C8 (at -4.64 11.6505) (layer B.SilkS))
    (fp_text value 2.2u (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer B.Cu) (tedit 5B218981)
    (at 106.096 74.285 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at -6.985 3.196 270) (layer B.SilkS))
    (fp_text value 2.2u (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 117.9705 84.318 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -9.582 -4.2705 90) (layer F.SilkS))
    (fp_text value 10p (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer B.Cu) (tedit 5B218981)
    (at 108.4836 79.123 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -3.277 -10.3836 90) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B218981)
    (at 112.446 84.445 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -7.155 -1.146 90) (layer F.SilkS))
    (fp_text value 10p (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:UFQFPN28 (layer F.Cu) (tedit 5B21886A)
    (at 109.652 80 180)
    (zone_connect 2)
    (fp_text reference U3 (at 2.286 -17.145 180) (layer F.SilkS))
    (fp_text value STM32F048G6 (at 0 3.125 180) (layer F.Fab))
    (pad 1 smd oval (at -2.125 -1.5 270) (size 0.3 0.65) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(C13-Pad1)") (zone_connect 2))
    (pad 2 smd oval (at -2.075 -1 270) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)") (zone_connect 2))
    (pad 3 smd oval (at -2.075 -0.5 270) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad2)") (zone_connect 2))
    (pad 4 smd oval (at -2.075 0 270) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (zone_connect 2))
    (pad 5 smd oval (at -2.075 0.5 270) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3) (zone_connect 2))
    (pad 6 smd oval (at -2.075 1 270) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 44 PA0) (zone_connect 2))
    (pad 7 smd oval (at -2.125 1.5 270) (size 0.3 0.65) (layers F.Cu F.Paste F.Mask)
      (net 50 RST) (zone_connect 2))
    (pad 8 smd oval (at -1.5 2.125 180) (size 0.3 0.65) (layers F.Cu F.Paste F.Mask)
      (net 23 TX) (zone_connect 2))
    (pad 9 smd oval (at -1 2.075 180) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 RX) (zone_connect 2))
    (pad 10 smd oval (at -0.5 2.075 180) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 33 LRCK) (zone_connect 2))
    (pad 11 smd oval (at 0 2.075 180) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 31 SCK) (zone_connect 2))
    (pad 12 smd oval (at 0.5 2.075 180) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R5-Pad2)") (zone_connect 2))
    (pad 13 smd oval (at 1 2.075 180) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R13-Pad2)") (zone_connect 2))
    (pad 14 smd oval (at 1.5 2.125 180) (size 0.3 0.65) (layers F.Cu F.Paste F.Mask)
      (zone_connect 2))
    (pad 15 smd oval (at 2.125 1.5 270) (size 0.3 0.65) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U12-Pad1)") (zone_connect 2))
    (pad 16 smd oval (at 2.075 1 270) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 17 smd oval (at 2.075 0.5 270) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 +1V8) (zone_connect 2))
    (pad 18 smd oval (at 2.075 0 270) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3) (zone_connect 2))
    (pad 19 smd oval (at 2.075 -0.5 270) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 DM) (zone_connect 2))
    (pad 20 smd oval (at 2.075 -1 270) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 DP) (zone_connect 2))
    (pad 21 smd oval (at 2.125 -1.5 270) (size 0.3 0.65) (layers F.Cu F.Paste F.Mask)
      (net 24 SWDIO) (zone_connect 2))
    (pad 22 smd oval (at 1.5 -2.125 180) (size 0.3 0.65) (layers F.Cu F.Paste F.Mask)
      (net 25 SWCLK) (zone_connect 2))
    (pad 23 smd oval (at 1 -2.075 180) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 43 PA15) (zone_connect 2))
    (pad 24 smd oval (at 0.5 -2.075 180) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 25 smd oval (at 0 -2.075 180) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 26 smd oval (at -0.5 -2.075 180) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 27 smd oval (at -1 -2.075 180) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 26 SCL) (zone_connect 2))
    (pad 28 smd oval (at -1.5 -2.125 180) (size 0.3 0.65) (layers F.Cu F.Paste F.Mask)
      (net 27 SDA) (zone_connect 2))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 128.6512 75.1232 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (zone_connect 2)
    (attr smd)
    (fp_text reference R15 (at 9.4488 -1.8796 90) (layer F.SilkS))
    (fp_text value 1M (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R14-Pad2)") (zone_connect 2))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:MOLEX-48037-1000-USB (layer B.Cu) (tedit 5B22D19A)
    (at 102.75 80 90)
    (descr "USB A connector female THT")
    (tags "USB USB_A_female THT")
    (zone_connect 2)
    (fp_text reference X1 (at 3.302 -6.56 90) (layer B.SilkS))
    (fp_text value USB_A (at 0.1 -10.34 90) (layer B.Fab))
    (pad 4 smd rect (at -3.5 2.6 90) (size 1.2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 3 smd rect (at -1 2.6 90) (size 1.2 2) (layers B.Cu B.Paste B.Mask)
      (net 19 DP) (zone_connect 2))
    (pad 2 smd rect (at 1 2.6 90) (size 1.2 2) (layers B.Cu B.Paste B.Mask)
      (net 20 DM) (zone_connect 2))
    (pad 1 smd rect (at 3.5 2.6 90) (size 1.2 2) (layers B.Cu B.Paste B.Mask)
      (net 6 +5V) (zone_connect 2))
    (pad "" thru_hole oval (at 5.7 0 90) (size 2.5 4) (drill oval 1.2 2.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad "" thru_hole circle (at 2.25 0 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad "" thru_hole circle (at -2.25 0 180) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad 5 thru_hole oval (at -5.7 0 90) (size 2.5 4) (drill oval 1.2 2.5) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)") (zone_connect 2))
  )
  (gr_text "32bit\nDAC" (at 126.8478 83.7338) (layer F.SilkS))
  (gr_text async (at 105.586888 82.178058) (layer F.SilkS))
  (gr_text UAC1 (at 105.60603 81.364676) (layer F.SilkS))
  (gr_text MODE (at 114.605 78.5522 180) (layer B.SilkS))
  (gr_text HP (at 137.3888 76.2916 180) (layer B.SilkS))
  (gr_text async (at 118.573658 73.141418 180) (layer B.SilkS))
  (gr_text UAC1 (at 118.599058 73.903418 180) (layer B.SilkS))
  (gr_text rev.A (at 134.8996 73.3198) (layer F.SilkS))
  (gr_text μDAC (at 128.6766 73.1928) (layer F.SilkS))
  (gr_text "©Lukaso 18" (at 115.9766 86.8326) (layer F.SilkS))
  (gr_text rev.A (at 134.8996 73.3706 180) (layer B.SilkS))
  (gr_text μDAC (at 123.876 73.8532 180) (layer B.SilkS))
  (dimension 39 (width 0.3) (layer Dwgs.User)
    (gr_text "39,000 mm" (at 119.5 91.35) (layer Dwgs.User))
    (feature1 (pts (xy 139 89) (xy 139 92.7)))
    (feature2 (pts (xy 100 89) (xy 100 92.7)))
    (crossbar (pts (xy 100 90) (xy 139 90)))
    (arrow1a (pts (xy 139 90) (xy 137.873496 90.586421)))
    (arrow1b (pts (xy 139 90) (xy 137.873496 89.413579)))
    (arrow2a (pts (xy 100 90) (xy 101.126504 90.586421)))
    (arrow2b (pts (xy 100 90) (xy 101.126504 89.413579)))
  )
  (dimension 16 (width 0.3) (layer Dwgs.User)
    (gr_text "16,000 mm" (at 148.299952 80 90) (layer Dwgs.User))
    (feature1 (pts (xy 140 72) (xy 149.649952 72)))
    (feature2 (pts (xy 140 88) (xy 149.649952 88)))
    (crossbar (pts (xy 146.949952 88) (xy 146.949952 72)))
    (arrow1a (pts (xy 146.949952 72) (xy 147.536373 73.126504)))
    (arrow1b (pts (xy 146.949952 72) (xy 146.363531 73.126504)))
    (arrow2a (pts (xy 146.949952 88) (xy 147.536373 86.873496)))
    (arrow2b (pts (xy 146.949952 88) (xy 146.363531 86.873496)))
  )
  (gr_arc (start 138 87) (end 139 87) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 138 73) (end 138 72) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 101 87) (end 101 88) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 101 73) (end 100 73) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 87) (end 100 80) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138 88) (end 101 88) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139 73) (end 139 87) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101 72) (end 138 72) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 80) (end 100 73) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.75 71.25) (xy 139.75 71.25) (xy 139.75 88.75) (xy 99.75 88.75)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.5 71) (xy 150 71) (xy 150 89) (xy 99.5 89)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 99.5 71) (xy 150 71) (xy 150 89) (xy 99.5 89)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer In2.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.2))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 100 71.5) (xy 109 71.5) (xy 109 80) (xy 116.5608 80) (xy 116.5608 88.5)
        (xy 100 88.5)
      )
    )
  )
  (zone (net 35) (net_name /+1V8OSC) (layer In2.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 121.75 74.75) (xy 124 77) (xy 125.5 77) (xy 125.5 81) (xy 117.5 81)
        (xy 117.5 74.75)
      )
    )
  )
  (zone (net 38) (net_name /+VP) (layer In2.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads (clearance 0.2))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 128.5 72) (xy 132.6 72) (xy 132.6 77.5) (xy 130.75 77.5) (xy 130.75 85.25)
        (xy 128.5 85.25)
      )
    )
  )
  (zone (net 37) (net_name /+1V8VA) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 131 72) (xy 139.5 72) (xy 139.5 88) (xy 131 88)
      )
    )
  )
  (zone (net 41) (net_name /+5VANA) (layer In2.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.2))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.127) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 110.5 72) (xy 110.5 77) (xy 117 77) (xy 117 74.3) (xy 122.1 74.3)
        (xy 123.25 75.5) (xy 127.75 75.5) (xy 127.75 79) (xy 128.25 79) (xy 128.25 72)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.8234 79.238) (xy 134.8234 79.619) (xy 135.941 79.619) (xy 136.449 80.127) (xy 137.338 80.127)
        (xy 137.719 80.127) (xy 137.719 79.492) (xy 137.592 79.365) (xy 136.576 79.365) (xy 136.449 79.238)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.798 80.889) (xy 134.798 81.27) (xy 135.941 81.27) (xy 136.195 81.651) (xy 136.703 81.651)
        (xy 136.83 81.524) (xy 136.83 81.016) (xy 136.703 80.889)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.25 80.75) (xy 136 81) (xy 136 81.5) (xy 136.25 81.75) (xy 136.25 82.5)
        (xy 137.25 82.5) (xy 137.25 79.5) (xy 137 79.25) (xy 136.5 79.25) (xy 136.25 79.5)
        (xy 136.25 80) (xy 136.5 80.25) (xy 136.5 80.5) (xy 136.5 80.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136 81) (xy 136.25 80.75) (xy 136.75 80.75) (xy 137 81) (xy 137 81.5)
        (xy 136.75 81.75) (xy 136.25 81.75) (xy 136 81.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.25 79.5) (xy 136.5 79.25) (xy 137 79.25) (xy 137.25 79.5) (xy 137.25 80)
        (xy 137 80.25) (xy 136.5 80.25) (xy 136.25 80)
      )
    )
  )
  (zone (net 3) (net_name "Net-(C2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.8128 83.5052) (xy 101.778 83.5052) (xy 101.778 85.6896) (xy 100.8128 85.6896)
      )
    )
  )
  (zone (net 36) (net_name /+1V8VD) (layer In2.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.2))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 120 83.5) (xy 128.25 83.5) (xy 130.75 83.5) (xy 130.75 88) (xy 120 88)
      )
    )
  )
  (zone (net 3) (net_name "Net-(C2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.887206 86.6802) (xy 103.887206 85.715) (xy 106.071606 85.715) (xy 106.071606 86.6802)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 108.5 70.75) (xy 129.5 70.75) (xy 129.5 89.5) (xy 108.25 89.5) (xy 108.25 70.75)
      )
    )
  )
)
