<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="35" x2="0" y2="5" width="0" layer="20"/>
<wire x1="0" y1="5" x2="5" y2="0" width="0" layer="20"/>
<wire x1="5" y1="0" x2="89.5" y2="0" width="0" layer="20"/>
<wire x1="89.5" y1="0" x2="91.5" y2="2" width="0" layer="20"/>
<wire x1="91.5" y1="2" x2="93.2688" y2="2.0066" width="0" layer="20"/>
<wire x1="93.2688" y1="2.0066" x2="93.8302" y2="2.0066" width="0" layer="20"/>
<wire x1="93.8302" y1="2.0066" x2="95.8368" y2="0" width="0" layer="20"/>
<wire x1="95.8368" y1="0" x2="180" y2="0" width="0" layer="20"/>
<wire x1="180" y1="0" x2="185" y2="5" width="0" layer="20"/>
<wire x1="185" y1="5" x2="185" y2="35" width="0" layer="20"/>
<wire x1="185" y1="35" x2="0" y2="35" width="0" layer="20"/>
<text>1% PRECISION</text>
<text>1% PRECISION</text>
<text>1% PRECISION</text>
<text>1% PRECISION</text>
<text>MusselBedHeater
RevF</text>
<text>Luke Miller 2020</text>
<text>MusselBedHeater
RevF</text>
<text>Luke Miller 2020
luke.miller@sdsu.edu</text>
<text>GND</text>
<text>DTR</text>
<text>VCC</text>
<text>GND</text>
<text>GND</text>
<text>+12V</text>
<text>+12V</text>
<text>GND</text>
<text>VCC</text>
<text>SCL</text>
<text>SDA</text>
<text>+</text>
<text>VRAW</text>
<text>GND</text>
<text>VRAW</text>
<text>GND</text>
<text>DATA</text>
<text>DATA</text>
<text>DATA</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>VCC</text>
<text>VCC</text>
<text>HEAT_GND</text>
<text>HEAT_GND</text>
<text>THERM</text>
<text>THERM</text>
<text>THERM</text>
<text>THERM</text>
<text>THERM</text>
<text>THERM</text>
<text>THERM</text>
<text>THERM</text>
<text>THERM</text>
<text>THERM</text>
<text>THERM</text>
<text>THERM</text>
<text>THERM</text>
<text>THERM</text>
<text>THERM</text>
<text>VRAW</text>
<text>VRAW</text>
<text>VRAW</text>
<text>VRAW</text>
<text>VRAW</text>
<text>VRAW</text>
<text>VRAW</text>
<text>VRAW</text>
<text>VRAW</text>
<text>VRAW</text>
<text>VRAW</text>
<text>HEAT_GND</text>
<text>HEAT_GND</text>
<text>HEAT_GND</text>
<text>HEAT_GND</text>
<text>HEAT_GND</text>
<text>HEAT_GND</text>
<text>HEAT_GND</text>
<text>HEAT_GND</text>
<text>HEAT_GND</text>
<text>HEAT_GND</text>
<text>HEAT_GND</text>
<text>HEAT_GND</text>
<text>HEAT_GND</text>
<text>HEAT_GND</text>
<text>HEAT_GND</text>
<text>THERM</text>
<text>THERM</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VRAW</text>
<text>GND</text>
<text>GND</text>
<text>VRAW</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>14</text>
<text>15</text>
<text>16</text>
<text>1</text>
<text>16</text>
<text>1</text>
<text>16</text>
<text>2</text>
<text>AREF</text>
<text>VCC</text>
<text>GND</text>
<text>SCK</text>
<text>MOSI</text>
<text>MISO</text>
<text>RST</text>
<text>CR1220
BATTERY</text>
<text>4-40</text>
<text>4-40</text>
<text>VCC</text>
<text>GND</text>
<text>RST</text>
<text>SCK</text>
<text>optional</text>
<text>0.1uF</text>
</plain>
<libraries>
<library name="miller">
<packages>
<package name="SOT-89">
<description>SOT-89 footprint&lt;br&gt;
Based on Diodes Incorporated footprint for AP2204 voltage regulator</description>
</package>
<package name="TERMINAL-2PIN-5.08MM_LARGEHOLE">
<description>2-pin terminal block, 5.08mm spacing, drill hole diameter 1.5mm</description>
</package>
<package name="PUSHBUTTON_SPST_PTS525_SERIES">
<description>C&amp;K PTS525 series tactile switch&lt;br&gt;
Small surface mount switches</description>
</package>
<package name="0603">
<description>0603 surface mount part</description>
</package>
<package name="PANASONIC_B">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package B&lt;/b&gt;</description>
</package>
<package name="DS3231M_SOIC8">
<description>Maxim DS3231M real time clock pattern&lt;br&gt;
This is the smaller cheaper DS3231M model, vs S model. This version does not have as many square wave output frequencies (just 32.768 kHz and 1Hz).</description>
</package>
<package name="1X06-RIGHT_ANGLE">
<description>1x06 0.1" spacing right angle header&lt;p&gt;
Example: Sullins PPPC061LGBN-RC, Digikey PN S5481-ND</description>
</package>
<package name="4-40-SCREW-HOLE">
<description>&lt;b&gt;4-40 size drill hole&lt;/b&gt;&lt;br&gt;
Sized to fit a 0.112" 4-40 screw fit through, with outer guidelines for a socket-head cap diameter of 0.183"&lt;br&gt;
See McMaster part 92185A110</description>
</package>
<package name="2X3_LOCK">
</package>
<package name="MOLEX_KK_254_4PIN_HEADER">
<description>Molex KK 254 series straight header. Through-hole, 2.54 (0.1") spacing. 4 pin. 
Molex PN# 47053-1000</description>
</package>
<package name="SOT23-3">
<description>SOT23-3 package&lt;br&gt;
Pad size 0.8 x 0.9mm</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip 0603 size</description>
</package>
<package name="TC2030-MCP-NL">
<description>&lt;B&gt;TAG-CONNECT ICSP Connector&lt;/B&gt;&lt;BR&gt;&lt;I&gt;Manufacturer:&lt;/I&gt; &lt;a href="www.tag-connect.com"&gt;Tag-Connect&lt;/a&gt;&lt;BR&gt;
&lt;BR&gt;Cable for easy In-Circuit Serial Programming. Designed for Microchip ICD2, suitable for many others.&lt;BR&gt;

&lt;TABLE cellspacing=0 cellpadding=0 border=0&gt;
&lt;TR&gt;&lt;TD width=20&gt;&lt;/TD&gt;&lt;TD&gt;
&lt;TABLE cellspacing=0 cellpadding=1 border=1&gt;
&lt;TR bgcolor=silver&gt;&lt;TD align=center&gt;PAD&lt;/TD&gt;&lt;TD align=center&gt;Description&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;1&lt;/TD&gt;&lt;TD&gt;MCLR/Vpp&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;2&lt;/TD&gt;&lt;TD&gt;Vdd&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;3&lt;/TD&gt;&lt;TD&gt;GND&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;4&lt;/TD&gt;&lt;TD&gt;PGD (ISPDAT)&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;5&lt;/TD&gt;&lt;TD&gt;PGC (ISPCLK)&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;6&lt;/TD&gt;&lt;TD&gt;nc (used for LVP)&lt;/TD&gt;&lt;/TR&gt;
&lt;/TABLE&gt;
&lt;/TD&gt;&lt;/TR&gt;&lt;/TABLE&gt;&lt;BR&gt;&lt;BR&gt;

©2009 ROFA.cz - modified and updated by Robert Darlington &amp;#8249;rdarlington@gmail.com&amp;#8250;</description>
</package>
<package name="SOT1210">
<description>&lt;li&gt;&lt;b&gt;SOT1210&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;Plastic single ended surface mounted package (LFPAK33); 8 leads
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: ---
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: ---&lt;/ul&gt;</description>
</package>
<package name="MICROSD_SOCKET_MOLEX_REVERSEMOUNT">
<description>&lt;b&gt;Molex micro SD card slot, push-push spring-loaded style "reverse mount"&lt;/b&gt;&lt;br&gt;
Molex PN 5027740891&lt;br&gt;
Digikey PN WM24066CT-ND&lt;br&gt;
This version has the surface mount pins easily accessible at the rear of the housing rather than underneath it like most other sockets.</description>
</package>
<package name="CR1220_BATTERY_HOLDER_SMD">
<description>CR1220 Battery Holder, SMD
Keystone Part # 3000</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="TO-277-3">
<description>TO-277-3 footprint&lt;br&gt;
Found on Schottky Diode FSV1060V On Semiconductor</description>
</package>
<package name="28-TSSOP">
<description>28-pin TSSOP package&lt;br&gt;
Body width 4.4 mm, body length 9.8mm, pitch between pads 0.65mm</description>
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="1X02_NOSILK">
<description>1x2 header, 0.1" pitch</description>
</package>
<package name="OLED_0.96_I2C_GND_PIN1_WIDE">
<description>OLED 0.96" screen 128x64&lt;br&gt;
GND on Pin 1 &lt;b&gt; CHECK YOUR PARTICULAR SCREEN FOR WIRING&lt;/b&gt;
&lt;br&gt;
Wider footprint found on DIYMALL units from Amazon</description>
</package>
<package name="TQFP48">
<description>Thin Plastic Quad Flat Pack [TQFP] 48-lead</description>
</package>
<package name="LED_RGB_SMD_1.6X1.6">
<description>RGB LED 1.6mm x 1.6mm SMD footprint&lt;br&gt;
Example: Kingbright APTF1616SEEZGKQBKC red green blue LED.</description>
</package>
<package name="PANASONIC_C">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Series, S-Series Package C&lt;/b&gt;</description>
</package>
<package name="I_0805">
<description>&lt;b&gt;0805 (2012) Inductor footprint&lt;br&gt;&lt;/b&gt;
Example:
Taiyo Yuden inductor # LBR2012T100K&lt;br&gt;
Digikey PN 587-2045-1-ND</description>
</package>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;&lt;br&gt;
Drill 0.04" (1.016mm), copper diameter 0.07" (1.778mm)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="AP2204_VREG" library="miller" package="SOT-89" value="AP2204R">
<attribute name="NAME"/>
</element>
<element name="BATT_INPUT1" library="miller" package="TERMINAL-2PIN-5.08MM_LARGEHOLE" value="TERMINAL-2PIN-5.08MMLARGEHOLE"/>
<element name="BATT_INPUT2" library="miller" package="TERMINAL-2PIN-5.08MM_LARGEHOLE" value="TERMINAL-2PIN-5.08MMLARGEHOLE"/>
<element name="BUTTON1" library="miller" package="PUSHBUTTON_SPST_PTS525_SERIES" value="PUSHBUTTON_DPST_SMD2SMALL">
<attribute name="NAME"/>
</element>
<element name="C1" library="miller" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="miller" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="miller" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="miller" package="0603" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="miller" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="miller" package="PANASONIC_B" value="1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="miller" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DS3231M" library="miller" package="DS3231M_SOIC8" value="DS3231MSOIC-8">
<attribute name="NAME"/>
</element>
<element name="FTDI" library="miller" package="1X06-RIGHT_ANGLE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="miller" package="4-40-SCREW-HOLE" value="HOLE-LAYOUT4-40-SOCKET-HEAD"/>
<element name="H2" library="miller" package="4-40-SCREW-HOLE" value="HOLE-LAYOUT4-40-SOCKET-HEAD"/>
<element name="ISP" library="miller" package="2X3_LOCK" value="AVR_SPI_PRG_62X3_LOCK">
<attribute name="NAME"/>
</element>
<element name="MUSSEL1" library="miller" package="MOLEX_KK_254_4PIN_HEADER" value="MOLEX_KK_254_4_PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="MUSSEL2" library="miller" package="MOLEX_KK_254_4PIN_HEADER" value="MOLEX_KK_254_4_PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="MUSSEL11" library="miller" package="MOLEX_KK_254_4PIN_HEADER" value="MOLEX_KK_254_4_PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="MUSSEL12" library="miller" package="MOLEX_KK_254_4PIN_HEADER" value="MOLEX_KK_254_4_PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="MUSSEL13" library="miller" package="MOLEX_KK_254_4PIN_HEADER" value="MOLEX_KK_254_4_PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="MUSSEL14" library="miller" package="MOLEX_KK_254_4PIN_HEADER" value="MOLEX_KK_254_4_PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="MUSSEL15" library="miller" package="MOLEX_KK_254_4PIN_HEADER" value="MOLEX_KK_254_4_PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="MUSSEL16" library="miller" package="MOLEX_KK_254_4PIN_HEADER" value="MOLEX_KK_254_4_PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="MUSSEL3" library="miller" package="MOLEX_KK_254_4PIN_HEADER" value="MOLEX_KK_254_4_PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="MUSSEL4" library="miller" package="MOLEX_KK_254_4PIN_HEADER" value="MOLEX_KK_254_4_PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="MUSSEL5" library="miller" package="MOLEX_KK_254_4PIN_HEADER" value="MOLEX_KK_254_4_PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="MUSSEL6" library="miller" package="MOLEX_KK_254_4PIN_HEADER" value="MOLEX_KK_254_4_PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="MUSSEL7" library="miller" package="MOLEX_KK_254_4PIN_HEADER" value="MOLEX_KK_254_4_PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="MUSSEL8" library="miller" package="MOLEX_KK_254_4PIN_HEADER" value="MOLEX_KK_254_4_PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="MUSSEL9" library="miller" package="MOLEX_KK_254_4PIN_HEADER" value="MOLEX_KK_254_4_PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="MUSSEL10" library="miller" package="MOLEX_KK_254_4PIN_HEADER" value="MOLEX_KK_254_4_PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="MOSFET-P" library="miller" package="SOT23-3" value="MOSFET-PCHANNELBSH203">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08285"/>
</element>
<element name="R10" library="miller" package="R0603" value="10ohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="miller" package="R0603" value="10ohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="miller" package="R0603" value="82ohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="miller" package="R0603" value="47k 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="miller" package="R0603" value="10k 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="miller" package="R0603" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="miller" package="R0603" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="miller" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="miller" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="miller" package="R0603" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RESET" library="miller" package="PUSHBUTTON_SPST_PTS525_SERIES" value="PUSHBUTTON_DPST_SMD2SMALL">
<attribute name="NAME"/>
</element>
<element name="TC2030_ISP" library="miller" package="TC2030-MCP-NL" value="">
<attribute name="NAME"/>
</element>
<element name="TEMP17" library="miller" package="MOLEX_KK_254_4PIN_HEADER" value="MOLEX_KK_254_4_PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="TEMP18" library="miller" package="MOLEX_KK_254_4PIN_HEADER" value="MOLEX_KK_254_4_PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="TEMP19" library="miller" package="MOLEX_KK_254_4PIN_HEADER" value="MOLEX_KK_254_4_PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="TEMP20" library="miller" package="MOLEX_KK_254_4PIN_HEADER" value="MOLEX_KK_254_4_PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="U$11" library="miller" package="SOT1210" value="MOSFET-N_LFPAK33"/>
<element name="U$12" library="miller" package="SOT1210" value="MOSFET-N_LFPAK33"/>
<element name="U$13" library="miller" package="SOT1210" value="MOSFET-N_LFPAK33"/>
<element name="U$14" library="miller" package="SOT1210" value="MOSFET-N_LFPAK33"/>
<element name="U$15" library="miller" package="SOT1210" value="MOSFET-N_LFPAK33"/>
<element name="U$16" library="miller" package="SOT1210" value="MOSFET-N_LFPAK33"/>
<element name="U$17" library="miller" package="SOT1210" value="MOSFET-N_LFPAK33"/>
<element name="U$18" library="miller" package="SOT1210" value="MOSFET-N_LFPAK33"/>
<element name="U$19" library="miller" package="SOT1210" value="MOSFET-N_LFPAK33"/>
<element name="U$2" library="miller" package="MICROSD_SOCKET_MOLEX_REVERSEMOUNT" value="MICROSD_MOLEX_REVERSECURRENT"/>
<element name="U$20" library="miller" package="SOT1210" value="MOSFET-N_LFPAK33"/>
<element name="U$21" library="miller" package="SOT1210" value="MOSFET-N_LFPAK33"/>
<element name="U$22" library="miller" package="SOT1210" value="MOSFET-N_LFPAK33"/>
<element name="U$23" library="miller" package="SOT1210" value="MOSFET-N_LFPAK33"/>
<element name="U$24" library="miller" package="SOT1210" value="MOSFET-N_LFPAK33"/>
<element name="U$25" library="miller" package="SOT1210" value="MOSFET-N_LFPAK33"/>
<element name="U$5" library="miller" package="CR1220_BATTERY_HOLDER_SMD" value="BATTERY_BUTTON_CELLCR1220_SMD"/>
<element name="BJT_NPN" library="miller" package="SOT23" value="BJT_NPN_FMMT619TA">
<attribute name="NAME"/>
</element>
<element name="U$7" library="miller" package="TO-277-3" value="SCHOTTKY_DIODE_TO-277-3">
<attribute name="NAME"/>
</element>
<element name="U$8" library="miller" package="TO-277-3" value="SCHOTTKY_DIODE_TO-277-3">
<attribute name="NAME"/>
</element>
<element name="PCA9685" library="miller" package="28-TSSOP" value="PCA968528">
<attribute name="VALUE"/>
</element>
<element name="ATMEGA328P" library="miller" package="TQFP32-08" value="ATMEGA328P">
<attribute name="VALUE"/>
</element>
<element name="VRAW_TEST" library="miller" package="1X02_NOSILK" value="PINHD-1X2NOSILK"/>
<element name="OLED" library="miller" package="OLED_0.96_I2C_GND_PIN1_WIDE" value="OLED_0.96_I2CGND_PIN1_WIDE">
<attribute name="NAME"/>
</element>
<element name="ADG725B" library="miller" package="TQFP48" value="ADG725_MUX">
<attribute name="NAME"/>
</element>
<element name="R34" library="miller" package="R0603" value="Rref_1%">
<attribute name="NAME"/>
</element>
<element name="U$10" library="miller" package="SOT1210" value="MOSFET-N_LFPAK33"/>
<element name="R18" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="miller" package="R0603" value="Rref_1%">
<attribute name="NAME"/>
</element>
<element name="R36" library="miller" package="R0603" value="Rref_1%">
<attribute name="NAME"/>
</element>
<element name="R37" library="miller" package="R0603" value="Rref_1%">
<attribute name="NAME"/>
</element>
<element name="R38" library="miller" package="R0603" value="Rref_1%">
<attribute name="NAME"/>
</element>
<element name="R39" library="miller" package="R0603" value="Rref_1%">
<attribute name="NAME"/>
</element>
<element name="R40" library="miller" package="R0603" value="Rref_1%">
<attribute name="NAME"/>
</element>
<element name="R41" library="miller" package="R0603" value="Rref_1%">
<attribute name="NAME"/>
</element>
<element name="R42" library="miller" package="R0603" value="Rref_1%">
<attribute name="NAME"/>
</element>
<element name="R43" library="miller" package="R0603" value="Rref_1%">
<attribute name="NAME"/>
</element>
<element name="R44" library="miller" package="R0603" value="Rref_1%">
<attribute name="NAME"/>
</element>
<element name="R45" library="miller" package="R0603" value="Rref_1%">
<attribute name="NAME"/>
</element>
<element name="R46" library="miller" package="R0603" value="Rref_1%">
<attribute name="NAME"/>
</element>
<element name="R47" library="miller" package="R0603" value="Rref_1%">
<attribute name="NAME"/>
</element>
<element name="R48" library="miller" package="R0603" value="Rref_1%">
<attribute name="NAME"/>
</element>
<element name="R49" library="miller" package="R0603" value="Rref_1%">
<attribute name="NAME"/>
</element>
<element name="RGB_LED" library="miller" package="LED_RGB_SMD_1.6X1.6" value="LED_3_COLOR_ANODE1">
<attribute name="NAME"/>
</element>
<element name="C9" library="miller" package="PANASONIC_C" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="miller" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="miller" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="INDUCTOR" library="miller" package="I_0805" value="INDUCTOR0805_TY">
<attribute name="NAME"/>
</element>
<element name="C11" library="miller" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PC1" library="miller" package="1X01" value="PINHD-1X1STANDARD">
<attribute name="NAME"/>
</element>
<element name="PC2" library="miller" package="1X01" value="PINHD-1X1STANDARD">
<attribute name="NAME"/>
</element>
<element name="MAX6103" library="miller" package="SOT23-3" value="MAX6100-MAX6107_VOLTAGE_REF">
<attribute name="NAME"/>
</element>
<element name="C12" library="miller" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="miller" package="0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AREF" library="miller" package="1X01" value="PINHD-1X1STANDARD">
<attribute name="NAME"/>
</element>
<element name="C14" library="miller" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$2" pad="MNT4"/>
<contactref element="U$2" pad="MNT3"/>
<contactref element="U$2" pad="MNT2"/>
<contactref element="U$2" pad="MNT1"/>
<contactref element="U$2" pad="GND6"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="DS3231M" pad="5"/>
<contactref element="FTDI" pad="5"/>
<contactref element="FTDI" pad="6"/>
<contactref element="ATMEGA328P" pad="5"/>
<contactref element="ATMEGA328P" pad="3"/>
<contactref element="ATMEGA328P" pad="21"/>
<contactref element="C3" pad="2"/>
<contactref element="RESET" pad="P$1"/>
<contactref element="RESET" pad="P$2"/>
<contactref element="TC2030_ISP" pad="6"/>
<contactref element="ISP" pad="6"/>
<contactref element="VRAW_TEST" pad="2"/>
<contactref element="AP2204_VREG" pad="P$2"/>
<contactref element="C7" pad="-"/>
<contactref element="C1" pad="2"/>
<contactref element="U$5" pad="GND"/>
<contactref element="BUTTON1" pad="P$1"/>
<contactref element="BUTTON1" pad="P$2"/>
<contactref element="R14" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="BJT_NPN" pad="2"/>
<contactref element="BATT_INPUT1" pad="P$2"/>
<contactref element="BATT_INPUT2" pad="P$2"/>
<contactref element="PCA9685" pad="14"/>
<contactref element="PCA9685" pad="25"/>
<contactref element="PCA9685" pad="2"/>
<contactref element="PCA9685" pad="3"/>
<contactref element="PCA9685" pad="4"/>
<contactref element="PCA9685" pad="5"/>
<contactref element="PCA9685" pad="24"/>
<contactref element="C8" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="U$11" pad="1"/>
<contactref element="U$11" pad="2"/>
<contactref element="U$11" pad="3"/>
<contactref element="R20" pad="2"/>
<contactref element="U$12" pad="1"/>
<contactref element="U$12" pad="2"/>
<contactref element="U$12" pad="3"/>
<contactref element="R21" pad="2"/>
<contactref element="U$13" pad="1"/>
<contactref element="U$13" pad="2"/>
<contactref element="U$13" pad="3"/>
<contactref element="R22" pad="2"/>
<contactref element="U$14" pad="1"/>
<contactref element="U$14" pad="2"/>
<contactref element="U$14" pad="3"/>
<contactref element="R23" pad="2"/>
<contactref element="U$15" pad="1"/>
<contactref element="U$15" pad="2"/>
<contactref element="U$15" pad="3"/>
<contactref element="R24" pad="2"/>
<contactref element="U$16" pad="1"/>
<contactref element="U$16" pad="2"/>
<contactref element="U$16" pad="3"/>
<contactref element="R25" pad="2"/>
<contactref element="U$17" pad="1"/>
<contactref element="U$17" pad="2"/>
<contactref element="U$17" pad="3"/>
<contactref element="R26" pad="2"/>
<contactref element="U$18" pad="1"/>
<contactref element="U$18" pad="2"/>
<contactref element="U$18" pad="3"/>
<contactref element="R27" pad="2"/>
<contactref element="U$19" pad="1"/>
<contactref element="U$19" pad="2"/>
<contactref element="U$19" pad="3"/>
<contactref element="R28" pad="2"/>
<contactref element="U$20" pad="1"/>
<contactref element="U$20" pad="2"/>
<contactref element="U$20" pad="3"/>
<contactref element="R29" pad="2"/>
<contactref element="U$21" pad="1"/>
<contactref element="U$21" pad="2"/>
<contactref element="U$21" pad="3"/>
<contactref element="R30" pad="2"/>
<contactref element="U$22" pad="1"/>
<contactref element="U$22" pad="2"/>
<contactref element="U$22" pad="3"/>
<contactref element="R31" pad="2"/>
<contactref element="U$23" pad="1"/>
<contactref element="U$23" pad="2"/>
<contactref element="U$23" pad="3"/>
<contactref element="R32" pad="2"/>
<contactref element="U$24" pad="1"/>
<contactref element="U$24" pad="2"/>
<contactref element="U$24" pad="3"/>
<contactref element="R33" pad="2"/>
<contactref element="U$25" pad="1"/>
<contactref element="U$25" pad="2"/>
<contactref element="U$25" pad="3"/>
<contactref element="MUSSEL1" pad="P$2"/>
<contactref element="MUSSEL2" pad="P$2"/>
<contactref element="MUSSEL3" pad="P$2"/>
<contactref element="MUSSEL4" pad="P$2"/>
<contactref element="MUSSEL5" pad="P$2"/>
<contactref element="MUSSEL6" pad="P$2"/>
<contactref element="MUSSEL7" pad="P$2"/>
<contactref element="MUSSEL8" pad="P$2"/>
<contactref element="MUSSEL9" pad="P$2"/>
<contactref element="MUSSEL10" pad="P$2"/>
<contactref element="MUSSEL11" pad="P$2"/>
<contactref element="MUSSEL12" pad="P$2"/>
<contactref element="MUSSEL13" pad="P$2"/>
<contactref element="MUSSEL14" pad="P$2"/>
<contactref element="MUSSEL15" pad="P$2"/>
<contactref element="MUSSEL16" pad="P$2"/>
<contactref element="TEMP20" pad="P$2"/>
<contactref element="TEMP19" pad="P$2"/>
<contactref element="TEMP18" pad="P$2"/>
<contactref element="TEMP17" pad="P$2"/>
<contactref element="OLED" pad="GND"/>
<contactref element="R18" pad="2"/>
<contactref element="U$10" pad="2"/>
<contactref element="U$10" pad="1"/>
<contactref element="U$10" pad="3"/>
<contactref element="C9" pad="-"/>
<contactref element="ADG725B" pad="23"/>
<contactref element="ADG725B" pad="24"/>
<contactref element="C6" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="MAX6103" pad="3"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="PCA9685" pad="1"/>
<contactref element="C14" pad="2"/>
</signal>
<signal name="CS_SD">
<contactref element="U$2" pad="CS2"/>
<contactref element="ATMEGA328P" pad="14"/>
</signal>
<signal name="VCC">
<contactref element="U$2" pad="VDD4"/>
<contactref element="C5" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="DS3231M" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="FTDI" pad="4"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="TC2030_ISP" pad="2"/>
<contactref element="ISP" pad="2"/>
<contactref element="AP2204_VREG" pad="P$3"/>
<contactref element="C7" pad="+"/>
<contactref element="PCA9685" pad="28"/>
<contactref element="C8" pad="1"/>
<contactref element="OLED" pad="VCC"/>
<contactref element="ADG725B" pad="43"/>
<contactref element="ADG725B" pad="13"/>
<contactref element="ADG725B" pad="14"/>
<contactref element="TEMP17" pad="P$4"/>
<contactref element="TEMP18" pad="P$4"/>
<contactref element="TEMP19" pad="P$4"/>
<contactref element="TEMP20" pad="P$4"/>
<contactref element="RGB_LED" pad="P$1"/>
<contactref element="C6" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="INDUCTOR" pad="P$2"/>
<contactref element="ATMEGA328P" pad="4"/>
<contactref element="ATMEGA328P" pad="6"/>
<contactref element="R5" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="MAX6103" pad="1"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="U$2" pad="SCK5"/>
<contactref element="ATMEGA328P" pad="17"/>
<contactref element="TC2030_ISP" pad="3"/>
<contactref element="ISP" pad="3"/>
<contactref element="ADG725B" pad="19"/>
</signal>
<signal name="MOSI">
<contactref element="U$2" pad="MOSI3"/>
<contactref element="ATMEGA328P" pad="15"/>
<contactref element="TC2030_ISP" pad="4"/>
<contactref element="ISP" pad="4"/>
<contactref element="ADG725B" pad="18"/>
</signal>
<signal name="MISO">
<contactref element="U$2" pad="MISO7"/>
<contactref element="ATMEGA328P" pad="16"/>
<contactref element="TC2030_ISP" pad="1"/>
<contactref element="ISP" pad="1"/>
</signal>
<signal name="VBAT">
<contactref element="U$5" pad="P$1"/>
<contactref element="U$5" pad="P$2"/>
<contactref element="DS3231M" pad="6"/>
</signal>
<signal name="SDA">
<contactref element="DS3231M" pad="7"/>
<contactref element="ATMEGA328P" pad="27"/>
<contactref element="R2" pad="1"/>
<contactref element="PCA9685" pad="27"/>
<contactref element="OLED" pad="SDA"/>
</signal>
<signal name="SCL">
<contactref element="DS3231M" pad="8"/>
<contactref element="ATMEGA328P" pad="28"/>
<contactref element="R3" pad="1"/>
<contactref element="PCA9685" pad="26"/>
<contactref element="OLED" pad="SCL"/>
</signal>
<signal name="32KHZ">
<contactref element="DS3231M" pad="1"/>
<contactref element="ATMEGA328P" pad="7"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="DTR">
<contactref element="C2" pad="1"/>
<contactref element="FTDI" pad="1"/>
</signal>
<signal name="TO_FTDI_RX">
<contactref element="FTDI" pad="2"/>
<contactref element="ATMEGA328P" pad="31"/>
</signal>
<signal name="TO_FTDI_TX">
<contactref element="FTDI" pad="3"/>
<contactref element="ATMEGA328P" pad="30"/>
</signal>
<signal name="BUTTON1">
<contactref element="ATMEGA328P" pad="32"/>
<contactref element="BUTTON1" pad="P$3"/>
<contactref element="BUTTON1" pad="P$4"/>
</signal>
<signal name="N$4">
<contactref element="U$2" pad="NC1"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U$2" pad="RES8"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="GRNLED">
<contactref element="R10" pad="2"/>
<contactref element="ATMEGA328P" pad="9"/>
</signal>
<signal name="BLUELED">
<contactref element="R11" pad="2"/>
<contactref element="ATMEGA328P" pad="10"/>
</signal>
<signal name="REDLED">
<contactref element="R12" pad="2"/>
<contactref element="ATMEGA328P" pad="13"/>
</signal>
<signal name="RESET">
<contactref element="TC2030_ISP" pad="5"/>
<contactref element="ATMEGA328P" pad="29"/>
<contactref element="R4" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="RESET" pad="P$3"/>
<contactref element="RESET" pad="P$4"/>
<contactref element="ISP" pad="5"/>
</signal>
<signal name="VRAW">
<contactref element="VRAW_TEST" pad="1"/>
<contactref element="AP2204_VREG" pad="P$1"/>
<contactref element="U$7" pad="P$3"/>
<contactref element="U$8" pad="P$3"/>
<contactref element="R16" pad="1"/>
<contactref element="MOSFET-P" pad="2"/>
<contactref element="C9" pad="+"/>
<contactref element="MUSSEL1" pad="P$1"/>
<contactref element="MUSSEL2" pad="P$1"/>
<contactref element="MUSSEL3" pad="P$1"/>
<contactref element="MUSSEL4" pad="P$1"/>
<contactref element="MUSSEL5" pad="P$1"/>
<contactref element="MUSSEL6" pad="P$1"/>
<contactref element="MUSSEL7" pad="P$1"/>
<contactref element="MUSSEL8" pad="P$1"/>
<contactref element="MUSSEL9" pad="P$1"/>
<contactref element="MUSSEL10" pad="P$1"/>
<contactref element="MUSSEL11" pad="P$1"/>
<contactref element="MUSSEL12" pad="P$1"/>
<contactref element="MUSSEL13" pad="P$1"/>
<contactref element="MUSSEL14" pad="P$1"/>
<contactref element="MUSSEL15" pad="P$1"/>
<contactref element="MUSSEL16" pad="P$1"/>
</signal>
<signal name="PC1">
<contactref element="ATMEGA328P" pad="24"/>
<contactref element="PC1" pad="1"/>
</signal>
<signal name="PC2">
<contactref element="ATMEGA328P" pad="25"/>
<contactref element="PC2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$8" pad="P$1"/>
<contactref element="U$8" pad="P$2"/>
<contactref element="BATT_INPUT2" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="BJT_NPN" pad="3"/>
<contactref element="MOSFET-P" pad="1"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="BJT_NPN" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="BATT_MONITOR_EN">
<contactref element="R15" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="ATMEGA328P" pad="2"/>
</signal>
<signal name="BATT_MONITOR">
<contactref element="R13" pad="2"/>
<contactref element="R14" pad="1"/>
<contactref element="ATMEGA328P" pad="22"/>
</signal>
<signal name="N$13">
<contactref element="R13" pad="1"/>
<contactref element="MOSFET-P" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="BATT_INPUT1" pad="P$1"/>
<contactref element="U$7" pad="P$1"/>
<contactref element="U$7" pad="P$2"/>
</signal>
<signal name="PWM1">
<contactref element="U$11" pad="4"/>
<contactref element="R19" pad="1"/>
<contactref element="PCA9685" pad="6"/>
</signal>
<signal name="HEATER1_GND">
<contactref element="U$11" pad="MB"/>
<contactref element="MUSSEL1" pad="P$4"/>
</signal>
<signal name="PWM2">
<contactref element="U$12" pad="4"/>
<contactref element="R20" pad="1"/>
<contactref element="PCA9685" pad="7"/>
</signal>
<signal name="HEATER2_GND">
<contactref element="U$12" pad="MB"/>
<contactref element="MUSSEL2" pad="P$4"/>
</signal>
<signal name="PWM3">
<contactref element="U$13" pad="4"/>
<contactref element="R21" pad="1"/>
<contactref element="PCA9685" pad="8"/>
</signal>
<signal name="HEATER3_GND">
<contactref element="U$13" pad="MB"/>
<contactref element="MUSSEL3" pad="P$4"/>
</signal>
<signal name="PWM4">
<contactref element="U$14" pad="4"/>
<contactref element="R22" pad="1"/>
<contactref element="PCA9685" pad="9"/>
</signal>
<signal name="HEATER4_GND">
<contactref element="U$14" pad="MB"/>
<contactref element="MUSSEL4" pad="P$4"/>
</signal>
<signal name="PWM5">
<contactref element="U$15" pad="4"/>
<contactref element="R23" pad="1"/>
<contactref element="PCA9685" pad="10"/>
</signal>
<signal name="HEATER5_GND">
<contactref element="U$15" pad="MB"/>
<contactref element="MUSSEL5" pad="P$4"/>
</signal>
<signal name="PWM6">
<contactref element="U$16" pad="4"/>
<contactref element="R24" pad="1"/>
<contactref element="PCA9685" pad="11"/>
</signal>
<signal name="HEATER6_GND">
<contactref element="U$16" pad="MB"/>
<contactref element="MUSSEL6" pad="P$4"/>
</signal>
<signal name="PWM7">
<contactref element="U$17" pad="4"/>
<contactref element="R25" pad="1"/>
<contactref element="PCA9685" pad="12"/>
</signal>
<signal name="HEATER7_GND">
<contactref element="U$17" pad="MB"/>
<contactref element="MUSSEL7" pad="P$4"/>
</signal>
<signal name="PWM8">
<contactref element="U$18" pad="4"/>
<contactref element="R26" pad="1"/>
<contactref element="PCA9685" pad="13"/>
</signal>
<signal name="HEATER8_GND">
<contactref element="U$18" pad="MB"/>
<contactref element="MUSSEL8" pad="P$4"/>
</signal>
<signal name="PWM9">
<contactref element="U$19" pad="4"/>
<contactref element="R27" pad="1"/>
<contactref element="PCA9685" pad="15"/>
</signal>
<signal name="HEATER9_GND">
<contactref element="U$19" pad="MB"/>
<contactref element="MUSSEL9" pad="P$4"/>
</signal>
<signal name="PWM10">
<contactref element="U$20" pad="4"/>
<contactref element="R28" pad="1"/>
<contactref element="PCA9685" pad="16"/>
</signal>
<signal name="HEATER10_GND">
<contactref element="U$20" pad="MB"/>
<contactref element="MUSSEL10" pad="P$4"/>
</signal>
<signal name="PWM11">
<contactref element="U$21" pad="4"/>
<contactref element="R29" pad="1"/>
<contactref element="PCA9685" pad="17"/>
</signal>
<signal name="HEATER11_GND">
<contactref element="U$21" pad="MB"/>
<contactref element="MUSSEL11" pad="P$4"/>
</signal>
<signal name="PWM12">
<contactref element="U$22" pad="4"/>
<contactref element="R30" pad="1"/>
<contactref element="PCA9685" pad="18"/>
</signal>
<signal name="HEATER12_GND">
<contactref element="U$22" pad="MB"/>
<contactref element="MUSSEL12" pad="P$4"/>
</signal>
<signal name="PWM13">
<contactref element="U$23" pad="4"/>
<contactref element="R31" pad="1"/>
<contactref element="PCA9685" pad="19"/>
</signal>
<signal name="HEATER13_GND">
<contactref element="U$23" pad="MB"/>
<contactref element="MUSSEL13" pad="P$4"/>
</signal>
<signal name="PWM14">
<contactref element="U$24" pad="4"/>
<contactref element="R32" pad="1"/>
<contactref element="PCA9685" pad="20"/>
</signal>
<signal name="HEATER14_GND">
<contactref element="U$24" pad="MB"/>
<contactref element="MUSSEL14" pad="P$4"/>
</signal>
<signal name="PWM15">
<contactref element="U$25" pad="4"/>
<contactref element="R33" pad="1"/>
<contactref element="PCA9685" pad="21"/>
</signal>
<signal name="HEATER15_GND">
<contactref element="U$25" pad="MB"/>
<contactref element="MUSSEL15" pad="P$4"/>
</signal>
<signal name="MAX_DATA">
<contactref element="ATMEGA328P" pad="12"/>
<contactref element="R8" pad="1"/>
<contactref element="TEMP20" pad="P$1"/>
<contactref element="TEMP19" pad="P$1"/>
<contactref element="TEMP18" pad="P$1"/>
<contactref element="TEMP17" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="ADG725B" pad="12"/>
<contactref element="R34" pad="2"/>
</signal>
<signal name="THERM1">
<contactref element="R34" pad="1"/>
<contactref element="ADG725B" pad="25"/>
<contactref element="MUSSEL1" pad="P$3"/>
</signal>
<signal name="CS_MUX">
<contactref element="ADG725B" pad="17"/>
<contactref element="ATMEGA328P" pad="11"/>
</signal>
<signal name="HEATER16_GND">
<contactref element="U$10" pad="MB"/>
<contactref element="MUSSEL16" pad="P$4"/>
</signal>
<signal name="PWM16">
<contactref element="U$10" pad="4"/>
<contactref element="R18" pad="1"/>
<contactref element="PCA9685" pad="22"/>
</signal>
<signal name="THERM16">
<contactref element="R49" pad="1"/>
<contactref element="ADG725B" pad="40"/>
<contactref element="MUSSEL16" pad="P$3"/>
</signal>
<signal name="THERM15">
<contactref element="R48" pad="1"/>
<contactref element="ADG725B" pad="39"/>
<contactref element="MUSSEL15" pad="P$3"/>
</signal>
<signal name="THERM14">
<contactref element="R47" pad="1"/>
<contactref element="ADG725B" pad="38"/>
<contactref element="MUSSEL14" pad="P$3"/>
</signal>
<signal name="THERM13">
<contactref element="R46" pad="1"/>
<contactref element="ADG725B" pad="37"/>
<contactref element="MUSSEL13" pad="P$3"/>
</signal>
<signal name="THERM12">
<contactref element="R45" pad="1"/>
<contactref element="ADG725B" pad="36"/>
<contactref element="MUSSEL12" pad="P$3"/>
</signal>
<signal name="THERM11">
<contactref element="R44" pad="1"/>
<contactref element="ADG725B" pad="35"/>
<contactref element="MUSSEL11" pad="P$3"/>
</signal>
<signal name="THERM10">
<contactref element="R43" pad="1"/>
<contactref element="ADG725B" pad="34"/>
<contactref element="MUSSEL10" pad="P$3"/>
</signal>
<signal name="THERM9">
<contactref element="R42" pad="1"/>
<contactref element="ADG725B" pad="33"/>
<contactref element="MUSSEL9" pad="P$3"/>
</signal>
<signal name="THERM8">
<contactref element="R41" pad="1"/>
<contactref element="ADG725B" pad="32"/>
<contactref element="MUSSEL8" pad="P$3"/>
</signal>
<signal name="THERM7">
<contactref element="R40" pad="1"/>
<contactref element="ADG725B" pad="31"/>
<contactref element="MUSSEL7" pad="P$3"/>
</signal>
<signal name="THERM6">
<contactref element="R39" pad="1"/>
<contactref element="ADG725B" pad="30"/>
<contactref element="MUSSEL6" pad="P$3"/>
</signal>
<signal name="THERM5">
<contactref element="R38" pad="1"/>
<contactref element="ADG725B" pad="29"/>
<contactref element="MUSSEL5" pad="P$3"/>
</signal>
<signal name="THERM4">
<contactref element="R37" pad="1"/>
<contactref element="ADG725B" pad="28"/>
<contactref element="MUSSEL4" pad="P$3"/>
</signal>
<signal name="THERM3">
<contactref element="R36" pad="1"/>
<contactref element="ADG725B" pad="27"/>
<contactref element="MUSSEL3" pad="P$3"/>
</signal>
<signal name="THERM2">
<contactref element="R35" pad="1"/>
<contactref element="ADG725B" pad="26"/>
<contactref element="MUSSEL2" pad="P$3"/>
</signal>
<signal name="N$28">
<contactref element="ADG725B" pad="11"/>
<contactref element="R35" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="ADG725B" pad="10"/>
<contactref element="R36" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="ADG725B" pad="9"/>
<contactref element="R37" pad="2"/>
</signal>
<signal name="N$34">
<contactref element="ADG725B" pad="8"/>
<contactref element="R38" pad="2"/>
</signal>
<signal name="N$36">
<contactref element="ADG725B" pad="7"/>
<contactref element="R39" pad="2"/>
</signal>
<signal name="N$38">
<contactref element="ADG725B" pad="6"/>
<contactref element="R40" pad="2"/>
</signal>
<signal name="N$40">
<contactref element="ADG725B" pad="5"/>
<contactref element="R41" pad="2"/>
</signal>
<signal name="N$42">
<contactref element="ADG725B" pad="4"/>
<contactref element="R42" pad="2"/>
</signal>
<signal name="N$44">
<contactref element="ADG725B" pad="3"/>
<contactref element="R43" pad="2"/>
</signal>
<signal name="N$46">
<contactref element="ADG725B" pad="2"/>
<contactref element="R44" pad="2"/>
</signal>
<signal name="N$48">
<contactref element="ADG725B" pad="1"/>
<contactref element="R45" pad="2"/>
</signal>
<signal name="N$50">
<contactref element="ADG725B" pad="48"/>
<contactref element="R46" pad="2"/>
</signal>
<signal name="N$52">
<contactref element="ADG725B" pad="47"/>
<contactref element="R47" pad="2"/>
</signal>
<signal name="N$54">
<contactref element="ADG725B" pad="46"/>
<contactref element="R48" pad="2"/>
</signal>
<signal name="N$56">
<contactref element="ADG725B" pad="45"/>
<contactref element="R49" pad="2"/>
</signal>
<signal name="ANALOG_0">
<contactref element="ATMEGA328P" pad="23"/>
<contactref element="ADG725B" pad="41"/>
<contactref element="C14" pad="1"/>
</signal>
<signal name="PWM_!OE">
<contactref element="PCA9685" pad="23"/>
<contactref element="ATMEGA328P" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="RGB_LED" pad="P$2"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="RGB_LED" pad="P$3"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="RGB_LED" pad="P$4"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="AVCC">
<contactref element="ATMEGA328P" pad="18"/>
<contactref element="C3" pad="1"/>
<contactref element="INDUCTOR" pad="P$1"/>
</signal>
<signal name="AREF">
<contactref element="MAX6103" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="ATMEGA328P" pad="20"/>
<contactref element="AREF" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
