<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="23.8" y2="0" width="0" layer="20"/>
<wire x1="23.8" y1="0" x2="23.8" y2="45.71" width="0" layer="20"/>
<wire x1="23.8" y1="45.71" x2="0" y2="45.71" width="0" layer="20"/>
<wire x1="0" y1="45.71" x2="0" y2="0" width="0" layer="20"/>
<text>GSG</text>
<text>Datalogger1
rev 1</text>
</plain>
<libraries>
<library name="Spark">
<packages>
<package name="PHOTON">
</package>
</packages>
</library>
<library name="TSL230R">
<packages>
<package name="DIP8">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R1210">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="Spark" package="PHOTON" value="PHOTON_WITH_HEADERS"/>
<element name="LIGHT1" library="TSL230R" package="DIP8" value="TSL230RDIP8"/>
<element name="U1" library="SparkFun-Sensors" package="TO-92" value=""/>
<element name="C1" library="adafruit" package="C1210" value="0.1u"/>
<element name="R1" library="adafruit" package="R1210" value="45.3k"/>
<element name="R2" library="adafruit" package="R1210" value="10k"/>
</elements>
<signals>
<signal name="VIN">
<contactref element="U$1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="21"/>
<contactref element="LIGHT1" pad="4"/>
<contactref element="U1" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="VBAT">
<contactref element="U$1" pad="22"/>
</signal>
<signal name="TMP36_VOUT">
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="U$1" pad="12"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="TSL230_VOUT">
<contactref element="LIGHT1" pad="6"/>
<contactref element="U$1" pad="10"/>
</signal>
<signal name="3V">
<contactref element="U$1" pad="24"/>
<contactref element="LIGHT1" pad="5"/>
</signal>
<signal name="S3">
<contactref element="LIGHT1" pad="8"/>
<contactref element="U$1" pad="16"/>
</signal>
<signal name="S2">
<contactref element="LIGHT1" pad="7"/>
<contactref element="U$1" pad="17"/>
</signal>
<signal name="S0">
<contactref element="LIGHT1" pad="1"/>
<contactref element="U$1" pad="18"/>
</signal>
<signal name="S1">
<contactref element="LIGHT1" pad="2"/>
<contactref element="U$1" pad="19"/>
</signal>
<signal name="OE">
<contactref element="LIGHT1" pad="3"/>
<contactref element="U$1" pad="20"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
