(kicad_pcb (version 4) (host pcbnew 4.0.3-1.fc24-product)
  (general
    (links 8)
    (no_connects 0)
    (area 15.050001 21.6 140.100001 89.200001)
    (thickness 1.6)
    (drawings 22)
    (tracks 20)
    (zones 0)
    (modules 11)
    (nets 30)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 VBAT)
  (net 2 GND)
  (net 3 MOSI)
  (net 4 SCK)
  (net 5 "Net-(P8-Pad1)")
  (net 6 "Net-(P8-Pad2)")
  (net 7 "Net-(P8-Pad3)")
  (net 8 "Net-(P8-Pad5)")
  (net 9 "Net-(P8-Pad6)")
  (net 10 "Net-(P8-Pad7)")
  (net 11 "Net-(P8-Pad8)")
  (net 12 "Net-(P8-Pad9)")
  (net 13 "Net-(P8-Pad10)")
  (net 14 "Net-(P8-Pad13)")
  (net 15 "Net-(P8-Pad14)")
  (net 16 "Net-(P8-Pad15)")
  (net 17 "Net-(P8-Pad16)")
  (net 18 "Net-(P9-Pad1)")
  (net 19 "Net-(P9-Pad2)")
  (net 20 "Net-(P9-Pad3)")
  (net 21 "Net-(P9-Pad4)")
  (net 22 "Net-(P9-Pad5)")
  (net 23 "Net-(P9-Pad6)")
  (net 24 "Net-(P9-Pad7)")
  (net 25 "Net-(P9-Pad8)")
  (net 26 "Net-(P9-Pad9)")
  (net 27 "Net-(P9-Pad11)")
  (net 28 VUSB)
  (net 29 VLED)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net MOSI)
    (add_net "Net-(P8-Pad1)")
    (add_net "Net-(P8-Pad10)")
    (add_net "Net-(P8-Pad13)")
    (add_net "Net-(P8-Pad14)")
    (add_net "Net-(P8-Pad15)")
    (add_net "Net-(P8-Pad16)")
    (add_net "Net-(P8-Pad2)")
    (add_net "Net-(P8-Pad3)")
    (add_net "Net-(P8-Pad5)")
    (add_net "Net-(P8-Pad6)")
    (add_net "Net-(P8-Pad7)")
    (add_net "Net-(P8-Pad8)")
    (add_net "Net-(P8-Pad9)")
    (add_net "Net-(P9-Pad1)")
    (add_net "Net-(P9-Pad11)")
    (add_net "Net-(P9-Pad2)")
    (add_net "Net-(P9-Pad3)")
    (add_net "Net-(P9-Pad4)")
    (add_net "Net-(P9-Pad5)")
    (add_net "Net-(P9-Pad6)")
    (add_net "Net-(P9-Pad7)")
    (add_net "Net-(P9-Pad8)")
    (add_net "Net-(P9-Pad9)")
    (add_net SCK)
  )
  (net_class POWER ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VBAT)
    (add_net VLED)
    (add_net VUSB)
  )
  (module ultim8x8_libs:Screw (layer F.Cu) (tedit 5815083B)
    (at 75.7 30)
    (fp_text reference P2 (at 0 -1.5875) (layer F.SilkS) hide)
    (fp_text value VLED (at 0 4.5) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.048) (layers *.Cu *.SilkS *.Mask)
      (net 29 VLED))
    (model RowGB_Libs/3D_Modules/vite_2mm5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.2 1.2 1.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module ultim8x8_libs:Screw (layer F.Cu) (tedit 58150834)
    (at 30 30)
    (fp_text reference P3 (at 0 -1.5875) (layer F.SilkS) hide)
    (fp_text value VLED (at 0 4.5) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.048) (layers *.Cu *.SilkS *.Mask)
      (net 29 VLED))
    (model RowGB_Libs/3D_Modules/vite_2mm5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.2 1.2 1.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module ultim8x8_libs:Screw (layer F.Cu) (tedit 5817FBD3)
    (at 75.7 75.7)
    (fp_text reference P4 (at 0 -1.5875) (layer F.SilkS) hide)
    (fp_text value GND (at 0 -4.2) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.048) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (model RowGB_Libs/3D_Modules/vite_2mm5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.2 1.2 1.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module ultim8x8_libs:Screw (layer F.Cu) (tedit 5817FBDF)
    (at 30 75.7)
    (fp_text reference P5 (at 0 -1.5875) (layer F.SilkS) hide)
    (fp_text value GND (at 0 -4.2) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.048) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (model RowGB_Libs/3D_Modules/vite_2mm5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.2 1.2 1.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module ultim8x8_libs:Screw (layer F.Cu) (tedit 5817F94C)
    (at 60.5 60.5)
    (fp_text reference P6 (at 0 -1.5875) (layer F.SilkS) hide)
    (fp_text value MOSI (at 6 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.048) (layers *.Cu *.SilkS *.Mask)
      (net 3 MOSI))
    (model RowGB_Libs/3D_Modules/vite_2mm5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.2 1.2 1.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module ultim8x8_libs:Screw (layer F.Cu) (tedit 5817F93C)
    (at 60.5 45.2)
    (fp_text reference P7 (at 0 -1.5875) (layer F.SilkS) hide)
    (fp_text value SCK (at 5.6 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.048) (layers *.Cu *.SilkS *.Mask)
      (net 4 SCK))
    (model RowGB_Libs/3D_Modules/vite_2mm5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.2 1.2 1.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module ultim8x8_libs:logo_MLlabs (layer F.Cu) (tedit 5814E899)
    (at 39.7 37.4)
    (fp_text reference P1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "Maniacal Labs" (at 0 6.604) (layer F.SilkS))
  )
  (module Pin_Headers:Pin_Header_Straight_1x16 (layer F.Cu) (tedit 58150B75)
    (at 74.4 50.4 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P8 (at 0 -2.6 270) (layer F.SilkS))
    (fp_text value CONN_01X16 (at 0 -3.1 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P8-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P8-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P8-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P8-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P8-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P8-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P8-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P8-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P8-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 SCK))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 MOSI))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P8-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P8-Pad14)"))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P8-Pad15)"))
    (pad 16 thru_hole oval (at 0 38.1 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P8-Pad16)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x16.wrl
      (at (xyz 0 -0.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x12 (layer F.Cu) (tedit 58150B6E)
    (at 36.3 70.6 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P9 (at 0 30.5 90) (layer F.SilkS))
    (fp_text value CONN_01X12 (at 0.1 30.9 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P9-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P9-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(P9-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(P9-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P9-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(P9-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(P9-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(P9-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(P9-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 VUSB))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(P9-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VBAT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ultim8x8_libs:logo_wyo_butterfly (layer F.Cu) (tedit 5814E891)
    (at 67.9 38.8)
    (fp_text reference P10 (at 0 0) (layer F.SilkS) hide)
    (fp_text value WyoLum (at -4.1 -5.1) (layer F.SilkS))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5817ECAE)
    (at 59.2 75 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP1 (at 0 7.6 270) (layer F.SilkS))
    (fp_text value JUMPER3 (at 0 -3.1 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 VUSB))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 VLED))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VBAT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text USB|BAT (at 61.5 77.8) (layer F.SilkS))
  (dimension 15.2 (width 0.3) (layer Dwgs.User)
    (gr_text "15.200 mm" (at 68.1 85.25) (layer Dwgs.User))
    (feature1 (pts (xy 60.5 80.7) (xy 60.5 86.6)))
    (feature2 (pts (xy 75.7 80.7) (xy 75.7 86.6)))
    (crossbar (pts (xy 75.7 83.9) (xy 60.5 83.9)))
    (arrow1a (pts (xy 60.5 83.9) (xy 61.626504 83.313579)))
    (arrow1b (pts (xy 60.5 83.9) (xy 61.626504 84.486421)))
    (arrow2a (pts (xy 75.7 83.9) (xy 74.573496 83.313579)))
    (arrow2b (pts (xy 75.7 83.9) (xy 74.573496 84.486421)))
  )
  (gr_line (start 75.7 25) (end 30 25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 15.2 (width 0.3) (layer Dwgs.User)
    (gr_text "15.200 mm" (at 21.55 68.1 90) (layer Dwgs.User))
    (feature1 (pts (xy 30 60.5) (xy 20.2 60.5)))
    (feature2 (pts (xy 30 75.7) (xy 20.2 75.7)))
    (crossbar (pts (xy 22.9 75.7) (xy 22.9 60.5)))
    (arrow1a (pts (xy 22.9 60.5) (xy 23.486421 61.626504)))
    (arrow1b (pts (xy 22.9 60.5) (xy 22.313579 61.626504)))
    (arrow2a (pts (xy 22.9 75.7) (xy 23.486421 74.573496)))
    (arrow2b (pts (xy 22.9 75.7) (xy 22.313579 74.573496)))
  )
  (gr_line (start 25 75.7) (end 25 30) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 30 80.7) (end 75.7 80.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 80.7 30) (end 80.7 75.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 75.7 30) (end 75.7 25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 75.7 75.7) (end 80.7 75.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 30 75.7) (end 30 80.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 30 30) (end 25 30) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 15.2 (width 0.3) (layer Dwgs.User)
    (gr_text "15.200 mm" (at 21.55 37.6 90) (layer Dwgs.User))
    (feature1 (pts (xy 30 30) (xy 20.2 30)))
    (feature2 (pts (xy 30 45.2) (xy 20.2 45.2)))
    (crossbar (pts (xy 22.9 45.2) (xy 22.9 30)))
    (arrow1a (pts (xy 22.9 30) (xy 23.486421 31.126504)))
    (arrow1b (pts (xy 22.9 30) (xy 22.313579 31.126504)))
    (arrow2a (pts (xy 22.9 45.2) (xy 23.486421 44.073496)))
    (arrow2b (pts (xy 22.9 45.2) (xy 22.313579 44.073496)))
  )
  (dimension 15.3 (width 0.3) (layer Dwgs.User)
    (gr_text "15.300 mm" (at 21.55 52.85 90) (layer Dwgs.User))
    (feature1 (pts (xy 30 45.2) (xy 20.2 45.2)))
    (feature2 (pts (xy 30 60.5) (xy 20.2 60.5)))
    (crossbar (pts (xy 22.9 60.5) (xy 22.9 45.2)))
    (arrow1a (pts (xy 22.9 45.2) (xy 23.486421 46.326504)))
    (arrow1b (pts (xy 22.9 45.2) (xy 22.313579 46.326504)))
    (arrow2a (pts (xy 22.9 60.5) (xy 23.486421 59.373496)))
    (arrow2b (pts (xy 22.9 60.5) (xy 22.313579 59.373496)))
  )
  (dimension 45.7 (width 0.3) (layer Dwgs.User)
    (gr_text "45.700 mm" (at 52.85 22.95) (layer Dwgs.User))
    (feature1 (pts (xy 75.7 30) (xy 75.7 21.6)))
    (feature2 (pts (xy 30 30) (xy 30 21.6)))
    (crossbar (pts (xy 30 24.3) (xy 75.7 24.3)))
    (arrow1a (pts (xy 75.7 24.3) (xy 74.573496 24.886421)))
    (arrow1b (pts (xy 75.7 24.3) (xy 74.573496 23.713579)))
    (arrow2a (pts (xy 30 24.3) (xy 31.126504 24.886421)))
    (arrow2b (pts (xy 30 24.3) (xy 31.126504 23.713579)))
  )
  (gr_text "1.8\" = 45.7mm\n0.6\" = 15.2mm\n0.8\" = 20.3mm" (at 94.7 50) (layer Cmts.User))
  (gr_text "Ultim8x8 Feather Shield" (at 53.1 27.5) (layer F.SilkS))
  (zone (net 29) (net_name VLED) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.7 25.4) (xy 79.1 26.6) (xy 80.2 30) (xy 80.2 75.8) (xy 79.1 79.1)
        (xy 75.7 80.2) (xy 30 80.2) (xy 26.6 79.1) (xy 25.5 75.7) (xy 25.5 30)
        (xy 26.7 26.7) (xy 30 25.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.7 25.4) (xy 79.1 26.6) (xy 80.2 30) (xy 80.2 75.8) (xy 79.1 79.1)
        (xy 75.7 80.2) (xy 30 80.2) (xy 26.6 79.1) (xy 25.5 75.7) (xy 25.5 30)
        (xy 26.7 26.7) (xy 30 25.5)
      )
    )
  )
)
