(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 2)
    (no_connects 0)
    (area 60.139809 34.3154 88.760907 71.183501)
    (thickness 0.8)
    (drawings 18)
    (tracks 6)
    (zones 0)
    (modules 12)
    (nets 3)
  )
  (page User 203.2 127)
  (title_block
    (title "Enable/Diable switch for AdaFruit Feather boards")
    (date 2017-03-27)
    (rev 1.0.0)
    (company "Sembazuru Circuits")
    (comment 1 "v1.0.0 - Initial release.")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3175)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00130_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref true)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "New folder/"))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.3175)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
  )
  (module CDE_misc:PAD_AdaFruit_Feather locked (layer F.Cu) (tedit 58D9CFE6)
    (at 71.12 43.18)
    (fp_text reference J1 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value En (at 0 1.778) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0.04 0) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
  )
  (module CDE_misc:PAD_AdaFruit_Feather locked (layer F.Cu) (tedit 58D9CFDA)
    (at 66.04 63.5)
    (fp_text reference J2 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value GND (at 0 -1.778) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0.04 0) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
  )
  (module CDE_misc:SW_ADAFRUIT_508 locked (layer F.Cu) (tedit 58D98DC6)
    (at 71.12 39.37)
    (descr https://cdn-shop.adafruit.com/datasheets/EG1218draw.pdf)
    (fp_text reference SW1 (at 2.54 -3.81) (layer F.SilkS) hide)
    (fp_text value "Slide Switch" (at 2.54 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0.04 0) (size 1.5 2.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.5 2.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 3 thru_hole oval (at 5.04 0) (size 1.5 2.5) (drill 0.9) (layers *.Cu *.Mask))
  )
  (module logos:crane_0.25in_silkscreen (layer B.Cu) (tedit 0)
    (at 73.66 53.975 180)
    (fp_text reference G*** (at 0 -2.27584 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 2.27584 180) (layer B.SilkS) hide)
  )
  (module Symbols:KiCad-Logo2_6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 71.12 54.61)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value KiCad-Logo2_6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module logos:OSHW_04mm_copper_noMask (layer B.Cu) (tedit 0)
    (at 66.675 54.61 180)
    (fp_text reference G*** (at 0 -2.35966 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 2.35966 180) (layer B.SilkS) hide)
  )
  (module CDE_misc:PAD-Clear_AdaFruit_Feather locked (layer F.Cu) (tedit 58D9D63D)
    (at 68.58 63.5)
    (fp_text reference MH6 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value A0 (at 0 2.54) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.04 0) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask)
      (solder_mask_margin 0.001) (zone_connect 0))
  )
  (module CDE_misc:PAD-Clear_AdaFruit_Feather locked (layer F.Cu) (tedit 58D9D63A)
    (at 63.5 63.5)
    (fp_text reference MH5 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value ARf (at 0 2.54) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.04 0) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask)
      (solder_mask_margin 0.001) (zone_connect 0))
  )
  (module CDE_misc:PAD-Clear_AdaFruit_Feather locked (layer F.Cu) (tedit 58D9D62C)
    (at 78.74 43.18)
    (fp_text reference MH4 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 12 (at 0 2.54) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.04 0) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask)
      (solder_mask_margin 0.001) (zone_connect 0))
  )
  (module CDE_misc:PAD-Clear_AdaFruit_Feather locked (layer F.Cu) (tedit 58D9D620)
    (at 68.58 43.18)
    (fp_text reference MH1 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value BAT (at 0 2.54) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.04 0) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask)
      (solder_mask_margin 0.001) (zone_connect 0))
  )
  (module CDE_misc:PAD_AdaFruit_Feather locked (layer F.Cu) (tedit 58D9DC1C)
    (at 73.66 43.18)
    (fp_text reference MH2 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value USB (at 0 2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0.04 0) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask))
  )
  (module CDE_misc:PAD_AdaFruit_Feather locked (layer F.Cu) (tedit 58D9DC08)
    (at 76.2 43.18)
    (fp_text reference MH3 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 13 (at 0 2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0.04 0) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask))
  )
  (gr_text "SCH v1.0.0\nPCB v1.0.0" (at 66.04 59.69) (layer B.SilkS))
  (gr_text "Enable/Disable\nSwitch for\nAdaFruit Feathers" (at 71.12 48.26) (layer B.SilkS))
  (gr_text "Sembazuru Circuits" (at 73.66 56.515) (layer B.SilkS))
  (gr_text "Solder this side\nagainst underside\nof Feather Board" (at 71.12 48.26) (layer F.SilkS))
  (dimension 15.24 (width 0.127) (layer Dwgs.User)
    (gr_text "0.6000 in" (at 71.12 70.104) (layer Dwgs.User))
    (feature1 (pts (xy 78.74 65.405) (xy 78.74 70.993)))
    (feature2 (pts (xy 63.5 65.405) (xy 63.5 70.993)))
    (crossbar (pts (xy 63.5 69.215) (xy 78.74 69.215)))
    (arrow1a (pts (xy 78.74 69.215) (xy 77.613496 69.801421)))
    (arrow1b (pts (xy 78.74 69.215) (xy 77.613496 68.628579)))
    (arrow2a (pts (xy 63.5 69.215) (xy 64.626504 69.801421)))
    (arrow2b (pts (xy 63.5 69.215) (xy 64.626504 68.628579)))
  )
  (dimension 27.94 (width 0.127) (layer Dwgs.User)
    (gr_text "1.1000 in" (at 84.074 50.8 270) (layer Dwgs.User))
    (feature1 (pts (xy 79.375 64.77) (xy 84.963 64.77)))
    (feature2 (pts (xy 79.375 36.83) (xy 84.963 36.83)))
    (crossbar (pts (xy 83.185 36.83) (xy 83.185 64.77)))
    (arrow1a (pts (xy 83.185 64.77) (xy 82.598579 63.643496)))
    (arrow1b (pts (xy 83.185 64.77) (xy 83.771421 63.643496)))
    (arrow2a (pts (xy 83.185 36.83) (xy 82.598579 37.956504)))
    (arrow2b (pts (xy 83.185 36.83) (xy 83.771421 37.956504)))
  )
  (gr_text Off (at 69.342 39.37 90) (layer B.SilkS))
  (gr_text On (at 77.978 39.37 90) (layer B.SilkS))
  (gr_line (start 63.5 45.085) (end 63.5 64.77) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.58 45.085) (end 63.5 45.085) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.58 36.83) (end 68.58 45.085) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 78.74 36.83) (end 68.58 36.83) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 78.74 58.42) (end 78.74 36.83) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.58 58.42) (end 78.74 58.42) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.58 64.77) (end 68.58 58.42) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 63.5 64.77) (end 68.58 64.77) (angle 90) (layer Edge.Cuts) (width 0.15))
)
