(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 28)
    (tracks 21)
    (zones 0)
    (modules 3)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 2 1)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module SamacSys_Parts:SKRR (layer F.Cu) (tedit 0)
    (at 185 67.5)
    (descr SKRR)
    (tags Switch)
    (attr smd)
    (fp_text reference S1 (at -0.315 -0.046) (layer F.SilkS))
    (fp_text value SKRR (at -0.315 -0.046) (layer F.SilkS) hide)
    (fp_text user %R (at -0.315 -0.046) (layer F.Fab))
    (pad 4 smd rect (at 3 2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 3 -2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -3 2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -3 -2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (model C:\Users\meeps\Downloads\LIBCAD\SamacSys_Parts.3dshapes\SKRRAAE010.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:SKRR (layer F.Cu) (tedit 0)
    (at 198.75 63.25)
    (descr SKRR)
    (tags Switch)
    (attr smd)
    (fp_text reference S0 (at -0.315 -0.046) (layer F.SilkS))
    (fp_text value SKRR (at -0.315 -0.046) (layer F.SilkS) hide)
    (fp_text user %R (at -0.315 -0.046) (layer F.Fab))
    (pad 4 smd rect (at 3 2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 3 -2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -3 2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -3 -2.5) (size 1 1.1) (layers F.Cu F.Paste F.Mask))
    (model C:\Users\meeps\Downloads\LIBCAD\SamacSys_Parts.3dshapes\SKRRAAE010.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:agb2 (layer F.Cu) (tedit 0)
    (at 137.75 113.25)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text v3 (at 190.75 71.75) (layer F.SilkS))
  (gr_line (start 193.5 55.5) (end 197.75 55.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 192 72.75) (end 192 71) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 192 72.75) (end 191.75 72.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 179.5 72.75) (end 191.75 72.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 179.5 62.75) (end 179.5 72.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 188.25 62.75) (end 179.5 62.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 189.25 61) (end 188.25 62.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 188.5 55.5) (end 188.496932 56.777608) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 193.5 55.5) (end 188.5 55.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 198.25 54.75) (end 197.75 55.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 201.25 54.75) (end 198.25 54.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 201.25 57.75) (end 201.25 54.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 202.247844 58.255031) (end 201.25 57.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 194.5 68.5) (end 202.75 68.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 188.25 59) (end 189.25 61) (angle -147.0947571) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 200 63.5) (end 202.75 68.5) (angle -127.9906157) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 193.5 70) (end 194.5 68.5) (angle -157.3801351) (layer Edge.Cuts) (width 0.05))
  (gr_text meeps (at 198.75 67.5) (layer F.SilkS))
  (gr_text TP1 (at 191 57) (layer F.SilkS))
  (gr_text TP0 (at 193.5 57) (layer F.SilkS))
  (gr_text GND (at 199 56.5) (layer F.SilkS))
)
