(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 12)
    (no_connects 0)
    (area 133.540499 88.836499 156.527501 107.759501)
    (thickness 1.6)
    (drawings 18)
    (tracks 32)
    (zones 0)
    (modules 8)
    (nets 5)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.3)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x011fc_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(IC1-Pad2)")
  (net 4 "Net-(IC1-Pad3)")
  (net_class Default "Dit is de standaard class."
    (clearance 0.3)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net GND)
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad3)")
    (add_net VCC)
  )
  (module BRICE:C_1206_HandSoldering (layer Top) (tedit 58CD0301)
    (at 146.304 90.932 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at -4.191 0.762 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers Top F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers Top F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module BRICE:ATTINY85-P (layer Top) (tedit 58CCFF70)
    (at 145.288 98.044)
    (descr "PDIP-8 Standard 300mil 8pin Dual In Line Package")
    (tags "Power Integrations P Package")
    (fp_text reference ATTINY85-P (at 0.635 0) (layer F.SilkS))
    (fp_text value ATTINY85-P (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.81 3.81) (size 1.905 1.905) (drill 0.762) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -1.27 3.81) (size 1.905 1.905) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(IC1-Pad2)"))
    (pad 3 thru_hole circle (at 1.27 3.81) (size 1.905 1.905) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(IC1-Pad3)"))
    (pad 4 thru_hole circle (at 3.81 3.81) (size 1.905 1.905) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at 3.81 -3.81) (size 1.905 1.905) (drill 0.762) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 1.27 -3.81) (size 1.905 1.905) (drill 0.762) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -1.27 -3.81) (size 1.905 1.905) (drill 0.762) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -3.81 -3.81) (size 1.905 1.905) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 VCC))
  )
  (module BRICE:Power_Pad_2x_1mmDrill (layer Top) (tedit 58CCFF4D)
    (at 153.924 92.964 90)
    (fp_text reference 5VCC (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value Power (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module BRICE:R_1206_HandSoldering (layer Top) (tedit 58C701D4)
    (at 146.812 105.664)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -1.85) (layer F.SilkS))
    (fp_text value 4700 (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers Top F.Paste F.Mask)
      (net 3 "Net-(IC1-Pad2)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers Top F.Paste F.Mask)
      (net 1 VCC))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module BRICE:DS18B20 placed (layer Top) (tedit 58CC3C73)
    (at 153.924 101.092 90)
    (fp_text reference S1 (at -5.08 0 180) (layer F.SilkS))
    (fp_text value DS18B20 (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(IC1-Pad2)"))
  )
  (module BRICE:FS1000A (layer Top) (tedit 58CCFF3D)
    (at 136.144 98.044 90)
    (fp_text reference "RF 433" (at -6.096 -0.254 90) (layer F.SilkS))
    (fp_text value FS1000A (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(IC1-Pad3)"))
    (pad 2 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Symbols:OSHW-Logo_5.7x6mm_SilkScreen (layer Bottom) (tedit 0)
    (at 137.16 104.14 270)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo_5.7x6mm_SilkScreen (at 0.75 0 270) (layer B.Fab) hide)
  )
  (module Symbols:WEEE-Logo_4.2x6mm_SilkScreen (layer Bottom) (tedit 0)
    (at 145.415 104.775 270)
    (descr "Waste Electrical and Electronic Equipment Directive")
    (tags "Logo WEEE")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value WEEE-Logo_4.2x6mm_SilkScreen (at 0.75 0 270) (layer B.Fab) hide)
  )
  (gr_line (start 156.464 91.44) (end 156.464 105.156) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 133.604 91.44) (end 133.604 105.156) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 153.924 91.44) (end 153.924 88.9) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 153.924 105.156) (end 156.464 105.156) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 136.144 88.9) (end 153.924 88.9) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 136.144 91.44) (end 133.604 91.44) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 136.144 107.696) (end 153.924 107.696) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 136.144 105.156) (end 136.144 107.696) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_text 2017 (at 139.065 92.075 90) (layer B.SilkS))
  (gr_text + (at 152.019 94.488) (layer F.SilkS))
  (gr_text - (at 152.019 91.313) (layer F.SilkS))
  (gr_text 2 (at 152.019 101.473) (layer F.SilkS))
  (gr_text 3 (at 152.019 104.013) (layer F.SilkS))
  (gr_text 1 (at 152.019 98.933) (layer F.SilkS))
  (gr_text "ZIONIII SONDE V1.0" (at 151.765 98.425 90) (layer B.SilkS))
  (gr_text 3 (at 138.176 96.012) (layer F.SilkS))
  (gr_text 2 (at 138.176 98.552) (layer F.SilkS))
  (gr_text 1 (at 138.176 101.092) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.604 88.9) (xy 156.464 88.9) (xy 156.464 107.696) (xy 133.604 107.696)
      )
    )
  )
)
