(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu16.04.1)
  (general
    (links 36)
    (no_connects 0)
    (area 142.799999 61.519999 194.385001 125.170001)
    (thickness 1.6)
    (drawings 19)
    (tracks 212)
    (zones 0)
    (modules 5)
    (nets 39)
  )
  (page A4)
  (title_block
    (title "B6525/6 METER PCB TO MOXA INTERFACE")
    (date 2018-04-06)
    (rev 1)
    (company ARQIVA)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(SV1-Pad1)")
  (net 2 "Net-(SV1-Pad2)")
  (net 3 "Net-(SV1-Pad4)")
  (net 4 "Net-(SV1-Pad11)")
  (net 5 "Net-(SV1-Pad12)")
  (net 6 "Net-(SV1-Pad13)")
  (net 7 "Net-(SV1-Pad16)")
  (net 8 "Net-(SV1-Pad17)")
  (net 9 "Net-(SV1-Pad18)")
  (net 10 "Net-(SV1-Pad19)")
  (net 11 "Net-(SV1-Pad20)")
  (net 12 "Net-(SV1-Pad28)")
  (net 13 "Net-(SV1-Pad29)")
  (net 14 "Net-(SV1-Pad14)")
  (net 15 "Net-(SV1-Pad15)")
  (net 16 "Net-(SV1-Pad3)")
  (net 17 "Net-(SV1-Pad5)")
  (net 18 "Net-(SV1-Pad6)")
  (net 19 "Net-(SV1-Pad7)")
  (net 20 "Net-(SV1-Pad8)")
  (net 21 "Net-(SV1-Pad9)")
  (net 22 "Net-(SV1-Pad10)")
  (net 23 "Net-(SV1-Pad21)")
  (net 24 "Net-(SV1-Pad22)")
  (net 25 "Net-(SV1-Pad23)")
  (net 26 "Net-(SV1-Pad24)")
  (net 27 "Net-(SV1-Pad25)")
  (net 28 "Net-(SV1-Pad26)")
  (net 29 "Net-(SV1-Pad27)")
  (net 30 "Net-(SV1-Pad30)")
  (net 31 "Net-(SV1-Pad31)")
  (net 32 "Net-(SV1-Pad32)")
  (net 33 "Net-(SV1-Pad33)")
  (net 34 "Net-(SV1-Pad34)")
  (net 35 "Net-(X2-PadL7.2)")
  (net 36 "Net-(X2-PadL7.1)")
  (net 37 "Net-(X2-PadL8.1)")
  (net 38 "Net-(X2-PadL8.2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(SV1-Pad1)")
    (add_net "Net-(SV1-Pad10)")
    (add_net "Net-(SV1-Pad11)")
    (add_net "Net-(SV1-Pad12)")
    (add_net "Net-(SV1-Pad13)")
    (add_net "Net-(SV1-Pad14)")
    (add_net "Net-(SV1-Pad15)")
    (add_net "Net-(SV1-Pad16)")
    (add_net "Net-(SV1-Pad17)")
    (add_net "Net-(SV1-Pad18)")
    (add_net "Net-(SV1-Pad2)")
    (add_net "Net-(SV1-Pad21)")
    (add_net "Net-(SV1-Pad22)")
    (add_net "Net-(SV1-Pad23)")
    (add_net "Net-(SV1-Pad24)")
    (add_net "Net-(SV1-Pad25)")
    (add_net "Net-(SV1-Pad26)")
    (add_net "Net-(SV1-Pad27)")
    (add_net "Net-(SV1-Pad28)")
    (add_net "Net-(SV1-Pad29)")
    (add_net "Net-(SV1-Pad3)")
    (add_net "Net-(SV1-Pad30)")
    (add_net "Net-(SV1-Pad31)")
    (add_net "Net-(SV1-Pad32)")
    (add_net "Net-(SV1-Pad33)")
    (add_net "Net-(SV1-Pad34)")
    (add_net "Net-(SV1-Pad4)")
    (add_net "Net-(SV1-Pad5)")
    (add_net "Net-(SV1-Pad6)")
    (add_net "Net-(SV1-Pad7)")
    (add_net "Net-(SV1-Pad8)")
    (add_net "Net-(SV1-Pad9)")
    (add_net "Net-(X2-PadL7.1)")
    (add_net "Net-(X2-PadL7.2)")
    (add_net "Net-(X2-PadL8.1)")
    (add_net "Net-(X2-PadL8.2)")
  )
  (net_class power ""
    (clearance 0.2)
    (trace_width 0.508)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(SV1-Pad19)")
    (add_net "Net-(SV1-Pad20)")
  )
  (module MountingHole_RevA_04Jul2011:MountingHole_4mm_RevA_Date21Jun2010 (layer F.Cu) (tedit 5AC7AC47)
    (at 168.91 113.665)
    (descr "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (fp_text reference MH (at 0 -5.4991) (layer F.SilkS) hide)
    (fp_text value MountingHole_4mm_RevA_Date21Jun2010 (at 0 5.99948) (layer Dwgs.User) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 4.0005) (layers))
  )
  (module 804-110:P-804-110 (layer F.Cu) (tedit 5AEC670D)
    (at 185.928 98.9584)
    (fp_text reference X1 (at -2.90798 -28.6988) (layer F.SilkS) hide)
    (fp_text value 804-110 (at -2.00512 28.8636) (layer F.SilkS) hide)
    (pad L2.1 thru_hole oval (at 0.8 -17) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(SV1-Pad16)"))
    (pad L2.2 thru_hole oval (at -4.2 -19.5) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(SV1-Pad16)"))
    (pad L1.1 thru_hole oval (at 0.8 -22) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(SV1-Pad17)"))
    (pad L1.2 thru_hole oval (at -4.2 -24.5) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(SV1-Pad17)"))
    (pad L3.1 thru_hole oval (at 0.8 -12) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(SV1-Pad18)"))
    (pad L3.2 thru_hole oval (at -4.2 -14.5) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(SV1-Pad18)"))
    (pad L4.1 thru_hole oval (at 0.8 -7) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(SV1-Pad16)"))
    (pad L4.2 thru_hole oval (at -4.2 -9.5) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(SV1-Pad16)"))
    (pad L5.2 thru_hole oval (at -4.2 -4.5) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(SV1-Pad12)"))
    (pad L5.1 thru_hole oval (at 0.8 -2) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(SV1-Pad12)"))
    (pad L6.2 thru_hole oval (at -4.2 0.5) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(SV1-Pad9)"))
    (pad L6.1 thru_hole oval (at 0.8 3) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(SV1-Pad9)"))
    (pad L7.2 thru_hole oval (at -4.2 5.5) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(SV1-Pad2)"))
    (pad L7.1 thru_hole oval (at 0.8 8) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(SV1-Pad2)"))
    (pad L8.1 thru_hole oval (at 0.8 13) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(SV1-Pad28)"))
    (pad L8.2 thru_hole oval (at -4.2 10.5) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(SV1-Pad28)"))
    (pad L9.1 thru_hole oval (at 0.8 18) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(SV1-Pad13)"))
    (pad L9.2 thru_hole oval (at -4.2 15.5) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(SV1-Pad13)"))
    (pad L10. thru_hole oval (at 0.8 23) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(SV1-Pad16)"))
    (pad L10. thru_hole oval (at -4.2 20.5) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(SV1-Pad16)"))
  )
  (module 804-110:P-804-110 (layer F.Cu) (tedit 5AEC6701)
    (at 151.384 98.9076)
    (fp_text reference X2 (at -2.90798 -28.6988) (layer F.SilkS) hide)
    (fp_text value 804-110 (at -2.00512 28.8636) (layer F.SilkS) hide)
    (pad L2.1 thru_hole oval (at 0.8 -17) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(SV1-Pad15)"))
    (pad L2.2 thru_hole oval (at -4.2 -19.5) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(SV1-Pad15)"))
    (pad L1.1 thru_hole oval (at 0.8 -22) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(SV1-Pad14)"))
    (pad L1.2 thru_hole oval (at -4.2 -24.5) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(SV1-Pad14)"))
    (pad L3.1 thru_hole oval (at 0.8 -12) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(SV1-Pad4)"))
    (pad L3.2 thru_hole oval (at -4.2 -14.5) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(SV1-Pad4)"))
    (pad L4.1 thru_hole oval (at 0.8 -7) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(SV1-Pad29)"))
    (pad L4.2 thru_hole oval (at -4.2 -9.5) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(SV1-Pad29)"))
    (pad L5.2 thru_hole oval (at -4.2 -4.5) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(SV1-Pad1)"))
    (pad L5.1 thru_hole oval (at 0.8 -2) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(SV1-Pad1)"))
    (pad L6.2 thru_hole oval (at -4.2 0.5) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(SV1-Pad2)"))
    (pad L6.1 thru_hole oval (at 0.8 3) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(SV1-Pad2)"))
    (pad L7.2 thru_hole oval (at -4.2 5.5) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(X2-PadL7.2)"))
    (pad L7.1 thru_hole oval (at 0.8 8) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(X2-PadL7.1)"))
    (pad L8.1 thru_hole oval (at 0.8 13) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(X2-PadL8.1)"))
    (pad L8.2 thru_hole oval (at -4.2 10.5) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(X2-PadL8.2)"))
    (pad L9.1 thru_hole oval (at 0.8 18) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(SV1-Pad19)"))
    (pad L9.2 thru_hole oval (at -4.2 15.5) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(SV1-Pad19)"))
    (pad L10. thru_hole oval (at 0.8 23) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(SV1-Pad20)"))
    (pad L10. thru_hole oval (at -4.2 20.5) (size 3.3 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(SV1-Pad20)"))
  )
  (module MountingHole_RevA_04Jul2011:MountingHole_4mm_RevA_Date21Jun2010 (layer F.Cu) (tedit 5AC79FD9)
    (at 168.91 88.265)
    (descr "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (fp_text reference MH (at 0 -5.4991) (layer F.SilkS) hide)
    (fp_text value MountingHole_4mm_RevA_Date21Jun2010 (at 0 5.99948) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 4.0005) (layers))
  )
  (module Connectors_Multicomp:Multicomp_MC9A12-3434_2x17x2.54mm_Straight (layer F.Cu) (tedit 56C61E6B)
    (at 148.2344 67.818)
    (descr http://www.farnell.com/datasheets/1520732.pdf)
    (tags "connector multicomp MC9A MC9A12")
    (fp_text reference SV1 (at -3 -7) (layer F.SilkS))
    (fp_text value ML34 (at 20.32 5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(SV1-Pad1)"))
    (pad 2 thru_hole circle (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(SV1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(SV1-Pad3)"))
    (pad 4 thru_hole circle (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(SV1-Pad4)"))
    (pad 5 thru_hole circle (at 5.08 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(SV1-Pad5)"))
    (pad 6 thru_hole circle (at 5.08 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(SV1-Pad6)"))
    (pad 7 thru_hole circle (at 7.62 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(SV1-Pad7)"))
    (pad 8 thru_hole circle (at 7.62 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(SV1-Pad8)"))
    (pad 9 thru_hole circle (at 10.16 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(SV1-Pad9)"))
    (pad 10 thru_hole circle (at 10.16 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(SV1-Pad10)"))
    (pad 11 thru_hole circle (at 12.7 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(SV1-Pad11)"))
    (pad 12 thru_hole circle (at 12.7 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(SV1-Pad12)"))
    (pad 13 thru_hole circle (at 15.24 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(SV1-Pad13)"))
    (pad 14 thru_hole circle (at 15.24 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(SV1-Pad14)"))
    (pad 15 thru_hole circle (at 17.78 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(SV1-Pad15)"))
    (pad 16 thru_hole circle (at 17.78 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(SV1-Pad16)"))
    (pad 17 thru_hole circle (at 20.32 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(SV1-Pad17)"))
    (pad 18 thru_hole circle (at 20.32 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(SV1-Pad18)"))
    (pad 19 thru_hole circle (at 22.86 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(SV1-Pad19)"))
    (pad 20 thru_hole circle (at 22.86 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(SV1-Pad20)"))
    (pad 21 thru_hole circle (at 25.4 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(SV1-Pad21)"))
    (pad 22 thru_hole circle (at 25.4 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(SV1-Pad22)"))
    (pad 23 thru_hole circle (at 27.94 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(SV1-Pad23)"))
    (pad 24 thru_hole circle (at 27.94 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(SV1-Pad24)"))
    (pad 25 thru_hole circle (at 30.48 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(SV1-Pad25)"))
    (pad 26 thru_hole circle (at 30.48 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(SV1-Pad26)"))
    (pad 27 thru_hole circle (at 33.02 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(SV1-Pad27)"))
    (pad 28 thru_hole circle (at 33.02 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(SV1-Pad28)"))
    (pad 29 thru_hole circle (at 35.56 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(SV1-Pad29)"))
    (pad 30 thru_hole circle (at 35.56 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(SV1-Pad30)"))
    (pad 31 thru_hole circle (at 38.1 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(SV1-Pad31)"))
    (pad 32 thru_hole circle (at 38.1 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(SV1-Pad32)"))
    (pad 33 thru_hole circle (at 40.64 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(SV1-Pad33)"))
    (pad 34 thru_hole circle (at 40.64 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(SV1-Pad34)"))
  )
  (gr_text POWER (at 160.6296 116.3828 90) (layer F.SilkS))
  (gr_text "CDT\n2018" (at 171.1452 104.5464 90) (layer F.SilkS))
  (gr_text "B6525/6 MOXA\n  INTERFACE" (at 165.4556 101.1936 90) (layer F.SilkS))
  (gr_text "V HT\n AI-7" (at 160.9852 97.4344 90) (layer F.SilkS))
  (gr_text "I SCREEN\n AI-6" (at 161.8996 88.0364 90) (layer F.SilkS))
  (gr_text "GRID FWD\n AI-5" (at 160.7312 78.4352 90) (layer F.SilkS))
  (gr_text "I GRID\n AI-2" (at 174.5488 98.0948 270) (layer F.SilkS))
  (gr_text "GRID REF\n AI-4" (at 174.8536 118.618 270) (layer F.SilkS))
  (gr_text "I ANODE\nAI-3" (at 176.3776 108.712 270) (layer F.SilkS))
  (gr_text "FEEDER FWD\n AI-1" (at 175.9204 88.0364 270) (layer F.SilkS))
  (gr_text "FEEDER REF\n AI-0" (at 172.974 77.3684 270) (layer F.SilkS))
  (dimension 25.4 (width 0.3) (layer Dwgs.User)
    (gr_text "1.0000 in" (at 160.575 100.965 270) (layer Dwgs.User))
    (feature1 (pts (xy 168.91 113.665) (xy 159.225 113.665)))
    (feature2 (pts (xy 168.91 88.265) (xy 159.225 88.265)))
    (crossbar (pts (xy 161.925 88.265) (xy 161.925 113.665)))
    (arrow1a (pts (xy 161.925 113.665) (xy 161.338579 112.538496)))
    (arrow1b (pts (xy 161.925 113.665) (xy 162.511421 112.538496)))
    (arrow2a (pts (xy 161.925 88.265) (xy 161.338579 89.391504)))
    (arrow2b (pts (xy 161.925 88.265) (xy 162.511421 89.391504)))
  )
  (dimension 51.424846 (width 0.3) (layer Dwgs.User)
    (gr_text "2.0246 in" (at 168.58254 145.267866 359.9717002) (layer Dwgs.User))
    (feature1 (pts (xy 194.30492 125.11532) (xy 194.294293 146.630566)))
    (feature2 (pts (xy 142.88008 125.08992) (xy 142.869453 146.605166)))
    (crossbar (pts (xy 142.870787 143.905166) (xy 194.295627 143.930566)))
    (arrow1a (pts (xy 194.295627 143.930566) (xy 193.168834 144.51643)))
    (arrow1b (pts (xy 194.295627 143.930566) (xy 193.169413 143.343589)))
    (arrow2a (pts (xy 142.870787 143.905166) (xy 143.997001 144.492143)))
    (arrow2b (pts (xy 142.870787 143.905166) (xy 143.99758 143.319302)))
  )
  (dimension 63.494936 (width 0.3) (layer Dwgs.User)
    (gr_text "2.4998 in" (at 226.7897 93.375991 89.95874375) (layer Dwgs.User))
    (feature1 (pts (xy 194.31 125.10008) (xy 228.11684 125.124423)))
    (feature2 (pts (xy 194.35572 61.60516) (xy 228.16256 61.629503)))
    (crossbar (pts (xy 225.462561 61.627559) (xy 225.416841 125.122479)))
    (arrow1a (pts (xy 225.416841 125.122479) (xy 224.831232 123.995553)))
    (arrow1b (pts (xy 225.416841 125.122479) (xy 226.004073 123.996398)))
    (arrow2a (pts (xy 225.462561 61.627559) (xy 224.875329 62.75364)))
    (arrow2b (pts (xy 225.462561 61.627559) (xy 226.04817 62.754485)))
  )
  (gr_line (start 142.875 61.595) (end 194.31 61.595) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.875 125.095) (end 142.875 61.595) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.8 125.095) (end 142.875 125.095) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 194.31 125.095) (end 177.8 125.095) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 194.31 61.595) (end 194.31 125.095) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 10) (net_name "Net-(SV1-Pad19)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 194.31 125.0696) (xy 142.8496 125.0696) (xy 142.8496 61.6204) (xy 194.31 61.6204)
      )
    )
  )
  (zone (net 10) (net_name "Net-(SV1-Pad19)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 194.31 125.0696) (xy 142.8496 125.0696) (xy 142.8496 61.6204) (xy 194.31 61.6204)
      )
    )
  )
)
